ETSI ES 201 873-1 V4.6.4 (2015-01)

Methods for Testing and Specification (MTS);

The Testing and Test Control Notation version 3;

Part 1: TTCN‑3 Core Language

**ETSI Standard**

Reference

RES/MTS-201873-1 T3ed461

Keywords

language, methodology, testing, TTCN-3

***ETSI***

650 Route des Lucioles

F-06921 Sophia Antipolis Cedex - FRANCE

Tel.: +33 4 92 94 42 00 Fax: +33 4 93 65 47 16

Siret N° 348 623 562 00017 - NAF 742 C

Association à but non lucratif enregistrée à la

Sous-Préfecture de Grasse (06) N° 7803/88

***Important notice***

The present document can be downloaded from:  
<http://www.etsi.org>

The present document may be made available in electronic versions and/or in print. The content of any electronic and/or print versions of the present document shall not be modified without the prior written authorization of ETSI. In case of any existing or perceived difference in contents between such versions and/or in print, the only prevailing document is the print of the Portable Document Format (PDF) version kept on a specific network drive within ETSI Secretariat.

Users of the present document should be aware that the document may be subject to revision or change of status. Information on the current status of this and other ETSI documents is available at <http://portal.etsi.org/tb/status/status.asp>

If you find errors in the present document, please send your comment to one of the following services:  
<http://portal.etsi.org/chaircor/ETSI_support.asp>

***Copyright Notification***

No part may be reproduced or utilized in any form or by any means, electronic or mechanical, including photocopying and microfilm except as authorized by written permission of ETSI.  
The content of the PDF version shall not be modified without the written authorization of ETSI.  
The copyright and the foregoing restriction extend to reproduction in all media.

© European Telecommunications Standards Institute 2014.

All rights reserved.

**DECT**TM, **PLUGTESTS**TM, **UMTS**TM and the ETSI logo are Trade Marks of ETSI registered for the benefit of its Members.  
**3GPP**TM and **LTE**™ are Trade Marks of ETSI registered for the benefit of its Members and  
of the 3GPP Organizational Partners.  
**GSM**® and the GSM logo are Trade Marks registered and owned by the GSM Association.

Contents

Intellectual Property Rights 11

Foreword 11

Modal verbs terminology 11

1 Scope 12

2 References 12

2.1 Normative references 12

2.2 Informative references 13

3 Definitions and abbreviations 13

3.1 Definitions 13

3.2 Abbreviations 18

4 Introduction 19

4.1 The core language and presentation formats 19

4.2 Unanimity of the specification 20

4.3 Conformance 21

5 Basic language elements 21

5.1 Identifiers and keywords 22

5.2 Scope rules 22

5.2.1 Scope of formal parameters 24

5.2.2 Uniqueness of identifiers 24

5.3 Ordering of language elements 25

5.4 Parameterization 25

5.4.1 Formal parameters 26

5.4.1.1 Formal parameters of kind value 26

5.4.1.2 Formal parameters of kind template 29

5.4.1.3 Formal parameters of kind timer 30

5.4.1.4 Formal parameters of kind port 31

5.4.2 Actual parameters 31

5.5 Cyclic Definitions 35

6 Types and values 35

6.1 Basic types and values 36

6.1.0 Simple basic types and values 36

6.1.1 Basic string types and values 37

6.1.1.1 Accessing individual string elements 38

6.1.2 Subtyping of basic types 39

6.1.2.1 Lists of templates 39

6.1.2.2 Lists of types 39

6.1.2.3 Ranges 39

6.1.2.4 String length restrictions 40

6.1.2.5 Pattern subtyping of character string types 41

6.1.2.6 Mixing subtyping mechanisms 41

6.1.2.6.1 Mixing patterns, lists and ranges 41

6.1.2.6.2 Using length restriction with other constraints 41

6.2 Structured types and values 42

6.2.1 Record type and values 43

6.2.1.1 Referencing fields of a record type 45

6.2.1.2 Optional elements in a record 46

6.2.1.3 Nested type definitions for field types 46

6.2.2 Set type and values 47

6.2.2.1 Referencing fields of a set type 47

6.2.2.2 Optional elements in a set 47

6.2.2.3 Nested type definition for field types 47

6.2.3 Records and sets of single types 47

6.2.3.1 Nested type definitions 50

6.2.3.2 Referencing elements of record of and set of types 50

6.2.4 Enumerated type and values 51

6.2.5 Unions 52

6.2.5.1 Referencing fields of a union type 52

6.2.5.2 Option and union 52

6.2.5.3 Nested type definition for field types 52

6.2.6 The anytype 53

6.2.7 Arrays 53

6.2.8 The default type 55

6.2.9 Communication port types 55

6.2.10 Component types 57

6.2.10.1 Component type definition 57

6.2.10.2 Reuse of component types 58

6.2.11 Component references 60

6.2.12 Addressing entities inside the SUT 62

6.2.13 Subtyping of structured types 64

6.2.13.1 Length subtyping of record ofs and set ofs 64

6.2.13.2 List subtyping of structured types and anytype 65

6.2.13.3 Subtyping of the iterated type of record ofs and set ofs 67

6.2.13.4 Mixing subtyping mechanisms 68

6.3 Type compatibility 69

6.3.1 Compatibility of non-structured types 69

6.3.2 Compatibility of structured types 70

6.3.2.1 Compatibility of enumerated types 70

6.3.2.2 Compatibility of record and record of types 71

6.3.2.3 Compatibility of set and set of types 72

6.3.2.4 Compatibility of union types 72

6.3.2.5 Compatibility of anytype types 73

6.3.2.6 Compatibility between sub-structures 73

6.3.3 Compatibility of component types 74

6.3.4 Type compatibility of communication operations 74

6.3.5 Type conversion 75

6.4 Type synonym 75

7 Expressions 75

7.1 Operators 76

7.1.1 Arithmetic operators 77

7.1.2 List operator 78

7.1.3 Relational operators 78

7.1.4 Logical operators 80

7.1.5 Bitwise operators 81

7.1.6 Shift operators 82

7.1.7 Rotate operators 82

7.2 Field references and list elements 83

8 Modules 83

8.1 Definition of a module 83

8.2 Module definitions part 84

8.2.1 Module parameters 85

8.2.2 Groups of definitions 86

8.2.3 Importing from modules 87

8.2.3.1 General format of import 88

8.2.3.2 Importing single definitions 94

8.2.3.3 Importing groups 94

8.2.3.4 Importing definitions of the same kind 95

8.2.3.5 Importing all definitions of a module 96

8.2.3.6 Import definitions from other TTCN‑3 editions and from non-TTCN‑3 modules 97

8.2.3.7 Importing of import statements from TTCN-3 modules 99

8.2.3.8 Compatibility of language specifications in imports 100

8.2.4 Definition of friend modules 100

8.2.5 Visibility of definitions 101

8.3 Module control part 102

9 Port types, component types and test configurations 103

9.1 Communication ports 103

9.2 Test system interface 105

10 Declaring constants 107

11 Declaring variables 107

11.1 Value variables 108

11.2 Template variables 109

12 Declaring timers 110

13 Declaring messages 111

14 Declaring procedure signatures 111

15 Declaring templates 113

15.1 Declaring message templates 114

15.2 Declaring signature templates 115

15.3 Global and local templates 117

15.4 In-line Templates 117

15.5 Modified templates 118

15.6 Referencing elements of templates or template fields 121

15.6.1 Referencing individual string elements 121

15.6.2 Referencing **record** and **set** fields 121

15.6.3 Referencing **record** **of** and **set** **of** elements 122

15.6.4 Referencing signature parameters 125

15.7 Template matching mechanisms 126

15.7.1 Specific values 127

15.7.2 Special symbols that can be used instead of values 128

15.7.3 Special symbols that can be used inside values 129

15.7.4 Special symbols which describe attributes of values 129

15.8 Template Restrictions 130

15.9 Match Operation 132

15.10 Valueof Operation 132

15.11 Concatenating templates of string and list types 133

16 Functions, altsteps and testcases 134

16.1 Functions 134

16.1.1 Invoking functions 137

16.1.2 Predefined functions 138

16.1.3 External functions 140

16.1.4 Invoking functions from specific places 140

16.2 Altsteps 141

16.2.1 Invoking altsteps 143

16.3 Test cases 144

17 Void 145

18 Overview of program statements and operations 145

19 Basic program statements 147

19.1 Assignments 148

19.2 The If-else statement 149

19.3 The Select case statement 149

19.4 The For statement 150

19.5 The While statement 151

19.6 The Do-while statement 151

19.7 The Label statement 152

19.8 The Goto statement 153

19.9 The Stop execution statement 154

19.10 The Return statement 154

19.11 The Log statement 155

19.12 The Break statement 157

19.13 The Continue statement 157

19.14 Statement block 158

20 Statement and operations for alternative behaviours 158

20.1 The snapshot mechanism 159

20.2 The Alt statement 159

20.3 The Repeat statement 163

20.4 The Interleave statement 164

20.5 Default Handling 166

20.5.1 The default mechanism 166

20.5.2 The Activate operation 167

20.5.3 The Deactivate operation 168

21 Configuration Operations 169

21.1 Connection Operations 170

21.1.1 The Connect and Map operations 170

21.1.2 The Disconnect and Unmap operations 172

21.2 Test case operations 173

21.2.1 Test case stop operation 173

21.3 Test Component Operations 174

21.3.1 The Create operation 174

21.3.2 The Start test component operation 175

21.3.3 The Stop test behaviour operation 176

21.3.4 The Kill test component operation 177

21.3.5 The Alive operation 178

21.3.6 The Running operation 179

21.3.7 The Done operation 180

21.3.8 The Killed operation 182

21.3.9 Summary of the use of any and all with components 183

22 Communication operations 183

22.1 The communication mechanisms 184

22.1.1 Principles of message-based communication 184

22.1.2 Principles of procedure-based communication 184

22.1.3 Principles of unicast, multicast and broadcast communication 185

22.1.4 General format of communication operations 185

22.1.4.1 General format of the sending operations 186

22.1.4.2 General format of the receiving operations 186

22.2 Message-based communication 187

22.2.1 The Send operation 188

22.2.2 The Receive operation 189

22.2.3 The Trigger operation 192

22.3 Procedure-based communication 194

22.3.1 The Call operation 194

22.3.2 The Getcall operation 198

22.3.3 The Reply operation 200

22.3.4 The Getreply operation 201

22.3.5 The Raise operation 203

22.3.6 The Catch operation 204

22.4 The Check operation 207

22.5 Controlling communication ports 209

22.5.1 The Clear port operation 209

22.5.2 The Start port operation 210

22.5.3 The Stop port operation 210

22.5.4 The Halt port operation 210

22.5.5 The Checkstate port operation 211

22.6 Use of any and all with ports 213

23 Timer operations 213

23.1 The timer mechanism 213

23.2 The Start timer operation 214

23.3 The Stop timer operation 214

23.4 The Read timer operation 215

23.5 The Running timer operation 215

23.6 The Timeout operation 216

23.7 Summary of use of any and all with timers 217

24 Test verdict operations 218

24.1 The Verdict mechanism 218

24.2 The Setverdict operation 219

24.3 The Getverdict operation 220

25 External actions 220

26 Module control 221

26.1 The Execute statement 221

26.2 The Control part 223

27 Specifying attributes 225

27.1 The Attribute mechanism 225

27.1.1 Scope of attributes 225

27.1.2 Overwriting rules for attributes 226

27.1.2.1 Additional overwriting rules for variant attributes 228

27.1.3 Changing attributes of imported language elements 228

27.2 The With statement 229

27.3 Display attributes 229

27.4 Encoding attributes 230

27.5 Variant attributes 231

27.6 Extension attributes 233

27.7 Optional attributes 233

Annex A (normative): BNF and static semantics 235

A.1 TTCN‑3 BNF 235

A.1.1 Conventions for the syntax description 235

A.1.2 Statement terminator symbols 235

A.1.3 Identifiers 235

A.1.4 Comments 235

A.1.5 TTCN‑3 terminals 236

A.1.5.1 Use of whitespaces and newlines 238

A.1.6 TTCN-3 syntax BNF productions 238

A.1.6.0 TTCN-3 module 238

A.1.6.1 Module definitions part 239

A.1.6.1.0 General 239

A.1.6.1.1 Typedef definitions 239

A.1.6.1.2 Constant definitions 241

A.1.6.1.3 Template definitions 241

A.1.6.1.4 Function definitions 243

A.1.6.1.5 Signature definitions 244

A.1.6.1.6 Testcase definitions 244

A.1.6.1.7 Altstep definitions 244

A.1.6.1.8 Import definitions 244

A.1.6.1.9 Group definitions 245

A.1.6.1.10 External function definitions 245

A.1.6.1.11 External constant definitions 245

A.1.6.1.12 Module parameter definitions 245

A.1.6.1.13 Friend module definitions 245

A.1.6.2 Control part 246

A.1.6.3 Local definitions 246

A.1.6.3.1 Variable instantiation 246

A.1.6.3.2 Timer instantiation 246

A.1.6.4 Operations 246

A.1.6.4.1 Component operations 246

A.1.6.4.2 Port operations 247

A.1.6.4.3 Timer operations 249

A.1.6.4.4 Testcase operation 249

A.1.6.5 Type 249

A.1.6.6 Value 250

A.1.6.7 Parameterization 250

A.1.6.8 Statements 251

A.1.6.8.1 With statement 251

A.1.6.8.2 Behaviour statements 251

A.1.6.8.3 Basic statements 252

A.1.6.9 Miscellaneous productions 255

Annex B (normative): Matching values 256

B.1 Template matching mechanisms 256

B.1.1 Matching specific values 256

B.1.2 Matching mechanisms instead of values 256

B.1.2.1 Template list 256

B.1.2.2 Complemented template list 257

B.1.2.3 Any value 258

B.1.2.4 Any value or none 258

B.1.2.5 Value range 259

B.1.2.6 SuperSet 260

B.1.2.7 SubSet 261

B.1.2.8 Omitting optional fields 262

B.1.3 Matching mechanisms inside values 263

B.1.3.1 Any element 263

B.1.3.1.1 Using single character wildcards 263

B.1.3.2 Any number of elements or no element 263

B.1.3.2.1 Using multiple character wildcards 264

B.1.3.3 Permutation 264

B.1.4 Matching attributes of values 265

B.1.4.1 Length restrictions 265

B.1.4.2 The IfPresent indicator 266

B.1.5 Matching character pattern 267

B.1.5.1 Set expression 269

B.1.5.2 Reference expression 269

B.1.5.3 Match expression n times 271

B.1.5.4 Match a referenced character set 271

B.1.5.5 Type compatibility rules for patterns 272

Annex C (normative): Predefined TTCN‑3 functions 273

C.0 General exception handling procedures 273

C.1 Conversion functions 273

C.1.1 Integer to character 273

C.1.2 Integer to universal character 273

C.1.3 Integer to bitstring 273

C.1.4 Integer to enumerated 274

C.1.5 Integer to hexstring 274

C.1.6 Integer to octetstring 274

C.1.7 Integer to charstring 275

C.1.8 Integer to float 275

C.1.9 Float to integer 275

C.1.10 Character to integer 275

C.1.11 Character to octetstring 275

C.1.12 Universal character to integer 276

C.1.13 Bitstring to integer 276

C.1.14 Bitstring to hexstring 276

C.1.15 Bitstring to octetstring 276

C.1.16 Bitstring to charstring 277

C.1.17 Hexstring to integer 277

C.1.18 Hexstring to bitstring 277

C.1.19 Hexstring to octetstring 278

C.1.20 Hexstring to charstring 278

C.1.21 Octetstring to integer 278

C.1.22 Octetstring to bitstring 278

C.1.23 Octetstring to hexstring 279

C.1.24 Octetstring to character string 279

C.1.25 Octetstring to character string, version II 279

C.1.26 Charstring to integer 280

C.1.27 Character string to hexstring 280

C.1.28 Character string to octetstring 280

C.1.29 Character string to float 281

C.1.30 Enumerated to integer 281

C.1.31 Octetstring to universal character string 282

C.1.32 Universal character string to octetstring 282

C.2 Length/size functions 283

C.2.1 Length of strings and lists 283

C.2.2 Number of elements in a structured value 284

C.3 Presence checking functions 285

C.3.1 The IsPresent function 285

C.3.2 The IsChosen function 286

C.3.3 The IsValue function 287

C.3.4 The IsBound function 288

C.4 String/list handling functions 289

C.4.1 The Regexp function 289

C.4.2 The Substring function 291

C.4.3 The Replace function 292

C.5 Codec functions 293

C.5.1 The encoding function 293

C.5.2 The decoding function 293

C.5.3 The encoding to universal charstring function 293

C.5.4 The decoding from universal charstring function 294

C.6 Other functions 295

C.6.1 The random number generator function 295

C.6.2 The testcasename function 295

C.6.3 The hostId function 296

Annex D (normative): Preprocessing macros 297

D.1 Preprocessing macro \_\_MODULE\_\_ 297

D.2 Preprocessing macro \_\_FILE\_\_ 297

D.3 Preprocessing macro \_\_BFILE\_\_ 297

D.4 Preprocessing macro \_\_LINE\_\_ 297

D.5 Preprocessing macro \_\_SCOPE\_\_ 298

Annex E (informative): Library of Useful Types 300

E.1 Limitations 300

E.2 Useful TTCN‑3 types 300

E.2.1 Useful simple basic types 300

E.2.1.0 Signed and unsigned single byte integers 300

E.2.1.1 Signed and unsigned short integers 300

E.2.1.2 Signed and unsigned long integers 301

E.2.1.3 Signed and unsigned longlong integers 301

E.2.1.4 IEEE 754 floats 301

E.2.2 Useful character string types 302

E.2.2.0 UTF-8 character string "utf8string" 302

E.2.2.1 BMP character string "bmpstring" 302

E.2.2.2 UTF-16 character string "utf16string" 302

E.2.2.3 ISO/IEC 10646 character string "iso8859string" 302

E.2.2.4 Status values for TTCN-3 objects 303

E.2.3 Useful structured types 303

E.2.3.0 Fixed-point decimal literal 303

E.2.4 Useful atomic string types 303

E.2.4.1 Single Recommendation ITU‑T T.50 character type 303

E.2.4.2 Single universal character type 304

E.2.4.3 Single bit type 304

E.2.4.4 Single hex type 304

E.2.4.5 Single octet type 304

Annex F (informative): Operations on TTCN‑3 active objects 305

F.1 Test components 305

F.1.1 Test component references 305

F.1.2 Dynamic behaviour of PTCs 306

F.1.3 Dynamic behaviour of the MTC 308

F.2 Timers 309

F.3 Ports 309

F.3.1 Configuration Operations 309

F.3.2 Port Controlling Operations 310

F.3.3 Communication Operations 311

Annex G (informative): Deprecated language features 312

G.1 Group style definition of module parameters 312

G.2 Recursive import 312

G.3 Using **all** in port type definitions 312

G.4 sizeof for length of lists 312

G.5 sizeoftype predefined function 312

G.6 Mixed ports 312

G.7 External constants 313

G.8 Prefixing enumerated values 313

G.9 Record of/arrays not compatible to record; set of not compatible with set 313

Annex H (informative): Bibliography 314

History 315

# Intellectual Property Rights

IPRs essential or potentially essential to the present document may have been declared to ETSI. The information pertaining to these essential IPRs, if any, is publicly available for **ETSI members and non-members**, and can be found in ETSI SR 000 314: *"Intellectual Property Rights (IPRs); Essential, or potentially Essential, IPRs notified to ETSI in respect of ETSI standards"*, which is available from the ETSI Secretariat. Latest updates are available on the ETSI Web server ([http://ipr.etsi.org](http://webapp.etsi.org/IPR/home.asp)).

Pursuant to the ETSI IPR Policy, no investigation, including IPR searches, has been carried out by ETSI. No guarantee can be given as to the existence of other IPRs not referenced in ETSI SR 000 314 (or the updates on the ETSI Web server) which are, or may be, or may become, essential to the present document.

# Foreword

This ETSI Standard (ES) has been produced by ETSI Technical Committee Methods for Testing and Specification (MTS).

The present document is part 1 of a multi-part deliverable covering the Testing and Test Control Notation version 3, as identified below:

**Part 1: "TTCN‑3 Core Language";**

Part 2: "TTCN‑3 Tabular presentation Format (TFT)";

Part 3: "TTCN‑3 Graphical presentation Format (GFT)";

Part 4: "TTCN‑3 Operational Semantics";

Part 5: "TTCN‑3 Runtime Interface (TRI)";

Part 6: "TTCN‑3 Control Interface (TCI)";

Part 7: "Using ASN.1 with TTCN‑3";

Part 8: "The IDL to TTCN-3 Mapping";

Part 9: "Using XML schema with TTCN-3";

Part 10: "TTCN-3 Documentation Comment Specification".

# Modal verbs terminology

In the present document "**shall**", "**shall not**", "**should**", "**should not**", "**may**", "**may not**", "**need**", "**need not**", "**will**", "**will not**", "**can**" and "**cannot**" are to be interpreted as described in clause 3.2 of the [ETSI Drafting Rules](http://portal.etsi.org/Help/editHelp!/Howtostart/ETSIDraftingRules.aspx) (Verbal forms for the expression of provisions).

"**must**" and "**must not**" are **NOT** allowed in ETSI deliverables except when used in direct citation.

# 1 Scope

The present document defines the Core Language of TTCN‑3. TTCN‑3 can be used for the specification of all types of reactive system tests over a variety of communication ports. Typical areas of application are protocol testing (including mobile and Internet protocols), service testing (including supplementary services), module testing, testing of CORBA based platforms, APIs, etc. TTCN‑3 is not restricted to conformance testing and can be used for many other kinds of testing including interoperability, robustness, regression, system and integration testing. The specification of test suites for physical layer protocols is outside the scope of the present document.

TTCN‑3 is intended to be used for the specification of test suites which are independent of test methods, layers and protocols. In addition to the textual format defined in this document, (ES 201 873-3 [i.2]) defines a graphical presentation format for TTCN‑3. The specification of these formats is outside the scope of the present document.

While the design of TTCN‑3 has taken the eventual implementation of TTCN‑3 translators and compilers into consideration the means of realization of Executable Test Suites (ETS) from Abstract Test Suites (ATS) is outside the scope of the present document.

# 2 References

References are either specific (identified by date of publication and/or edition number or version number) or non‑specific. For specific references, only the cited version applies. For non-specific references, the latest version of the reference document (including any amendments) applies.

Referenced documents which are not found to be publicly available in the expected location might be found at <http://docbox.etsi.org/Reference>.

NOTE: While any hyperlinks included in this clause were valid at the time of publication ETSI cannot guarantee their long term validity.

## 2.1 Normative references

The following referenced documents are necessary for the application of the present document.

[1] ETSI ES 201 873-4: "Methods for Testing and Specification (MTS); The Testing and Test Control Notation version 3; Part 4: TTCN-3 Operational Semantics".

[2] ISO/IEC 10646 (2012): "Information technology -- Universal Coded Character Set (UCS)".

[3] Recommendation ITU-T X.292: "OSI conformance testing methodology and framework for protocol Recommendations for ITU-T applications - The Tree and Tabular Combined Notation (TTCN)".

NOTE: The corresponding ISO/IEC standard is ISO/IEC 9646-3: "Information technology -- Open Systems Interconnection -- Conformance testing methodology and framework -- Part 3: The Tree and Tabular Combined Notation (TTCN)".

[4] Recommendation ITU-T T.50: "International Reference Alphabet (IRA) (Formerly International Alphabet No. 5 or IA5) - Information technology - 7-bit coded character set for information interchange".

NOTE: The corresponding ISO/IEC standard is ISO/IEC 646: "Information technology -- ISO 7-bit coded character set for information interchange".

[5] Recommendation ITU-T X.290: "OSI conformance testing methodology and framework for protocol Recommendations for ITU-T applications - General concepts".

NOTE: The corresponding ISO/IEC standard is ISO/IEC 9646-1: "Information technology -- Open Systems Interconnection -- Conformance testing methodology and framework; Part 1: General concepts".

[6] IEEE™ 754: "IEEE Standard for Floating-Point Arithmetic".

## 2.2 Informative references

The following referenced documents are not necessary for the application of the present document but they assist the user with regard to a particular subject area.

[i.1] Void.

[i.2] ETSI ES 201 873-3: "Methods for Testing and Specification (MTS); The Testing and Test Control Notation version 3; Part 3: TTCN-3 Graphical presentation Format (GFT)".

[i.3] ETSI ES 201 873-5: "Methods for Testing and Specification (MTS); The Testing and Test Control Notation version 3; Part 5: TTCN-3 Runtime Interface (TRI)".

[i.4] ETSI ES 201 873-6: "Methods for Testing and Specification (MTS); The Testing and Test Control Notation version 3; Part 6: TTCN-3 Control Interface (TCI)".

[i.5] ETSI ES 201 873-7: "Methods for Testing and Specification (MTS); The Testing and Test Control Notation version 3; Part 7: Using ASN.1 with TTCN-3".

[i.6] ETSI ES 201 873-8: "Methods for Testing and Specification (MTS); The Testing and Test Control Notation version 3; Part 8: The IDL to TTCN-3 Mapping".

[i.7] ETSI ES 201 873-9: "Methods for Testing and Specification (MTS); The Testing and Test Control Notation version 3; Part 9: Using XML schema with TTCN-3".

[i.8] ETSI ES 201 873-10: "Methods for Testing and Specification (MTS); The Testing and Test Control Notation version 3; Part 10: TTCN-3 Documentation Comment Specification".

[i.9] Void.

[i.10] Object Management Group (OMG) (2001): "The Common Object Request Broker: Architecture and Specification - IDL Syntax and Semantics". Version 2.6, FORMAL/01-12-01.

[i.11] ETSI ES 202 781: "Methods for Testing and Specification (MTS); The Testing and Test Control Notation version 3; TTCN-3 Language Extensions: Configuration and Deployment Support".

[i.12] ETSI ES 202 784: "Methods for Testing and Specification (MTS); The Testing and Test Control Notation version 3; TTCN-3 Language Extensions: Advanced Parameterization".

[i.13] ETSI ES 202 785: "Methods for Testing and Specification (MTS); The Testing and Test Control Notation version 3; TTCN-3 Language Extensions: Behaviour Types".

[i.14] ETSI ES 202 782: "Methods for Testing and Specification (MTS); The Testing and Test Control Notation version 3; TTCN-3 Language Extensions: TTCN-3 Performance and Real Time Testing".

[i.15] ISO/IEC 10646 (2003): "Information technology -- Universal Coded Character Set (UCS)".

# 3 Definitions and abbreviations

## 3.1 Definitions

For the purposes of the present document, the terms and definitions given in Recommendation ITU‑T X.290 [5], Recommendation ITU‑T X.292 [3] and the following apply:

**actual parameter:** value, expression, template or name reference (identifier) to be passed as parameter to the invoked entity (function, test case, altstep, etc.) as defined at the place of invoking

**assignment notation:** notation that can be used for record, set, record of and set of values, where the fields or the elemens to which a value is assigned are identified explicitly within a pair of curly brackets ("{" and "}") by the field names or the positions of the elements

**basic types:** set of predefined TTCN‑3 types described in clauses 6.1.0 and 6.1.1 of the present document

NOTE: Basic types are referenced by their names.

**communication port:** abstract mechanism facilitating communication between test components

NOTE: A communication port is modelled as a FIFO queue in the receiving direction. Ports can be message‑based or procedure-based.

**compatible type:** TTCN‑3 is not strongly typed but the language does require type compatibility

NOTE: Variables, constants, templates, etc. have compatible types if conditions in clause 6.3 are met.

**completely initialized:** values and templates of simple types are completely initialized if they are partially initialized

NOTE: Values and templates of structured types and arrays are completely initialized if all their fields and elements are completely initialized. In case of record of, set of, and array values and templates, this means at least the first n elements are initialized, where n is the minimal length imposed by the type length restriction or array definition (thus in case of n equals 0, the value "{}" also completely initializes a record of, a set of or an array).

**component constant:** constant defined in a component type

**component port:** port defined in a component type

**component template:** template defined in a component type

**component timer:** timer defined in a component type

**component variable:** variable defined in a component type

**data types:** common name for simple basic types, basic string types, structured types, the special data type anytype and all user defined types based on them

NOTE: See table 3 of the present document.

**defined types (defined TTCN‑3 types):** set of all predefined TTCN‑3 types (basic types, all structured types, the type anytype, the address, port and component types and the default type) and all user-defined types declared either in the module or imported from other TTCN‑3 modules

**deterministic function:** function that for the same input in the in and inout parameters always yields the same output both for the return result as well as the inout and out parameters

NOTE 1: A non-deterministic function is one that is not deterministic.

NOTE 2: In general, it cannot be decided if a function is deterministic or not. However, a function can be specified to be deterministic, i.e. the function is supposed to be deterministic. In this case, a violation of the determinism can be detected and handled accordingly. The handling however is tool-specific.

**dynamic parameterization:** form of parameterization, in which actual parameters are dependent on runtime events

EXAMPLE: The value of the actual parameter is a value received during runtime or depends on a received value by a logical relation.

**exception:** in cases of procedure-based communication, an exception (if defined) is raised by an answering entity if it cannot answer a remote procedure call with the normal expected response

**formal parameter:** typed name or typed template reference (identifier) not resolved at the time of the definition of an entity (function, test case, altstep, etc.) but at the time of invoking it

NOTE: Actual values or templates (or their names) to be used at the place of formal parameters are passed from the place of invoking the entity (see also the definition of actual parameter).

**fuzzy value or template:** If a value or template instance is declared to be fuzzy, the expression, initializing or partly initializing it (including actual parameters passed to in formal parameters), is subject to lazy evaluation. During execution, this expression is re-evaluated each time when the fuzzy object is referenced, except when at the left hand side of an assignment or passing it to a fuzzy or lazy formal parameters. The result of this (re)evaluation is used as the actual value or template of the fuzzy instance. When new content is assigned to a fuzzy instance or to its subpart, the right hand side of the assignment is subject to lazy evaluation again.

**global visibility:** Attribute of an entity (module parameter, constant, template, etc.) that its identifier can be referenced anywhere within the module where it is defined including all functions, test cases and altsteps defined within the same module and the control part of that module.

**implementation conformance statement (ICS):** See Recommendation ITU‑T X.290 [5].

**implementation extra information for testing (IXIT):** See Recommendation ITU‑T X.290 [5].

**implementation under test (IUT):** See Recommendation ITU‑T X.290 [5].

**in parameterization:** kind of parameterization where the value of the actual parameter (the argument) is assigned to the formal parameter when the parameterized object is invoked, but the value of the formal parameter is not passed back to the actual parameter when the invoked object completes. In **in** parameterization, parameters are passed by value

NOTE 1: The arguments are evaluated before the parameterized object is entered.

NOTE 2: Only the values of the arguments are passed and changes to the arguments within the invoked object have no effect on the arguments as seen by the invoking object.

**index notation:** notation to access individual elements of record of, set of, array and string values or templates. The element to be accessed is identified explicitly by an index value enclosed in square brackets ("[" and "]") which specifies the position of that element within the referenced value or template. The index value is either an integer value, array of integers or record of integers. Integer values used for indexing (either directly or as elements of the record of or array values) always lie within the index range of the type of the referenced value or template. Except for those arrays which are defined with an explicit index range, the index range always has 0 as the index for the first element

**inout parameterization:** kind of parameterization that uses passing by reference When the parameterized object is invoked, the formal parameter is linked with the actual parameter and gets direct access to the same data content that is currently represented by the actual parameter

NOTE 1: The invoked object uses the actual parameter directly, so that all changes made in the formal parameter become immediately effective on the actual parameter. If the same actual parameter is passed to two distinct formal parameters, a change in one formal parameter becomes immediately effective in the other one (and in the actual parameter).

NOTE 2: Inout parameters can be used for functions, altsteps, and test cases only, if not restricted by further rules, e.g. altsteps activated as defaults.

**known types:** set of all TTCN‑3 predefined types, types defined in a TTCN‑3 module and types imported into that module from other TTCN‑3 modules or from non-TTCN‑3 modules

**lazy evaluation:** Lazy evaluation means that evaluation of an expression is delayed during execution until the value or template instance, to which the result of the evaluation should have been assigned or passed to as actual parameter, is first referenced at an other place than the left hand side of an assignment or an actual parameter passed to a fuzzy or lazy formal parameter. During execution, this delayed evaluation is carried out at the first actual reference, even when the result is to be used in an expression that is also subject to lazy evaluation. For the evaluation the actual values at the time of the evaluation to be used (not the actual values at the time of the assignment or parameter passing). This implies that components of the expression may be uninitialized at the time, when execution reaches the assignment or parameter passing, but may be initialized by the time of the evaluation that can lead to successful evaluation. If, by the time of the evaluation, execution has left the scope unit, in which one or more components of the expression is defined, the actual values of the component(s) at the time of leaving the scope unit are to be stored for the purpose of the delayed evaluation (but only for that, i.e. the values are not accessible for the user).

**lazy value or template:** A value or template instance is called lazy, when the expression, initializing or partly initializing it (including actual parameters passed to in formal parameters), is subject to lazy evaluation. When, during execution, the delayed (lazy) evaluation is taking place, its result is stored in the lazy value or template and the lazy instance is used further on like ordinary values and templates, until the next use of the lazy variable or parameter on the left hand side of an assignment. When a new content is assigned to a lazy instance or to its subpart, the right hand side of the assignment is subject to lazy evaluation again. If, during execution, no expression referencing the lazy object is evaluated, the lazy value or template instance is never evaluated.

**left hand side (of assignment):** value or template variable identifier or a field name of a structured type value or template variable (including array index if any), which stands left to an assignment symbol (:=)

NOTE: A constant, module parameter, timer, structured type field name or a template header (including template type, name and formal parameter list) standing left of an assignment symbol (:=) in declarations and or a modified template definitions are out of the scope of this definition as not being part of an assignment.

**local visibility:** attribute of an entity (constant, variable, etc.) that its identifier can be referenced only within the function, test case or altstep where it is defined

**main test component (MTC):** See Recommendation ITU‑T X.292 [3].

**out parameterization:** kind of parameterization where the actual parameter’s content (the argument) is not passed to the formal parameter when the parameterized object is invoked, but the value of the formal parameter is passed back to the actual parameter when the invoked object completes. In **out** parameterization, parameters are passed by value

NOTE 1: Out parameters can be used for functions, altsteps, and test cases only, if not restricted by further rules, e.g. **altstep**s activated as defaults.

NOTE 2: An **out** formal parameter is uninitialized (unbound) when the invoked object is entered.

NOTE 3: The value is passed back to the actual parameter only if within the invoked object a value is assigned to it. If no value is assigned, the actual parameter remains unchanged when the invoked object completes.

**parallel test component (PTC):** See Recommendation ITU‑T X.292 [3].

**partially initialized:** values are partially initialized if a concrete value has been assigned to it or to at least one of its fields or elements

NOTE 1: A template variable is initialized if a matching mechanism has been assigned to it or to at least one of its fields or elements, directly or indirectly via expansion (see clause 15.6). A template is initialized if a matching mechanism has been assigned to it, directly or indirectly via expansion (see clause 15.6).

NOTE 2: TTCN-3 data objects (both value and template) are initialized if they or at least one of their fields or elements have been used on the left hand side of an assignment (including initial value assignment at declaration), except of uninitialized **record**s and **set**s, when the assignment does not change any of its fields. Note that for example an empty pair of curly brackets used for a record value may change the optional fields of the value via the implicit omit mechanism (see clause 27.7).

**passing by reference:** ability to link an actual parameter with a formal parameter of a function, altstep or test case and to control its actual value within the function, altstep or test case by using the formal parameter reference. When parameters are passed by reference, no copy of the data content is made and the actual and formal parameters share the same data content.

**passing by value**: ability to make a copy of a data content of an actual or formal parameter before passing it to a formal or actual parameter. When parameters are passed by value, the actual and formal parameters do not share the same data content.

**port parameterization:** ability to pass a port as an actual parameter into a parameterized object via a port parameter

NOTE: This actual port parameter is added to the specification of that object and may complete it.

**qualified name:** TTCN-3 elements can be identified unambiguously by qualified names

NOTE: For modules, the qualified name is the <module name>. For global definitions such as testcases, functions, etc., the qualified name is <module name>.<definition name>. For control, the qualified name is <module name>.control. For local definitions, such as variables, local templates, etc. within a global definition, the qualified name is <module name>.<global definition name>.<local definition name>.

**right hand side (of assignment):** expression, template reference or signature parameter identifier which stands right to an assignment symbol (:=)

NOTE: Expressions and template references standing right of an assignment symbol (:=) in constant, module parameter, timer, template or modified template declarations are out of the scope of this definition as not being part of an assignment.

**root type:** root types of types derived from TTCN-3 basic types are the respective basic types

NOTE 1: The root type of user defined record types is **record**, the root type of user defined record of and array types is **record of**, the root type of user defined set types is **set**, the root type of user defined set of types is **set of**. The root type of user defined union types is **union** and the root type of anytypes is **anytype**. The root types of special configuration types are **default** or **component,** respectively. Port types do not have a root type.

NOTE 2: As **address** is more a predefined type name than a distinct type with its own properties, the root type of an **address** type and all of its derivatives are the same, as the root type was, if the type was defined with a name different from **address**.

**static parameterization:** form of parameterization, in which actual parameters are independent of runtime events; i.e. known at compile time or in case of module parameters are known by the start of the test suite execution

NOTE 1: A static parameter is to be known from the test suite specification, (including imported definitions), or the test system is aware of its value before execution time.

NOTE 2: All types are known at compile time, i.e. are statically bound.

**strong typing:** strict enforcement of type compatibility by type name equivalence with no exceptions

**system under test (SUT):** See Recommendation ITU‑T X.290 [5].

**template:** TTCN-3 data objects are values or templates by definition. A TTCN‑3 template identifies a subset of the values of its type (where the subset may contain a single instance of the type, several instances or all instances) or the matching mechanism **omit**. Templates are defined by global and local templates, template variable definitions, or formal template parameters. Any of those are templates from the point of view of their usage, irrespective of their actual content; for example, a template variable containing a specific value is a template.

**template parameterization:** ability to pass a template as an actual parameter into a parameterized object via a template parameter

NOTE 1: This actual template parameter is added to the specification of that object and may complete it.

NOTE 2: Values passed to formal template parameters are considered to be in-line templates (see clause 15.4).

**test behaviour:** (or behaviour) test case or a function started on a test component when executing an **execute** or a **start** component statement and all functions and altsteps called recursively

NOTE: During a test case execution each test component has its own behaviour and hence several test behaviours may run concurrently in the test system (i.e. a test case can be seen as a collection of test behaviours).

**test case:** See Recommendation ITU‑T X.290 [5].

**test case error:** See Recommendation ITU‑T X.290 [5].

**test suite:** set of TTCN‑3 modules that contains a completely defined set of test cases, optionally supplemented with one or more TTCN‑3 control parts

**test system:** See Recommendation ITU‑T X.290 [5].

**test system interface:** test component that provides a mapping of the ports available in the (abstract) TTCN‑3 test system to those offered by the SUT

**timer parameterization:** ability to pass a timer as an actual parameter into a parameterized object via a timer parameter

NOTE: This actual timer parameter is added to the specification of that object and may complete it.

**type compatibility:** language feature that allows to use values, expressions or templates of a given type as actual values of another type

EXAMPLE: At assignments, as actual parameters at calling a function, referencing a template, etc. or as a return value of a function.

**type context:** "In the context of a type" means that at least one object involved in the given TTCN-3 action (an assignment, operation, parameter passing, etc.) identifies a concrete type unambiguously

NOTE: Either directly (e.g. an in-line template) or by means of a typed TTCN-3 object (e.g. via a constant, variable, formal parameter, etc.).

**unqualified name:** unqualified name of a TTCN-3 element is its name without any qualification

**user-defined type:** type that is defined by subtyping of a basic type or declaring a structured type

NOTE: User-defined types are referenced by their identifiers (names).

**value:** TTCN-3 data objects are values or templates by definition. A TTCN‑3 value is an instance of its type

NOTE: Values are defined by module parameters, constants, value variables, or formal value parameters. Any of those are value objects from the point of view of their usage. A template containing only specific value matching - though referring to a single instance of its type - is not a value object, but is a template object.

**value list notation:** notation that can be used for record, set, record of and set of values, where the values of the subsequent fields or elements are listed within a pair of curly brackets ("{" and "}"), without an explicit identification of the field name or element position

**value notation:** notation by which an identifier is associated with a given value or range of a particular type

NOTE: Values may be constants or variables.

**value parameterization:** ability to pass a value as an actual parameter into a parameterized object via a value parameter

NOTE: This actual value parameter is added to the specification of that object and may complete it.

## 3.2 Abbreviations

For the purposes of the present document, the following abbreviations apply:

API Application Programming Interface

ASN Abstract Syntax Notation

ASP Abstract Service Primitive

NOTE: See Recommendation ITU‑T X.290 [5].

ATS Abstract Test Suite

BER Basic Encoding Rules

BMP Basic Multilingual Plane

BNF Backus-Nauer Form

BOM Byte order mark

CORBA Common Object Request Broker Architecture

ETS Executable Test Suite

FIFO First In First Out

GFT Graphical presentation Format

ICS Implementation Conformance Statement

IDL Interface Definition Language

IRV International Reference Version

IUT Implementation Under Test

IXIT Implementation eXtra Information for Testing

LHS Left Hand Side (of assignment)

MTC Main Test Component

PDU Protocol Data Unit

NOTE: See Recommendation ITU‑T X.290 [5].

PTC Parallel Test Component

RHS Right Hand Side (of assignment)

SDL Specification and Description Language

SUT System Under Test

TCI TTCN-3 Control Interfaces

TFT Tabular presentation Format

TRI TTCN-3 Runtime Interfaces

TSI Test System Interface

TTCN-3 Testing and Test Control Notation version 3

UCS Universal Character Set

UID UCS Universal Character Set

USI UCS Short Identifier

UTF UCS Transformation Format

UTF-8 Unicode Transformation Format-8

UTF-16 Unicode Transformation Format-16

UTF-16BE Unicode Transformation Format-16 big-endian

UTF-16LE Unicode Transformation Format-16 little-endian

UTF-32 Unicode Transformation Format-32

UTF-32BE Unicode Transformation Format-32 big-endian

UTF-32LE Unicode Transformation Format-32 little-endian

XML eXtensible Markup Language

# 4 Introduction

TTCN‑3 is a flexible and powerful language applicable to the specification of all types of reactive system tests over a variety of communication interfaces. Typical areas of application are protocol testing (including mobile and Internet protocols), service testing (including supplementary services), module testing, testing of CORBA based platforms, API testing, etc. TTCN‑3 is not restricted to conformance testing and can be used for many other kinds of testing including interoperability, robustness, regression, system and integration testing.

TTCN‑3 includes the following essential characteristics:

* the ability to specify dynamic concurrent testing configurations;
* operations for procedure-based and message-based communication;
* the ability to specify encoding information and other attributes (including user extensibility);
* the ability to specify data and signature templates with powerful matching mechanisms;
* value parameterization;
* the assignment and handling of test verdicts;
* test suite parameterization and test case selection mechanisms;
* combined use of TTCN‑3 with other languages;
* well-defined syntax, interchange format and static semantics;
* different presentation formats (e.g. tabular and graphical presentation formats);
* a precise execution algorithm (operational semantics).

NOTE: The present document uses the following model of concept description: concepts, principles and mechanisms are explained in (introductory) text at the beginning of a clause. For every concept having concrete syntax, the syntactical structure of that concept is presented afterwards. The syntactical structure follows the conventions for the TTCN-3 syntax description in clause A.1.1 and uses rules of the TTCN-3 BNF given in clause A.1. A semantic description follows the syntactic structure. The restrictions on the concept are listed subsequently. Finally, examples on the usage of the concept are given.

In case of a contradiction between the body of the present document (clauses 5 to 27) and annex A of the present document, annex A has the priority.

## 4.1 The core language and presentation formats

The TTCN‑3 specification is separated into several parts (see figure 1).

The first part, defined in the present document, is the core language.

The second part, defined in ES 201 873-2 [i.1], is the tabular presentation format.

The third part, defined in ES 201 873-3 [i.2], is the graphical presentation format.

The fourth part, ES 201 873-4 [1], contains the operational semantics of the language.

The fifth part, ES 201 873-5 [i.3], defines the TTCN‑3 Runtime Interface (TRI).

The sixth part, ES 201 873-6 [i.4], defines the TTCN‑3 Control Interfaces (TCI).

The seventh part, ES 201 873-7 [i.5], specifies the use of ASN.1 definitions with TTCN‑3.

The eight part, ES 201 873-8 [i.6], specifies the use of IDL definitions with TTCN‑3.

The ninth part, ES 201 873-9 [i.7] specifies the use of XML definitions with TTCN‑3.

The tenth part, ES 201 873-10 [i.8] specifies documentation tags for TTCN‑3.

The core language serves three purposes:

a) as a generalized text-based test language in its own right;

b) as a standardized interchange format of TTCN‑3 test suites between TTCN‑3 tools;

c) as the semantic basis (and where relevant, the syntactical basis) for various presentation formats.

The core language may be used independently of the presentation formats. However, neither the tabular format nor the graphical format can be used without the core language. Use and implementation of these presentation formats will be done on the basis of the core language.

The tabular format and the graphical format are the first in an anticipated set of different presentation formats. These other formats may be standardized presentation formats or they may be proprietary presentation formats defined by TTCN‑3 users themselves. These additional formats are not defined in the present document.

TTCN-3 may optionally be used with TTCN-3 packages, which define additional concepts for specific purposes.

TTCN‑3 may optionally be used with other type-value notations in which case definitions in other languages may be used as alternative data type and value syntax. Other parts of the TTCN-3 standard specify use of some other languages with TTCN‑3. The support of other languages is not limited to those specified in the ES 201 873 series of documents but to support languages for which combined use with TTCN‑3 is defined, rules given in the present document apply.



Figure 1: User's view of the core language, its packages and the various presentation formats

The core language is defined by a complete syntax (see annex A) and operational semantics (ES 201 873-4 [1]). It contains minimal static semantics (provided in the body of the present document and in annex A) which do not restrict the use of the language due to some underlying application domain or methodology.

## 4.2 Unanimity of the specification

The language is specified syntactically and semantically in terms of a textual description in the body of the present document (clauses 5 to 27) and in a formalized way in annex A. In each case, when the textual description is not exhaustive, the formal description completes it. If the textual and the formal specifications are contradictory, the latter shall take precedence.

## 4.3 Conformance

For an implementation claiming to conform to this version of the language, all features specified in the present document shall be implemented consistently with the requirements given in the present document and in ES 201 873‑4 [1].

# 5 Basic language elements

The top-level unit of TTCN‑3 is a module. A module cannot be structured into sub-modules. A module can import definitions from other modules. Modules can have module parameters to allow test suite parameterization.

A module consists of a definitions part and a control part. The definitions part of a module defines test components, communication ports, data types, constants, test data templates, functions, signatures for procedure calls at ports, test cases, etc.

The control part of a module calls the test cases and controls their execution. The control part may also declare (local) variables, etc. Program statements (such as **if**-**else** and **do-while**) can be used to specify the selection and execution order of individual test cases. The concept of global variables is not supported in TTCN‑3.

TTCN‑3 has a number of predefined basic data types as well as structured types such as records, sets, unions, enumerated types and arrays.

A special kind of data structure called a template provides parameterization and matching mechanisms for specifying test data to be sent or received over the test ports. The operations on these ports provide both message-based and procedure-based communication capabilities. Procedure calls may be used for testing implementations which are not message based.

Dynamic test behaviour is expressed as test cases. TTCN‑3 program statements include powerful behaviour description mechanisms such as alternative reception of communication and timer events, interleaving and default behaviour. Test verdict assignment and logging mechanisms are also supported.

Finally, TTCN‑3 language elements may be assigned attributes such as encoding information and display attributes. It is also possible to specify (non-standardized) user-defined attributes.

The TTCN-3 language elements are summarized in table 1.

Table 1: Overview of TTCN‑3 language elements

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Language element | Associated keyword | Specified in module definitions | Specified in module control | Specified in functions/ altsteps/ test cases | Specified in test component type |
| TTCN‑3 module definition | **module** |  |  |  |  |
| Import of definitions from other module | **import** | Yes |  |  |  |
| Grouping of definitions | **group** | Yes |  |  |  |
| Data type definitions | **type** | Yes |  |  |  |
| Communication port definitions | **port** | Yes |  |  |  |
| Test component definitions | **component** | Yes |  |  |  |
| Signature definitions | **signature** | Yes |  |  |  |
| External function definitions | **external** | Yes |  |  |  |
| Constant definitions | **const** | Yes | Yes | Yes | Yes |
| Data/signature template definitions | **template** | Yes | Yes | Yes | Yes |
| Function definitions | **function** | Yes |  |  |  |
| Altstep definitions | **altstep** | Yes |  |  |  |
| Test case definitions | **testcase** | Yes |  |  |  |
| Value variable declarations | **var** |  | Yes | Yes | Yes |
| Template variable declarations | **var template** |  | Yes | Yes | Yes |
| Timer declarations | **timer** |  | Yes | Yes | Yes |
| NOTE: The notions "definition" and "declaration" of variables, constants, types and other language elements are used interchangeably throughout the present document. The distinction between both notions is useful only for implementation purposes, as it is the case in programming languages like C and C++. On the level of TTCN‑3, the notions have equal meaning. | | | | | |

## 5.1 Identifiers and keywords

TTCN‑3 identifiers are case sensitive. TTCN‑3 keywords shall be written in all lowercase letters (see annex A). TTCN‑3 keywords shall neither be used as identifiers of TTCN‑3 objects nor as identifiers of objects imported from modules of other languages. The same rules apply to names of predefined TTCN‑3 functions (see annex C).

Special TTCN-3 modifiers are identifiers prefixed with the @-symbol (see annex A). They modify the default semantics of the language element they are applied to in the specified way. If more than one modifier is applied to a language element, they may be applied in any order.

NOTE: These modifiers are useful for refining or modifying existing language features, for example in the context of the optional extension packages of TTCN-3 since they cannot lead to backward incompabilities with existing reserved keywords or identifiers.

## 5.2 Scope rules

TTCN‑3 provides nine basic units of scope:

a) module definitions part;

b) control part of a module;

c) component types;

d) functions;

e) altsteps;

f) test cases;

g) statement blocks;

h) templates;

i) user defined named types.

NOTE 1: Additional scoping rule for groups is given in clause 8.2.2.

NOTE 2: Additional scoping rule for counters of **for** loops is given in clause 19.4.

NOTE 3: Statement blocks may include declarations. They may occur as stand-alone statement blocks, embedded in another statement block or within compound statements, e.g. as body of a **while** loop.

NOTE 4: Built in TTCN-3 types like **integer**, **charstring**, **anytype**, etc. are not scope units, but all named user defined types are scope units, independent of their kinds.

Each unit of scope consists of (optional) declarations. The scope units: control part of a module, functions, test cases, altsteps and statement blocks may additionally specify some form of behaviour by using the TTCN‑3 program statements and operations (see clause 18).

Definitions made in the module definitions part but outside of other scope units are globally visible, i.e. may be used elsewhere in the module, including all functions, test cases and altsteps defined within the module and the control part. Identifiers imported from other modules are also globally visible throughout the importing module.

Definitions made in the module control part have local visibility, i.e. can be used within the control part only.

Definitions made in a test component type may be used in a component type extending this component type definition, and in functions, test cases and altsteps referencing that component type or a compatible test component type (see clause 6.3.3) by a **runs on** clause.

Test cases, altsteps and functions are individual scope units without any hierarchical relation between them, i.e. declarations made at the beginning of their body have local visibility and shall only be used in the given test case, altstep or function (e.g. a declaration made in a test case is not visible in a function called by the test case or in an altstep used by the test case).

Stand-alone statement blocks and statements within compound statements, like e.g. **if-else**, **while**, **do-while**, or **alt** statements may be used within the control part of a module, test cases, altsteps, functions, or may be embedded in other statement blocks or compound statements, e.g. an **if-else** statement that is used within a **while** loop.

Statement blocks and embedded statement blocks have a hierarchical relation both to the scope unit including the given statement block and to any embedded statement block. Declarations made within a statement block have local visibility.

The hierarchy of scope units is shown in figure 2. Declarations of a scope unit at a higher hierarchical level are visible in all units at lower levels within the same branch of the hierarchy. Declarations of a scope unit in a lower level of hierarchy are not visible to those units at a higher hierarchical level.



Figure 2: Hierarchy of scope units

EXAMPLE 1: Local scopes

**module** MyModule

{ :

**const** **integer** MyConst := 0; // MyConst is visible to MyBehaviourA and MyBehaviourB

:

**function** MyBehaviourA()

{ :

**const** **integer** A := 1; // The constant A is only visible to MyBehaviourA

:

}

**function** MyBehaviourB()

{ :

**const** **integer** B := 1; // The constant B is only visible to MyBehaviourB

:

}

}

EXAMPLE 2: Component type scopes

**type** **component** MyComponentType {

**const** **integer** MyConst := 1;

...

}

**type** **component** MyExtendedComponentType **extends** MyComponentType {

**var** **integer** MyVar:= 2 \* MyConst; // using MyConst of MyComponentType

...

}

### 5.2.1 Scope of formal parameters

The scope of formal parameters in a parameterized object (e.g. in a function definition) shall be restricted to the definition in which the parameters appear and to the lower levels of scope in the same scope hierarchy. That is they follow the scope rules for local definitions (see clause 5.2).

### 5.2.2 Uniqueness of identifiers

TTCN‑3 requires uniqueness of identifiers, i.e. all identifiers in the same scope hierarchy shall be distinctive. This means that a declaration in a lower level of scope shall not re-use the same identifier as a declaration in a higher level of scope in the same branch of the scope hierarchy.

The identifier of a module (its module name) or of an imported module belongs to the scope unit of the module and cannot be used as identifier for other definitions inside this module. Identifiers for fields of structured types, enumerated values and groups do not have to be globally unique, however in the case of enumerated values the identifiers shall only be reused for enumerated values within other enumerated types. The rules of identifier uniqueness shall also apply to identifiers of formal parameters.

EXAMPLE 1: Nested scopes

**module** MyModule

{ :

**const** **integer** A := 1;

:

**function** MyBehaviourA()

{ :

**const** **integer** A := 1; // Is NOT allowed: clash with global constant A

**:**

**if**(…)

{ :

**const** **boolean** A := **true;** // Is NOT allowed: clash with local constant A

:

}

}

}

EXAMPLE 2: Independent scopes

// The following IS allowed as the constants are not declared in the same scope hierarchy

// (assuming there is no declaration of A in module header)

**function** MyBehaviourA()

{ :

**const** **integer** A := 1;

**:**

}

**function** MyBehaviourB()

{ :

**const** **integer** A := 1;

**:**

}

EXAMPLE 3: Module scopes

**module** MyModuleB {

**import** **from** MyModuleA { **…** }

**function** MyFunction() {

**var** **integer** MyModuleB:= 1; // Is NOT allowed: class with module name

**:**

}

**type** **boolean** MyModuleA; // Is NOT allowed: class with imported module name

}

## 5.3 Ordering of language elements

Generally, the order in which declarations can be made is arbitrary. Inside a statement block, such as a function body or a branch of an **if-else** statement, all declarations (if any), shall be made at the beginning of the statement block only.

EXAMPLE:

// This is a legal mixing of TTCN‑3 declarations

:

**var** MyVarType MyVar2 := 3;

**const** **integer** MyConst:= 1;

**if** (MyVar2+MyConst > 10)

{

**var** **integer** MyVar1:= 1;

**:**

MyVar1:= MyVar1 + 10;

**:**

}

:

Declarations in the module definitions part and in a component type definition may be made in any order. However inside the module control part, test case definitions, functions, altsteps, and statement blocks, all required declarations shall be given beforehand. This means in particular, local variables, local timers, and local constants shall never be used before they are declared. The only exceptions to this rule are labels. Forward references to a label may be used in **goto** statements before the label occurs (see clause 19.8).

## 5.4 Parameterization

TTCN-3 allows to parameterize modules, templates, functions, altsteps and testcases. Values, templates, timers, and ports may be used as actual parameters. A summary of which language elements can be parameterized and what can be passed to them as parameters is given in table 2.

NOTE: Type parameterization for TTCN-3 is defined in the optional package [i.12].

Table 2: Overview of parameterizable TTCN‑3 objects

|  |  |  |  |
| --- | --- | --- | --- |
| Keyword | Allowed kind of Parameterization | Allowed form of Parameterization | Allowed types in formal parameter lists |
| **module** | Value parameterization | Static at start of runtime | all basic types, all user-defined types and **address** type. |
| **template** | Value and template parameterization | Dynamic at runtime | all basic types, all user-defined types, **address** type and **template.** |
| **function** | Value, template, port and timer parameterization | Dynamic at runtime | all basic types, all user-defined types, **address** type, **component** type, **port** type, **default**, **template** and **timer**. |
| **altstep** | Value, template, port and timer parameterization | Dynamic at runtime | all basic types, all user-defined types, **address** type, **component** type, **port** type, **default**, **template** and **timer**. |
| **testcase** | Value, template, port and timer parameterization | Dynamic at runtime | all basic types and of all user-defined types, **address** type and **template**. |
| NOTE: Signatures are not shown in the table, because a signature declares parameters only. The templates for the signatures can be parameterized, however. | | | |

### 5.4.1 Formal parameters

TTCN-3 modules, structured types, templates, functions, altsteps, and testcases may be defined incompletely, i.e. some entities (variables, templates, ports, timers, etc.) used by the above objects may not be resolved in the definition of the object. These objects are called parameterized objects. Formal entities replacing the unresolved entities in the parameterized object's definition are called formal parameters.

Formal parameters of parameterized templates, functions, altsteps, and testcases are defined in formal parameter lists. Formal parameters of modules are defined in module parameter definitions (see clause 8.2.1).

Formal parameters shall be **in**, **inout** or **out** parameters (see definitions in clause 3.1). If not stated otherwise, a formal parameter is an **in** parameter. For all these three sorts of parameter passing, the formal parameters can both be read and set (i.e. get new values being assigned) within the parameterized object. Formal parameters can be used directly as actual parameters for other parameterized objects, e.g. as actual parameters in function invocations or as actual parameters in template instances.

If parameters are passed by value (i.e. in case of **in** and **out** parameters), type compatibility rules specified in 6.3 apply. When parameters are passed by reference, strong typing is required. Both the actual and formal parameter shall be of the same type.

Formal **in** parameters may have default values. This default value is used when no actual parameter is provided.

NOTE 1: Although **out** parameters can be read within the parameterized object, they do not inherit the value of their actual parameter; i.e. they should be set before they are read.

Formal value or template parameters may be declared lazy using the @lazy modifier. The behaviour of lazy parameters is defined in clause 3.1, definition of lazy values or templates. See examples in clause 5.4.1.1.

Formal value or template parameters may be declared fuzzy using the @fuzzy modifier. The behaviour of lazy parameters is defined in clause 3.1, definition of fuzzy values or templates. See examples in clause 5.4.1.1.

NOTE 2: The actual values of component variables used in the delayed evaluation of a lazy or fuzzy parameter may differ from their values at the time, when the parameterized function or alstep was called.

Assigning default values for lazy and fuzzy formal parameters does not change the parameters' semantics: when the default values are used as actual values for the parameters, they shall be evaluated the same way (i.e. delayed) as if an actual parameter was provided.

Lazy and fuzzy properties are valid only in the scope, where the parameters' names are visible. For example, if a fuzzy parameter is passed to a formal parameter declared without a modifier, it losts its fuzzy feature inside the called function. Similarly, if it is passed to a lazy formal parameter, it becomes lazy within the called function.

#### 5.4.1.1 Formal parameters of kind value

Values of all basic types, all user-defined types, address type, component type, and default can be passed as value parameters.

***Syntactical Structure***

[ ( **in** | **inout** | **out** ) ] [ **@lazy** | **@fuzzy** ] *Type* *ValueParIdentifier* [":=" ( *Expression* | "-" ) ]

***Semantic Description***

Value formal parameters can be used within the parameterized object the same way as values, for example in expressions.

Value formal parameters may be in, inout or out parameters. The default for value formal parameters is **in** parameterization which may optionally be denoted by the keyword **in**. Using of inout or out kind of parameterization shall be specified by the keywords **inout** or **out** respectively.

In parameters may have a default value, which is given by an expression assigned to the parameter. Formal parameters of modified templates may inherit the default values from the corresponding parameters of their parent templates; this shall explicitly be denoted by using a dash (don't change) symbol at the place of the modified template parameters' default value.

TTCN‑3 supports value parameterization according to the following rules:

* the language element **module** allows *static* value parameterization to support test suite parameters, i.e.this parameterization may or may not be resolvable at compile-time but shall be resolved by the commencement of runtime (i.e. *static* at runtime). This means that, at runtime, module parameter values are globally visible but not changeable (see more details in clause 8.2);
* the language elements **template**, **testcase,** **altstep** and **function** support *dynamic* value parameterization (i.e. this parameterization shall be resolved at runtime).

NOTE: Component and default references are also handled as value parameters. In the case of component references, the corresponding component type is the type of the formal parameter. In the case of default references the TTCN-3 type **default** is the type of the formal parameter.

***Restrictions***

a) Language elements which cannot be parameterized are: **const**, **var**, **timer**, **control**, **record** **of**, **set** **of**, **enumerated**, **port**, **component** and subtype definitions, **group** and **import**.

b) Formal value parameters of templates, and of altsteps activated as defaults (see clause 20.5.2) shall always be **in** parameters.

c) Restrictions on module parameters are given in clause 8.2.

d) Default values can be provided for **in** parameters only.

e) The expression of the formal parameters' default value has to be compatible with the type of the parameter. The expression shall not refer to elements of the component type of the optional **runs on** clause. The expression shall not refer to other parameters of the same parameter list. The expression shall not contain the invocation of functions with a **runs on** clause.

f) Default values of component type formal parameters shall be one of the special values **null, mtc, self**, or **system**.

g) Default values of default type formal parameters shall be the special value **null**.

h) The dash (don't change) symbol shall be used with formal parameters of modified templates only (see also clause 15.5).

i) For formal value parameters of templates the restrictions specified in clause 15 shall apply.

j) Only in parameters can be declared lazy or fuzzy.

k) When parameters are referenced (e.g. in assignments, expressions, template bodies, etc.), the rules for variables shall apply.

***Examples***

EXAMPLE 1: In, out and inout formal parameters

**function** MyFunction1(**in boolean** MyReferenceParameter){ … };

// MyReferenceParameter is an in value parameter. The parameter can be read. It can also be set // within the function, however, the assignment is local to the function only

**function** MyFunction2(**inout boolean** MyReferenceParameter){ … };

// MyReferenceParameter is an inout value parameter. The parameter can be read and set

// within the function - the assignment is not local

**function** MyFunction3(**out template boolean** MyReferenceParameter){ … };

// MyReferenceParameter is an out value parameter. The parameter can be set within the function,   
 // the assignment is not local. It can also be read, but only after it has been set.

EXAMPLE 2: Reading and setting parameters

**type** **record** MyMessage {

**integer** f1,

**integer** f2

}

**function** f\_MyMessage (**integer** p\_int) **return** MyMessage {

**var** **integer** f1, f2;

f1 := f\_mult2 (p\_int);

// parameter p\_int is passed on; as the parameter of the called function f\_mult2 is

// defined as an inout parameter, it passes back the changed value for p\_int,

f2 := p\_int;

**return** {f1, f2};

}

**function** f\_mult2 (**inout** **integer** p\_integer) **return** **integer** {

p\_integer := 2 \* p\_integer;

// the value of the formal parameter is changed; this new value is passed back when

// f\_mult2 completes

**return** p\_integer-1

}

**testcase** tc\_01 () **runs** **on** MTC\_PT {

...

P1.**send** (f\_MyMessage(5))

// the value sent is { f1 := 9 , f2 := 10 }

...

}

EXAMPLE 3: Function with default value for parameter

**function** f\_comp (**in integer** p\_int1, **in** **integer** p\_int2 := 3) **return** **integer** {

**var** **integer** v := p\_int1 + p\_int2;

:

**return** v;

}  
  
 **function** f () {

**var** **integer** w;  
 …

w := f\_comp(1); // same as calling f\_comp(1,3);  
 w := f\_comp(1,2); // value 2 is taken for parameter p\_int2 and not its default value 3

…

}

EXAMPLE 4: Direct passing of formal parameters to functions

**function** f\_MyFunc2(**in** **bitstring** p\_refPar1, **inout** **integer** p\_refPar2) **return** **integer** {

:

}

**function** f\_MyFunc1(**inout bitstring** p\_refPar1, **out** **integer** p\_refPar2) **return** **integer** {

:

**return** f\_MyFunc2(p\_refPar1, p\_refPar2);

}

// p\_refPar1 and p\_refPar2 can be passed directly to a function invocation

EXAMPLE 5: Lazy and fuzzy parameters

**type component** MyComp { **var integer** v\_int }

**function** f\_MyLazyFuzzy(**in** **@lazy** **integer** p\_lazy, **in** **@fuzzy** **integer** p\_fuzzy) **runs on** MyComp {

//When called from MyCalling:

v\_int := 1;

**log**(p\_lazy); //will log 2 as function double with actual parameter v\_int equals 1 is called

//here; 2 is stored in p\_lazy (also, function double stores 2 in v\_int)

**log**(p\_lazy); //will log 2 again as p\_lazy is not re-evaluated

**log**(p\_fuzzy);//will log 4 as function double with actual parameter v\_int equals 2 is called

// here (also, function double stores 4 in v\_int)

**log**(p\_fuzzy) //will log 8 as function double is re-evaluated with actual parameter 4

}

**function double** (**in integer** p\_in) **runs on** MyComp **return integer**{

p\_in := 2\* p\_in;

v\_int := p\_in;

**return** p\_in

}

**testcase** tc\_MyCalling() **runs on** MyComp {

v\_int := 0;

f\_MyLazyFuzzy (double(v\_int), double(v\_int) )

}

EXAMPLE 6: Difference between passing by value and passing by reference

**function** f\_byValue (**in integer** p\_int1, **in** **integer** p\_int2) {

p\_int2 := p\_int2 + 1;

log(p\_int1);

log(p\_int2);

}

**function** f\_byReference (**inout integer** p\_int1, **inout** **integer** p\_int2) {

p\_int2 := p\_int2 + 1;

log(p\_int1);

log(p\_int2);

}

**function** f () {

**var** **integer** v\_int := 1;

f\_byValue(v\_int, v\_int); // prints 1 and 2

log(v\_int); // prints 1

f\_byReference(v\_int, v\_int); // prints 2 and 2

log(v\_int); // prints 2

}

#### 5.4.1.2 Formal parameters of kind template

Template kind parameters are used to pass templates into parameterizable objects.

***Syntactical Structure***

[ **in** | **inout** | **out** ] **template** [ *Restriction* ] *Type* *ValueParIdentifier* [":=" ( *TemplateInstance* | "-" )]

***Semantic Description***

Templates parameters can be defined for templates, functions, altsteps, and test cases.

To enable a parameterized object to accept templates or matching symbols as actual parameters, the extra keyword **template** shall be added before the type field of the corresponding formal parameter. This makes the parameter a template parameter and in effect extends the allowed actual parameters for the associated type to include the appropriate set of matching attributes (see annex B) as well as the normal set of values.

Formal template parameters can be used within the parameterized object the same way as templates and template variables.

Formal template parameters may be in, inout or out parameters. The default for formal template parameters is **in** parameterization.

In parameters may have a default template, which is given by a template instance assigned to the parameter. Formal template parameters of modified templates may inherit their default templates from the corresponding parameters of their parent templates; this shall explicitly be denoted by using a dash (don't change) symbol at the place of the modified template parameter's default template.

Formal template parameters can be restricted to accept actual parameters containing a restricted set of matching mechanisms only. Such limitations can be expressed by the restrictions **omit**, **present**, and **value**. The restriction **template (omit)** can be replaced by the shorthand notation **omit**. The meaning of the restrictions is explained in clause 15.8.

***Restrictions***

a) Only **function, testcase**, **altstep** and **template** definitions may have formal template parameters.

b) Formal template parameters of **templates**, of **function**s started as test component behaviour (see clause 21.3.2) and of **altstep**s activated as defaults (see clause 20.5.2) shall always be **in** parameters.

c) Default templates can be provided for in parameters only.

d) The default template instance has to be compatible with the type of the parameter. The template instance shall not refer to elements of the component type in a runs on clause. The template instance shall not refer to other parameters in the same parameter list. The template instance shall not contain the invocation of functions with a runs on clause.

e) Default templates of component type formal parameters shall be built from the special values **null, mtc, self**, or **system**.

f) Restrictions specified in clause 15 shall apply.

g) The dash (don't change) symbol shall be used with formal parameters of modified templates only (see also clause 15.5).

h) Only in template parameters can be declared lazy or fuzzy.

i) When template parameters are referenced (e.g. in assignments, expressions, template bodies, etc.), the rules for template variables shall apply.

***Examples***

EXAMPLE 1: Template with template parameter

// The template

**template** MyMessageType MyTemplate (**template** **integer** MyFormalParam):=

{ field1 := MyFormalParam,

field2 := **pattern** "abc\*xyz",

field3 := **true**

}

// could be used as follows

pco1.**receive**(MyTemplate(?));

// Or as follows

pco1.**receive**(MyTemplate(**omit**)); // provided that field1 is declared in MyMessageType as optional

EXAMPLE 2: Function with template parameter

**function** MyBehaviour(**template** MyMsgType MyFormalParameter)

**runs on** MyComponentType

{ :

pco1.**receive**(MyFormalParameter);

:

}

EXAMPLE 3: Template with restricted parameter

// The template

**template** MyMessageType MyTemplate1 (**template** ( **omit** ) **integer** MyFormalParam):=

{ field1 := MyFormalParam,

field2 := **pattern** "abc\*xyz",

field3 := **true**

}

// could be used as follows

pco1.**send**(MyTemplate1(**omit**));

// but not as follows

pco1.**receive**(MyTemplate1(?)); // AnyValue is not within the restriction

// the same template can be written shorter as

**template** MyMessageType MyTemplate2 (**omit** **integer** MyFormalParam):=

{ field1 := MyFormalParam,

field2 := **pattern** "abc\*xyz",

field3 := **true**

}

#### 5.4.1.3 Formal parameters of kind timer

Functions and altsteps can be parameterized with timers.

***Syntactical Structure***

[ **inout** ] **timer** *TimerParIdentifier*

***Semantic Description***

Timers passed into a parameterized object are known inside the behaviour definition of that object. Timer parameters can be used within the parameterized object like any other timer, i.e. they need not to be declared inside the parameterized object.

Timer parameters shall preserve their current state, i.e. only the timer is made known within the parameterized object. For example, also a started timer continues to run, i.e. it is not stopped implicitly. Thereby, possible timeout events can be handled inside the function or altstep to which the timer is passed.

Formal timer parameters are identified by the keyword **timer**.

***Restrictions***

a) Formal timer parameters shall be inout parameters, which can optionally be indicated by the keyword **inout**.

b) Only **function** - with the exception of functions started as test component behaviour (see clause 21.3.2) - and **altstep** definitions may have formal timer parameters.

***Examples***

// Function definition with a timer in the formal parameter list

**function** MyBehaviour (**timer** MyTimer)

{ :

MyTimer.**start**;

:

}

// could be used as follows

**function** MyBehaviour2 ()

{ :

**timer** t;

MyBehaviour(t);

:

}

#### 5.4.1.4 Formal parameters of kind port

Functions and altsteps can be parameterized with ports.

***Syntactical Structure***

[ **inout** ] *PortTypeIdentifier**PortParIdentifier*

***Semantic Description***

Ports passed into a parameterized object are known inside the behaviour definition of that object. Port parameters can be used within the parameterized object like any other port, i.e. they need not to be made visible by a **runs on** clause.

Ports passed in as parameters shall preserve their current state, only the port is made known within the parameterized object's body. For example, a started port continues to send/receive messages, i.e. it is not stopped implicitly; thereby, possible port events can be handled inside the function or altstep to which the port is passed to.

***Restrictions***

a) Formal port parameters shall be inout parameters, which can optionally be indicated by the keyword **inout**.

b) Only **function** - with the exception of functions started as test component behaviour (see clause 21.3.2) ‑ and **altstep** definitions may have formal port parameters.

***Examples***

// Altstep definition with a port in the formal parameter list

**altstep** MyBehaviour (MyPortType MyPort)

{ :

[] MyPort.**receive** { **setverdict**(**fail**); **stop**; }

:

}

### 5.4.2 Actual parameters

Values, templates, timers and/or ports can be passed into parameterized TTCN-3 objects as actual parameters. Actual parameters can be provided both as a list in the same order as the formal parameters as well as in an assignment notation explicitly using the associated formal parameter names.

***Syntactical Structure***

( *Expression* | // for value parameter

*TemplateInstance* | // for template parameter

*TimerRef* | // for timer parameter

*Port* | // for port parameter

"-" ) | // to skip a parameter with default  
 *ParameterId* ":=" ( Expression | TemplateInstance | TimerRef | Port ) )

***Semantic Description***

Actual parameters that are passed by value to **in** formal value parameters shall be variables, literal values, module parameters, constants, variables, value returning (external) functions, formal value parameters (of in, inout or out parameterization) of the current scope or expressions composed of the above.

Actual parameters that are passed to **inout** formal value parameters shall be variables or formal value parameters (of in, inout or out parameterization) or references to elements of variables or formal value parameters of structured types.

NOTE: Reference to a string element cannot be passed by reference as string types are not structured types.

Actual parameters that are passed to **in** formal template parameters shall be literal values, module parameters, constants, variables, value or template returning (external) functions, formal value parameters (of in, inout or out parameterization) of the current scope or expressions composed of the above, as well as templates, template variables or formal template parameters (of in, inout or out parameterization) of the current scope.

Actual parameters that are passed to **out** formal template parameters shall be variables, template variables, formal value parameters, formal template parameters or references to elements of variables, template variables, formal value parameters or formal template parameters of structured types.

Actual parameters that are passed to **inout** formal template parameters shall be variables, template variables, formal value or template parameters (of in, inout or out parameterization) of the current scope or references to elements of (template) variables or formal (template) parameters of structured types.

When actual parameters that are passed to **in** formal value or template parameters contain a value or template reference, rules for using references on the right hand side of assignments apply. When actual parameters that are passed to **inout** and **out** formal value or template parameters contain a value or template reference, rules for using references on the left hand side of assignments apply.

The values of **out** formal parameters are passed to the actual parameters in the same order as is the order of formal parameters in the definition of the parameterized TTCN-3 object.

Actual parameters that are passed to formal timer parameters shall be component timers, local timers or formal timer parameters of the current scope.

Actual parameters that are passed to formal port parameters shall be component ports or formal port parameters of the current scope.

It is allowed to pass elements of structured values or templates (record, set, record of, set of, union and anytype values or templates) by reference. Modification of parameters passed this way affects the original structured value or template. Before passing the actual parameter, the rules for referencing the element on the left hand side of assignments are applied, expanding the structured value so that the referenced element becomes accessible (see clauses 6.2 and 15.6 for more details).

When a formal parameter has been defined with a default value or template, respectively, then it is not necessary to provide an actual parameter. The actual parameters are evaluated in the order of their appearance. If for some formal parameters, no actual parameter has been provided, their default values are taken and evaluated in the order of the formal parameter list.

The empty brackets for instances of parameterized templates that have only parameters with default values are optional when no actual parameters are provided, i.e. all formal parameters use their default values.

***Restrictions***

a) When using list notation, the order of elements in the actual parameter list shall be the same as their order in the corresponding formal parameter list. For each formal parameter without a default there shall be an actual parameter. The actual parameter of a formal parameter with default value can be skipped by using dash "-" as actual parameter. An actual parameter can also be skipped by just leaving it out if no other actual parameter follows in the actual parameter list - either because the parameter is last or because all following formal parameters have default values and are left out.

b) Either list notation or assignment notation shall be used in a single parameter list. They shall not be mixed.

c) When using assignment notation, each formal parameter shall be assigned an actual parameter at most once. For each formal parameter without default value, there shall be an actual parameter. In order to use the default value of a formal parameter, no assignment for this specific parameter shall be provided.

d) The type of each actual parameter shall be compatible with the type of each corresponding formal parameter. Strong typing is required for parameters passed by reference.

e) Actual parameters passed to restricted formal template parameters shall obey the restrictions given in clause 15.8.

f) All parameterized entities specified as an actual parameter shall have their own parameters resolved in the top‑level actual parameter list.

g) If the formal parameter list of TTCN‑3 objects **function**, **testcase**, **signature, altstep** or **external** **function** is empty, then the empty parentheses shall be included both in the declaration and in the invocation of that object. In all other cases the empty parentheses shall be omitted.

h) Restrictions on the use of signature parameters are given in clauses 15.2 and 22.3.

i) Restrictions on parameters passed to altsteps are given in clauses 16.2.1 and 20.5.2.

j) Unless specified differently in the relevant clause(s), actual parameters passed to **in** or **inout** formal parameters shall be at least partially initialized (for an exemption see e.g. clause 16.1.2 of the present document).

k) Functions, called by actual parameters passed to fuzzy or lazy formal parameters of the calling function, shall not have inout or out formal parameters. The called functions may use other functions with inout or out parameters internally.

l) Actual parameters passed to **out** and **inout** parameters shall not be references to lazy or fuzzy variables.

m) Whenever a value or template of a record, set, union, record of, set of, array and anytype type is passed as an actual parameter to an inout parameter, none of the fields or elemens of this structured value or template shall be passed as an actual parameter to another inout parameter of the same parameterized TTCN-3 object. This restriction applies recursively to all sub-elements of the structured value or template in any level of nesting.

n) If two or more actual parameters passed to **inout** parameters of the same parameterized TTCN-3 object contain a reference to distinct alternatives of the same union or anytype value, an error shall be produced.

***Examples***

EXAMPLE 1: Formal and actual parameter lists have to match

// A function definition with a formal parameter list

**function** MyFunction(**integer** FormalPar1, **boolean** FormalPar2, **bitstring** FormalPar3) { … }

// A function call with an actual parameter list

MyFunction(123, **true**,'1100'B);

// A function call with assignment notation for actual parameters

MyFunction(FormalPar1 := 123, FormalPar3 := '1100'B, FormalPar2 := **true**);

EXAMPLE 2: In parameters

**function** MyFunction(**in** **template** MyTemplateType MyValueParameter){ … };

// MyValueParameter is in parameter, the in keyword is optional

// A function call with an actual parameter

MyFunction(MyGlobalTemplate);

EXAMPLE 3: Inout and out parameters

**function** MyFunction(**inout boolean** MyReferenceParameter){ … };

// MyReferenceParameter is an inout parameter

// A function call with an actual parameter

MyFunction(MyBooleanVariable);

// The actual parameter can be read and set within the function

**function** MyFunction(**out template boolean** MyReferenceParameter){ … };

// MyReferenceParameter is an out parameter

// A function call with an actual parameter

MyFunction(MyBooleanVariable);

// The actual parameter is initially unbound, but can be set and read within the function.

**type** **record** **of** **integer** RoI;

**function** f\_swapElements (**inout integer** p\_int1, **inout** **integer** p\_int2) {

**var** **integer** v\_tmp := p\_int1;

p\_int1 := p\_int2;

p\_int2 := p\_tmp;

}

**function** f\_testReferences (**inout** RoI p\_roi, **inout** **integer** p\_elem) { … }

:

**var** RoI v\_roi := { 0, 1, 2, 3, 4, 5 };

f\_swapElements(v\_roi[0], v\_roi[5]); // after the function call, v\_roi is { 5, 1, 2, 3, 4, 0 }

f\_testReferences(v\_roi, v\_roi[2]); // produces an error as elements of v\_roi are not allowed

// to be passed by reference if the parent structure (v\_roi) is passed by reference too.

EXAMPLE 4: Empty parameter lists

// A function definition with an empty parameter list shall be written as

**function** MyFunction(){ … }

// and shall be called as

MyFunction();

// A record definition with an empty parameter list shall be written as

**type record** MyRecord { … }

// and shall be used as

**template** MyRecord Mytemplate := { … }

EXAMPLE 5: Nested parameter lists

// Given the message definition

**type record** MyMessageType

{

**integer** field1,

**charstring** field2,

**boolean** field3

}

// A message template might be

**template** MyMessageType MyTemplate(**integer** MyValue) :=

{

field1 := MyValue,

field2 := **pattern** "abc\*xyz",

field3 := **true**

}

// A test case parameterized with a template might be

**testcase** TC001(**template** MyMessageType RxMsg) **runs on** PTC1 **system** TS1 {

:

MyPCO.**receive**(RxMsg);

}

// When the test case is called in the control part and the parameterized template is

// passed as an actual parameter, the template's actual parameters shall be provided

**control**

{ :

**execute**(TC001(MyTemplate(7)));

:

}

EXAMPLE 6: A typical use case for lazy parameterization

**modulepar** **boolean** logMessage := true;

**function** logMsg(**@lazy** **charstring** complex) {

**if** (logMessage) {

**log**(complex);

}

}

**function** computeComplexMessage() **return charstring** {

// some complicated computation

}

logMsg(computeComplexMessage()); // computeComplexMessage() is only invoked if

// logMessage is false

EXAMPLE 7: Actual parameters passed to lazy and fuzzy formal parameters

**type** **record** MyMessage { **integer** id, **float** number }

**type** **port** MyPortType **message** { **inout** MyMessage }

**type** **component** MyMTC {

**var** **integer** v\_id;

**port** MyPortType P;

}

**testcase** TC\_shootingMessages () **runs** **on** MyMTC {

**connect**(**self**:P,**self**:P);

sendLazy({v\_id, rnd()}); //note that at this point v\_id is unintialized yet

sendFuzzy({v\_id, rnd()})

}

**function** sendLazy(@lazy MyMessage pdu) **runs** **on** MyMTC {

**for** (v\_id := 1; v\_id<9; v\_id:=v\_id+1){

P.**send**(pdu); // the actual parameter passed to the formal parameter pdu is evaluated only in

// the first loop;let say rnd() returns 0.924946; the message { 1, 0.924946 } is

// sent out 8 times

}

**setverdict**(**pass**,"messages has been sent out")

}

**function** sendFuzzy(@fuzzy MyMessage pdu) **runs** **on** MyMTC {

**for** (v\_id := 1; v\_id<9; v\_id:=v\_id+1){

P.**send**(pdu); // the actual parameter passed to the formal parameter pdu is evaluated in each

// loop; let say rnd() returns 0.924946, 0.680497, 0.630836, 0.648681, 0.428501,

// 0.262539, 0.646990, 0.265262 in subsuent calls; the messages 1, 0.924946 },

// {{ 2, 0.680497 }, { 3, 0.630836 }, { 4, 0.648681 }, { 5, 0.428501 },

// { 6, 0.262539 }, { 7, 0.646990 } and { 8, 0.265262 } are sent out in sequence

}

**setverdict**(**pass**,"messages has been sent out")

}

EXAMPLE 8: Order of out parameters

**function** f\_initValues (**out** **integer** p\_par1, **out** **integer** p\_par2) {

p\_par1 := 1**;**

p\_par2 := 2;

}

**function** f(){

**var** **integer** v\_var1;

f\_initValues(p\_par2 := v\_var1, p\_par1 := v\_var1);

// After this function call, v\_var1 will contain 2, as parameters are assigned in

// the same order as in the definition of the f\_initValues function. Thus p\_par1 is

// assigned first to v\_var1 and p\_par2 after that ovewriting the previous value.

}

## 5.5 Cyclic Definitions

Direct and indirect cyclic definitions are not allowed with the exception of the following cases:

a) for recursive type definitions (see clause 6.2);

b) function and altstep definitions (i.e. recursive function or altstep calls);

c) cyclic import definitions, if the imported definitions only form allowed cyclic definitions.

NOTE 1: Indirect cyclic definitions may be a result of imports of definitions that are needed for the usage of a definition but do not need to be known in the importing module (see clause 8.2.3.1).

NOTE 2: For the detection of cycles only the main identifiers of the definition are used. For example, field identifiers are not used.

***Examples***

EXAMPLE 1: Module with cyclic constant definition that is not allowed

**module** MyModule {

:

**type record** ARecordType { **integer** a, **integer** b };

:

// The following two lines include a cycle that is not allowed

**const** ARecordType cConst := { 1 , dConst.b}; // cConst refers to dConst

**const** ARecordType dConst := { 1 , cConst.b}; // dConst refers to cConst

}

EXAMPLE 2: Modules with cyclic import that is allowed

**module** MyModuleA {

**import** **from** MyModuleB { **type** MyInteger }

**type** **record** **of** MyInteger MyIntegerList;

}

**module** MyModuleB {

**type** **integer** MyInteger;

**import** **from** MyModuleA { **type** MyIntegerList }

}

# 6 Types and values

TTCN‑3 supports a number of predefined basic types. These basic types include ones normally associated with a programming language, such as **integer**, **boolean** and string types, as well as some TTCN‑3 specific ones such as **verdicttype**. Structured types such as **record** types, **set** types and **union** types can be constructed from these basic types. **enumerated** types are specific structured types being constructed of enumerated values.

The special data type **anytype** is defined as the union of all known data types and the address type within a module.

Special types associated with test configurations such as **address**, **port** and **component** may be used to define the architecture of the test system (see clause 21).

The special type **default** may be used for the default handling (see clause 20.5).

The TTCN‑3 types are summarized in table 3.

Table 3: Overview of TTCN‑3 types

|  |  |  |
| --- | --- | --- |
| Class of type | Keyword | Subtype |
| Simple basic types | **integer** | range, list |
| **float** | range, list |
| **boolean** | list |
| **verdicttype** | list |
| Basic string types | **bitstring** | list, length |
| **hexstring** | list, length |
| **octetstring** | list, length |
| **charstring** | range, list, length, pattern |
| **universal charstring** | range, list, length, pattern |
| Structured types | **record** | list (see note) |
| **record of** | list (see note), length |
| **set** | list (see note) |
| **set of** | list (see note), length |
| **enumerated** | list (see note) |
| **union** | list (see note) |
| Special data type | **anytype** | list |
| Special configuration types | **address** |  |
| **port** |  |
| **component** |  |
| Special default type | **default** |  |
| NOTE: List subtyping of these types is possible when defining a new constrained type from an already existing parent type but not directly at the declaration of the first parent type. | | |

NOTE: Behaviour types for TTCN-3 are defined in the optional package [i.13].

## 6.1 Basic types and values

### 6.1.0 Simple basic types and values

TTCN‑3 supports the following basic types:

a) **integer:** a type with distinguished values which are the positive and negative whole numbers, including zero.

Values of integer type shall be denoted by one or more digits; the first digit shall not be zero unless the value is 0; the value zero shall be represented by a single zero.

b) **float:** a type to describe floating-point numbers and special float values.

In general, floating point numbers can be defined as:<*mantissa>* × <*base><exponent>*,

where *<mantissa>* is a positive or negative integer, *<base>* a positive integer (in most cases 2, 10 or 16) and *<exponent>* a positive or negative integer.

In TTCN‑3, the floating-point number value notation is restricted to a base with the value of 10. Floating point values can be expressed by using two forms of value notations:

* the decimal notation with a dot in a sequence of numbers like, 1.23 (which represents 123×10-2), 2.783 (i.e. 2783 × 10-3) or -123.456789 (which represents -123 456 789 × 10-6); or
* by two numbers separated by E where the first number specifies the mantissa and the second specifies the exponent, for example 12.3E4 (which represents 123 × 103) or -12.3E-4 (which represents ‑123 × 10‑5).

NOTE 1: In contrast to the general definition of float values, the mantissa of in theTTCN‑3 value notation, beside integers, allows decimal numbers as well.

The special values of the float type consist of **infinity** (positive infinity), **-infinity** (negative infinity) and the value **not\_a\_number**. For the ordering of special values see clauses 7.1.1 and 7.1.3.

NOTE 2: **-not\_a\_number** (i.e. minus not a number) is not to be used.

c) **boolean:** a type consisting of two distinguished values.

Values of boolean type shall be denoted by **true** and **false**.

d) **verdicttype:** a type for use with test verdicts consisting of 5 distinguished values. Values of **verdicttype** shall be denoted by **pass**, **fail**, **inconc**, **none** and **error**.

### 6.1.1 Basic string types and values

TTCN‑3 supports the following basic string types:

NOTE 1: The general term string or string type in TTCN‑3 refers to **bitstring**, **hexstring**, **octetstring**, **charstring** and **universal charstring**.

a) **bitstring:** a type whose distinguished values are the ordered sequences of zero, one, or more bits.

Values of type **bitstring** shall be denoted by an arbitrary number (possibly zero) of the bit digits: 0 1, preceded by a single quote ( ' ) and followed by the pair of characters 'B.

EXAMPLE 1: '01101'B.

b) **hexstring:** a type whose distinguished values are the ordered sequences of zero, one, or more hexadecimal digits, each corresponding to an ordered sequence of four bits.

Values of type **hexstring** shall be denoted by an arbitrary number (possibly zero) of the hexadecimal digits (uppercase and lowercase letters can equally be used as hex digits):

0 1 2 3 4 5 6 7 8 9 a b c d e f A B C D E F

preceded by a single quote ( ' ) and followed by the pair of characters'H; each hexadecimal digit is used to denote the value of a semi-octet using a hexadecimal representation.

EXAMPLE 2: 'AB01D'H  
'ab01d'H  
'Ab01D'H

c) **octetstring:** a type whose distinguished values are the ordered sequences of zero or a positive even number of hexadecimal digits (every pair of digits corresponding to an ordered sequence of eight bits).

Values of type **octetstring** shall be denoted by an arbitrary, but even, number (possibly zero) of the hexadecimal digits (uppercase and lowercase letters can equally be used as hex digits):

0 1 2 3 4 5 6 7 8 9 a b c d e f A B C D E F

preceded by a single quote ( ' ) and followed by the pair of characters 'O; each hexadecimal digit is used to denote the value of a semi-octet using a hexadecimal representation.

EXAMPLE 3: 'FF96'O  
'ff96'O  
'Ff96'O

d) **charstring:** are types whose distinguished values are zero, one, or more characters of the version of Recommendation ITU‑T T.50 [4] complying with the International Reference Version (IRV) as specified in clause 8.2 of Recommendation ITU‑T T.50 [4].

NOTE 2: The IRV version of Recommendation ITU‑T T.50 [4] is equivalent to the IRV version of the International Reference Alphabet (former International Alphabet No.5 - IA5), described in Recommendation ITU‑T T.50 [4].

Values of **charstring** type shall be denoted by an arbitrary number (possibly zero) of non-control characters from the relevant character set, preceded and followed by double quote ("). Graphical characters include the range from SP(32) to TILDE (126). Values of **charstring** type can also be calculated using the predefined conversion function int2char with the positive integer value of their encoding as argument (see clause C.1).

NOTE 3: The predefined conversion function is able to return single-character-length values only.

In cases where it is necessary to define strings that include the character double quote (") the character is represented by a pair of double quotes on the same line with no intervening space characters.

EXAMPLE 4: The charstring "ab"cd" is written in TTCN-3 code as in the following constant declaration. Each of the 3 quote characters that are part of the string is preceded by an extra quote character and the whole character string is delimited by quote characters, e.g.  
**var** **charstring** vl\_char:= """ab""cd""";

e) The character string type preceded by the keyword **universal** denotes types whose distinguished values are zero, one, or more characters from ISO/IEC 10646 [2].


**universal** **charstring** values can also be denoted by an arbitrary number (possibly zero) of characters from the relevant character set, preceded and followed by double quote ("), calculated using a predefined conversion function (see clause C.1.2) with the positive integer value of their encoding as argument, by a "quadruple" or using the USI-like notation.

NOTE 4: If applying the double quote format all characters from any character set defined in ISO/IEC 10646 [2] are allowed. Users should be aware of the character set capabilities of their editing tool and the TTCN-3 module transfer syntax UTF-8 (see chapter 8).

NOTE 5: The predefined conversion function is able to return single-character-length values only.

In cases where it is necessary to define strings that include the character double quote (") the character is represented by a pair of double quotes on the same line with no intervening space characters.

The "quadruple" is only capable to denote a single character and denotes the character by the decimal values of its group, plane, row and cell according to ISO/IEC 10646 [2], preceded by the keyword **char** included into a pair of brackets and separated by commas (e.g. **char** ( 0, 0, 1, 113) denotes the Latin small letter u with double acute: "ű"). In cases where it is necessary to denote the character double quote (") in a string assigned according to the first method (within double quotes), the character is represented by a pair of double quotes on the same line with no intervening space characters. The two methods may be mixed within a single notation for a string value by using the concatenation operator.

EXAMPLE 5: The expression: "the Braille character" & **char** (0, 0, 40, 48) & "looks like this" represents the literal string: the Braille character  looks like this.

The UCS sequence identifier-like (USI-like) notation (see also clause 6.6 of ISO/IEC 10646 [2]) can be used to denote 1..N characters, using their short identifiers of code point (similar to UIDs described in clause 6.5 of ISO/IEC 10646 [2]). The USI-like notation is composed of the keyword **char** followed by parentheses. The parentheses enclose a comma-separated list of short identifiers . Each short identifier represents a single character and it shall be composed of a letter **U** or **u** followed by an optional “+” PLUS SIGN character, followed by 1..8 hexadecimal digits. The hexadecimal digits represent the numeric code point of the character. (e.g. char(U0171) denotes the Latin small letter u with double acute: "ű"). In the USI-like notation, the leading zeroes can be omitted, (i.e. char(U171)is equal to char(U0171)).

EXAMPLE 6: The expression: **char** (U4E2D, U56FD) represents the literal string: 中国.

NOTE 6: Control characters can be denoted by using the predefined conversion function, the quadruple form or the USI-like notation.

By default, **universal charstring** shall conform to the UTF-32 encoding specified in clause 9.3 of ISO/IEC 10646 [2].

NOTE 7: UTF-32 is an encoding format, which represents any UCS character on a fixed, 32 bits‑length field.

This default encoding can be overridden using the defined variant attributes (see clause 27.5). The useful character string types utf8string, bmpstring, utf16string and iso8859string using these attributes are defined in annex E.

#### 6.1.1.1 Accessing individual string elements

Individual elements in a string type may be accessed using an array-like syntax. Only single elements of the string may be accessed.

Units of length of different string type elements are indicated in table 4.

Indexing shall begin with the value zero (0). The index shall be between zero and the length of the string minus one for retrieving an element from a string. For assigning an element to the end of a string, the length of the string should be used as index.

EXAMPLE 1: Accessing an existing element

// Given

MyBitString := '11110111'B;

// Then doing

MyBitString[4] := '1'B;

// Results in the bitstring '11111111'B

EXAMPLE 2: Specific cases

**var** **bitstring** MyBitStringA, MyBitStringB, MyBitStringC;

MyBitStringA := '010'B;  
 MyBitStringA[1] := '11'B; //causes an error as only individual elements can be accessed  
  
 MyBitStringB := '1'B;  
 MyBitStringB[4] := '1'B; //causes an error as the index is larger than the length of the lhs  
  
 MyBitStringC := ''B;  
 MyBitStringC[0] := '1'B; // value of MyBitStringC is '1'B

MyBitStringC[1] := '0'B; // value of MyBitStringC is '10'B

### 6.1.2 Subtyping of basic types

User-defined types shall be denoted by the keyword **type**. With user-defined types it is possible to create subtypes (such as lists, ranges and length restrictions) on basic types, structured types and anytype according to table 3.

#### 6.1.2.1 Lists of templates

TTCN‑3 permits the specification of a list of distinguished templates as listed in table 3. The templates in the list shall be instances of the type being constrained and the set of values matching at least one of these templates shall be a subset of the values defined by the type being constrained. The subtype defined by this list restricts the allowed values of the subtype to those values matching at least one of the templates in the list. The templates in the list shall only (directly or indirectly) reference other templates or constant expressions. Constant expressions used (directly or indirectly) in the template expressions shall meet with the restrictions in clause 10 for constant expressions used in type definitions.

EXAMPLE:

**type** **bitstring** MyListOfBitStrings ('01'B, '10'B, '11'B);

**type** **float** pi (3.1415926);

**type** **charstring** MyStringList ("abcd", "rgy", "xyz");

**type** **universal charstring** SpecialLetters   
 (**char**(0, 0, 1, 111), **char**(0, 0, 1, 112), **char**(0, 0, 1, 113));

#### 6.1.2.2 Lists of types

TTCN‑3 permits the specification of a list of subtypes as listed in table 3 for value lists. The types in the list shall be subtypes of the root type. The subtype defined by this list restricts the allowed values of the subtype to the union of the values of the referenced subtypes.

EXAMPLE:

**type** **bitstring** BitStrings1 ('0'B, '1'B );

**type** **bitstring** BitStrings2 ('00'B, '01'B, '10'B, '10'B);

**type bitstring** BitStrings\_1\_2 (Bitstrings1, Bitstrings2);

#### 6.1.2.3 Ranges

TTCN‑3 permits the specification of range constraints for the types **integer, charstring,** **universal charstring** and **float** (or derivations of these types). For **integer** and **float**, the subtype defined by the range restricts the allowed values of the subtype to the values in the range including or excluding the lower boundary and/or the upper boundary. The upper boundary shall be greater than or equal to the lower boundary.

In order to specify an infinite integer range, the keyword -**infinity** or **infinity** can be used instead of a value indicating that there is no lower or upper boundary; **-infinity** shall not be used as the upper bound and **infinity** shall not be used as the lower bound for integer ranges.

Also for **float**, **‑infinity** or **infinity** can be used as the bounds in range restrictions. Using the special value **‑infinity** as the lower bound shall indicate that the allowed numerical values are not restricted downward and the special value **‑infinity** is also included. If both the lower and upper bounds denote **‑infinity**, no numerical values are included, only the special value **‑infinity**. Using the special value **infinity** as the upper bound shall indicate that the allowed numerical values are not restricted upward and the special value **infinity** is also included. If both the lower and upper bounds denote **infinity**, no numerical values are included, only the special value **infinity**. If exclusive bounds (!**infinity** or !**-infinity)** is used instead, only the respective numerical float values are included in the range. In case of **float**, the special value **not\_a\_number** is not allowed in a range constraint.

In the case of **charstring** and **universal charstring** types, the range restricts the allowed values for each separate character in the strings. The boundaries shall evaluate to valid character positions according to the coded character set table(s) of the type (e.g. the given position shall not be empty). Empty positions between the lower and the upper boundaries are not considered to be valid values of the specified range.

Constants used in the constant expressions defining the values shall meet with the restrictions in clause 10.

EXAMPLE 1:

**type** **integer** MyIntegerRange (0 .. 255); // range from 0..255

// (with inclusive boundaries)

**type** **integer** MyIntegerRange (-**infinity** .. -1); // all negative integer numbers

**type** **integer** MyIntegerRange (0 .. !256); // the same range as above (with left

// inclusive and right exclusive boundary)

**type** **integer** MyIntegerRange (!-1 .. 255); // the same range as above(with left

// exclusive and right inclusive boundary)

**type** **integer** MyIntegerRange (!-1 .. !256); // the same range as above

// (with exclusive boundaries)

**type** **float** piRange (3.14 .. 3142E-3);

**type** **float** LessThanPi (-**infinity** .. 3142E-3);

**type** **float** Numbers (-**infinity** .. **infinity**); //includes all float values but **not\_a\_number**

**type** **float** Wrong (-**infinity** .. **not\_a\_number**); // causes an error as not\_a\_number is not

// allowed in range subtyping

EXAMPLE 2:

**type** **charstring** MyCharString ("a" .. "z");

// Defines a string type of any length with each character within the specified range

**type** **universal** **charstring** MyUCharString1 ("a" .. !"z");

// Defines a string type of any length with each character within the range from a to y

// (character codes from 97 to 121), like "abxy";

// strings containing any other character (including control characters), like

// "abc2" are disallowed.

**type** **universal** **charstring** MyUCharString2 (**char**(0, 0, 1, 111) .. **char**(0, 0, 1, 113));

// Defines a string type of any length with each character within the range specified using

// the quadruple notation

#### 6.1.2.4 String length restrictions

TTCN‑3 permits the specification of length restrictions on string types. The length boundaries are based on different units depending on the string type with which they are used. In all cases, these boundaries shall be inclusive boundaries only and evaluate to non‑negative **integer** values (or derived **integer** values).

EXAMPLE:

**type** **bitstring** MyByte **length**(8); // Exactly length 8

**type** **bitstring** MyByte **length**(8 .. 8); // Exactly length 8

**type** **bitstring** MyNibbleToByte **length**(4 .. 8); // Minimum length 4, maximum length 8

Table 4 specifies the units of length for different string types.

Table 4: Units of length used in field length specifications

|  |  |
| --- | --- |
| Type | Units of Length |
| **bitstring** | bits |
| **hexstring** | hexadecimal digits |
| **octetstring** | octets |
| **character strings** | characters |

For the upper bound the keyword **infinity** may also be used to indicate that there is no upper limit for the length. The upper boundary shall be greater than or equal to the lower boundary.

#### 6.1.2.5 Pattern subtyping of character string types

TTCN‑3 allows using character patterns specified in clause B.1.5 to constrain permitted values of **charstring** and **universal charstring** types. The type constraint shall use the **pattern** keyword followed by a character pattern. All values denoted by the pattern shall be a subset of the type being sub typed. Constants used in the constant expressions defining the values shall meet with the restrictions in clause 10.

NOTE: Pattern subtyping can be seen as a special form of list constraint, where members of the list are not defined by listing specific character strings but via a mechanism generating elements of the list.

EXAMPLE:

**type** **charstring** MyString (**pattern** "abc\*xyz");

// all permitted values of MyString have prefix abc and postfix xyz

**type** **charstring** MyStringCaseAgnostic (**pattern** **@nocase** "abc\*xyz");

// all permitted values of MyStringCaseAgnostic have a

// prefix abc or Abc or aBc or abC or ABc or aBC or AbC or ABC, and a

// postfix xyz or Xyz or xYz or xyZ or XYz or xYZ or XyZ or XYZ;

**type** **universal** **charstring** MyUString (**pattern** "\*\r\n")

// all permitted values of MyUString are terminated by CR/LF

**type** **charstring** MyString2 (**pattern** "abc?\q{0,0,1,113}");

// causes an error because the character denoted by the quadruple {0,0,1,113} is not a

// legal character of the TTCN‑3 charstring type

**type** MyString MyString3 (**pattern** "d\*xyz");

// causes an error because the type MyString does not contain a value starting with the

// character d

#### 6.1.2.6 Mixing subtyping mechanisms

##### 6.1.2.6.1 Mixing patterns, lists and ranges

Within **integer** and **float** (or derivations of these types) subtype definitions it is allowed to mix lists and ranges. It is possible to mix both template list and type list subtyping with each other and with range subtyping. Overlapping of different constraints is not an error.

EXAMPLE 1:

**type** **integer** MyIntegerRange (1, 2, 3, 10 .. !20, 99, 100);

**type** **float** lessThanPiAndNaN (-**infinity** .. 3142E-3, **not\_a\_number**);

Within **charstring** and **universal charstring** subtype definitions it is not allowed to mix pattern, template list, type list, or range constraints.

EXAMPLE 2:

**type** **charstring** MyCharStr0 ("gr", "xyz");

// contains character strings gr and xyz;

**type** **charstring** MyCharStr1 ("a".."z");

// contains character strings of arbitrary length containing characters a to z.

**type** **charstring** MyCharStr2 (pattern "[a-z]#(3,9)");

// contains character strings of length from 3 to 9 characters containing characters a to z

##### 6.1.2.6.2 Using length restriction with other constraints

Within **bitstring**, **hexstring,** **octetstring** subtype definitions lists and length restriction may be mixed in the same subtype definition.

Within **charstring** and **universal charstring** subtype definitions it is allowed to add a length restriction to constraints containing list, range or pattern subtyping in the same subtype definition.

When mixed with other constraints the length restriction shall be the last element of the subtype definition. The length restriction takes effect jointly with other subtyping mechanisms (i.e. the value set of the type consists of the common subset of the value sets identified by the list, range or pattern subtyping and the length restriction).

EXAMPLE:

**type** **charstring** MyCharStr5 ("gr", "xyz") **length** (1..9);

// contains the character strings gr and xyz;

**type** **charstring** MyCharStr6 ("a".."z") **length** (3..9);

// contains character strings of length from 3 to 9 characters and containing characters

// a to z

**type** **charstring** MyCharStr7 (**pattern** "[a-z]#(3,9)") **length** (1..9);

// contains character strings of length from 3 to 9 characters containing characters

// a to z

**type** **charstring** MyCharStr8 (**pattern** **@nocase** "[a-z]#(3,9)") **length** (1..8);

// contains character strings of length from 3 to 8 characters containing characters

// a to z and A to Z

**type** **charstring** MyCharStr9 (**pattern** "[a-z]#(1,8)") **length** (1..9);

// contains any character strings of length from 1 to 8 characters containing characters

// a to z

**type** **charstring** MyCharStr10 ("gr", "xyz") **length** (4);

// causes an error as it contains no value

## 6.2 Structured types and values

The **type** keyword is also used to specify structured types such as **record** types, **record** **of** types, **set** types, **set** **of** types, **enumerated** types and **union** types.

Values of these types may be given using an explicit assignment notation or a short-hand value list notation.

EXAMPLE 1:

**const** MyRecordType MyRecordValue:= //assignment notation

{

field1 := '11001'B,

field2 := **true**,

field3 := "A string"

}

// Or

**const** MyRecordType MyRecordValue:= {'11001'B, **true**, "A string"} //value list notation

The assignment notation can be used for **record, record of**, **set**, **set of** and **union** value notations and for arrays. The value list notation can be used for **record, record of**, **set** and **set of** value notations and for arrays. The index notation can be used for **record of** and **set of** value notations and for arrays. See more details in the subsequent clauses.

EXAMPLE 2:

**var** MyRecordType MyVariable:= //assignment notation

{

field1 := '11001'B,

// field2 implicitly unspecified

field3 := "A string"

}

// Or  
 **var** MyRecordType MyVariable:= //assignment notation

{

field1 := '11001'B,  
 field2 := -, // field2 explicitly unspecified

field3 := "A string"

}

// Or

**var** MyRecordType MyVariable:= {'11001'B, -, "A string"} //value list notation

It is not allowed to mix the two value notations in the same (immediate) context.

EXAMPLE 3:

// This is disallowed

**const** MyRecordType MyRecordValue:= {MyIntegerValue, field2 := **true**, "A string"}

Where applicable TTCN‑3 type definitions may be recursive. The user, however, shall ensure that all type recursion is resolvable and that no infinite recursion occurs.

In case of record and set types, to avoid infinite recursion, fields referencing to its own type, shall be optional.

EXAMPLE 4:

// Valid recursive record type definition

**type** **record** MyRecord1  
    {   
        FieldType1 field1,  
        MyRecord1 field2 **optional**,

        FieldType3 field3   
    }

// Invalid recursive record type definition causing an error

**type** **record** MyRecord2  
    {   
        FieldType1 field1,  
        MyRecord2 field2,

        FieldType3 field3   
    }

In case of union types, to avoid infinite recursion, at least one of the alternatives shall not reference its own type.

EXAMPLE 5:

// Valid recursive union type definition

**type** **union** MyUnion1

{

MyUnion1 choice1,

**charstring** choice2

}

// Invalid recursive union type definition causing an error

**type** **union** MyUnion2

{

MyUnion2 choice1,

MyUnion2 choice2

}

### 6.2.1 Record type and values

TTCN‑3 supports ordered structured types known as **record**. The elements of a **record** type may be any of the basic types or user-defined data types (such as other records, sets or arrays). The values of a **record** shall be compatible with the types of the **record** fields. The element identifiers are local to the **record** and shall be unique within the **record** (but do not have to be globally unique).

EXAMPLE 1:

**type** **record** MyRecordType

{

**integer** field1**,**

MyOtherRecordType field2 **optional,**

**charstring** field3

}

**type** **record** MyOtherRecordType

{

**bitstring** field1**,**

**boolean** field2

}

Records may be defined with no fields, i.e. as empty records.

EXAMPLE 2:

**type** **record** MyEmptyRecord {}

A **record** value is assigned on an individual element basis. The order of field values in the value list notation shall be the same as the order of fields in the related type definition.

EXAMPLE 3:

**var** **integer** MyIntegerValue := 1;

**const** MyOtherRecordType MyOtherRecordValue:=

{

field1 := '11001'B,

field2 := **true**

}

**var** MyRecordType MyRecordValue :=

{

field1 := MyIntegerValue,

field2 := MyOtherRecordValue,

field3 := "A string"

}

The same value specified with a value list.

EXAMPLE 4:

MyRecordValue:= {MyIntegerValue, {'11001'B, **true**}, "A string"};

When the assignment notation is used for **record**‑s, fields wished to be changed shall be identified explicitly and a value, the not used symbol "-" or the **omit** keyword can be associated with them. The **omit** keyword shall only be used for optional fields. Its result is that the given field is not present in the given value.

NOTE: Pleases note the difference between omitted and uninitialized fields. Omitted optional fields are not present in the record or set value intentionally, i.e. the field is initialized and it does not prevent the whole record or set from being completely initialized.

When the assignment notation is used in a scope, where the **optional** attribute is implicitly or explicitly set to **"explicit** **omit"**, fields, not explicitly referred to in the notation, shall remain unchanged. In particular, when specifying partial values (i.e. setting the value of only a subset of the fields) using the assignment notation, for example, at initialization, only the fields or elements to be assigned values shall be specified. Fields or elements not mentioned are implicitly left uninitialized. It is also possible to leave fields explicitly unspecified using the not used symbol "-". When re-assigning a previously initialized value, using the not used symbol or just skipping a field or element in an assignment notation, will cause that field or element to remain unchanged.

EXAMPLE 5:

**var** MyRecordType MyVariable :=

{

field1 := '111'B,

field2 := **false,**

field3 := -

}

MyVariable := { '10111'B, -, - };

// after this, MyVariable contains:

// { '10111'B, **false** /\* unchanged \*/, <undefined> /\* unchanged \*/ }

MyVariable :=

{

field2 := **true**

}

// after this, MyVariable contains:

// { '10111'B /\* unchanged \*/, **true**, <undefined> /\* unchanged \*/ }

MyVariable :=

{

field1 := -,

field2 := **false,**

field3 := -

}

// after this, MyVariable contains:

// { '10111'B /\* unchanged \*/, **false**, <undefined> /\* unchanged \*/}

When the assignment notation is used in a scope, where the **optional** attribute is set to **"implicit** **omit"**, optional fields, not directly referred to in the notation, shall implicitly be set to omit, while mandatory fields shall remain unchanged (see also clause 27.7).

When using the value list notation, all fields in the structure shall be specified either with a value, the not used symbol "‑" or the **omit** keyword. The **omit** keyword shall only be used for optional fields. Its result is that the given field is not present in the given value. The first component of the list (a value, a "-" or **omit**) is associated with the first field, the second list component is associated with the second field, etc. No empty assignment is allowed (i.e. two commas, the second immediately following the first or only with white space between them). Fields or elements to be left unchanged shall be explicitly skipped in the list by using the not-used-symbol "-".

When the value list notation is used in a scope, where the **optional** attribute is implicitly or explicitly set to **"explicit** **omit**, already initialized fields or elements left without an associated component in a value list notation (i.e. at the end of a value ) are becoming uninitialized. In this way, a value with initialized fields or elements can be made empty by using an empty pair of curly brackets ("{}").

When using value list notation in a scope where the **optional** attribute is set to **"implicit omit"**, optional fields wished to be omitted by the implicit mechanism, but followed by fields to which a value or template is assigned explicitly, shall be skipped by using the not used symbol "-". When all remaining fields at the end of the type definition are optional and they are wished to be omitted by the implicit mechanism, either the not used symbol "-" can be used for some or all of them or they can simply be left out from the notation.

EXAMPLE 6:

**type** **record** R {  
 **integer** f1,  
 **integer** f2 **optional**,  
 **integer** f3,  
 **integer** f4 **optional**,  
 **integer** f5 **optional**  
 }  
  
 **var** R x := { 1, -, 2 } **with** { **optional** "implicit omit" }  
 // after the assignment x contains { 1, omit, 2, omit, omit }  
 **var** R x2 := { 1, 2 } **with** { **optional** "implicit omit" }  
 // after the assignment x2 contains { 1, 2, <undefined>, omit, omit }

#### 6.2.1.1 Referencing fields of a record type

Elements of a **record** shall be referenced by the dot notation *TypeIdOrExpression.ElementId*, where *TypeIdOrExpression* resolves to the name of a structured type or an expression of a structured type such as variable, formal parameter, module parameter, constant, template, or function invocation. *ElementId* shall resolve to the name of a field in the structured type. Fields of record type definitions shall not reference themselves.

EXAMPLE 1:

MyVar1 := MyRecord1.myElement1;

// If a record is nested within another type then the reference may look like this

MyVar2 := MyRecord1.myElement1.myElement2;

EXAMPLE 2:

**type** **record** MyType

{

**integer** field1,

MyType.field2 field2 **optional**, // this circular reference is NOT ALLOWED

**boolean** field3

}

If a field in a **record** type or a subtype of a **record** type is referenced by the dot notation, the resulting type is the set of values allowed for that field imposed by the constraints of the field declaration itself (i.e. any constraints applied to the **record** type itself are ignored).

EXAMPLE 3:

**type** **record** MyType2

{

**integer** field1 (1 .. 10),

**charstring** field2 **optional**

}

**type** MyType2 MyType3 ({1, omit}, {2, "foo"}, {3, "bar"}) ;

**type** MyType3.field1 MyType4; // MyType4 is the integer type constrained to  
 // the values 1..10

**type** MyType3.field2 MyType5; // MyType5 is the charstring type

**type** MyType2.field1 MyType6; // MyType6 is the integer type constrained to  
 // the values 1..10

**type** MyType2.field2 MyType7; // MyType7 is the charstring type

Referencing a subfield of an uninitialized or omitted record field or value on the right hand side of an assignment shall cause an error.

EXAMPLE 4:

**type record** MyType4

{

**integer** field1 **optional**,

**record**

{

**integer** subfield1,

**integer** subfield2

} field2 **optional**

}

...

**var** MyType4 v\_rec := { field1 := 1, field2 := omit }

**var** integer v\_int := v\_rec.field2.subfield1;

// causes an error as v\_rec.field2 is omitted

When referencing a field of an uninitialized record value or field or omitted field (including omitting a field at a higher level of the embedding hierarchy) on the left hand side of an assignment, the reference shall recursively be expanded up to and including the depth of the referenced subfield as follows:

1. When expanding a value or value field of record type, the subfield referenced in the dot notation shall be set to present and all unreferenced mandatory subfields shall be left uninitialized; when the assignment is used in a scope where the **optional** attribute is equal to "explicit omit", all unreferenced optional subfields shall be left undefined. When the assignment is used in a scope where the optional attribute is equal to "implicit omit", all unreferenced optional subfields shall be set to **omit**.
2. Expansion of **record of/set of/array**, **union** and **set** values and intermediate fields shall follow the rules of item a) in clauses 6.2.3 and 6.2.5.1, and clause 6.2.2.1 correspondingly.

At the end of the expansion, the value at the right hand side of the assignment shall be assigned to the referenced subfield.

EXAMPLE 5:

**var** MyType4 v\_rec;

v\_rec.field2.subfield1 := 5;

// after the assignment v\_rec is { field1 := <undefined>, field2 := { subfield1 := 5,

// subfield2 := <undefined> } }

#### 6.2.1.2 Optional elements in a record

Optional elements in a **record** shall be specified using the **optional** keyword.

EXAMPLE 1:

**type** **record** MyMessageType

{

FieldType1 field1,

FieldType2 field2 **optional**,

:

FieldTypeN fieldN

}

Optional fields shall be omitted using the omit symbol.

EXAMPLE 2:

MyRecordValue:= {MyIntegerValue, **omit** , "A string"};

// Note that this is not the same as writing,

// MyRecordValue:= {MyIntegerValue, -, "A string"};

// which would mean the value of field2 is unchanged

#### 6.2.1.3 Nested type definitions for field types

TTCN‑3 supports the definition of types for record fields nested within the **record** definition. Both the definition of new structured types (**record**, **set**, **enumerated**, **set** **of**, **record** **of**, and **union**) and the specification of subtype constraints are possible.

EXAMPLE:

// record type with nested structured type definitions

**type** **record** MyNestedRecordType  
 {  
 **record**   
 {  
 **integer** nestedField1,   
 **float** nestedField2  
 } outerField1,  
 **enumerated** {  
 nestedEnum1,  
 nestedEnum2  
 } outerField2,  
 **record** **of** **boolean** outerField3  
 }

// record type with nested subtype definitions

**type** **record** MyRecordTypeWithSubtypedFields

{

**integer** field1 (1 .. 100),

**charstring** field2 **length** ( 2 .. 255 )

}

### 6.2.2 Set type and values

TTCN‑3 supports unordered structured types known as **set**. Set types and values are similar to records except that the ordering of the **set** fields is not significant.

EXAMPLE:

**type** **set** MySetType

{

**integer** field1,

**charstring** field2

}

The field identifiers are local to the set and shall be unique within the set (but do not have to be globally unique).

NOTE: When the value list notation is used for values of **set** types, the values are assigned to the fields in the sequential order of the fields in the type definition.

#### 6.2.2.1 Referencing fields of a set type

Elements of a **set** shall be referenced by the dot notation (see clause 6.2.1.1). Elements of set type definitions shall not reference themselves. For referencing field types of **set** types, the same rules apply as in clause 6.2.1.1 for fields of **record** types.

EXAMPLE:

MyVar3 := MySet1.myElement1;

// If a set is nested in another type then the reference may look like this

MyVar4 := MyRecord1.myElement1.myElement2;

// Note, that the set type, of which the field with the identifier 'myElement2' is referenced,

// is embedded in a record type

#### 6.2.2.2 Optional elements in a set

Optional elements in a **set** shall be specified using the **optional** keyword.

#### 6.2.2.3 Nested type definition for field types

TTCN‑3 supports the definition of types for set fields nested within the **set** definition, similar to the mechanism for record types described in clause 6.2.1.3.

### 6.2.3 Records and sets of single types

TTCN‑3 supports the specification of records and sets whose elements are all of the same type. These are denoted using the keyword **of**. These records and sets do not have element identifiers and can be considered similar to an ordered array and an unordered collection respectively.

NOTE 1: Subtyping of record of and set of types see in clause 6.2.13.

EXAMPLE 1:

**type** **set of** **boolean** MySetOfType; // is an unlimited set of boolean values

When the assignment notation is used for **record of**‑s and **set of**‑s, elements wished to be changed are identified explicitly and either a value or the not used symbol "-" can be assigned to them. Other fields, not referred to in the notation, shall remain unchanged. In particular, when specifying partial values (i.e. setting the value of only a subset of the fields) using the assignment notation, for example, at initialization, only the elements to be assigned values shall be specified: elements not mentioned are implicitly left uninitialized. It is also possible to leave fields explicitly unspecified using the not used symbol "-". When re-assigning a previously initialized value, using the not used symbol or just skipping a field or element in an assignment notation, will cause that field or element to remain unchanged.

EXAMPLE 2:

**var** MyRecordOfType MyVariable := {

[0] := '111'B,

[1] := '101'B,

[2] := -

}

MyVariable := { '10111'B, -, - };

// after this, MyVariable contains:

// { '10111'B, '101'B /\* unchanged \*/, <undefined> /\* unchanged \*/ }

MyVariable :=

{

[1] := '010'B,

}

// after this, MyVariable contains:

// { '10111'B/\* unchanged \*/, '010'B, <undefined>/\* unchanged \*/ }

MyVariable :=

{

[0] := -,

[1] := '001'B**,**

[2] := -

}

// after this, MyVariable contains:

// { '10111'B/\* unchanged \*/, '001'B, <undefined> /\* unchanged \*/}

When using the value list notation, all elements in the structure shall be specified either with a value or the not used symbol "-". The first member of the list is assigned to the first element, the second list member is assigned to the second element, etc. No empty assignment is allowed (e.g. two commas, the second immediately following the first or only with white space between them). Elements to be left out of the assignment shall be explicitly skipped in the list by use of the not-used-symbol "-". Already initialized elements left without a corresponding list member in a value list notation (i.e. at the end of a list) are becoming uninitialized. In this way, a value with initialized elements can be made empty by using the empty value list notation ("{}").

Index notations can be used on both the right-hand side and left-hand side of assignments. For nested record of or set of types, an array or record of integer restricted to a single size can be used as a short-hand notation for a nested index notation. The index notation, when used on the right hand side, refers to the value of the identified element of a **record of** or a **set of**. When it is used at the left hand side, only the value of the identified single element is changed, values assigned to other elements already remain unchanged. The index of the first element shall be zero and the index value shall not exceed the limitation placed by length subtyping.

If the value of the element indicated by the index at the right-hand of an assignment is undefined (uninitialized), this shall cause a semantic or runtime error. Referencing an identified element of an uninitialized or omitted record of or set of field or value on the right hand side of an assignment shall cause an error.

If an indexing operator at the left-hand side of an assignment refers to a non-existent element, the value at the right-hand side is assigned to the element and all elements with an index smaller than the actual index and without assigned value are created with an uninitialized value.

When referencing an element of an uninitialized record of or set of value or field or omitted field (including omitting a field at a higher level of the embedding hierarchy) on the left hand side of an assignment, the reference shall recursively be expanded up to and including the depth of the referenced element as follows:

1. When expanding a value or value field of **record of** or **set of** type, the element referenced by the index notation shall be set to present and all elements with a smaller index shall be created with an uninitialized value.
2. Expansion of **record**, **union** and **set** values and intermediate fields shall follow the rules of item a) in clauses 6.2.1.1 and 6.2.5.1, and clause 6.2.2.1 correspondingly.
3. At the end of the expansion, the value at the right hand side of the assignment shall be assigned to the referenced element.

Uninitialized elements are permitted only in transient states (while the value remains invisible). Sending a **record of** or **set of** value with uninitialized elements shall cause an error.

NOTE 2: When using on the right hand side of an assignment for **record of-**s or **set of-**s, the assignment notation and the indexed notation have similar effect, with the exception that the assignment notation is able to address multiple elements in one notation, while the index notation is able to address a single element only.

EXAMPLE 3:

// Given

**type** **record of integer** MyRecordOf;

**type** **record** **of** MyRecordOf RoRoI;

**var integer** MyVar;

// Using the value list notation

**var** MyRecordOf MyRecordOfVar := { 0, 1, 2, 3, 4 };

// The same record of, defined with the assignment notation  
 **var** MyRecordOf MyRecordOfVarAssignment := {  
 [0] := 0,  
 [1] := 1,  
 [2] := 2,

[3] := 3,  
 [4] := 4

};

**var** RoRoI v\_recof;

// Using an index notation

MyVar := MyRecordOfVar[0]; // the first element of the "record of" value (integer 0)

// is assigned to MyVar

// Index notations are permitted on the left-hand side of assignments as well:

MyRecordOfVar[1] := MyVar; // MyVar is assigned to the second element

// value of MyRecordOfVar is { 0, 0, 2, 3, 4 }

// The assignment

MyRecordOfVar := { 0, 1, -, 2 };

// will change the value of MyRecordOfVar to{ 0, 1, 2 <unchanged>, 2};  
 // Note, that the 3rd element would be undefined if had no previous assigned value.

// The assignment

MyRecordOfVar[6] := 6;

// will change the value of MyRecordOfVar to

// { 0, 1, 2 , 2, <uninitialized>, <uninitialized>, 6 };  
 // Note the 5th and 6th elements (with indexes 4 and 5) had no assigned value before this

// last assignment and are therefore undefined.

MyRecordOfVar[4] := 4; MyRecordOfVar[5] := 5;

// will complete MyRecordOfVar to the fully defined value { 0, 1, 2 , 2, 4 , 5 , 6 };

// Expansion of uninitialized record of value:

v\_recof[1][2] := 0;

// after the assignment v\_recof is { <undefined>, { <undefined>, <undefined>, 0 } }

// Pls. Note the difference between the two index assignment notations the following example:

**var** MyRecordOf ix := { 0,1,2 }

ix := { [3] := 2\*ix[2]+1 }

// the value of ix is: { 0, 1, 2, 5 }

// The same result can be achieved by using an index notation on the left hand side of

// the assignment:

**var** MyRecordOf ix := { 0,1,2 }

ix[3] := 2\*ix[2]+1

// the value of ix is: { 0, 1, 2, 5 }

NOTE 3: The index notation makes it possible e.g. to copy **record of** values element by element in a for loop. For example, the function below reverses the elements of a **record of** value:

**function** reverse(**in** MyRecordOf src) **return** MyRecordOf  
 {  
 **var** MyRecordOf dest;  
 **var integer** i, srcLength := **lengthof** (src);  
 **for**(i := 0; i < srcLength; i := i + 1) {  
 dest[srcLength - 1 - i] := src[i];  
 }  
 **return** dest;  
 }

Embedded **record of** and **set of** types will result in a data structure similar to multidimensional arrays (see clause 6.2.7).

EXAMPLE 4:

// Given **type** **record of** **integer** MyBasicRecordOfType;  
 **type** **record of** MyBasicRecordOfTypeMy2DRecordOfType;

// Then, the variable myRecordOfArray will have similar attributes to a two-dimensional array:  
 **var** My2DRecordOfType myRecordOfArray;  
 // and reference to a particular element would look like this  
 // (value of the second element of the third 'MyBasicRecordOfType' construct)   
 myRecordOfArray [2][1] := 1;

//with

**var** **integer** i[2] := { 1, 2 };  
 myRecordOfArray [i] := 2;

// is the same as assigning element myRecordOfArray[i[0]][i[1]]

#### 6.2.3.1 Nested type definitions

TTCN‑3 supports the definition of the aggregated type nested with the **record** **of** or **set** **of** definition. Both the definition of new structured types (**record**, **set**, **enumerated**, **set** **of** and **record** **of**) and the specification of subtype constraints are possible.

EXAMPLE:

**type record of enumerated** { red, green, blue } ColorList;

**type record length** (10) **of record length** (10) **of integer** Matrix;

**type set of record** { **charstring** id, **charstring** val } GenericParameters;

#### 6.2.3.2 Referencing elements of record of and set of types

It is also allowed to reference the inner type of **record of** and **set of** types by using the index notation but with a dash. The notation *TypeId[-]*, where *TypeId* resolves to the name of a **record of** or **set of** type, references the inner type of *TypeId*. If the type definition restricts the element type of the **record of** or **set of** type, referencing the inner type of that type yields a type which contains all values from the constrained type.

EXAMPLE:

//Provided the definitions below

**type** **record** **of** **integer** MyRecordOfInt;

**type** **record** **of** **record** {

**integer** f1,

**set** { **integer** s1, **boolean** s2 } f2

} MyRecordOfRecord;

**type** **record** **of** **record** **of** **integer** MyRecordOfRecordOfInt;

**type** **record** **of** **record** {

**integer** f1,

**record** **of** **boolean** f2

} MyRecordOfRecord2;

// Referencing the inner integer type

**type** MyRecordOfInt[-] MyInteger;

**const** MyRecordOfInt[-] c\_MyInteger:= 5;

// Referencing the nested record type

**type** MyRecordOfRecord[-] MyInnerRecord;

**const** MyRecordOfRecord[-] c\_MyRecord := { f1 = 5; f2 := { s1 := 0; s2 := **true** }}

// Referencing the set type nested in the inner record

**type** MyRecordOfRecord[-].f2 MyNestedSet;

**const** MyRecordOfRecord[-].f2 c\_MySet := { s1 := 0; s2 := **true** }

// Referencing the innermost boolean

**type** MyRecordOfRecord[-].f2.s2 MyBoolean;

**const** MyRecordOfRecord[-].f2.s2 c\_MyBool := **false**;

// Referencing the inner record of

**type** MyRecordOfRecordOfInt[-] MyInnerRecordOfInt;

**const** MyRecordOfRecordOfInt[-] c\_MyInnerRecordOfInt := { 0, 1, 2, 3 };

// Referencing the integer type within the inner record of

**type** MyRecordOfRecordOfInt[-][-] MyInteger2;

**const** MyRecordOfRecordOfInt[-][-] c\_MyInteger2 := 1;

// Referencing the boolean type within the nested record

**type** MyRecordOfRecord2[-].f2[-] MyInnermostBoolean;

**const** MyRecordOfRecord2[-].f2[-] c\_MyInnermostBoolean := **true** ;

**type** **record length** (5) **of** **record of integer** ConstrainedRecordOfInt (1 .. 10);

**type** ConstrainedRecordOfInt[-] ConstrainedInt;

// defines the type record of integer, where the integer values are restricted

// to the range 1 .. 10 but the record of has no length restriction

### 6.2.4 Enumerated type and values

TTCN‑3 supports **enumerated** types. Enumerated types are used to model types that take only a distinct named set of values. Such distinct values are called enumerated values. Each enumerated value shall have an identifier. Operations on enumerated types shall only use these identifiers and are restricted to assignment, equivalence and ordering operators. The identifiers of enumerated values shall be unique within the enumerated type (but do not have to be globally unique) and are consequently visible in the context of the given type only. The identifiers of enumerated values shall only be reused within other structured type definitions and shall not be used for identifiers of local or global visibility at the same or a lower level of the same branch of the scope hierarchy (see scope hierarchy in clause 5.2).

EXAMPLE 1: Declaration of enumerated types and values

**type** **enumerated** MyFirstEnumType {

Monday, Tuesday, Wednesday, Thursday, Friday

};

**type** **integer** Monday;

// This definition does not clash with the previous one

// as Monday in MyFirstEnumType is of local scope

**type** **enumerated** MySecondEnumType {

Saturday, Sunday, Monday

};

// This definition is legal as it reuses the Monday identifier within

// a different enumerated type

**type** **record** MyRecordType {

**integer** Monday

};

// This definition is legal as it reuses the Monday identifier within

// a distinct structured type as identifier of a given field of this type

**type** **record** MyNewRecordType {

MyFirstEnumType firstField,

**integer** secondField

};

**var** MyNewRecordType newRecordValue := { Monday, 0 }

// MyFirstEnumType is implicitly referenced via the firstField element of MyNewRecordType

Each enumerated value may optionally have a user-assigned integer value, which is defined after the name of the enumerated value in parenthesis. Each user-assigned integer number shall be distinct within a single **enumerated** type. For each enumerated value without an assigned integer value, the system successively associates an integer number in the textual order of the enumerated values, starting at the left-hand side, beginning with zero, by step 1 and skipping any number occupied by any of the enumerated values with a manually assigned value. These values are only used by the system to allow the use of relational operators. The user shall not directly use associated integer values but can access them and convert integer values into enumerated values by using the predefined functions **enum2int** and **int2enum** (see clauses 16.1.2, C.1.30 and C.1.4).

NOTE 1: The integer value also may be used by the system to encode/decode enumerated values. This, however is outside the scope of the present document (with the exception that TTCN‑3 allows the association of encoding attributes to TTCN‑3 items).

For any instantiation or value reference of an **enumerated** type, the given type shall be implicitly or explicitly referenced.

NOTE 2: If the enumerated type is an element of a user defined structured type, the enumerated type is implicitly referenced via the given element (i.e. by the identifier of the element or the position of the value in a value list notation) at value assignment, instantiation, etc.

EXAMPLE 2: Using enumerated types (see also example 4 of clause 8.2.3.1)

// Valid instantiations of MyFirstEnumType and MySecondEnumType would be

**var** MyFirstEnumType Today := Tuesday;

**var** MySecondEnumType Tomorrow := Monday;

// The following statements however cause an error as the two variables are instances

// of different enumeration types

Today := Tomorrow;

Today == Tomorrow;

// The following operation is correct

**if** (Today == Monday ) {...}

// the type of variable Today identifies the type context of MyFirstEnumType for the

// equality operator

// But the following causes an error

**if** ( Tuesday == Wednesday ) {...}

// there is no TTCN-3 type(d) object to establish the type context for the equality operator

// Please note that the values Tuesday and Wednesday are defined within the type

// MyFirstEnumType only, but this is not sufficient to establish the type context

When a TTCN-3 module parameter, formal parameter, constant, variable, non-parameterized template or parameterized template with all formal parameters having default values of an imported enumerated type is defined, the name of that definition shall not be the same as any of the enumerated values of that type.

### 6.2.5 Unions

TTCN‑3 supports the **union** type. The **union** type is a collection of alternatives, each one identified by an identifier. Only one of the specified alternatives will ever be present in an actual union value. Union types are useful to model data which can take one of a finite number of known types.

EXAMPLE:

**type** **union** MyUnionType

{

**integer** number,

**charstring** string

};

// A valid instantiation of MyUnionType would be

**var** MyUnionType age, oneYearOlder;

**var integer** ageInMonths;

age.number := 34; // value notation by referencing the field. Note, that this   
 // notation makes the given field to be the chosen one

oneYearOlder := {number := age.number+1};

ageInMonths := age.number \* 12;

The assignment notation shall be used for **union**-s, and the notation shall assign a value to one field only. This field becomes the chosen field. Neither the not used symbol "-" nor **omit** is allowed in union value notations.

The value list notation shall not be used for setting values of **union** types.

#### 6.2.5.1 Referencing fields of a union type

Alternatives of a **union** type shall be referenced by the dot notation *TypeIdOrExpression.AlternativeId*, where *TypeIdOrExpression* resolves to the name of a union type or an expression of a union type such as variable, formal parameter, module parameter, constant, template, or function invocation. *AlternativeId* shall resolve to the name of an alternative in the union type. Alternatives of union type definitions shall not reference themselves. Alternatives of union type definitions shall not reference themselves.

EXAMPLE 1:

MyVar5 := MyUnion1.myChoice1;

// If a union type is nested in another type then the reference may look like this

MyVar6 := MyRecord1.myElement1.myChoice2;

// Note, that the union type, of which the field with the identifier 'myChoice2' is referenced,

// is embedded in a record type

If an alternative in a union type or a subtype of a union type is referenced by the dot notation, the resulting type is the set of values allowed for that alternative imposed by the constraints of the alternative declaration itself (i.e. any constraints applied to the union type itself are ignored).

When an alternative of a union type is referenced on the right hand side of an assignment an error shall occur if the referenced alternative is not the currently chosen alternative or if the referenced union field or value is omitted or uninitialized.

EXAMPLE 2:

**type** **union** MyUnion2

{

**integer** choice1,

**charstring** choice2

}

**type** **record** MyRecordEmbedsUnion

{

MyUnion2 field1 **optional**

}

...

**var** MyUnion2 v\_un2 := { choice1 := 1 }

**var** **charstring** v\_char := v\_un2.choice2; // causes an error as v\_un.choice2 is not chosen

**var** MyRecordEmbedsUnion v\_rec := { field1 := **omit** }

**var** **integer** v\_int := v\_rec.field1.choice1; // causes an error as v\_rec.field1 is omitted

When referencing an alternative of a union type on the left hand side of an assignment, the referenced alternative shall become the chosen one. This rule shall apply recursively if the reference contains alternatives of nested unions, choosing all the referenced alternatives.

When referencing an alternative of an uninitialized union value or field or omitted field (including omitting a field at a higher level of the embedding hierarchy) on the left hand side of an assignment, the reference shall recursively be expanded up to and including the depth of the referenced alternative as follows:

1. When expanding a value or value field of **union** type, the alternative referenced in the dot notation becomes the chosen one.
2. Expansion of **record**, **record of**, **set**, **set of**, and **array** values and intermediate fields shall follow the rules of item a) in clauses 6.2.1.1and 6.2.3, and clause 6.2.2.1 correspondingly.
3. At the end of the expansion, the value at the right hand side of the assignment shall be assigned to the referenced alternative.

EXAMPLE 3:

**type** **union** MyUnion3

{

**integer** choice1,

**union**

{

**bitstring** subchoice1,

**charstring** subchoice2

} choice2

}

...

**var** MyUnion3 v\_un3 := { choice1 := 1 }

**var** MyRecordEmbedsUnion v\_rec2 := { field1 := **omit** }

v\_un3.choice2.subchoice2 := "Hello!";

// after the assignment v\_un3 equals to { choice2 := { subchoice2 := "Hello!" } }

v\_rec2.field1.choice1 := 10; // after the assignment v\_rec2 equals to  
 // { field1 := { choice1 := 10 } }

#### 6.2.5.2 Option and union

Optional fields are not allowed for the **union** type, which means that the **optional** keyword shall not be used with **union** types.

#### 6.2.5.3 Nested type definition for field types

TTCN‑3 supports the definition of types for union alternatives nested within the union definition, similar to the mechanism for record types described in clause 6.2.1.3.

### 6.2.6 The anytype

The special type **anytype** is defined as a shorthand for the union of all known data types and the address type in a TTCN‑3 module. The definition of the term known types is given in clause 3.1, i.e. the anytype shall comprise all the known data types but not the port, component, and default types. The address type shall be included if it has been explicitly defined within that module.

The fieldnames of the **anytype** shall be uniquely identified by the corresponding type names.

NOTE 1: As a result of this requirement imported types with clashing names (either with an identifier of a definition in the importing module or with an identifier imported from a third module) cannot be reached via the anytype of the importing module.

EXAMPLE:

// A valid usage of anytype would be

**var** **anytype** MyVarOne, MyVarTwo;

**var integer** MyVarThree;

MyVarOne.**integer** := 34;

MyVarTwo := {**integer** := MyVarOne.integer + 1};

MyVarThree := MyVarOne.integer \* 12;

The **anytype** is defined locally for each module and (like the other predefined types) cannot be directly imported by another module. However, a user defined type of the type **anytype** can be imported by another module. The effect of this is that all types of that module are imported.

NOTE 2: The user-defined type of **anytype** "contains" all types imported into the module where it is declared. Importing such a user-defined type into a module may cause side effects and hence due caution should be given to such cases.

### 6.2.7 Arrays

Arrays can be used in TTCN-3 as a shorthand notation to specify record of types. They may be specified also at the point of a variable declaration. Arrays may be declared as single or multi-dimensional. Array dimensions shall be specified using constant expressions, which shall evaluate to a positive **integer** values. Constants used in the constant expressions shall meet with the restrictions in clause 10.

EXAMPLE 1:

**type integer** MyArrayType1[3]; // A type with 3 integer elements

**type** **record** **length** (3) **of** **integer** MyRecordOfType1; // The corresponding record of

**var** MyArrayType1 a1:= { 7, 8, 9 };

**var** MyRecordOfType1 r1:= a1; // MyArrayType1 and MyRecordOfType1 are compatible

**var** **integer** myArray1[3]:= r1; // Instantiates an integer array of 3 elements

// with the index 0 to 2

// being compatible to MyArrayType1 and MyRecordOfType1

**var** **integer** myArray2[2][3]; // Instantiates a two-dimensional integer array of 2 × 3 elements // with indexes from (0,0) to (1,2)

Array elements are accessed by means of the index notation ([]), which shall specify a valid index within the array's range. Individual elements of multi-dimensional arrays can be accessed by repeated use of the index notation. An array or record of integer restricted to a single size can be used in the index notation as a short-hand for the repeated index notation. Accessing elements outside the array's range will cause a compile-time or test case error.

EXAMPLE 2:

MyArray1[1] := 5;  
 MyArray2[1][2] := 12;

MyArray1[4] := 12; // ERROR: index shall be between 0 and 2  
 MyArray2[3][2] := 15; // ERROR: first index shall be 0 or 1

Array dimensions may also be specified using ranges (with inclusive boundaries only). In such cases, the lower and upper values of the range define the lower and upper index values. Such an array is corresponding to a record of with a fixed length restriction computed as the difference between upper and lower index bound plus 1 and indexing starting from the lower bound of the array definition.

EXAMPLE 3:

**type integer** MyArrayType2[2 .. 5]; // A type with 4 integer elements, indices starting with 2

**type** **record** **length** (4) **of** **integer** MyRecordOfType2; // The corresponding record of

**var** **integer** MyArray3[1 .. 5]; // Instantiates an integer array of 5 elements

// with the index 1 to 5

MyArray3[1] := 10; // Lowest index

MyArray3[5] := 50; // Highest index

**var** **integer** MyArray4[1 .. 5][2 .. 3 ]; // Instantiates a two-dimensional integer array of  
 // 5 × 2 elements with indexes from (1,2) to (5,3)

NOTE: It is not possible to define an array type with a variable amount of elements. Neither is it possible to define an unlimited array with a lower bound on the array index.

The values of array elements shall be compatible with the corresponding variable or type declaration. Values may be assigned individually by a value list notation or index notation or more than one or all at once by a value list notation or index assignment notation. When the value list notation is used, the first value of the list is assigned to the first element of the array (the element with index 0 or the lower bound if an index range has been given), the second value to the next element, etc. Elements to be left out from the assignment shall be explicitly skipped in the list by using dash. For using the assignment notation for arrays, the rules described in 6.2.3 are valid for arrays as well.

Index notation can be used on both the right-hand side and left-hand side of assignments. The index of the first element shall be zero or the lower bound if an index range has been given. The index shall not exceed the limitations given by either the length or the upper bound of the index. If the value of the element indicated by the index at the right‑hand of an assignment is undefined or if the index notation is applied to an uninitialized or omitted array value on the right hand side of an assignment, error shall be caused. Sending an array value with undefined elements shall cause an error. All elements in an array value that are not set explicitly are undefined. When referencing an element of an uninitialized array value or field or omitted field on the left hand side of an assignment, the rules for record of values specified in 6.2.3 apply.

For assigning values to multi-dimensional arrays, each dimension that is assigned shall resolve to a set of values enclosed in curly braces. When specifying values for multi-dimensional arrays, the leftmost dimension corresponds to the outermost structure of the value, and the rightmost dimension to the innermost structure. The use of array slices of multi-dimensional arrays, i.e. when the number of indexes of the array value is less than the number of dimensions in the corresponding array definition, is allowed. Indexes of array slices shall correspond to the dimensions of the array definition from left to right (i.e. the first index of the slice corresponds to the first dimension of the definition). Slice indexes shall conform to the related array definition dimensions.

EXAMPLE 4:

MyArray1[0]:= 10;

MyArray1[1]:= 20;

MyArray1[3]:= 30;

// or using an value list

MyArray1:= {10, 20, **-**, 30};

MyArray4:= {{1, 2}, {3, 4}, {5, 6}, {7, 8}, {9, 10}};

// the array value is completely defined

**var** **integer** MyArray5[2][3][4] :=

{  
 {  
 {1, 2, 3, 4}, // assigns a value to MyArray5 slice [0][0]  
 {5, 6, 7, 8}, // assigns a value to MyArray5 slice [0][1]  
 {9, 10, 11, 12} // assigns a value to MyArray5 slice [0][2]  
 }, // end assignments to MyArray5 slice [0]   
 {  
 {13, 14, 15, 16}, {17, 18, 19, 20}, {21, 22, 23, 24}

} // assigns a value to MyArray5 slice [1]

};

MyArray4[2] := {20, 20};

// yields {{1, 2}, {3, 4}, {20, 20}, {7, 8}, {9, 10}};  
 MyArray5[1] := { {0, 0, 0, 0}, {0, 0, 0, 0}, {0, 0, 0, 0}};  
 // yields {{{1, 2, 3, 4}, {5, 6, 7, 8}, {9, 10, 11, 12}},  
 // {{0, 0, 0, 0}, {0, 0, 0, 0}, {0, 0, 0, 0}}};

MyArray5[0][2] := {3, 3, 3, 3};

// yields {{{1, 2, 3, 4}, {5, 6, 7, 8}, {3, 3, 3, 3}},

// {{0, 0, 0, 0}, {0, 0, 0, 0}, {0, 0, 0, 0}}};

**var integer** MyArrayInvalid[2][2];

MyArrayInvalid := { 1, 2, 3, 4 }

// causes an error as the dimension of the value notation

// does not correspond to the dimensions of the definition

MyArrayInvalid[2] := { 1, 2 }

// causes an error as the index of the slice should be 0 or 1

### 6.2.8 The default type

TTCN‑3 allows the activation of altsteps (see clause 16.2) as defaults to capture recurring behaviour. Default references are unique references to activated defaults. Such a unique default reference is generated by a test component when an altstep is activated as a default, i.e. a default reference is the result of an **activate** operation (see clause 20.5.2).

Default references have the special and predefined type **default**. Variables of type **default** can be used to handle activated defaults in test components. The special value **null** represents an unspecific default reference, e.g. can be used for the initialization of variables of default type.

Default references are used in **deactivate** operations (see clause 20.5.3) in order to identify the default to be deactivated.

Default references have meaning only within the test component instances they are activated, i.e. a default reference assigned to a default variable in test component instance "a1" of type "A" has no meaning in test component instance "a2" of type "A".

The actual data representation of the **default** type shall be resolved externally by the test system. This allows abstract test cases to be specified independently of any real TTCN‑3 runtime environment, in other words TTCN‑3 does not restrict the implementation of a test system with respect to the handling and identification of defaults.

### 6.2.9 Communication port types

Ports facilitate communication between test components and between test components and the test system interface.

TTCN‑3 supports message-based and procedure-based ports. Each port shall be defined as being message-based or procedure-based. Message-based ports shall be identified by the keyword **message** and procedure-based ports shall be identified by the keyword **procedure** within the associated port type definition.

Ports are bidirectional. The directions are specified by the keywords **in** (for the in direction), **out** (for the out direction) and **inout** (for both directions). Directions shall be seen from the point of view of the test component owning the port with the exception of the test system interface, where **in** identifies the direction of message sending or procedure call and **out** identifies the direction of message receive, get reply or catch exception from the point of view of the test component connected to the test system interface port.

Each port type definition shall have one or more lists indicating the allowed collection of (message) types or procedure signatures together with the allowed communication direction.

For configuration purposes the port type may have one **map** **param** and one **unmap param** declaration indicating the allowed additional parameters for the respective operation. These formal parameters shall be value parameters.

Whenever a signature (see also clause 14) is defined in the **out** direction of a procedure-based port, the types of all its **inout** and **out** parameters, its return type and its exception types are automatically part of the **in** direction of this port. Whenever a signature is defined in the **in** direction for a procedure-based port, the types of all its **inout** and **out** parameters, its return type and its exception types are automatically part of the **out** direction of this port.

Ports used for the communication with the SUT may need to address specific entities within the SUT. In addition, several address schemes may be supported by one SUT at different ports. To support such addressing schemes, TTCN-3 allows to bind an **address** type to a port. Values of this type may be used for addressing purposes in communication operations (see clause 22.1) and be stored in variables. The handling of address types bound to different ports by means of the dot notation is explained in clause 6.2.12.

***Syntactical Structure***

Message-based port:

**type** **port** *PortTypeIdentifier* **message** "{"

{ (**address** *Type* ";") |

(**map** **param** "(" { *FormalValuePar* [","] }+ ")") |

(**unmap** **param** "(" { *FormalValuePar* [","] }+ ")") |

((**in** | **out** | **inout**) { *MessageType* [ "," ] }+ ";") }

"}"

Procedure-based port:

**type** **port** *PortTypeIdentifier* **procedure** "{"

{ (**address** *Type* ";" ) |

(**map** **param** "(" { *FormalValuePar* [","] }+ ")") |

(**unmap** **param** "(" { *FormalValuePar* [","] }+ ")") |

((**in** | **out** | **inout**) { *Signature* [ "," ] }+ ";") }

"}"

***Restrictions***

In addition to the general static rules of TTCN‑3 given in clause 5, the following restrictions apply:

a) At most one address type should be bound to a port type.

b) At most one map parameter list should be defined for a port type.

c) At most one unmap parameter list should be defined for a port type.

d) Formal parameters of **map param** and **unmap param** declarations shall be value parameters and not be of **port**, **component**, **timer** or **default** type or of structured types having fields of **port**, **component**, **timer** or **default** type.

e) *MessageType* shall be a data type as defined in section 3.1.

***Examples***

EXAMPLE 1: Message-based port

// Message-based port which allows types MsgType1 and MsgType2 to be received at, MsgType3 to be

// sent via and any integer value to be send and received over the port

**type** **port** MyMessagePortTypeOne **message**

{

**in** MsgType1, MsgType2;

**out** MsgType3;

**inout integer**

}

EXAMPLE 2: Procedure-based port

// Procedure-based port which allows the remote call of the procedures Proc1, Proc2 and Proc3.

// Note that Proc1, Proc2 and Proc3 are defined as signatures

**type** **port** MyProcedurePortType **procedure**

{

**out** Proc1, Proc2, Proc3

}

EXAMPLE 3: Message-based port with address type definition

**type** **port** MyMessagePortTypeTwo **message**

{

**address integer**; // if addressing is used on ports of type MyMessagePortTypeTwo

// the addresses have to be of type integer

**inout** MsgType1, MsgType2;

}

NOTE: The term message is used to mean both messages as defined by templates and actual values resulting from expressions. Thus, the list restricting what may be used on a message-based port is simply a list of type names.

EXAMPLE 4: Usage of param in port declaration

// Message based port which allows MsgType4 to be send and received over the port

// and MsgType5 and MsgType6 as configuration parameter type

**type** **port** MyMessagePortType **message**

{

**inout** MsgType4;

**map** **param** (**in** MsgType5 p1, **out** MsgType6 p2);

}

// Procedure based port which allows the remote call of the procedure Proc1

// and MsgType5 as configuration parameter type

**type** **port** MyProcedurePortType **procedure**

{

**out** Proc1;

**unmap** **param** (MsgType5 p1);

}

### 6.2.10 Component types

#### 6.2.10.1 Component type definition

The component type defines which ports are associated with a component (see figure 3). The port names in a component type definition are local to that component type, i.e. another component type may have ports with the same names. Port names in the same component type definition shall all have unique names.



Figure 3: Typical components

It is also possible to declare constants, variables, templates and timers local to a particular component type. These declarations are visible to all testcases, functions and altsteps that run on an instance of the given component type. This shall be explicitly stated using the **runs** **on** keyword (see clause 16) in the testcase, function or altstep header. Component type definitions are associated with the component instance and follow the scope rules defined in clause 5.2. Each new instance of a component type will thus have its own set of constants, variables, templates and timers as specified in the component type definition (including any initial values, if stated). Constants used in the constant expressions of type declarations for variables, constants or ports shall meet with the restrictions in clause 10, however constants used in the constant expressions of initial values for variables, constants, templates or timers do not have to obey these restrictions.

***Syntactical Structure***

**type** **component** *ComponentTypeIdentifier* "{"

{ ( *PortInstance*

| *VarInstance*

| *TimerInstance*

| *ConstDef*

| *TemplateDef* ) }

"}"

***Semantic Description***

Component type definitions specify the creation, declaration and initialization of ports and component constants, variables, templates and timers during the creation of an instance of a component type. These instances can be used as the main test component, as the test system interface or as a parallel test component. Every instance of a component type has its own fresh copy of the port, constant, variable, template and timer instances defined in the component type definition.

***Restrictions***

No specific restrictions in addition to the general static rules of TTCN‑3 given in clause 5.

***Examples***

EXAMPLE 1: Component type with port instances only

**type component** MyPTCType

{

**port** MyMessagePortType PCO1, PCO4;

**port** MyProcedurePortType PCO2;

**port** MyAllMesssagesPortType PCO3

}

EXAMPLE 2: Component type with variable, timer and port instance

**type component** MyMTCType

{

**var** integer MyLocalInteger;

**timer** MyLocalTimer;

**port** MyMessagePortType PCO1

}

EXAMPLE 3: Component type with port instance arrays

**type component** MyCompType

{

**port** MyMessageInterfaceType PCO[3]

**port** MyProcedureInterfaceType PCOm[3][3]

// Defines a component type which has an array of 3 message ports and a two‑dimensional

// array of 9 procedure ports.

}

#### 6.2.10.2 Reuse of component types

It is possible to define component types as the extension of other component types, using the **extends** keyword.

***Syntactical Structure***

**type** **component** *ComponentTypeIdentifier* **extends** *ComponentTypeIdentifier*   
 { "," ComponentTypeIdentifier} "{"

{ ( *PortInstance*

| *VarInstance*

| *TimerInstance*

| *ConstDef*

| *TemplateDef* ) }

"}"

***Semantic Description***

In such a definition, the new type definition is referred to as the *extended type*, and the type definition following the **extends** keyword is referred to as the *parent type*. The effect of this definition is that the extended type will implicitly also contain all definitions from the parent type. It is called the *effective type definition*.

It is allowed to have one component type extending several parent types in one definition, which have to be specified as a comma-separated list of types in the definition. Any of the parent types may also be defined by means of extension. The effective component type definition of the extended type is obtained as the collection of all constant, variable, template, timer and port definitions contributed by the parent types (determined recursively if a parent type is also defined by means of an extension) and the definitions declared in the extended type directly. The effective component type definition shall be name clash free.

NOTE 1: It is not considered to be a different declaration and hence causes no error if a specific definition is contributed to the extended type by different parent types (via different extension paths).

The semantics of component types with extensions are defined by simply replacing each component type definition by its effective component type definition as a pre-processing step prior to using it.

NOTE 2: For component type compatibility, this means that a component reference c of type CT1, which extends CT2, is compatible with CT2, and test cases, functions and altsteps specifying CT2 in their **runs on** clauses can be executed on c (see clause 6.3.3).

***Restrictions***

In addition to the general static rules of TTCN‑3 given in clause 5, the following restrictions apply:

a) When defining component types by extension, there shall be no name clash between the definitions being taken from the parent type and the definitions being added in the extended type, i.e. there shall not be a port, variable, constant or timer identifier that is declared both in the parent type (directly or by means of extension) and the extended type. It is not considered to be a name clash if a specific definition is contributed to the extended type via different extension paths.

b) When defining component types by extending more than one parent type, there shall be no name clash between the definitions of the different parent types, i.e. there shall not be a port, variable, constant or timer identifier that is declared in any two of the parent types (directly or by means of extension). It is not considered to be a name clash if a specific definition is contributed to the extended type via different extension paths.

c) It is allowed to extend component types that are defined by means of extension, as long as no cyclic chain of definition is created.

***Examples***

EXAMPLE 1: A component type extension and its effective type definition

**type** **component** MyMTCType

{

**var** integer MyLocalInteger;

**timer** MyLocalTimer;

**port** MyMessagePortType PCO1

}

**type** **component** MyExtendedMTCType **extends** MyMTCType

{

**var** **float** MyLocalFloat;

**timer** MyOtherLocalTimer;

**port** MyMessagePortType PCO2;

}

// effectively, the above definition is equivalent to this one:

**type component** MyExtendedMTCType

{

/\* the definitions from MyMTCType \*/

**var** integer MyLocalInteger;

**timer** MyLocalTimer;

**port** MyMessagePortType PCO1

/\* the additional definitions \*/

**var** float MyLocalFloat;

**timer** MyOtherLocalTimer;

**port** MyMessagePortType PCO2;

}

EXAMPLE 2: A component type extension chain and forbidden cyclic extensions

**type component** MTCTypeA **extends** MTCTypeB { /\* … \*/ };  
 **type component** MTCTypeB **extends** MTCTypeC { /\* … \*/ };  
 **type component** MTCTypeC **extends** MTCTypeA { /\* … \*/ }; // ERROR - cyclic extension

**type** **component** MTCTypeD **extends** MTCTypeD { /\* … \*/ }; // ERROR - cyclic extension

EXAMPLE 3: Component type extensions with name clashes

**type component** MyExtendedMTCType **extends** MyMTCType

{

**var** **integer** MyLocalInteger; // ERROR - already defined in MyMTCType (see above)

**var float** MyLocalTimer; // ERROR - timer with that name exists in MyMTCType

**port** MyOtherMessagePortType PCO1; // ERROR - port with that name exists in MyMTCType

}  
  
 **type component** MyBaseComponent { **timer** MyLocalTimer };  
 **type component** MyInterimComponent **extends** MyBaseComponent { **timer** MyOtherTimer };

**type component** MyExtendedComponent **extends** MyInterimComponent

{

**timer** MyLocalTimer; // ERROR - already defined in MyInterimComponent via extension

}

EXAMPLE 4: Component type extension from several parent types

**type component** MyCompB { **timer** T };

**type component** MyCompC { **var integer** T };

**type component** MyCompD **extends** MyCompB, MyCompC {}

// ERROR - name clash between MyCompB and MyCompC

// MyCompB is defined above

**type component** MyCompE **extends** MyCompB {

**var integer** MyVar1 := 10;

}

**type component** MyCompF **extends** MyCompB {

**var float** MyVar2 := 1.0;

}

**type component** MyCompG **extends** MyCompB, MyCompE, MyCompF {

// No name clash.

// All three parent types of MyCompG have a timer T, either directly or via extension of

// MyCompB; as all these stem (directly or via extension) from timer T declared in MyCompB,

// which make this form of collision legal.

/\* additional definitions here \*/

}

### 6.2.11 Component references

Component references are unique references to the test components created during the execution of a test case.

***Syntactical Structure***

**system** | **mtc** | **self** | *VariableRef | FunctionInstance*

***Semantic Description***

A unique component reference is generated by the test system at the time when a component is created. It is the result of a **create** operation (see clause 21.2.1). In addition, component references are returned by the predefined operations **system** (returns the component reference of the test system interface, which is automatically created when testcase execution is started), **mtc** (returns the component reference of the MTC, which is automatically created when testcase execution started) and **self** (returns the component reference of the component in which **self** is called).

Component references are used in the configuration operations such as **connect**, **map** and **start** (see clause 21) to set-up test configurations and in the **from**, **to** and **sender** parts of communication operations of ports connected to test components other than the test systeminterface for addressing purposes (see clause 22 and figure 6).

In addition, the special value **null** is available to indicate an undefined component reference, e.g. for the initialization of variables to handle component references.

The actual data representation of component references shall be resolved externally by the test system. This allows abstract test cases to be specified independently of any real TTCN‑3 runtime environment, in other words TTCN‑3 does not restrict the implementation of a test system with respect to the handling and identification of test components.

A component reference includes component type information. This means, for example, that a variable for handling component references shall use the corresponding component type name in its declaration.

The configuration operations (see clause 21) do not work directly on arrays of components. Instead a specific element of the array shall be provided as the parameter to these operations. For components, the effect of an array is achieved by using an array of component references and assigning the relevant array element to the result of the **create** operation.

***Restrictions***

In addition to the general static rules of TTCN‑3 given in clause 5, the following restrictions apply:

a) The only operations allowed on component references are assignment, equality and non-equality.

b) The variable associated with *VariableRef* (being a component type variable, a component type parameter, etc.) or the return type associated with *FunctionInstance* shall be of component type.

***Examples***

EXAMPLE 1: Component references with component type variables

// A component type definition

**type component** MyCompType {

**port** PortTypeOne PCO1;

**port** PortTypeTwo PCO2

}

// Declaring one variable for the handling of references to components of type MyCompType

// and creating a component of this type

**var** MyCompType MyCompInst := MyCompType.**create**;

EXAMPLE 2: Usage of component references in configuration operations

// referring to the component created above

**connect**(**self**:MyPCO1, MyCompInst:PCO1);

**map**(MyCompInst:PCO2, **system**:ExtPCO1);

MyCompInst.**start**(MyBehavior(**self**)); // self is passed as a parameter to MyBehavior

EXAMPLE 3: Usage of component references in from- and to- clauses

MyPCO1.**receive from** MyCompInst;

:

MyPCO2.**receive**(**integer**:?) -> **sender** MyCompInst;

:

MyPCO1.**receive**(MyTemplate) **from** MyCompInst;

:

MyPCO2.**send**(**integer**:5) **to** MyCompInst;

EXAMPLE 4: Usage of component references in one-to-many connections

// The following example explains the case of a one-to-many connection at a Port PCO1

// where values of type M1 can be received from several components of the different types

// CompType1, CompType2 and CompType3 and where the sender has to be retrieved.

// In this case the following scheme may be used:

:

**var** M1 MyMessage, MyResult;

**var** MyCompType1 MyInst1 := **null**;

**var** MyCompType2 MyInst2 := **null**;

**var** MyCompType3 MyInst3 := **null**;

:

**alt** {

[] PCO1.**receive**(M1:?) **from** MyInst1 -> **value** MyMessage **sender** MyInst1 {}

[] PCO1.**receive**(M1:?) **from** MyInst2 -> **value** MyMessage **sender** MyInst2 {}

[] PCO1.**receive**(M1:?) **from** MyInst3 -> **value** MyMessage **sender** MyInst3 {}

}

:

MyResult := MyMessageHandling(MyMessage); // some result is retrieved from a function

:

**if** (MyInst1 != **null**) {PCO1.**send**(MyResult) **to** MyInst1};

**if** (MyInst2 != **null**) {PCO1.**send**(MyResult) **to** MyInst2};

**if** (MyInst3 != **null**) {PCO1.**send**(MyResult) **to** MyInst3};

:

EXAMPLE 5: Usage of self

**var** MyComponentType MyAddress;

MyAddress := **self**; // Store the current component reference

EXAMPLE 6: Usage of component arrays

// This example shows how to model the effect of creating, connecting and running arrays of

// components using a loop and by storing the created component reference in an array of

// component references.

**testcase** MyTestCase() **runs on** MyMtcType **system** MyTestSystemInterface

{

:

**var integer** i;

**var** MyPTCType1 MyPtc[11];

:

**for** (i:= 0; i<=10; i:=i+1)

{

MyPtc[i] := MyPTCType1.**create**;

**connect**(**self**:PtcCoordination, MyPtc[i]:MtcCoordination);

MyPtc[i].**start**(MyPtcBehaviour());

}

:

}

### 6.2.12 Addressing entities inside the SUT

An SUT may consist of several entities which can be addressed individually. The global **address** data type may be used if only one data type is needed. If several data types at different ports are needed for addressing SUT entities, the type used for addressing via a port instance shall be declared in the corresponding port type definition.

***Syntactical Structure***

*TemplateInstance*

***Semantic Description***

The actual data representation of the global **address** type is resolved either by an explicit global address type definition within the test suite, address type definitions within port definitions, or externally by the test system (i.e. the **address** type is left as an open type within the TTCN‑3 specification). This allows abstract test cases to be specified independently of any real address mechanism specific to the SUT.

If an **address** type is bound to a port type definition, addressing of SUT instances (i.e. **to**- and **from**-directives in communication operations) via instances of that port type shall be restricted to values of the bound **address** type.

If several address types exist within a test suite, ambiguities shall be resolved by means of the dot notation. For example, a type reference within a variable definition used to store an SUT address may be prefixed by a port type identifier or a module identifier. If both a global address type definition and port definitions with an address type definition exist in a module, the global address type shall only affect ports without an explicit address type definition. The consistent use of explicit address type definitions within port definitions is recommended over the use of global address type definitions.

Explicit SUT addresses for a globally defined address type shall only be generated inside a TTCN‑3 module if the type is defined inside the module itself. If the type is not defined inside the module, explicit SUT addresses for a global address type shall only be passed in as parameters or be received in message fields or as parameters of remote procedure calls.

In addition, the special value **null** is available for the **address** type to indicate an undefined address, e.g. for the initialization of variables of the address type.

If a port type definition includes the declaration of a type that shall be used for addressing SUT entities, only values of that type shall be used in **to**, **from** and **sender** parts of receive and send operations of port instances of that type mapped to the test system interface.

***Restrictions***

In addition to the general static rules of TTCN‑3 given in clause 5, the following restrictions apply:

a) *TemplateInstance* shall be of type **address** or of the type of the address declaration in a port type definition. If *TemplateInstance* is of type **address**, it and can be an address type value, an address type variable, etc.

b) For addressing purposes, the **address** data type shall only be used in the **to**, **from** and **sender** parts of receive and send operations of ports mapped to the test system interface.

c) The **address** data type shall not be used in the **to**, **from** and **sender** parts of receive and send operations of connected ports, i.e, ports used for the communication among test components.

***Examples***

EXAMPLE 1: Global address type

// Associates the type integer to the open type address

**type integer address**;

:

// new address variable initialized with null

**var address** MySUTentity := **null**;

:

// receiving an address value and assigning it to variable MySUTentity

PCO.**receive**(**address**:?) -> **value** MySUTentity;

:

// usage of the received address for sending template MyResult

PCO.**send**(MyResult) **to** MySUTentity;

:

// usage of the received address for receiving a confirmation template

PCO.**receive**(MyConfirmation) **from** MySUTentity;

EXAMPLE 2: Port type-specific address type

**type** record MyAddressType { // user-defined type

integer field1;

boolean field2;

}

**type** **port** MyPortType **message** {

**address** MyAddressType; // address declaration

**inout** **integer**;

}

**type component** MyComponentType

{

**port** MyPortType PCO;

}

**function myFunction () runs on MyComponentType {**

**var** MyAddressType SUT\_Address := { 5, **true**}; // address value for addressing via ports

// of MyPortType

:

PCO.**send**(**integer:** 5) **to** SUT\_Address; // use of address value in to

:

PCO**.receive**(**integer:** ?)from **SUT\_Address**; // use of address value in from

:

}

EXAMPLE 3: Elaborated address example

**type** AddressType1 **address**; // address type definition on module level

**type** **port** MyPortType1 **message** {

**inout** MsgType1;

}

// address types bound to port types

**type** **port** MyPortType2 **message** {

**address** AddressType2; // values of type AddressType2 can be

// used to address SUT entities.

**inout** MsgType2;

}

**type** **port** MyMessagePort3 **message** {

**address** AddressType3; // values of type AddressType3 can be

// used to address SUT entities.

**inout** MsgType3;

}

// component type definition

**type component** MyComponentType

{

**port** MyPortType1 PCO1;

**port** MyPortType2 PCO2;

**port** MyPortType3 PCO3

}

// The following behaviour is considered to be executed on an instance of MyComponentType.

// Furthermore, it is considered that the ports PCO1, PCO2 and PCO3 are mapped ports, i.e.

// used for the communication with the SUT.

:

// new address variable initialized with null

**var address** MySUTentity1 := **null**; // type of MySUTentity1 is AddressType1

**var** MyPortType2.**address** MySUTentity2 := **null**; // type of MySUTentity2 is AddressType2

**var** MyPortType3.**address** MySUTentity3 := **null**; // type of MySUTentity3 is AddressType3

:

// receiving an address values and assigning them to variables

PCO1.**receive**(MsgType1:?) **from** **address**:? -> sender MySUTentity1;

// Address type of module scope,

// no prefix needed

PCO2.**receive**(MsgType2:?) **from** MyPortType2.**address**:? -> **sender** MySUTentity2;

// Resolution of address type

// by means of a prefix

PCO3.**receive**(MsgType3:?) **from** MyPortType3.**address**:? -> **sender** MySUTentity3;

:

// usage of the received address values for addressing purposes

PCO1.**send**(MyResult) **to** MySUTentity1;

:

PCO2.**receive**(MyConfirmation) **from** MySUTentity2;

:

PCO3.**send**(MyRequest) **to** MySUTentity3;

:

### 6.2.13 Subtyping of structured types

TTCN-3 allows subtyping of structured types as given in table 3.

#### 6.2.13.1 Length subtyping of record ofs and set ofs

TTCN-3 permits constraining the number of elements in instances of **record of** and **set of** types.

The **length** keyword followed by a value or a range (with inclusive boundaries only) within brackets and used between the **record** or **set** and the **of** keywords, restricts the allowed lengths of the given **record of** or **set of** type. The value or the bounds within the brackets shall be non-negative integer values, except when the **infinity** keyword is used at the place of the upper bound, in which case the maximum number of the elements is not constrained.

Record of and set of type definitions may be used to define new **record of** or **set of** subtypes. In this case the rules of the previous paragraph apply, except that the **length** keyword and the value or range defining the allowed number of iterations (within brackets) shall be placed following the identifier of the new type.

Constants used in the constant expressions of length subtyping shall meet with the restrictions in clause 10.

EXAMPLE 1: Length restrictions of record of and set of types

**type** **record length**(10) **of** **integer** MyRecordOfType10;

// is a record of exactly 10 integers

**type** **record length**(0..10) **of** **integer** MyRecordOfType0\_10;

// is a record of a maximum of 10 integers

**type** **record length**(10..**infinity**) **of** **integer** MyRecordOfType10up;

// record of at least 10 integers

**type** **record length**(0..**infinity**) **of** **integer** MyRecordOfType0up;

// an unrestricted record of integer type

EXAMPLE 2: Length subtyping of referenced record of types

**type** **record** **of** **charstring** StringArray;

// is an unlimited record of, each element shall be a charstring

**type** StringArray StringArray34 **length**(4 .. 5);

// is a record of 4 or 5 elements, each element is a charstring

// it is equivalent to

// **type** **record** **length**(4 .. 5) **of** **charstring** StringArray34a;

**type** StringArray34 StringArray34again **length**(4 .. 5);

// the same as StringArray34

**type** StringArray34 StringArray6 **length**(6);

// causes an error as record ofs with 6 elements are not legal values of StringArray34

EXAMPLE 3: Length subtyping of referenced set of types

**type record** MyCapsule{

**set of integer** mySetOfInt

}

**type** MyCapsule.mySetOfInt MySetOfIntSub **length**(5..10);

// unordered list of 5 to 10 integers

#### 6.2.13.2 List subtyping of structured types and anytype

List subtyping is possible when defining a new type based on an existing parent type, but not directly at the declaration of the first parent type (see table 3).

Subtypes defined by a list subtyping restrict the allowed values of the subtype to the values matched by at least one of the constraints in the list. In case of list subtyping of **record**, **set**, **record of**, **set of**, **union** and **anytype** types, the list may contain both subtypes and possibly partial templates of the parent types. Subtype references shall be resolved in a recursive way: the collection of templates denoted by the subtype(s) referenced in the list become members of the new subtype definition with an expanded list containing only possibly partial templates. When constraining **record of**, **set of**, **union** and **anytype** types, all templates of the expanded list (i.e. after resolving the subtype references) shall be valid (i.e. complete) templates of the first parent type. When constraining **record** and **set** types, templates of the expanded list defined using the value list notation shall be valid (i.e. complete) templates, while templates of the expanded list defined using the field assignment notation may be partial (i.e. incomplete). In the latter case, the fields that are not explicitly present shall be considered as containing *AnyValue* for mandatory fields and *AnyValueOrNone* for optional fields.

NOTE: Users should assign new values to single fields of values/templates based on types using list subtyping cautiously: it may happen that the new field value would be valid with other combination(s) of the rest of the fields but causes an erroneous record/set value, when combining with the actual values of the other fields. See example below.

In case of **enumerated** types, the template list subtyping shall contain only values of the parent type.

EXAMPLE 1: List subtyping of record types

**type** **record** MyRecord {

integer f1 **optional**,

charstring f2,

charstring f3

}

**type** MyRecord MyRecordSub1 (

{ f1 **:= omit**, f2 **:=** "user"**,** f3 **:=** "password" }**,**

{ f1 **:=** 1, f2 **:=** "User", f3 **:=** "Password" }

) // a valid subtype of MyRecord containing 2 values

**type** MyRecord MyRecordSub2 (

MyRecordSub1,

{ f1 := 2, f2 := "uname", f3 := "pswd" },

{f1 := 3, f2 := "Uname", f3 := "Pswd" }

) // a valid subtype of MyRecord, containing 4 values; notice that values of

// MyRecordSub1 are identified by referencing MyRecordSub1

**type** MyRecordSub1 MyRecordSub3 (

{f1 := 1, f2 := "user", f3 := "password" },

{ f1 := 1, f2 := "User", f3 := "Password" }

) // invalid type as { f1 := 1, f2 := "user", f3 := "password" } is not a legal value of

// MyRecordSub1 (notice field f1)

**type** MyRecord MyRecordSub4 (

{f2 := "user", f3 := "password" },

{ f2 := "User", f3 := "Password" }

) // any valid value of MyRecord, where the combination of f2 and f3 is  
 // f2 := "user" AND f3 := "password" or f2 := "User" AND f3 := "Password"

// i.e. field f1 is considered as if it was present and contained *AnyValueOrNone*

**type** MyRecord MyRecordSub5 (

{f2 := "user", f3 := pattern "password|Password" },

{ f1 := (1 .. 10), f2 := "User" }

) // a valid subtype of MyRecord containing all values which match one of the given

// templates

// { f1 := \*, f2 := "user", f3 := pattern "password|Password" } or

// { f1 := (1 .. 10), f2 := "User", f3 := ? }

**type** **record** R { **integer** k, **integer** i, **integer** j }

**type** R R2 ({ k:= 1, i := 2}, { k:= 2, i := 3})

**function** inc(**inout** **integer** p) {

  p := p + 1;

}

**function** f() {

**var** R2 x := { 1, 2, 5 }

x.k := 2; // error, as the value {2,2,5} is not allowed

inc(x.i); // error, as the value {1,3,5} is not allowed

// (previous erroneous assignment is ignored here)

inc(x.j); // allowed

}

EXAMPLE 2: List subtyping of record of types

**type** **record** **of** **charstring** StringArray;

**type** StringArray StringArrayList1 (

{ "aa" },

{ "bbb", "cc" },

{ "ddd", "ee", "ff" }

); // valid subtype of StringArray

**type** StringArrayList1 StringArrayList2 (

{ "aa" },

{ "bbb", "cc" }

); // valid subtype of StringArrayList1

**type** StringArrayList1 StringArrayList3 (

StringArrayList2,

{ "ddd", "ee", "ff" }

); // valid, but equivalent to StringArrayList1

**type** StringArrayList1 StringArrayList4 (

StringArrayList2,

{ "ddd", "ee", "fff" }

); // empty type as { "ddd", "ee", "fff" } is not a value of StringArrayList1

// (notice the extra character f in the third element)

EXAMPLE 3: List subtyping of union types

**type union** MyUnion {

**integer** c1,

**charstring** c2,

**charstring** c3

};

**type** MyUnion MyUnionSub1 (

{ c1 := 0 },

{ c1 := 1 }

); // a valid subtype of MyUnion containing two values

**type** MyUnion MyUnionSub2 (

MyUnionSub1,

{ c2 := "mine" },

{ c3 := "yours" }

); // a valid subtype of MyUnion containing four values; notice that values of

// MyUnionSub1 are identified by referencing MyUnionSub1

**type** MyUnionSub1 MyUnionSub3 (

{ c1 := 0 },

{ c1 := 2 }

); // causes an error as { c1 := 2 } is not a value of MyUnionSub1

EXAMPLE 4: List subtyping of enumerated types

**type** **enumerated** MyEnum { first, second, third, fourth, fifth };

**type** MyEnum EnumSub1 ( first, second, third );

// a valid subtype of MyEnum

**type** EnumSub1 EnumSub2 ( first, second );

// a valid subtype of EnumSub1

**type** EnumSub1 EnumSub3 ( first, second, fourth );

// causes an error as fourth is not a value of EnumSub1

**type** MyEnum EnumSub4 ( EnumSub1, fourth);

// causes an error as type references are not allowed in the template list

// of enumerated types

EXAMPLE 5: List subtyping of anytype

**type** **anytype** MyAnySub1 (

{ **integer** := 5 },

{ **boolean** := false },

{ **bitstring** := '0011'B },

{ **charstring** := "mine" },

{ MyEnum := first }

); // a valid subtype of anytype, consisting of 5 values

**type** MyAnySub1 MyAnySub2 (

{ **integer** := 5 },

{ **boolean** := false },

{ **bitstring** := '0011'B }

); // a valid subtype of MyAnySub1, consisting of 3 values

**type** **anytype** MyAnySub3 (

MyAnySub2,

{ **octetstring** := 'FF'O }

); // a valid subtype of anytype, consisting of 4 values, 3 of which are defined

// by referring to MyAnySub2

**type** MyAnySub1 MyAnySub4 (

{ **integer** := 5 },

{ **boolean** := false },

{ MyEnum := second }

); // causes an error as { MyEnum := second } is not a value of MyAnySub1

**type** MyAnySub1 MyAnySub5 (

MyAnySub3,

{ MyEnum := first }

); // causes an error as { **octetstring** := 'FF'O } (defined via referencing MyAnySub3) is

// not a value of MyAnySub1

**type** **record** R { **integer** k, **integer** i, **integer** j }

**type** R R2 ({ k:= 1, i := 2}, { k:= 2, i := 3})

**function** g() {

**var** R2 x := { 1, 2 }

x.k := 2; // error

}

#### 6.2.13.3 Subtyping of the iterated type of record ofs and set ofs

A type restriction following the identifier of a newly defined **record of** or **set of** type (i.e. when the keywords **record** and **of** or **set** and **of** are used in the definition) shall constrain the innermost type. The newly defined iterated type shall be a subset of the innermost type. If the innermost type is a basic type, the subtyping rules in clause 6.1.2 shall apply. If the innermost type is referencing a structured type or **anytype**, the rules in clauses 6.2.13.1 and 6.2.13.2 shall apply.

EXAMPLE 1: Subtyping of basic innermost types of record ofs and set ofs

**type** **record** **of** **charstring** String23Array **length**(2 .. 3);

// is an unlimited record of, each element shall be a charstring of 2 or 3 characters

**type** **record length**(0..10) **of** **charstring** String12Array10 **length**(12);

// is a record of a maximum of 10 strings each with exactly 12 characters

**type** **record of** **record of** **charstring** String12Array2D **length**(12);

// is a two-dimensional unlimited array of strings each with exactly 12 characters

**type** **set length**(5) **of** **set length**(6) **of** **charstring** String12Array2D56 **length**(12);

// is an unordered two-dimensional array of the size 5\*6 strings, each with

// exactly 12 characters

**const** String23Array c\_str23arr\_a := { "aa", "bbb", "cc", "ddd", "ee", "ff" };

// valid, all charstrings are 2 or 3 characters long

**const** String23Array c\_str23arr\_b := { "a", "bbbb", "cc", "ddd", "ee", "ff" };

// causes an error as "a" and "bbbb" are not 2 or 3 characters long

**const** String12Array2D56 c\_str12arr2D56\_a := {

{ "aa", "aaa", "bb", "bbb", "cc", "ccc" },

{ "dd", "ddd", "ee", "eee", "ff", "fff" },

{ "gg", "ggg", "hh", "hhh", "ii", "iii" },

{ "jj", "jjj", "kk", "kkk", "ll", "lll" },

{ "mm", "mmm", "nn", "nnn", "oo", "ooo" }

}; // valid, a 5\*6 matrix of charstrings being 2 or 3 characters long

**const** String12Array2D56 c\_str12arr2D56\_b := {

{ "a", "aaa", "bb", "bbbb", "cc", "ccc" },

{ "dd", "ddd", "ee", "eee", "ff", "fff" },

{ "gg", "ggg", "hh", "hhh", "ii", "iii" },

{ "jj", "jjj", "kk", "kkk", "ll", "lll" },

{ "mm", "mmm", "nn", "nnn", "oo", "ooo", "pp" }

}; // causes an error as "a" and "bbbb" are not 2 or 3 characters long and

// the 5th inner record of has 7 elements

EXAMPLE 2: Length subtyping of structured innermost types of record ofs

**type** **record of** String23Array String23Array45 **length**(4 .. 5);

// is a two-dimensional array, the first dimension is unlimited,

// the second dimension is restricted to 4 or 5 elements and each element

// is a charstring of 2 or 3 characters. It is equivalent to:

// **type** **record of** **record** **length**(4 .. 5) **of** **charstring** String23Array45 **length**(2 .. 3);

**const** String23Array45 c\_str23arr45\_a := {

{ "aa", "bbb", "cc", "ddd" },

{ "ee", "fff", "gg", "hhh", "ii" }

}; // valid, 4 or 5 elements in the inner record of, all containing 2 or 3 characters

**const** String23Array45 c\_str23arr45\_b := {

{ "aa" , "bbb", "cc" }

}; //causes an error as there are only 3 elements in the inner record of

**const** String23Array45 c\_str23arr45\_c := {

{ "aa", "bbbb", "cc", "dd" }

}; //causes an error as "bbbb" contains 4 characters

**type** **record length**(0 .. 1) **of** String23Array String23Array0145 **length**(4 .. 5);

// is a two-dimensional array, the first dimension is limited to 0 or 1 elements,

// the second dimension is restricted to 4 or 5 elements, each element is a

// charstring of 2 or 3 characters.

**const** String23Array0145 c\_str23arr0145\_a := {

{ "aa", "bbb", "cc", "ddd" },

}; // a valid 1\*4 array of charstrings, each of 2 or 3 characters

**const** String23Array0145 c\_str23arr0145\_a := {

{ "aa", "bbb", "cc", "ddd" },

{ "ee", "fff", "gg", "hhh", "ii" }

}; // causes an error as there are two elements in the outer record of

**const** String23Array0145 c\_str23arr0145\_b := {

{ "aa" , "bbb", "cc" }

}; // causes an error as there are only 3 elements in the inner record of

**const** String23Array0145 c\_str23arr0145\_c := {

{"aa", "bbbb", "cc", "dd" }

}; // causes an error as "bbbb" contains 4 characters

**type** **record of** String23Array45 String23Array6 **length**(6);

// empty type as String23Array45 is restricted to 4 or 5 elements,

// thus length restriction 6 is outside the allowed range

#### 6.2.13.4 Mixing subtyping mechanisms

In the case of structured types and the special type **anytype**, it is forbidden to mix different subtyping mechanisms (e.g. list and length) in the same definition.

## 6.3 Type compatibility

Generally, TTCN‑3 requires type compatibility of values at assignments, instantiations and comparison.

For the purpose of this clause the actual value to be assigned, passed as parameter, etc., is called value "b". The type of value "b" is called type "B". The type of the formal parameter, which is to obtain the actual value of value "b" is called type "A".

NOTE: As **address** is more a predefined type name than a distinct type with its own properties, the same type compatibility rules apply to an **address** type and to its derivatives as the rules were if the type was defined with a name different from **address**.

### 6.3.1 Compatibility of non-structured types

For variables, constants, templates, etc. of simple basic types and basic string types the value "b" is compatible to type "A" if type "B" resolves to the same root type as type "A" (e.g. **integer**) and it does not violate subtyping (e.g. ranges, length restrictions) of type "A". Compatibility between charstring and universal charstring is defined below.

EXAMPLE 1: Compatibility of integers

// Given

**type** **integer** MyInteger(1 .. 10);

:

**var** **integer** x;

**var** MyInteger y;

// Then

y := 5; // is a valid assignment

x := y;

// is a valid assignment, because y has the same root type as x and no subtyping is violated

x := 20; // is a valid assignment

y := x;

// is NOT a valid assignment, because the value of x is out of the range of MyInteger

x := 5; // is a valid assignment

y := x;

// is a valid assignment, because the value of x is now within the range of MyInteger

EXAMPLE 2: Compatibility of floats

// Given

**type** **float** PositiveFloats(0.0 .. **infinity**);

:

**var** PositiveFloats x;

**var** **float** y;

// Then

y := 5.0; // is a valid assignment

x := y;

// is a valid assignment, because y has the same root type as x and no subtyping is violated

y := -20.0; // is a valid assignment

x := y;

// causes an error, because the value of y is out of the range of PositiveFloats

y := not\_a\_number; // is a valid assignment

x := y;

// causes an error, because the value **not\_a\_number** is out of the range of PositiveFloats

EXAMPLE 3: Compatibility of charstrings

//Given

**type** **charstring** MyChar **length** (1);

**type** **charstring** MySingleChar **length** (1);

**var** MyChar myCharacter;

**var** **charstring** myCharString;

**var** MySingleCharmySingleCharString := "B";

//Then

myCharString := mySingleCharString;

//is a valid assignment as charstring restricted to length 1 is compatible with charstring.

myCharacter := mySingleCharString;

//is a valid assignment as two single-character-length charstrings are compatible.

//Given

myCharString := "abcd";

//Then

myCharacter := myCharString[1];

//is valid as the r.h.s. notation addresses a single element from the string

//Given

**var** **charstring** myCharacterArray [5] := {"A", "B", "C", "D", "E"}

//Then

myCharString := myCharacterArray[1];

//is valid and assigns the value "B" to myCharString;

For variables, constants, templates, etc. of **charstring** type, value 'b' is compatible with a **universal charstring** type 'A' unless it violates any type constraint specification (range, list or length) of type "A".

For variables, constants, templates, etc. of **universal charstring** type, value 'b' is compatible with a **charstring** type 'A' if all characters used in value 'b' have their corresponding characters (i.e. the same control or graphical character using the same character code) in the type **charstring** and it does not violate any type constraint specification (range, list or length) of type "A".

EXAMPLE 4: Compatibility of character and universal character strings

//Given

**type** **charstring** MyChar **length** (1);

...

**var** MyChar myCharacter;

**var** **charstring** myCharString;

**var** **universal** **charstring** myUnivCharString;

// Given

myCharString := "abcd";

// Then

myUnivCharString := myCharString

//is valid as charstring and universal charstring are compatible

myCharacter := myUnivCharString [1];

// is valid as the r.h.s. notation addresses a single element of the string,

// containing a character compatible with charstring

// Given

myUnivCharString := "bet" & **char** ( 0, 0, 1, 113);

// Then

myCharString := myUnivCharString;

// is **in**valid as myUnivCharString contains a character not in ISO 646.

// Given

**var** **charstring** myCharacterArray [5] := {"A", "B", "C", "D", "E"}

// Then

myCharString := myCharacterArray[1];

// is valid and assigns the value "B" to myCharString;

### 6.3.2 Compatibility of structured types

This clause defines compatibility rules for structured types. In subsequent clauses, "value "b"" is called the value to be assigned, e.g. when passed as parameter, to an object of type "A".

#### 6.3.2.1 Compatibility of enumerated types

Enumerated types are only compatible to synonym types (see clause 6.4) and not compatible with other basic or structured types.

#### 6.3.2.2 Compatibility of record and record of types

**record** types are compatible if the number, and optional aspect of the fields in the textual order of definition are identical, the types of each field are compatible and the value of each existing field of the value "b" is compatible with the type of its corresponding field in type "A". The value of each field in the value "b" is assigned to the corresponding field in the value of type "A".

EXAMPLE 1:

// Given

**type record** AType {

**integer** a(0..10) **optional**,

**integer** b(0..10) **optional,**

**boolean**  c

}

**type record** BType {

**integer** a **optional**,

**integer** b(0..10) **optional,**

**boolean**  c

}

**type record** CType { // type with different field names

**integer**  d **optional**,

**integer** e **optional,**

**boolean**  f

}

**type record** DType { // type with field c optional

**integer**  a **optional**,

**integer** b **optional,**

**boolean**  c **optional**

}

**type record** EType { // type with an extra field d

**integer**  a **optional**,

**integer** b **optional,**

**boolean**  c,

**float**  d **optional**

}

**var** AType MyVarA := { -, 1, **true**};

**var** BType MyVarB := { omit, 2, **true**};

**var** CType MyVarC := { 3, **omit**, **true**};

**var** DType MyVarD := { 4, 4, **true**};

**var** EType MyVarE := { 5, 5, **true**, **omit**};

// Then

MyVarA := MyVarB; // is a valid assignment,

// new value of MyVarA is ( a :=omitted, b:= 2, c:= true)

MyVarC := MyVarB; // is a valid assignment

// new value of MyVarC is ( d :=omitted, e:= 2, f:= true)

MyVarA := MyVarD; // is NOT a valid assignment because the optionality of fields does not

// match

MyVarA := MyVarE; // is NOT a valid assignment because the number of fields does not match

MyVarC := { d:= 20 };// actual value of MyVarC is { d:=20, e:=2,f:= true }

MyVarA := MyVarC // is NOT a valid assignment because field 'd' of MyVarC violates subtyping

// of field 'a' of AType

**record** **of** types and arrays are compatible if their element types are compatible and value "b" does not violate any length subtyping of the **record** **of** type "A" or dimensions of the array type. Values of elements of the value "b" shall be assigned sequentially to the instance of type "A", including undefined elements.

Two array types are compatible if their corresponding **record of** types are compatible.

EXAMPLE 2:

// Given

**type record** HType {

**integer** a,

**integer** b **optional**,

**integer** c

}

**type record of integer** IType

**var** HType MyVarH := { 1, **omit**, 2};

**var** IType MyVarI;

**var** **integer** MyArrayVar[2];

// Then

MyArrayVar := MyVarH;  
 // is NOT a valid assignment as type of MyArrayVar and HType are incompatible

MyVarI := MyVarH;

// is NOT a valid assignment as the types are incompatible

MyVarI := { 3, 4 };

MyVarH := MyVarI;

// is NOT a valid assignment as the mandatory field 'c' of Htype receives no value

#### 6.3.2.3 Compatibility of set and set of types

**set** types are only compatible with other **set** types and **set** **of** types are only compatible with other **set of** types. For **set** types the same compatibility rules shall apply as to **record** types and for **set** **of** types the same compatibility rules shall apply as to **record** **of** types.

NOTE 1: This implies that though the order of elements at sending and receipt is unknown, when determining type compatibility for **set** types, the textual order of the fields in the type definition is decisive.

NOTE 2: In **set** values the order of fields may be arbitrary, however this does not affect type compatibility as field names unambiguously identify, which fields of the related **set** type correspond to which **set** value fields.

EXAMPLE:

// Given

**type set** FType {

**integer** a optional,

**integer** b optional,

**boolean** c

}

**type set** GType {

**integer** d optional,

**integer** e optional,

**boolean** f

}

**var** FType MyVarF := { a:=1, c:=**true** };

**var** GType MyVarG := { f:=**true**, d:=7};

// Then

MyVarF := MyVarG; // is a valid assignment as types FType and GType are compatible

MyVarF := MyVarA; // is NOT a valid assignment as MyVarA is a record type

#### 6.3.2.4 Compatibility of union types

**union** types are only compatible with other **union** types. A union value "a" of union type "A" is compatible with union type "B" if the alternative selected in "a" has a corresponding alternative with identical name in "B" and the value of the selected alternative in "a" is compatible to the type of the corresponding alternative in "B".

EXAMPLE:

**type** **union** U1 {**integer** i};

**type** **union** U2 {**integer** i, **boolean** b};

**var** U1 u1 := {i := 1};

**var** U2 u2 := u1; // correct

u1:= u2; // correct as the alternative i is selected in u2 and is compatible  
 // to i in U1

u2:= {b := true};

u1:= u2; // incorrect as u1 has no alternative b

**var** **anytype** x := u1; // incorrect as the anytype is not a **union** type.

#### 6.3.2.5 Compatibility of anytype types

**anytype** types are only compatible with other **anytype** types. An anytype value "a" of anytype type "A" is compatible with anytype type "B" if the alternative selected in "a" has a corresponding alternative with identical name in "B" and the value of the selected alternative in "a" is compatible to the type of the corresponding alternative in "B". Identical alternative names in this case mean the name of a TTCN-3 basic type or the name of the same user defined type definition (considering also the module in which the type is defined).

EXAMPLE:

**module** A {

**type** **integer** I (0..2);

**type float** F;

**type** **anytype** Atype //anytype composed of TTCN-3 built-in basic types, I, and F

}

**module** B {

**type** **integer** I (0..2);

**type** **anytype** Atype

}

**module** C {

**import from** A **all**;

**import from** B **all**;

**type union** U {

**integer** I (0..2)

}

**control** {

**var** A.Atype aa;

**var** A.Atype aaI := { I := 1 }

**var** A.Atype aaF := { F := 1.0 }

**var** B.Atype ba := { integer := 1 }

**var** B.Atype baI := { I := 1 }

**var** U u := { I := 1 }

aa := ba; // correct, the value of aa1 becomes { integer := 1 }

aa := baI; // incorrect, type B.I is not present in the anytype A.Atype

aa := u; // incorrect, type of u is not anytype but a user defined union type

ba := { float := 1.0 }; // correct, assigning a literal value

ba := aaI; // incorrect, type A.I is not present in the anytype B.Atype

ba := aaF; // incorrect, type A.F is not present in the anytype B.Atype

}

}

#### 6.3.2.6 Compatibility between sub-structures

The rules defined in this clause for structured types compatibility are also valid for the sub-structure of such types.

EXAMPLE:

// Given

**type record** JType {

HTypeH,

**integer** b **optional**,

**integer** c

}

**var** JType MyVarJ

// If considering the declarations above, then

MyVarJ.H := MyVarH;  
 // is a valid assignment as the type of field H of JType and HType are compatible

MyVarI := MyVarJ.H;  
 // is a valid assignment as IType and the type of field H of JType are compatible

### 6.3.3 Compatibility of component types

Type compatibility of component types has to be considered in different conditions:

1. Compatibility of a component reference value with a component type (e.g. when passing a component reference as an actual parameter to a function or an altstep or when assigning a component reference value to a variable of different component type): a component reference "b" of component type "B" is compatible with component type "A" if all definitions of "A" have identical definitions in "B".
2. Runs on compatibility: a function or altstep referring to component type "A" in its runs on clause may be called or started on a component instance of type 'B' if all the definitions of "A" have identical definitions in "B".
3. Mtc compatibility: a function or altstep referring to component type "A" in its mtc clause may be called or started in any context that has a mtc clause of type "B" or a testcase with a runs on clause of type "B" if all the port definitions of "A" have identical definitions in "B". If the type of the mtc is unknown in the calling function, this can lead to runtime errors if the component type "A" is not mtc-compatible with the type of the running mtc.
4. System compatibility: a function or altstep referring to component type "A" in its system clause may be called or started in any context that has a system clause of type "B" or a test case with a runs on clause of type "B" and no system clause if all the port definitions of "A" have identical definitions in "B". If the type of the system is unknown in the calling function, this can lead to runtime errors if the component type "A" is not system-compatible with the type of the system the current test case was started on.

Identity of definitions in "A" with definitions of "B" is determined based on the following rules:

a) For port instances, both the type and the identifier shall be identical.

b) For timer instances, identifiers shall be identical and either both shall have identical initial durations or both shall have no initial duration.

c) For variable instances and constant definitions, the identifiers, the types and initialization values shall be identical (in case of variables this means that either the values are missing in both definitions or are the same).

d) For local template definitions, the identifiers, the types, the formal parameter lists and the assigned template or template field values shall be identical.

### 6.3.4 Type compatibility of communication and connection operations

The communication operations (see clause 22) **send**, **receive**, **trigger**, **call**, **getcall**, **reply**, **getreply** and **raise** and connection operations **connect, map, disconnect** and **unmap** (see clause 21.1) are exceptions to the weaker rule of type compatibility and require strong typing. The types of values or templates directly used as parameters to these operations shall also be explicitly defined in the associated port type definition. Strong typing also applies to storing the received value, address or component reference during a **receive** or **trigger** operation.

EXAMPLE:

**type** **record** MyRec {...} // user defined type

**type** MyRec MyRecAlias; // a type alias

**type** **port** MyPort **message** { **inout** MyRec**,** MyRecAlias; } // port that can transport both types

**type component** MyComponent { **port** MyPortP; }

**template** MyRecAlias t\_MyRecAlias:= {...} // a template of the alias type

**var** MyComponentmyComp1 **:=** MyComponent**.create,** myComp2 **:=** MyComponent**.create;**

**connect** (myComp1:P, myComp2:P) // two connected PTCs via ports that can

// transport the user-defined and the alias type

// in myComp1:

P.**send** (t\_MyRecAlias); // sending of template of alias type

// in myComp2:

P.**receive** (MyRec:?);

// shall not match as the transmitted template is of the alias type and

// not of the user-defined type

// in myComp2:

**var** MyRec x;

P.**receive** (MyRecAlias:?) -> **value** x;

// shall cause an error since also storing the value requires strong typing

### 6.3.5 Type conversion

If it is necessary to convert values of one type to values of another type, because their types have different root types, then either one of the predefined conversion functions defined in clause 16.1.2 or a user defined function shall be used.

EXAMPLE:

// To convert an integer value to a hexstring value use the predefined function int2hex

MyHstring := **int2hex**(123, 4);

## 6.4 Type synonym

A type can be defined as a synonym to another type. Type synonyms can be defined for all kinds of types. Synonym types are compatible.

EXAMPLE:

**type** MyType1 MyType2; // MyType2 is synonym to MyType1

# 7 Expressions

TTCN‑3 allows the specification of expressions. TTCN-3 expressions may be template references, value references or literals (i.e. no operation is involved), and may be composed of the operators defined in clause 7.1.

NOTE: Templates can be used at the RHS of assignment, parameter passing and (predefined) functions where template passing is explicitly allowed.

***Syntactical Structure***

*SingleExpression* |

"{" { ( *FieldReference* ":=" ( Expression | "-" )) [","] } "}" | // compound expression

"{" [ { ( Expression | "-" ) [","] } ] "}" // compound expression

***Semantic Description***

Expressions may be built from other (simple) expressions. Functions used in expressions shall have a return clause. The operands of the operators used in an expression shall be values and their root types shall be the types specified for the appropriate operator in the subsequent clauses.

Compound expressions are used for expressions of array, record, record of and set of types.

***Restrictions***

In addition to the general static rules of TTCN‑3 given in clause 5, the following restrictions apply:

a) At the point, when an expression is evaluated, the evaluated values of the operands used in expressions shall be completely initialized except where explicitly stated otherwise in the specific clause of the operator.

b) The root types of the operands shall be the types specified for the appropriate operand.

c) With the exception of the equality and non-equality operators, the special value **null** shall not be used as an operand of expressions (see clause 7.1.3).

This means also that all fields and elements of structured types referenced in an expression shall contain completely initialized values, while other fields and elements, not used in the expression, may be uninitialized or contain **omit**.

***Examples***

(x + y - increment(z))\*3 // single expression

{ a:= 1, b:= **true** } // compound expression, field expression list

{ 1, **true** } // compound expression, value list

## 7.1 Operators

TTCN‑3 supports a number of predefined operators that may be used in the terms of TTCN‑3 expressions. The predefined operators fall into seven categories:

a) arithmetic operators;

b) list operator;

c) relational operators;

d) logical operators;

e) bitwise operators;

f) shift operators;

g) rotate operators.

***Restrictions***

In addition to the general static rules of TTCN‑3 given in clause 5, the following restrictions apply:

a) When an expression is evaluated, the evaluated values used as the operands of operators shall be completely initialized, except for those operands for which it is explicitly allowed to be partially initialized (see clause 11.1).

These operators are listed in table 5.

Table 5: List of TTCN‑3 operators

| Category | Operator | Symbol or Keyword |
| --- | --- | --- |
| **Arithmetic operators** | addition | **+** |
| subtraction | **-** |
| multiplication | **\*** |
| division | **/** |
| modulo | **mod** |
| remainder | **rem** |
| **String operators** | concatenation | **&** |
| **Relational operators** | equal | **==** |
| less than | **<** |
| greater than | **>** |
| not equal | **!=** |
| greater than or equal | **>=** |
| less than or equal | **<=** |
| **Logical operators** | logical not | **not** |
| logical and | **and** |
| logical or | **or** |
| logical xor | **xor** |
| **Bitwise operators** | bitwise not | **not4b** |
| bitwise and | **and4b** |
| bitwise or | **or4b** |
| bitwise xor | **xor4b** |
| **Shift operators** | shift left | **<<** |
| shift right | **>>** |
| **Rotate operators** | rotate left | **<@** |
| rotate right | **@>** |

The precedence of these operators is shown in table 6. Within any row in this table, the listed operators have equal precedence. If more than one operator of equal precedence appears in an expression, the operations are evaluated from left to right. Parentheses may be used to group operands in expressions, in which case a parenthesized expression has the highest precedence for evaluation.

Table 6: Precedence of Operators

|  |  |  |
| --- | --- | --- |
| Priority | Operator type | Operator |
| highest  Lowest | Unary  Binary  Binary  Unary  Binary  Binary  Binary  Binary  Binary  Binary  Unary  Binary  Binary  Binary | **( … )**  **+, -**  **\*, /**, **mod**, **rem**  **+, -, &**  **not4b**  **and4b**  **xor4b**  **or4b**  **<<, >>, <@, @>**  **<, >, <=, >=**  **==, !=**  **not**  **and**  **xor**  **or** |

### 7.1.1 Arithmetic operators

The arithmetic operators represent the operations of addition, subtraction, multiplication, division, modulo and remainder. Operands of these operators shall be of **integer** values (including derivations of **integer**) or floating‑point numbers (including derivations of **float**, containing numeric values only), except for **mod** and **rem** which shall be used with **integer** (including derivations of **integer**) types only.

The usage of the special float values **infinity**, **-infinity** and **not\_a\_number** in arithmetic operators shall follow the rules defined in IEEE 754 [6].

With **integer** types, the result type of arithmetic operations is **integer**. With float types, the result type of arithmetic operations is **float**.

In the case where plus (+) or minus (-) is used as the unary operator the rules for operands apply as well. The result of using the minus operator is the negative value of the operand if it was positive and vice versa. The result of using the plus operator is the value of the operand, i.e. a positive value if the operand value was positive and a negative value if the operand value was negative.

The result of performing the division operation (/) on two:

a) **integer** values gives the whole **integer** part of the value resulting from dividing the first **integer** by the second (i.e. fractions are discarded);

b) numeric **float** values gives the **float** value resulting from dividing the first **float** by the second (i.e. fractions are not discarded).

The operators **rem** and **mod** compute on operands of type **integer** and have a result of type **integer**. The operations x **rem** y and x **mod** y compute the rest that remains from an integer division of x by y. Therefore, they are only defined for non-zero operands y. For positive x and y, both x **rem** y and x **mod** y have the same result but for negative arguments they differ.

Formally, **mod** and **rem** are defined as follows:

x **rem** y = x - y \* (x/y)

x **mod** y = x **rem** |y| when x >= 0

= 0 when x < 0 and x **rem** |y| = 0

= |y| + x **rem** |y| when x < 0 and x **rem** |y| < 0

Table 7 illustrates the difference between the **mod** and **rem** operator:

Table 7: Effect of mod and rem operator

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| x | -3 | -2 | -1 | 0 | 1 | 2 | 3 |
| x mod 3 | 0 | 1 | 2 | 0 | 1 | 2 | 0 |
| x rem 3 | 0 | -2 | -1 | 0 | 1 | 2 | 0 |

### 7.1.2 List operator

The predefined list operator (&) performs concatenation of values of string types, **record of**, **set of**, or **array** of the same root types. The operation is a simple concatenation from left to right. No form of arithmetic addition is implied. The result type is the root type of the operands.

NOTE 1: In case of the list types, both the outer type (i.e. **record of**, **set of** or **array**) and the iterated inner type need to have the same root type in a recursive manner.

NOTE 2: It is also possible to concatenate two or more value list notation expressions if the result is to be used as a **record of** or **array** of the same root type as the concatenated expressions.

***Restrictions***

In addition to the general static rules of TTCN‑3 given in clause 5, the following restrictions apply:

a) When the list concatenation operator is used for record of-s, set of-s and arrays, its operands shall be at least partially initialized.

EXAMPLE:

'1111'B & '0000'B & '1111'B gives '111100001111'B

{1,2} & {3,4} & {5,6} gives the following record of integer {1,2,3,4,5,6}

### 7.1.3 Relational operators

The predefined relational operators are equality (==), less than (<), greater than (>), non‑equality to (!=), greater than or equal to (>=) and less than or equal to (<=). The result type of all these operations is **boolean**.

The relational operators less than (<), greater than (>), greater than or equal to (>=), and less than or equal to (<=) shall have only operands of type **integer** (including derivations of **integer**), **float** (including derivations of **float**), or instances of the same **enumerated** type. It is not allowed to compare instances of different root types.

The **address** type is allowed for the equality (==) and non-equality (!=) operators, independent of its actual type, but when its actual type differs from the types specified above, it can be compared to the literal special value **null** only.

Operands of equality (==) and non-equality (!=) shall be completely initialized values or field references of type compatible root types and the values or field references being compared shall obey the following rules. This implies that instances of types not mentioned below shall not be operands of equality and non-equality.

* Two field references are equal if the referenced fields are both **optional** fields and both fields are set to **omit** or if both referenced fields (regardless if they are optional or not) are initialized with values and these values are equal. A field reference is equal to a value if the referenced field is initialized with a value and both values are equal.
* Two integer values are equal if and only if they contain the same value. Otherwise, normal mathematical ordering is applied.
* Two floating-point numbers are equal if and only if they contain the same value. The values minus zero and plus zero are two distinct values (e.g. they are encoded differently in some standardized languages) and minus zero is less than plus zero, which represents zero. Otherwise, normal mathematical ordering is applied. The special values **‑infinity,** **infinity** and **not\_a\_number** are equal to themselves only. The special value **‑infinity** is less than any other float value. The special value **infinity** is greater than any numerical float values and **-infinity**. The special value **not\_a\_number** is greater than any other float value (including **infinity)**.
* Two charstring or two universal charstring values are equal if and only if they have equal lengths and the characters at all positions are the same.
* For values of bitstring, hexstring or octetstring types, the same equality rule applies as for charstring values with the exception, that fractions which shall equal at all positions are bits, hexadecimal digits or pairs of hexadecimal digits accordingly.
* Two record values, or set values are equal respectively if and only if they are mutually compatible with the type of the other operand (see clause 6.3), the actual values of all present fields are equal to their corresponding fields and all fields corresponding to omitted fields are also omitted in the peer value.
* Two record of values, set of values or array values, respectively, are equal if and only if they are mutually compatible with the type of the other operand (see clause 6.3), they both have the same length, and and each element of one value is equal to the corresponding element of the other value. Record of values and array values may also be compared, in which case the corresponding record of type of the array is being considered.
* Values of the same union type, and values of different union types in which at least one of the alternatives is compatible with the other type (see clause 6.3.2.4) can be compared (independent if a compatible alternative is the selected one or not). Two values of union types are equal if and only if in both values the name of the selected alternative is identical, they are compatible with the type of the other value, and the actual values of the chosen fields are equal.
* Values of the same or any two anytype types can be compared. For anytype values the same rule apply as to union values, with the addition that names of types defined with the same name in different modules do not denote the same name of the selected alternatives.
* Two default or two component values are equal if and only if they contain the same value (i.e. they designate the same default or test component, independent of the actual state of the denoted object).
* It is also possible to use compound expressions (field assignment or value list notation) directly as operands of comparison operations of structured types. If there is a compound expression on both sides of the comparison operator, they shall both be value list notation expressions where the elements shall be of the same root type and they shall be compared like record of values with elements of that root type. If only one operand of the comparison operation is a compound expression it shall be compatible with the root type of the other operand and they shall be compared like values of that root type.

EXAMPLE:

// Given

**type** **set** S1 {

**integer** a1 **optional**,

**integer** a2 **optional**,

**integer** a3 **optional**

};

**type** **set** S2 {

**integer** b1 **optional**,

**integer** b2 **optional**,

**integer** b3 **optional**

};

**type** **set** S3 {

**integer** c1 **optional**,

**integer** c2 **optional**,

};

**type** **set** **of** **integer** SI;

**type** **union** U1 {

**integer** d1,

**integer** d2,

};

**type** **union** U2 {

**integer** e1,

**integer** e2,

};

**type** **union** U3 {

**integer** d1,

**integer** d2,

**boolean** d3

};

// And

**const** S1 s1 := { a1 := 0, a2 := **omit**, a3 := 2 };

// Notice that the order of defining values of the fields does not matter

**const** S2 s2a := { b1 := 0, b3 := 2, b2 := **omit** };

**const** S2 s2b := { b2 := 0, b3 := 2, b1 := **omit** };

**const** S3 s3 := { c1 := 0, c2 :=2 };

**var** SI v\_si:= { 0, -, 2 };

**const** SI si := { 0, 2 };

**const** U1 u1 := { d1:= 0 };

**const** U2 u2 := { e1:= 0 };

**const** U3 u3; := { d1:= 0 };

// Then

s1 == s2a;

// returns **true**

s1 == s2b;

// returns **false**, because neither a1 nor a2 are equal to their counterparts

// (the corresponding element is not omitted)

s1 == s3;

// returns **false**, because the effective value structures of s1 and s3 are not compatible

s1 == v\_si;

// causes test case error as v\_si is not completely initialized  
 // (2nd element is left uninitialized)

s1 == si;

// returns **false**, as the counterpart of the omitted a2 is 2,

// but the counterpart of a3 is undefined

s3 == si;

// returns **true**

u1 == u2;

// causes error as U1 and U2 have no common subset of alternatives

u1 == u3;

// returns **true**, as alternatives with the same names are chosen and

// the actual values in the selected alternatives are equal

{ 0, omit, 2 } == s1;

// returns true

s2a == { b1 := 0, b2:= omit, b3 := 2 };

// returns true

{ s1, s2b } == { s2a, s1 };

// returns false because s2b != s1

{ s1, s2b, s2a } == { s1 };

// returns false because of different length

s1.a1 == s2a.b1;

// returns true, both fields are initialized with values and the values are equal

s1.a2 == s2a.b2;

// returns true, both fields are omit

s1.a1 == s2a.b2;

// returns false, value vs. omit

s1.a1 == omit;

// error, omit is neither a value nor a field reference

s1.a2 == 3;

// false, omit vs. value

### 7.1.4 Logical operators

The predefined **boolean** operators perform the operations of negation, logical **and**, logical **or** and logical **xor**. Their operands shall be of root type **boolean**. The result type of logical operations is **boolean**.

The logical **not** is the unary operator that returns the value **true** if its operand was of value **false** and returns the value **false** if the operand was of value **true**.

The logical **and** returns the value **true** if both its operands are **true**; otherwise it returns the value **false**.

The logical **or** returns the value **true** if at least one of its operands is **true**; it returns the value **false** only if both operands are **false**.

The logical **xor** returns the value **true** if one of its operands is **true**; it returns the value **false** if both operands are **false** or if both operands are **true**.

Short circuit evaluation for boolean expressions is used, i.e. the evaluation of operands of logical operators is stopped once the overall result is known: in the case of the **and** operator, if the left argument evaluates to **false**, then the right argument is notevaluated and the whole expression evaluates to **false**. In the case of the **or** operator, if the left argument evaluates to **true**, then the right argument is not evaluated and the whole expression evaluates to **true**.

### 7.1.5 Bitwise operators

The predefined bitwise operators perform the operations of bitwise **not**, bitwise **and**, bitwise **or** and bitwise **xor**. These operators are known as **not4b**, **and4b**, **or4b** and **xor4b** respectively.

NOTE: To be read as "not for bit", "and for bit", etc.

Their operands shall be of root type **bitstring, hexstring** or **octetstring**. In the case of **and4b, or4b** and **xor4b** the operands shall be of the same root types. The result type of the bitwise operators shall be the root type of the operands.

The bitwise **not4b** unary operator inverts the individual bit values of its operand. For each bit in the operand a 1 bit is set to 0 and a 0 bit is set to 1. That is:

**not4b** '1'B gives '0'B

**not4b** '0'B gives '1'B

EXAMPLE 1:

**not4b** '1010'B gives '0101'B

**not4b** '1A5'H gives 'E5A'H

**not4b** '01A5'O gives 'FE5A'O

The bitwise **and4b** operator accepts two operands of equal length. For each corresponding bit position, the resulting value is a 1 if both bits are set to 1, otherwise the value for the resulting bit is 0. That is:

'1'B **and4b** '1'B gives '1'B

'1'B **and4b** '0'B gives '0'B

'0'B **and4b** '1'B gives '0'B

'0'B **and4b** '0'B gives '0'B

EXAMPLE 2:

'1001'B **and4b** '0101'B gives '0001'B

'B'H **and4b** '5'H gives '1'H

'FB'O **and4b** '15'O gives '11'O

The bitwise **or4b** operator accepts two operands of equal length. For each corresponding bit position, the resulting value is 0 if both bits are set to 0, otherwise the value for the resulting bit is 1. That is:

'1'B **or4b** '1'B gives '1'B

'1'B **or4b** '0'B gives '1'B

'0'B **or4b** '1'B gives '1'B

'0'B **or4b** '0'B gives '0'B

EXAMPLE 3:

'1001'B **or4b** '0101'B gives '1101'B

'9'H **or4b** '5'H gives 'D'H

'A9'O **or4b** 'F5'O gives 'FD'O

The bitwise **xor4b** operator accepts two operands of equal length. For each corresponding bit position, the resulting value is 0 if both bits are set to 0 or if both bits are set to 1, otherwise the value for the resulting bit is 1. That is:

'1'B **xor4b** '1'B gives '0'B

'0'B **xor4b** '0'B gives '0'B

'0'B **xor4b** '1'B gives '1'B

'1'B **xor4b** '0'B gives '1'B

EXAMPLE 4:

'1001'B **xor4b** '0101'B gives '1100'B

'9'H **xor4b** '5'H gives 'C'H

'39'O **xor4b** '15'O gives '2C'O

### 7.1.6 Shift operators

The predefined shift operators perform the shift left (**<<**) and shift right (**>>**)operations. Their left-hand operand shall be of root type **bitstring, hexstring** or **octetstring.** Their right-hand operand shall be a non-negative **integer**. The result type of these operators shall be the same as the root type of the left operand.

The shift operators behave differently based upon the type of their left-hand operand. If the type of the left-hand operand is:

a) **bitstring** then the shift unit applied is 1 bit;

b) **hexstring** then the shift unit applied is 1 hexadecimal digit;

c) **octetstring** then the shift unit applied is 1 octet.

The shift left (**<<**) operator accepts two operands. It shifts the left-hand operand by the number of shift units to the left as specified by the right-hand operand. Excess shift units (bits, hexadecimal digits or octets) are discarded. For each shift unit shifted to the left, a zero ('0'B, '0'H, or '00'O determined according to the type of the left­-hand operand) is inserted from the right-hand side of the left operand.

EXAMPLE 1:

'111001'B **<<** 2 gives '100100'B

'12345'H **<<** 2 gives '34500'H

'1122334455'O **<<** (1+1) gives '3344550000'O

The shift right **(>>)**operator accepts two operands. It shifts the left-hand operand by the number of shift units to the right as specified by the right-hand operand. Excess shift units (bits, hexadecimal digits or octets) are discarded. For each shift unit shifted to the right, a zero ('0'B, '0'H, or '00'O determined according to the type of the left-hand operand) is inserted from the left-hand side of the left operand.

EXAMPLE 2:

'111001'B >> 2 gives '001110'B

'12345'H >> 2 gives '00123'H

'1122334455'O >> (1+1) gives '0000112233'O

### 7.1.7 Rotate operators

The predefined rotate operators perform the rotate left (**<@)** and rotate right (**@>)** operators. Their left-hand operand shall be of root type **bitstring**, **hexstring**, **octetstring**, **charstring**, **universal charstring**, **record of**, or **set of**. Their right-hand operand shall be a non-negative **integer**. The result type of these operators shall be the same as the root type of the left-hand operand.

NOTE: Please note that the root types of arrays is **record of**, therefore arrays are allowed as left-hand operands of rotate operators.

The rotate operators behave differently based upon the type of their left-hand operand. If the type of the left-hand operand is:

a) **bitstring** then the rotate unit applied is 1 bit;

b) **hexstring** then the rotate unit applied is 1 hexadecimal digit;

c) **octetstring** then the rotate unit applied is 1 octet;

d) **charstring** or **universal charstring** then the rotate unit applied is one character;

e) **record of, set of,** or **array** then the rotate unit applied is one element.

The rotate left **(<@)** operator accepts two operands. It rotates the left-hand operand by the number of shift units to the left as specified by the right-hand operand. Excess shift units (bits, hexadecimal digits, octets, characters, or elements) are re‑inserted into the left-hand operand from its right-hand side.

***Restrictions***

In addition to the general static rules of TTCN‑3 given in clause 5, the following restrictions apply:

a) When the rotate operator is used for **record of**-s, **set of**-s and arrays, its left hand operand shall be at least partially initialized.

NOTE: Please note that for the right hand operand restriction a) in clause 7 further on applies.

EXAMPLE 1:

'101001'B **<@** 2 gives '100110'B

'12345'H **<@** 2 gives '34512'H

'1122334455'O **<@** (1+2) gives '4455112233'O

"abcdefg" **<@** 3gives "defgabc"

The rotate right **(@>)** operator accepts two operands. It rotates the left-hand operand by the number of shift units to the right as specified by the right-hand operand. Excess shift units (bits, hexadecimal digits, octets, characters, or elements) are re‑inserted into the left-hand operand from its left-hand side.

EXAMPLE 2:

'100001'B **@>** 2 gives '011000'B

'12345'H **@>** 2 gives '45123'H

'1122334455'O **@>** (1+2) gives '3344551122'O

"abcdefg" **@>** 3gives "efgabcd"

## 7.2 Field references and list elements

Within expressions, fields of record and set types are referenced with the dot notation **".field"**. Elements of record of, set of, array and string types are referenced with the index notation **"[index]"**. Dot and brackets have the same binding power. Field references and list elements are evaluated from left to right.

# 8 Modules

The principal building blocks of TTCN‑3 are modules. A module may define a fully executable test suite or just a library. A module may refer to the TTCN-3 language version and to package versions being used. A module consists of a (optional) definitions part, and a (optional) module control part.

NOTE: The term test suite is synonymous with a complete TTCN‑3 module containing test cases and a control part.

The transfer syntax of TTCN-3 modules shall be UTF-8, i.e. each character of the module shall be individually encoded and decoded according to the UCS Transformation Format 8 (UTF-8) as defined in annex R of ISO/IEC 10646 [2] and no characters not corresponding to any character of the module shall be present.

## 8.1 Definition of a module

A module is defined with the keyword **module**.

NOTE 1: The treatment of TTCN‑3 modules in files, repositories and alike is outside the scope of the present document.

***Syntactical Structure***

**module** *ModuleIdentifier* [ **language** *FreeText* { "," *FreeText* } ] "{"

[ *ModuleDefinitionsPart* ]

[ *ModuleControlPart* ]

"}"

***Semantic Description***

A TTCN‑3 module groups a set of (typically cohesive) TTCN‑3 definitions. TTCN‑3 modules have an explicit import interface to use definitions from other TTCN‑3 or non-TTCN‑3 modules. It is possible to hide definitions in a TTCN‑3 module (see clause 8.2.5). TTCN‑3 modules can be compiled/interpreted separately. They are reusable and parameterizable.

Module names are of the form of a TTCN‑3 identifier.

NOTE 2: The module identifier is the informal text name of the module.

In addition, a module specification can carry an optional attribute identified by the **language** keyword that identifies the edition of the TTCN‑3 language, in which the module is specified. The following language strings are to be used:

"TTCN‑3:2001" - to be used with modules complying with version 1.1.2 of the present document (see annex H)*.*  
 "TTCN‑3:2003" - to be used with modules complying with version 2.2.1 of the present document (see annex H).  
 "TTCN‑3:2005" - to be used with modules complying with version 3.1.1 of the present document (see annex H).  
 "TTCN‑3:2007" - to be used with modules complying with version 3.2.1 of the present document (see annex H).  
 "TTCN‑3:2008" - to be used with modules complying with version 3.3.2 of the present document (see annex H).  
 "TTCN‑3:2008 Amendment 1" - to be used with modules complying with version 3.4.1 of the present document  
 (see annex H).  
 "TTCN‑3:2009" - to be used with modules complying with version 4.1.1 of the present document (see annex H).  
 "TTCN‑3:2010" - to be used with modules complying with version 4.2.1 of the present document (see annex H).  
 "TTCN‑3:2011" - to be used with modules complying with version 4.3.1 of the present document (see annex H).  
 "TTCN‑3:2012" - to be used with modules complying with version 4.4.1 of the present document (see annex H).  
 "TTCN‑3:2013" - to be used with modules complying with version 4.5.1 of the present document (see annex H).  
 "TTCN‑3:2014" - to be used with modules complying with version 4.6.1 of the present document (see annex H).  
 "TTCN‑3:2015" - to be used with modules complying with the present document.

Furthermore, the optional attribute identified by the **language** keyword may identify package versions being used by this module. The package tags are defined in ES 202 781 [i.11], ES 202 782 [i.14], ES 202 784 [i.12], and ES 202 785 [i.13]. The language identifier and the package identifier are to be written as a comma-separated list.

***Restrictions***

In addition to the general static rules of TTCN 3 given in clause 5, the following restrictions apply:

1. At most one language string per module shall be given to define the core language version in which the module is defined.
2. Per extension package, at most one extension package string of that extension package shall be used by a module.

***Examples***

**module** MyTestSuite **language** "TTCN‑3:2003"

{ … }

## 8.2 Module definitions part

The module definitions part specifies the top-level definitions of the module and may import visible identifiers from other modules. Visibility rules are given in clause 8.2.5. Scope rules for declarations made in the module definitions part and imported declarations are given in clause 5.3. Those language elements which may be defined in a TTCN‑3 module are listed in table 1. Every definition can be associated with attributes using the with statement defined in clause 27. Visible module definitions may be imported by other modules.

***Syntactical Structure***

{

[ *Visibility* ] (

*TypeDef* |

*ConstDef* |

*TemplateDef* |

*ModuleParDef* |

*FunctionDef* |

*SignatureDef* |

*TestcaseDef* |

*AltstepDef* |

*ImportDef* |

*GroupDef* |

*ExtFunctionDef* |

*FriendDef*

) [ *WithStatement* ]

[ ";" ]

}+

***Semantic Description***

Definitions in the module definitions part may be made in any order.

Such definitions, i.e. top-level definitions outside of other scope units, are globally visible within the module. They may be used elsewhere in the module. This includes identifiers imported from other modules.

Declarations of dynamic language elements such as variables or timers shall only be made in the control part, test cases, functions, altsteps or component types.

TTCN‑3 does not support the declaration of variables in the module definitions part, i.e. global variables cannot be defined in TTCN‑3. However, variables defined in a test component type may be used by all test cases, functions, etc. running on components of that component type and variables defined in the control part provide the ability to keep their values independently of test case execution.

***Restrictions***

No specific restrictions in addition to the general static rules of TTCN‑3 given in clause 5.

***Examples***

**module** MyModule

{ // This module contains definitions only

:

**const** **integer** MyConstant := 1;

**type record** MyMessageType { … }

:

**function** TestStep(){ … }

**:**

}

### 8.2.1 Module parameters

Module parameters define a set of values that are supplied by the test environment at runtime. Module parameters do not change their value during test execution. They can be used on right hand side of assignments, in expressions, in actual parameters, and in template definitions, but not within type definitions.

***Syntactical Structure***

Single type, single module parameter form:

[ *Visibility* ] **modulepar** *ModuleParType* *ModuleParIdentifier* [ ":=" *ConstantExpression* ] ";"

Single type, multiple module parameter form:

[ *Visibility* ] **modulepar** *ModuleParType*

{ *ModuleParIdentifier* [ ":=" *ConstantExpression* ] **","** }

*ModuleParIdentifier* [ ":=" *ConstantExpression* ] ";"

***Semantic Description***

Module parameters behave as global constants at runtime. For module parameterization, TTCN-3 only supports value parameterization which has to be resolved static at start of runtime.

Module parameters allow to customize a TTCN‑3 test suite for a specific IUT, test setup or test campaign. Module parameters are declared by specifying the type and listing their identifiers following the keyword **modulepar**.

It is allowed to specify default values for module parameters. This shall be done by an assignment in the module parameter list. A default value can merely be assigned at the place of the declaration of the module parameter.

If the test system does not provide an actual runtime value for a module parameter, the default value shall be used during test execution, otherwise the actual value provided by the test system. Actual runtime values shall be literals only.

If functions are used for the initialization of module parameters, it is strongly advised to adhere to the rules defined in clause 16.1.4. Not following these rules may cause non-deterministic test executions.

Visible module parameters can be imported.

Optional fields of record and set module parameters or module parameter fields can be initialized explicitly or implicitly. For implicit initialization of the optional fields of a module parameter or a module parameter field, an **optional** attribute with the value "**implicit omit**" (see clause 27.7) shall be associated with it either directly or via the attribute distribution (scoping) mechanism (see clause 27.1.1).

***Restrictions***

In addition to the general static rules of TTCN‑3 given in clause 5, the following restrictions apply:

a) During test execution these values shall be treated as constants.

b) Module parameters shall not be of port type, default type or component type.

c) A module parameter shall only be of type address if the address type is explicitly defined within the associated module.

d) Module parameters shall be declared within the module definition part only.

e) More than one occurrence of module parameters declaration is allowed but each parameter shall be declared only once (i.e. redefinition of the module parameter is not allowed).

f) The constant expression for the default value of a module parameter shall respect the limitations given in clause 16.1.4.

g) Module parameters shall not be used in type or array definitions.

***Examples***

**module** MyTestSuiteWithParameters

{

// single type, single module parameter, which is per default public

**modulepar** **boolean** TS\_Par0 := **true**;

// single type, multiple module parameters with an explicit public visibility

**public** **modulepar** **integer** TS\_Par1, TS\_Par2 := 1 + char2int("a");

...

}

### 8.2.2 Groups of definitions

In the module definitions part, definitions can be collected in named groups. Grouping is done to aid readability and to add logical structure to the module if required. If necessary, the dot notation shall be used to identify sub-groups within the group hierarchy uniquely, e.g. for the import of a specific sub-group.

***Syntactical Structure***

[ **public** ] **group** *GroupIdentifier* "{"

{ *ModuleDefinition* [ ";" ] }

"}"

***Semantic Description***

A group of definitions can be specified wherever a single definition is allowed. Groups may be nested, i.e. groups may contain other groups. This allows the test suite specifier to structure, among other things, collections of test data or functions describing test behaviour.

Groups and nested groups have no scoping. Please note however, attributes given to a group by an associated with statement apply to all elements of a group (see clause 27). Import statements may import groups so that all visible elements of a group are imported (see clause 8.2.3.3).

***Restrictions***

In addition to the general static rules of TTCN‑3 given in clause 5, the following restrictions apply:

1. Group identifiers across the whole module need not necessarily be unique. However, top-level group identifiers and all group identifiers of subgroups of a single group shall be unique.
2. Only **public** visibility can be defined for groups as they are always public.

***Examples***

**module** MyModule {

:

// A collection of definitions

**group** MyGroup {

**const** **integer** MyConst:= 1;

:

**type record** MyMessageType { … };

**group** MyGroup1 { // Sub-group with definitions

**type** **record** AnotherMessageType { … };

**const** **boolean** MyBoolean := **false**

}

}

// A group of altsteps

**group** MyStepLibrary {

**group** MyGroup1 { // Sub-group with the same name as the sub-group with definitions

**altstep** MyStep11() { … }

**altstep** MyStep12() { … }

:

**altstep** MyStep1n() { … }

}

**group** MyGroup2 {

**altstep** MyStep21() { … }

**altstep** MyStep22() { … }

:

**altstep** MyStep2n() { … }

}

}

:

}

// An import statement that imports MyGroup1 within MyStepLibrary

**import** **from** MyModule {

**group** MyStepLibrary.MyGroup1

}

### 8.2.3 Importing from modules

It is possible to re-use visible definitions specified in different modules using the **import** statement. Every definition in a TTCN‑3 module has an associated visibility, which is by default **public** (see clause 8.2.5).

NOTE: Groups are **public** only. Importing a group means that only the visible elements of the group are being imported.

#### 8.2.3.1 General format of import

An import statement can be used anywhere in the module definitions part.

***Syntactical Structure***

[ *Visibility* ] **import** **from** *ModuleId*

(

( **all** [ **except** "{" *ExceptSpec* "}" ] )

|

( "{" *ImportSpec* "}" )

)

[ ";" ]

***Semantic Description***

TTCN‑3 supports the import of the following definitions: module parameters, user defined types, signatures, constants, data templates, signature templates, functions, external functions, altsteps and test cases. Each definition has a *name* (defines the identifier of the definition, e.g. a function name), a *specification* (e.g. a type specification or a signature of a function) and in the case of functions, altsteps and test cases an associated *behaviour description*. In addition, import statements of one module can be explicitly imported by another module (see clause 8.2.3.7). Only definitions or import statements visible from the importing module can be imported (see clause 8.2.5).

In contrast to module definitions, which are by default public, import statements are by default private.

EXAMPLE 1a:

|  |  |  |  |
| --- | --- | --- | --- |
|  | Name | Specification | Behaviour description |
| **function** | MyFunction | (**inout** MyType1 MyPar) **return** MyType2 **runs on** MyCompType | {  const MyType3 MyConst := …;  : // further behaviour  } |

|  |  |  |  |
| --- | --- | --- | --- |
|  | Specification | Name | Specification |
| **type** | **record** | MyRecordType | {  MyType4 field1,  integer field2  } |

|  |  |  |  |
| --- | --- | --- | --- |
|  | Specification | Name | Specification |
| **template** | MyType5 | MyTemplate | := {  field1 := 1,  field2 := MyConst, // MyConst is a module constant  field3 := ModulePar // ModulePar is module parameter  } |

Behaviour descriptions have no effect on the import mechanism, because their internals are considered to be invisible to the importer when the corresponding functions, altsteps or test cases are imported. Thus, they are not considered in the following descriptions.

The specification part of an importable definition contains *local definitions* (e.g. field names of structured type definitions or values of enumerated types) and *referenced definitions* (e.g. references to type definitions, templates, constants or module parameters). For the examples above, this means:

|  |  |  |  |
| --- | --- | --- | --- |
|  | Name | Local definitions | Referenced definitions |
| **function** | MyFunction | MyPar | MyType1, MyType2, MyCompType |
| **type** | MyRecordType | field1, field2 | MyType4, integer |
| **template** | MyTemplate |  | MyType5, field1, field2, field3, MyConst, ModulePar |

NOTE 1: The local definitions column refers to identifiers only that are newly defined in the importable definition. Values assigned to individual fields of importable definitions, e.g. in template definitions, may also be considered as local definitions, but they are not important for the explanation of the import mechanism.

NOTE 2: The referenced definitions field1, field2 and field3 of template MyTemplate are the field names of MyType5, i.e. they are referenced via MyType5.

Referenced definitions are also importable definitions, i.e. the source of a referenced definition can again be structured into a name and a specification part and the specification part also contains local and referenced definitions. In other words, an importable definition may be built up recursively from other importable definitions.

The TTCN‑3 import mechanism is related to the local and referenced definitions used in the specification part of the importable definitions. Table 8 specifies the possible local and referenced definitions of importable definitions.

Table 8: Possible local and referenced definitions of importable definitions

|  |  |  |
| --- | --- | --- |
| Importable Definition | Possible Local Definitions | Possible Referenced Definitions |
| Module parameter |  | Module parameter type |
| User-defined type (for all) |  |  |
| * enumerated type | Concrete values |  |
| * structured type | Field names, nested type definitions | Field types |
| * port type |  | Message types, signatures |
| * component type | Constant names, variable names, timer names and port names | Constant types, variable types, port types |
| Signature | Parameter names | Parameter types, return type, types of exceptions |
| Constant |  | Constant type |
| Data Template | Parameter names | Template type, parameter types, constants, module parameters, functions |
| Signature template |  | Signature definition, constants, module parameters functions |
| Function | Parameter names | Parameter types, return type, component type (**runs on** clause) |
| External function | Parameter names | Parameter types, return type |
| Altstep | Parameter names | Parameter types, component type (**runs on** clause) |
| Test case | Parameter names | Parameter types, component types (**runs on**- and **system** clause) |
| NOTE 1: For the import of import statements see clause 8.2.3.7.  NOTE 2: For the import of groups see clause 8.2.3.3. | | |

The TTCN‑3 import mechanism distinguishes between the *identifier of a referenced definition* and the *information necessary for the usage of a referenced definition* within the imported definition. For the usage, the identifier of a referenced definition is not required and therefore not imported automatically.

EXAMPLE 1b: Differentiation between *information necessary for the usage* and the identifier.

**module** A {

**type** **record** MyRec1 {

**integer** field1,

**charstring** field2

}

}

**module** B {

**import** **from** A **all**;

**type** **record** MyRec2 {

MyRec1 myField1,

// "myField1" is the local definition, "MyRec1" is a referenced definition;

// the *name* "MyRec1" shall be imported in this case as is directly referenced

**boolean** myField2

}

}

**module** C {

**import** **from** B **all**;

**const** MyRec2 t\_MyRec2 := {

myField1 := { field1 := 5, field2 := "A" },

// to define myField1 of MyRec2 the name "MyRec1" is not needed, the

// *information necessary for the usage* is its type information,

// i.e. names and types of its fields field1 and field2

// which is embeddded in the imported definition of MyRec2

myField2 := **true**

}

}

If an imported definition has attributes (defined by means of a **with** statement) then the attributes shall also be imported. The mechanism to change attributes of imported definitions is explained in clause 27.1.3.

NOTE 3: If the module has global attributes they are associated to definitions without these attributes.

The use of **import** on single definitions, groups of definitions, definitions of the same kind, etc. may lead to situations where the *same definition is referred to more than once*. Such cases shall be resolved by the system and definitions shall be imported only once.

NOTE 4: The mechanisms to resolve such ambiguities, e.g. overwriting and sending warnings to the user, are outside the scope of the present document and should be provided by TTCN‑3 tools.

All **import** statements and definitions within import statements are considered to be treated independently one after the other in the order of their appearance.

All TTCN‑3 modules shall have their own name space in which all definitions shall be uniquely identified. *Name clashes* may occur due to import, e.g. import from different modules. Name clashes shall be resolved using qualified name(s) for the imported definition(s), i.e. prefixing the imported definition (which causes the name clash) by the identifier of the module in which it has been defined; the prefix and the identifier shall be separated by a dot ("."). If the type of the component referenced in a connection operation is known (either when the component reference is a variable or value returned from a function or the type is defined the runs on, mtc or system clause of the calling function), the referenced port declaration shall be present in this component type.

There is one exception to this rule: when **in the context** of an enumerated type (see clause 6.2.4), an enumerated value is clashing with the name of a definition in the importing module, the enumerated value shall take precedence and the definition in the importing module shall be referenced by using its qualified name (see example 4 below in this clause).

In cases where there are no ambiguities the prefixing need not (but may) be present when the imported definitions are used. When the definition is referenced in the same module where it is defined, the module identifier of the module (the current module) also may be used for prefixing the identifier of the definition. For the latter case, prefixing shall only be used for definitions with global visibility for the module.

***Restrictions***

In addition to the general static rules of TTCN‑3 given in clause 5, the following restrictions apply:

a) An import statement shall only be used in the module definitions part and not be used within a control part, function definition, and alike.

b) Only top-level visible definitions of a module may be imported. Definitions which are top-level but invisible to the importing module or which occur at a lower scope (e.g. local constants defined in a function) shall not be imported.

c) A definition is imported together with its name and all local definitions.

NOTE 5: A local definition, e.g. a field name of a user-defined record type or an enumerated value, has only meaning in the context of the definitions in which it is defined, e.g. a field name of a record type can only be used to access a field of the record type and not outside this context.

In particular, importing an enumerated type does not impose the restriction given in clause 6.2.4 on global names defined in the importing module.

d) A definition is imported together with all information of referenced definitions that are necessary for the usage of the imported definition, independent of the visibility of the referenced definitions (see clause 8.2.5).

NOTE 6: If module C imports a definition from module B that uses a type reference defined in module A, the corresponding information necessary for the usage of that type is automatically imported into module C (see example 5 below in this clause). Identifiers of referenced definitions are not automatically imported.

In particular, if module C imports global value or template definitions (e.g. constants, module parameters, templates) or local definitions (e.g. formal parameters of templates, functions, etc., or constants and variables of component types) of an enumerated type from module B, the enumerated values of this type (i.e. the identifiers) are implicitly and automatically imported to module C. That is, the enumerated values are known when an enumerated value or template is used in module C (e.g. when an actual parameter is passed or a value is assigned to a component variable). Note that this implicit importing does not impose the restriction given in clause 6.2.4 on global names defined in module C.

e) If the referenced definitions are wished to be used in the importing module, they shall be explicitly imported either directly from its source module or indirectly by importing the import statements of a module importing it (see clause 8.2.3.7).

f) When importing a function, altstep or test case the corresponding behaviour specifications and all definitions used inside the behaviour specifications remain invisible for the importing module.

g) The language specification (see clause 8.1) of the import statement shall not override the language specification of the importing module.

h) The language specification of the import statement shall be identical to the language specification of the source module from which definitions are imported (see clause 8.2.3.8) provided a language specification is defined in the source module. If not, the language specification in the import statement is taken as the language specification of the source module. If the source module uses however language concepts not being part of that language specification, this causes an error for the import statement.

***Examples***

EXAMPLE 1: Selected import examples

**module** MyModuleA

{ :

// Scope of the imported definitions is global to MyModuleA

**import** **from** MyModuleB **all**; // import of all definitions from MyModuleB

**import from** MyModuleC { // import of selected definitions from MyModuleC

**type** MyType1, MyType2; // import of types MyType1 and MyType2

**template** **all** // import of all templates

}

:

**function** MyBehaviourC()

{

// import cannot be used here

:

}

**:**

**control**

{

// import cannot be used here

:

}

}

EXAMPLE 2: Use of imported definitions and visibility of definitions referenced by them

**module** ModuleONE {

**modulepar** **integer** ModPar1 := …;

**type** **record** RecordType\_T1 {

**integer** Field1\_T1,

**:**

}

**type** **record** RecordType\_T2 {

RecordType\_T1 Field1\_T2,

:

}

**const** **integer** MyConst := …;

**template** RecordType\_T2 Template\_T2 (RecordType\_T1 TempPar\_T2):= { // parameterized template

Field1\_T2 := …,

:

}

} // end module ModuleONE

**module** ModuleTWO {

**import** **from** ModuleONE {

**template** Template\_T2

}

// Only the names Template\_T2 and TempPar\_T2 will be visible in ModuleTWO. Please note, that

// the identifier TempPar\_T2 can only be used when modifying Template\_T2. All information

// necessary for the usage of Template\_T2, e.g. for type checking purposes, are imported

// for the referenced definitions RecordType\_T1, Field1\_T2, etc., but their identifiers are

// not visible in ModuleTWO.

// This means, e.g. it is not possible to use the constant MyConst or to declare a

// variable of type RecordType\_T1 or RecordType\_T2 in ModuleTWO without explicitly importing  
 // these types.

**import** **from** ModuleONE {

**modulepar** ModPar2

}

// The module parameter ModPar2 of ModuleONE is imported from ModuleONE and

// can be used like an integer constant

} // end module ModuleTWO

**module** ModuleTHREE {

**import** **from** ModuleONE **all**; // imports all definitions from ModuleONE

**type port** MyPortType **message** {

**inout** RecordType\_T2 // Reference to a type defined in ModuleONE

}

**type component** MyCompType {

**var integer** MyComponentVar := ModPar2;

// Reference to a module parameter of ModuleONE

**:**

}

**function** MyFunction () **return** **integer** {

**return** MyConst // Reference to a module constant of ModuleONE

}

**testcase** MyTestCase (**out** RecordType\_T2 MyPar) **runs** **on** MyCompType {

:

MyPort.**send**(Template\_T2); // Sending a template defined in ModuleONE

:

}

} // end ModuleTHREE

**module** ModuleFOUR {

**import from** ModuleTHREE {

**testcase** MyTestCase

}

// Only the name MyTestCase will be visible and usable in ModuleFOUR.

// Type information for RecordType\_T2 is imported via ModuleTHREE from ModuleONE and

// Type information for MyCompType is imported from ModuleTHREE. All definitions

// used in the behaviour part of MyTestCase remain hidden for the user of ModuleFOUR.

} // end ModuleFOUR

EXAMPLE 3: Handling of name clashes

**module** MyModuleA {

:

**type** **bitstring** MyTypeA;

**import from** SomeModuleC {

**type** MyTypeA, // Where MyTypeA is of type character string

MyTypeB // Where MyTypeB is of type character string

}

**:**

**control** {

:

**var** SomeModuleC.MyTypeA MyVar1 := "Test String"; // Prefix shall be used

**var** MyTypeA MyVar2 := '10110011'B; // This is the original MyTypeA

:

**var** MyTypeB MyVar3 := "Test String"; // Prefix need not be used …

**var** SomeModuleC.MyTypeB MyVar3 := "Test String"; // … but it can be if wished

:

}

}

NOTE 7: Definitions with the same name defined in different modules are always assumed to be different, even if the actual definitions in the different modules are identical. For example, importing a type that is already defined locally, even with the same name, would lead to two different types being available in the module.

EXAMPLE 4: Name clash between enumerated values and global definitions

**module** A {

**type** **enumerated** MyEnumType {enumX, enumY, enumZ}

**type** **enumerated** MyEnumType2 {enumX, enumY, enumZ}

}

**module** B {

**import** **from** A **all**;

**const** MyEnumType enumY := enumX; // this is not allowed as enumerated values restrict

// global names (see clause 6.2.4)

**const** MyEnumType2 enumX := enumX;// this is likewise not allowed

**const** **integer** enumZ := 0;

**modulepar** MyEnumType px\_MyModulePar1 := enumY

// the default value of the module parameter will be the value enumY, as the type of

// px\_MyModulePar1 creates the context of MyEnumType and in this context enumerated values

// take precedence over global definition names; note that for the same context reason there

// in no name clash between the enumerated values defined in MyEnumType and in MyEnumType2

**modulepar** MyEnumType px\_MyModulePar2 := B.enumY

// the default value of the module parameter will be the value enumX, as the prefix

// identifies the constant definition enumY unambiguously, which has the value enumX

**modulepar** **integer** px\_IntegerPar := enumZ;

// the default value of the module parameter will be 0 as this assignment is not in the

// context of an enumerated type, hence no name clash occurs

**modulepar** MyEnumType px\_MyModulePar3 := B.enumX

// causes an error as px\_MyModulePar3 and the constant enumX has different types

}

EXAMPLE 5: Importing local definitions transitively

**module** A {

**type enumerated** MyEnum\_Type { enumX, enumY, enumZ}

**type record** MyRec { **integer** a, **integer** b }

**type component** MyComp { **var** MyRec v\_Rec := { a := 5 } }

}

**module** B {

**import** **from** A **all**;

**modulepar** MyEnum\_Type px\_MyModulePar := enumY;

**type component** MyCompUser **extends** MyComp {}

}

**module** C {

**import from** B **all**;

**testcase** TC() **runs on** MyCompUser {

**if** (px\_MyModulePar == enumY) {

// the enumerated value enumY is know in C without explicitly importing it from A

**setverdict**(**pass**)

}

**if** (v\_Rec.a == 5) {

v\_Rec.b := v\_Rec.a;

// Both the variable name v\_Rec and the record field names are known in C without

// explicitly importing them from A

**setverdict** (**pass**)

}

}

}

#### 8.2.3.2 Importing single definitions

Single visible definitions can be imported by referring to the definition kind and the definition name(s). The import of single definitions can be used in combination with imports of groups (see clause 8.2.3.3), with imports of definitions of the same kind (see clause 8.2.3.4), and with imports of import statements (see clause 8.2.3.7).

***Syntactical Structure***

[ *Visibility* ] **import** **from** *ModuleId* "{"

{

(

( **type** { *TypeDefIdentifier* [ "," ] } ) |

( **template** { *TemplateIdentifier* [ "," ] } ) |

( **const** { *ConstIdentifier* [ "," ] } ) |

( **testcase** { *TestcaseIdentifier* [ "," ] } ) |

( **altstep** { *AltstepIdentifier* [ "," ] } ) |

( **function** { *FunctionIdentifier* [ "," ] } ) |

( **signature** { *SignatureIdentifier* [ "," ] } ) |

( **modulepar** { *ModuleParIdentifier* [ "," ] } )

)

[ ";" ]

}

"}" [ ";" ]

***Semantic Description***

See clause 8.2.3. Import of an invisible definition shall cause an error.

***Restrictions***

In addition to the general static rules of TTCN‑3 given in clause 5, the following restrictions apply:

1. The definition to be imported shall be defined in the module from which it is to be imported and shall be visible to the importing module.
2. See the restrictions given in clause 8.2.3.

***Examples***

**import from** MyModuleA {

**type** MyType1 // imports one type definition from MyModuleA only

}

**import from** MyModuleB {

**type** MyType2, Mytype3, MyType4; // imports three types,

**template** MyTemplate1; // imports one template, and

**const** MyConst1, MyConst2 // imports two constants

}

#### 8.2.3.3 Importing groups

Groups of definitions may be imported. The import of groups can be used in combination with imports of single definitions (see clause 8.2.3.2), with imports of definitions of the same kind (see clause 8.2.3.4), and with imports of import statements (see clause 8.2.3.7).

It is allowed to import sub‑groups (i.e. a group which is defined within another group) directly, i.e. without the groups in which the sub-group is embedded. If the name of a sub-group that should be imported is identical to the name of another sub-group in the same module (see clause 8.2.2), the dot notation shall be used to identify the sub-group to be imported uniquely.

If some visible definitions of a group are wished not to be imported, their kinds and identifiers shall be listed in the exception list within a pair of curly brackets following the **except** keyword. The **all** keyword is also allowed to be used in the exception list; this will exclude all definitions of the same kind from the import statement.

***Syntactical Structure***

[ *Visibility*] **import** **from** *ModuleId* "{"

{

( **group** { *QualifiedIdentifier* [ **except** "{" *ExceptSpec* "}" ] [ "," ] } )

[ ";" ]

}

"}" [ ";" ]

***Semantic Description***

The effect of importing a group is identical to an **import** statement that lists all visible definitions (including sub‑groups) of this group except of those that are listed in the except specification. See also clause 8.2.3. Import statements contained in the group or in its subgroups are not part of this list, only definitions are.

It is important to point out, that the except statement does not exclude the definitions listed from being imported in general; all statements importing definitions of the same kind can be seen as a shorthand notation for an equivalent list of identifiers of single definitions. The **except** statement excludes definitions from this single list only.

***Restrictions***

In addition to the general static rules of TTCN‑3 given in clause 5, the following restrictions apply:

1. The group to be imported shall be defined in the module from which it is to be imported.
2. See the restrictions given in clause 8.2.3.

***Examples***

**import from** MyModule { **group** MyGroup } // includes all visible definitions from MyGroup

**import from** MyModule {

**group** MyGroup **except** {

**type** MyType3, MyType5; // excludes the two types from the import statement,

**template all** // excludes all templates defined in MyGroup

// from the import statement

// but imports all other visible definitions of MyGroup

}

}

**import from** MyModule{

**group** MyGroup

**except** { **type** MyType3 };// imports all visible types of MyGroupexcept MyType3

**type** MyType3 // imports MyType3 explicitly

}

#### 8.2.3.4 Importing definitions of the same kind

The **all** keyword may be used to import all visible definitions of the same kind of a module. The **all** keyword used with the **constant** keyword identifies all visible constants declared in the definitions part of the module the import statement refers to. Similarly the **all** keyword used with the **function** keyword identifies all visible functions and all visible external functions defined in the module the import statement denotes.

If some visible declarations of a kind are wished to be excluded from the given import statement, their identifiers shall be listed following the **except** keyword.

The import of visible definitions of the same kind can be used in combination with imports of single visible definitions (see clause 8.2.3.2), with imports of groups (see clause 8.2.3.3), and with imports of import statements (see clause 8.2.3.7).

***Syntactical Structure***

[ *Visibility*] **import** **from** *ModuleId* "{"

{

(

( **type** **all** [ **except** { *TypeDefIdentifier* [ "," ] } ] ) |

( **template** **all** [ **except** { *TemplateIdentifier* [ "," ] } ] ) |

( **const** **all** [ **except** { *ConstIdentifier* [ "," ] } ] ) |

( **testcase** **all** [ **except** { *TestcaseIdentifier* [ "," ] } ] ) |

( **altstep** **all** [ **except** { *AltstepIdentifier* [ "," ] } ] ) |

( **function** **all** [ **except** { *FunctionIdentifier* [ "," ] } ] ) |

( **signature** **all** [ **except** { *SignatureIdentifier* [ "," ] } ] ) |

( **modulepar** **all** [ **except** { *ModuleParIdentifier* [ "," ] } ] )

)

[ ";" ]

}

"}" [ ";" ]

***Semantic Description***

The effect of importing definitions of the same kind is identical to an **import** statement that lists all visible definitions of that kind except of those that are listed in the except specification. See also clause 8.2.3.

NOTE: If the list of all visible definitions of that kind except of those that are listed in the **except** specification is empty, the import statement has no effect. This case does not lead to an error.

***Restrictions***

In addition to the general static rules of TTCN‑3 given in clause 5, the following restrictions apply:

1. See the restrictions given in clause 8.2.3.

***Examples***

**import from** MyModule {

**type all**; // imports all types of MyModule

**template all** // imports all templates of MyModule

}

**import from** MyModule {

**type** **all** **except** MyType3, MyType5; // imports all types except MyType3 and MyType5

**template** **all** // imports all templates defined in Mymodule

}

#### 8.2.3.5 Importing all definitions of a module

All visible definitions of a module definitions part may be imported using the **all** keyword next to the module name.

If some visible definitions are wished not to be imported, their kinds and identifiers shall be listed in the exception list within a pair of curly brackets following the **except** keyword. The **all** keyword is also allowed to be used in the exception list; this will exclude all visible declarations of the same kind from the import statement.

NOTE 1: If the list of all visible definitions of a module except of those that are listed in the **except** specification is empty, the import statement has no effect. This case does not lead to an error.

NOTE 2: Importing all definitions of a module imports only definitions declared directly in that module, but does not import the import statements of that module (see also clause 8.2.3.7).

***Syntactical Structure***

[ *Visibility*] **import** **from** *ModuleId*

**all**

[

{

**except** "{"

( **group** { *QualifiedIdentifier* [ "," ] } | **all** ) |

( **type** { *TypeDefIdentifier* [ "," ] } | **all** ) |

( **template** { *TemplateIdentifier* [ "," ] } | **all** ) |

( **const** { *ConstIdentifier* [ "," ] } | **all** ) |

( **testcase** { *TestcaseIdentifier* [ "," ] } | **all** ) |

( **altstep** { *AltstepIdentifier* [ "," ] } | **all** ) |

( **function** { *FunctionIdentifier* [ "," ] } | **all** ) |

( **signature** { *SignatureIdentifier* [ "," ] } | **all** ) |

( **modulepar** { *ModuleParIdentifier* [ "," ] } | **all** )

"}"

[ ";" ]

}

]

[ ";" ]

***Semantic Description***

The effect of importing all visible definitions of a module is identical to an **import** statement that lists all importable definitions of that module except of those that are listed in the except specification. See also clause 8.2.3.

***Restrictions***

In addition to the general static rules of TTCN‑3 given in clause 5, the following restrictions apply:

1. If all visible definitions of a module are imported by using the all keyword, no other form of import (import of single definitions, import of the same kind, etc.) shall be used for the same import statement.
2. In the set of except statements for an all import, only one except statement per kind of definition (i.e. for a group, type, etc.) is allowed.

***Examples***

**import from** MyModule **all**; // includes all definitions from MyModule

**import from** MyModule **all except** {

**type** MyType3, MyType5; // excludes these two types from the import statement and

**template all** // excludes all templates declared in MyModule,

// from the import statement

// but imports all other definitions of MyModule

}

#### 8.2.3.6 Import definitions from other TTCN‑3 editions and from non-TTCN‑3 modules

In cases when visible definitions are imported from modules from other TTCN‑3 editions or from other sources than TTCN‑3 modules, the language specification (see clause 8.1) shall be used to denote the language (may be together with a version number) of the source (e.g. module, package, library or even file) from which definitions are imported. It consists of the **language** keyword and a subsequent textual declaration of the denoted language.

The use of the language specification is optional when importing from a TTCN‑3 module of the same edition as the importing module. The TTCN‑3 language identifiers defined in clause 8.1 are to be used. Package identifiers from ES 202 781 [i.11], ES 202 782 [i.14], ES 202 784 [i.12] and ES 202 785 [i.13] can be used in addition. Identifiers for other languages are defined in the language mapping parts of TTCN‑3, i.e. in ES 201 873-7 [i.5], ES 201 873‑8 [i.6] and ES 201 873-9 [i.7].

When an incompatibility is discovered between the language and/or package identification (including implicit identification by omitting the language specification) and the syntax of the module from which definitions are imported, tools shall provide reasonable effort to resolve the conflict.

***Syntactical Structure***

[ *Visibility*] **import** **from** *ModuleIdentifier* [ *LanguageSpec* ] … [ ";" ]

***Semantic Description***

TTCN‑3 supports the referencing of elements defined in other TTCN‑3 editions (*versioned elements*) or other languages (*foreign elements*) from within TTCN‑3 modules. Such elements can be used in a TTCN‑3 module of a given edition only if they have a TTCN‑3 view in that TTCN‑3 edition. The term TTCN‑3 view can be best explained by considering the case when the definition of a TTCN‑3 element is based on another TTCN‑3 element, the information content of the referenced element shall be available and is used for the new definition. For example, when a template is defined based on a structured type, the identifiers and types of fields of the base type shall be accessible and are used for the template definition. In a similar way, when a base type is a versioned or foreign element it shall provide the same information content as would be required from a TTCN‑3 type declaration. The versioned or foreign element, naturally, may contain more information than required by TTCN‑3. The TTCN‑3 view of a versioned or foreign element means that part of the information carried by that element, which is necessary to use it in TTCN‑3. Obviously, the TTCN‑3 view of a versioned or foreign element may be the full set or a subset of the information content of that element but never a superset. There may be versioned or foreign element without a TTCN‑3 view (zero TTCN‑3 view), i.e. for some reason no TTCN‑3 definition in the given edition could be based on them.

To make declarations of versioned or foreign element visible in TTCN‑3 modules, their names shall be imported just like definitions in other TTCN‑3 modules of the given edition. When imported, only the TTCN‑3 view of the versioned or foreign element will be seen from the importing TTCN‑3 module. There are two main differences between importing TTCN‑3 elements of the same editions and versioned or foreign elements:

* to import from a TTCN‑3 module of another edition or from a non-TTCN‑3 module, the import statement shall contain an appropriate language identifier string;
* only versioned or foreign elements with a TTCN‑3 view of a given edition are importable into a TTCN‑3 module of that edition.

Importing can be done automatically using the all directive, in which case all importable objects shall automatically be selected by the testing tool, or done manually by listing names of elements to be imported. Naturally, in the second case only importable elements are allowed in the list.

When importing definitions from a non-TTCN-3 language, two principle approaches exist:

* With an implicit language mapping, non-TTCN-3 definitions are mapped internally in the TTCN-3 tool to the respective TTCN-3 definitions as defined by the language mapping; the importing module works with the internal representations of the imported definitions.
* With an explicit language mapping, non-TTCN-3 definitions are mapped directly to separate TTCN-3 definitions; the importing module imports the generated TTCN-3 and works with the mapped TTCN-3 definitions.

These lead to three options when using non-TTCN-3 language modules in a TTCN-3 specification:

* The import statement imports the non-TTCN-3 module; the tool uses the internal representation of the implicit mapping of the non-TTCN-3 module's definitions according to the language mapping specification of that language.
* The import statement imports the non-TTCN-3 module; the tool imports from a TTCN-3 module which is an explicit mapping of the non-TTCN-3 module's definitions according to the language mapping specification of that language.
* The import statement imports the explicit TTCN-3 representation of the non-TTCN-3 module; the tool imports the TTCN-3 module which is an explicit mapping of the non-TTCN-3 module according to the language mapping specification of that language.

***Restrictions***

In addition to the general static rules of TTCN‑3 given in clause 5, the following restrictions apply:

1. The language specification may only be omitted if the referenced module contains TTCN‑3 notation and the TTCN‑3 version is known.
2. Definitions imported from non-TTCN-3 language sources have by default public visibility provided that no other rules are defined in the respective language mapping (see ES 201 873-7 [i.5], ES 201 873-8 [i.6] or ES 201 873-9 [i.7], respectively).

***Examples***

**module** MyNewModule {

**import from** MyOldModule **language** "TTCN‑3:2003" {

**type** MyType

}

}

**module** MyNewestModule {

**import** **from** MyNewModule **language** "TTCN‑3:2010" { **import** **all** };

// the language specifications shall be identical, see clause 8.2.3.8

}

NOTE: The import mechanism is designed to allow the re-use of definitions from other TTCN‑3 editions or from other non-TTCN-3 language sources. The rules for importing definitions from specifications written in other languages, e.g. SDL packages, may follow the TTCN‑3 rules or may have to be defined separately.

#### 8.2.3.7 Importing of import statements from TTCN-3 modules

Visible import statements of TTCN-3 modules can be imported by other TTCN‑3 modules.

***Syntactical Structure***

[ *Visibility* ] **import** **from** *ModuleIdentifier* [ *LanguageSpec* ]

"{" **import** **all** [ ";" ] "}" [ ";" ]

***Semantic Description***

TTCN‑3 supports importing of visible import statements from other TTCN-3 modules. This means that import statements of the module, from which the import statements are imported, are re-imported to the importing module. For example, if module B imports the import statements of module A, everything that is imported by A using import statements visible for module B, is also imported by B. If another module C imports all import statements from B, then C imports all what A is importing - provided that the import statements are visible to modules B and C.

It is not possible to import individual import statements of another module.

The import of import statements can be used in combination with imports of single definitions (see clause 8.2.3.2), with imports of groups (see clause 8.2.3.3), and with imports of definitions of the same kind (see clause 8.2.3.4).

***Restrictions***

In addition to the general static rules of TTCN‑3 given in clause 5, the following restrictions apply:

a) The restrictions given in clause 8.2.3.1 apply.

b) The restrictions given in clause 8.2.3.6 apply.

c) Importing of import statements is only possible from other TTCN-3 modules, i.e. the language specification (see clause 8.1) shall denote a TTCN-3 edition only, not a non-TTCN-3 language.

***Examples***

EXAMPLE: Importing of visible import statements

**module** A {

**type** **integer** T1;

**type** **integer** T2;

**template** T1 t1 := ?;

**template** T2 t2 := \*;

:

}

**module** B {

**public** **import** **from** A { **type** T1 }

**type** **charstring** T2;

**template** T1 t1 := ( 1, 2, 3 );

:

}

**module** C {

**public** **import** **from** B { **import** **all** } // imports the import statements only

**public** **import** **from** B { **type** T2 } // imports the type B.T2

**import** **from** A { **template** **all** }

:

}

**module** D {

**private** **import** **from** C { **import** **all** } // imports the import statements only

:

}

**module** E {

**import** **from** D { **import** **all** }

:

}

// yields the following

// module A knows

// A.T1 (defined)

// A.T2 (defined)

// A.t1 (defined)

// A.t2 (defined)

//

// module B knows

// A.T1 (imported)

// B.T2 (defined)

// B.t1 (defined)

//

// module C knows

// A.T1 (imported from B importing it from A)

// B.T2 (imported)

// A.t1 (imported)

// A.t2 (imported)

//

// module D knows

// A.T1 (imported from C importing it from B importing it from A)

// B.T2 (imported from C importing it from B)

// A.t2 and A.t2 are not imported as their imports are private to C

//

// module E "knows" nothing

// as the imports of D are private and not visible to E

#### 8.2.3.8 Compatibility of language specifications in imports

When importing into a TTCN-3 module, the language specification (see clause 8.1) of the importing module, the language specification of the import statement and the language specification of the source module, where the imported definitions are defined, have to be compatible according to the following rules.

***Restrictions***

In addition to the general static rules of TTCN‑3 given in clause 5, the following restrictions apply:

a) A TTCN-3 module of any TTCN-3 edition can import from a non-TTCN-3 language source provided that a TTCN-3 view for the non-TTCN-3 language exists (see clause 8.2.3.6).

b) Definitions or import statements are imported according to the language specification in which the definition or the import statement is defined. If no language specification is given in this module, the language specification of the import statement with which those definitions or import statements are to be imported, is used instead. If the module, within which the definitions or the import statements are defined, and the import statement for these definitions or import statements provide both a language specification, then they shall be identical. If none of the two has a language specification, the language specification has to be known from other sources, which is tool specific.

c) A TTCN-3 module shall only import from earlier or same editions of TTCN-3 but not from later editions, e.g. the TTCN-3 language specification in an import statement has to be lower or equal to the TTCN-3 language specification of the importing module.

### 8.2.4 Definition of friend modules

Modules can define other modules to be friends.

***Syntactical Structure***

[ **private** ] **friend module** *ModuleIdentifier* { **","** *ModuleIdentifier* } **";"**

***Semantic Description***

Friendship to modules is defined by the exporting module (the module that declares the definitions) not by the importing module (the module that uses the module definitions of another module). Friendship can be cyclic.

If a module is friend to a module from which it imports top-level definitions, all top-level definitions with public and friend visibility are visible to the friend module. For non-friend modules, public top-level definitions are visible only.

Missing friend modules shall not cause an error.

NOTE: Friend modules can be checked by tools, however at most warning are to be issued if a friend module is missing.

***Restrictions***

In addition to the general static rules of TTCN 3 given in clause 5, the following restrictions apply:

a) Only private visibility can be defined for friend definitions as they are always private.

***Examples***

**module** MyModuleA {

**friend** **module** MyModuleB,MyModuleC;

}

// MyModuleB and MyModuleC are friends of MyModuleA

**module** MyModuleB {

**friend** **module** MyModuleA;

}

// MyModuleA is friend of MyModuleB

**module** MyModuleC {

}

### 8.2.5 Visibility of definitions

Top-level module definitions and import statements have a visibility, which can be explicitly set. They are by default **public** except for imported and friend definitions. Import definitions are by default **private**. Friend definitions are **private** only. Group definitions are **public** only.

***Syntactical Structure***

[ **public** | **friend** | **private** ]

***Semantic Description***

The visibility controls whether a top-level definition or an import statement is importable by another module.

Three visibilities are distinguished:

* A top-level definition or an import statement with **public** visibility is importable by any other module.
* A top-level definition or an import statement with **friend** visibility is importable by friend modules only (see clause 8.2.4).
* A top-level definition or an import statement with **private** visibility cannot be imported at all.

NOTE: As specified in restriction e) of clause 8.2.3.1, this means that importable definitions are imported together with all information of referenced definitions that are necessary for the usage of the importable definition, even if the referenced definition is private. Only the identifier of the referenced definition is not visible in the importing TTCN-3 module.

The visibility of groups is always **public**. The visibility of imported definitions is by default **private**. All other module definitions are by default **public**.

The visibility of a top-level definition or an import statement defines their importability by another module. If the top‑level definition or the import statement is part of a group, this has no effect on the importability of the module definition. The importability of a top-level definition by another module is summarized in table 9, the importability of import statements in table 10.

Table 9: Visibility and import of module definitions

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Visibility of module definition | Module definition importable directly by a  non-friend module | Module definition importable directly by a  friend module | Module definition importable via group import by a non-friend module | Module definition importable via group import by a friend module |
| **public** | yes | yes | yes | yes |
| **friend** | no | yes | no | yes |
| **private** | no | no | no | no |

Table 10: Visibility and import of import statements

|  |  |  |
| --- | --- | --- |
| Visibility of import | Import imported by a non-friend module | Import imported by a friend module |
| **public** | yes | yes |
| **friend** | no | yes |
| **private** | no | no |

***Restrictions***

No specific restrictions in addition to the general static rules of TTCN‑3 given in clause 5.

***Examples***

**module** MyModuleA {

**friend** **module** MyModuleC;

**private** **type** **integer** MyInteger;

// MyInteger is not visible to other modules

**friend** **type** **charstring** MyString;

// MyString is visible to friend modules

**public** **type** **boolean** MyBoolean;

// MyBoolean is visible to all modules

}

**module** MyModuleB {

**import** **from** MyModuleA **all**;

// MyString and MyInteger are not visible and are not imported

// MyBoolean is imported

}

**module** MyModuleC {

**import** **from** MyModuleA **all**;

// MyInteger is not visible and is not imported

// MyString and MyBoolean are imported

}

## 8.3 Module control part

The module control part may contain local definitions (i.e. constants or templates), local instances (i.e. variables or timers) and describe the selection, parameterization and execution order (possibly repetitive) of the actual test cases. A test case shall be defined in the module definitions part or imported from another module, and called in the control part.

The control part of a module calls the test cases with actual parameters and controls their execution. Program statements can be used to specify the selection and execution order of the test cases. Definitions made in the module control part have local visibility, i.e. can be used within the control part only.

This is explained in more detail in clause 26.

EXAMPLE:

**module** MyTestSuite

{ // This module contains definitions …

:

**const** **integer** MyConstant := 1;

**type record** MyMessageType { … }

**template** MyMessageType MyMessage := { … }

:

**function** MyFunction1() { … }

**function** MyFunction2() { … }

**:**

**testcase** MyTestcase1() **runs on** MyMTCType { … }

**testcase** MyTestcase2() **runs on** MyMTCType { … }

:

// … and a control part so it is executable

**control**

{

**var** **boolean** MyVariable; // local control variable

:

**execute**( MyTestCase1()); // sequential execution of test cases

**execute**( MyTestCase2());

**:**

}

}

# 9 Port types, component types and test configurations

TTCN‑3 allows the (dynamic) specification of concurrent test configurations (or configuration for short). A configuration consists of a set of inter-connected test components with well-defined communication ports and an explicit test system interface which defines the borders of the test system (see figure 4).

NOTE: Additional configuration and deployment support for TTCN-3 is defined in the optional package [i.11].



Figure 4: Conceptual view of a typical TTCN‑3 test configuration

Within every configuration there shall be one (and only one) Main Test Component (MTC). Test components that are not MTCs are called parallel test components or PTCs. The MTC shall be created by the system automatically at the start of each test case execution. The behaviour defined in the body of the test case shall execute on this component. During execution of a test case, other components can be created dynamically by the explicit use of the **create** operation.

Test case execution shall end when the MTC terminates. All other PTCs are treated equally i.e. there is no explicit hierarchical relationship among them and the termination of a single PTC terminates neither other components nor the MTC. When the MTC terminates, the test system has to stop all PTCs not terminated by the moment when the test case execution is ended.

Communication between test components and between the components and the test system interface is achieved via communication ports (see clause 9.1).

Test component types and port types, denoted by the keywords **component** and **port**, shall be defined in the module definitions part. The actual configuration of components and the connections between them is achieved by performing **create** and **connect** operations within the test case behaviour. The component ports are connected to the ports of the test system interface by means of the **map** operation (see clause 21.1.1).

## 9.1 Communication ports

Test components are connected via their ports, i.e. connections among components and between a component and the test system interface are port-oriented. Each port is modelled as an infinite FIFO queue which stores the incoming messages or procedure calls until they are processed by the component owning that port (see figure 5).

NOTE: While TTCN‑3 ports are infinite in principle in a real test system they may overflow. This is to be treated as a test case error (see clause 24.1).



Figure 5: The TTCN‑3 communication port model

TTCN‑3 connections are port-to-port and port-to-test system interface connections (see figure 6). There are no restrictions on the number of connections a component may maintain. One-to-many connections are also allowed (e.g. figure 6 (g) or (h)).

***Restrictions***

In addition to the general static rules of TTCN‑3 given in clause 5, the following restrictions apply:

a) The following connections are not allowed (see figure 7):

* A port owned by a component A shall not be connected with two or more ports owned by the same component (figure 7 (a) and (e)).
* A port of a test system interface cannot have connection with more than one port owned by a component A. This means, connections as shown in figure 7 (b) are not allowed**.**
* A port owned by a component A shall not be connected with two or more ports owned by a component B (see figure 7(c)).
* A port owned by a component A can only have a one-to-one connection with the test system interface. This means, connections as shown in figure 7 (d) are not allowed.
* Connections within the test system interface are not allowed (see figure 7 (f)).
* A port that is connected shall not be mapped and a port that is mapped shall not be connected (see figure 7 (g)).

b) Since TTCN‑3 allows dynamic configurations and addresses, the restrictions on connections cannot always be checked at compile-time. The checks shall be made at runtime and shall lead to a test case error when failing.



Figure 6: Allowed connections



Figure 7: NOT allowed connections

## 9.2 Test system interface

TTCN‑3 is used to test implementations. The object being tested is known as the Implementation Under Test or IUT. The IUT may offer direct interfaces for testing or it may be part of system in which case the tested object is known as a System Under Test or SUT. In the minimal case the IUT and the SUT are equivalent. In the present document the term SUT is used in a general way to mean either SUT or IUT.

In a real test environment test cases need to communicate with the SUT. However, the specification of the real physical connection is outside the scope of TTCN‑3. Instead, a well defined (but abstract) test system interface shall be associated with each test case. A test system interface definition is identical to a component definition, i.e. it is a list of all possible communication ports through which the test case is connected to the SUT.

The test system interface statically defines the number and type of the port connections to the SUT during a test run. However, the connections between the test system interface and the TTCN‑3 test components are dynamic in nature and may be modified during a test run by using **map** and **unmap** operations (see clause 21.1).

A component type definition is used to define the test system interface because, conceptually, component type definitions and test system interface definitions have the same form (both are collections of ports defining possible connection points). When used as test system interfaces, components cannot make use of any constants, variables and timers declared in the component type.

***Syntactical Structure***

The same as a component type definition (see clauses 6.2.10 and 6.2.10.1).

***Semantic Description***

Generally, a component type reference defining the test system interface shall be associated with every test case using more than one test component. The ports of the test system interface shall automatically be instantiated by the system together with the MTC when the test case execution starts.

The operation returning the component reference of the test system interface is **system**. This shall be used to address the ports of the test system.

In the case where the MTC is the only component that is instantiated during test execution, a test system interface need not be associated to the test case. In this case, the component type definition associated with the MTC implicitly defines the corresponding test system interface.

Variables, timers and constants declared in component types, which are used as test system interfaces will have no effect.

***Restrictions***

In addition to the general static rules of TTCN‑3 given in clause 5, the following restrictions apply:

1. The same as for component type definitions (see clauses 6.2.10 and 6.2.10.1).

***Examples***

EXAMPLE 1: Explicit definition of a test system interface

**type** **component** MyMTCType

{

**var** integer MyLocalInteger;

**timer** MyLocalTimer;

**port** MyMessagePortType PCO1

}

**type component** MyTestSystemInterface

{

**port** MyMessagePortType PCO1, PCO2;

**port** MyProcedurePortType PCO3

}

// MyTestSystemInterface is the test system interface

**testcase** MyTestcase1 () **runs** **on** MyMTCType **system** MyTestSystemInterface {

// establishing the port connections

**map**(**mtc**:PCO1, **system**:PCO2);

// the testcase behaviour

// …

}

EXAMPLE 2: Implicit definition of a test system interface

// MyMTCType is the test system interface

**testcase** MyTestcase2 () **runs** **on** MyMTCType {

// map statements are not needed

// the testcase behaviour

// …

}

# 10 Declaring constants

TTCN-3 constants are runtime constants. After value assignment, they do not change their value during test execution. They can be used on the right hand side of assignments, in expressions, in actual parameters, and in template definitions. Constants used within type definitions have to have values known at compile-time.

***Syntactical Structure***

**const** *Type* { *ConstIdentifier* [ *ArrayDef* ] ":=" *ConstantExpression* [ "," ] } [ ";" ]

***Semantic Description***

A constant assigns a name to a fixed value. A value is assigned only once to a constant, at the place of its declaration. The constant does not change its value during test execution. The constant is defined only once, but can be referenced multiple times in a TTCN-3 module.

If functions are used for the initialization of constants, it is strongly advised to adhere to the rules defined in clause 16.1.4. Not following these rules may cause non-deterministic test executions.

Optional fields of record and set constants or constant fields can be initialized explicitly or implicitly. For implicit initialization of the optional fields of a constant or a constant field, an **optional** attribute with the value **"implicit omit"** (see clause 27.7) shall be associated with it either directly or via the attribute distribution (scoping) mechanism (see clause 27.1.1).

***Restrictions***

In addition to the general static rules of TTCN‑3 given in clause 5, the following restrictions apply:

a) Constants shall not be of port type.

NOTE: The only value that can be assigned to global constants or component constants of default or component types is the special value **null**.

b) Constant expressions initializing constants, which are used in type and array definitions, shall only contain literals, predefined functions except of rnd (see clause 16.1.2), operators specified in clause 7.1, and other constants obeying the limitations of this clause.

c) Using the dot notation (see clauses 6.2.1.1, 6.2.2.1 and 6.2.5.1) and index notation (see clauses 6.2.3 and 6.2.7) for referencing a field, alternative or element of an **address** value, which actual value is **null** shall cause an error.

***Examples***

**const** **integer** MyConst1 := 1;

**const** **boolean** MyConst2 := **true**, MyConst3 := **false**;

# 11 Declaring variables

TTCN-3 variables are statically typed variables. Variables are either value variables to store values or template variables to store templates.

Variables can be of simple basic types, basic string types, structured types, special data types (including subtypes derived from these types) as well as address, component or default types.

Variables can be declared and used in the module control part, test cases, functions and altsteps. Additionally, variables can be declared in component type definitions. These variables can be used in test cases, altsteps and functions which are running on a given component type.

Variables can be declared lazy using the @lazy modifier.

Alternatively, variables can be declared fuzzy using the @fuzzy modifier.

Lazy and fuzzy features are valid only in the scope, where the variables' names are visible. For example, if a fuzzy variable is passed to a formal parameter declared without a modifier, it loses its fuzzy feature inside the called function. Similarly, if it is passed to a lazy formal parameter, it becomes lazy within the called function.

Whenever a lazy or fuzzy variable is assigned, the TE is required to save the lexical environment (the set of directly or indirectly referenced values and templates) valid at the time of the assignment, so that it is possible to resolve the expression at the time of evaluation of the lazy or fuzzy value or template. If the assignment was made on a lower scope than the evaluation, saving the lexical environment extends lifetime of the referenced variables defined on that lower scope.

***Example***

**var** **@fuzzy** **integer** v\_fuzzy := 1;

**var integer** v\_var;

**var** **boolean** v\_condition := true;

**if** (v\_condition) {

**var boolean** v\_local := 0;

v\_fuzzy := v\_local;

v\_local := 10;

}

// although v\_local is no longer valid at this point, v\_fuzzy still evaluates to 10 because

// the lexical environment is available to the fuzzy variable:

v\_var := v\_fuzzy;

## 11.1 Value variables

A TTCN-3 value variable stores values. It is declared by the **var** keyword followed by a type identifier and a variable identifier. An initial value can be assigned at variable declaration.

It may be used at the right hand side as well as at the left hand side of assignments, in expressions, following the **return** keyword in bodies of functions with a return clause in their headers and may be passed to both value and template-type formal parameters.

***Syntactical Structure***

**var** [ **@lazy** | **@fuzzy** ] *Type* *VarIdentifier* [ *ArrayDef* ] [ ":=" *Expression* ]

{ [ "," ] *VarIdentifier* [ *ArrayDef* ] [ ":=" *Expression* ] } [ ";" ]

***Semantic Description***

A value variable associates a name with the location of a value. A value variable may change its value during test execution several times. A value can be assigned several times to a value variable. The value variable can be referenced multiple times in a TTCN-3 module.

***Restrictions***

In addition to the general static rules of TTCN‑3 given in clause 5, the following restrictions apply:

a) *Expression* shall be of type *Type*.

b) Value variables shall store values only.

c) Value variables shall not be declared or used in a module definitions part (i.e. global variables are not supported in TTCN‑3).

d) Use of uninitialized value variables at other places than the left hand side of assignments, in return statements, or as actual parameters passed to formal parameters shall cause an error.

e) The initialization or assignment of a fuzzy or lazy variable shall not contain function calls of functions with inout or out parameters. The called functions may use other functions with inout or out parameters internally.

f) If lazy or fuzzy value variables are used in deterministic contexts (i.e. during the evaluation of a snapshot or initialization of global non-fuzzy templates), the same restrictions apply to all functions used in the value assigned to the variable as for functions described in clause 16.1.4.

g) The expression assigned to a lazy or fuzzy variable might contain a direct or indirect reference to this variable. Evaluation of such an expression shall cause a dynamic error.

h) Using the dot notation (see clauses 6.2.1.1, 6.2.2.1 and 6.2.5.1) and index notation (see clauses 6.2.3 and 6.2.7) for referencing a field, alternative or element of an **address** value, which actual value is **null** shall cause an error.

***Examples***

**var** **integer** MyVar0;

**var** **integer** MyVar1 := 1;

**var** **boolean** MyVar2 := **true**, MyVar3 := **false**;

**var** @**lazy** **integer** MyLazyVar1 := MyVar1+1;

MyVar1 := 2;

MyVar2 := MyLazyVar1; // MyLazyVar1 evaluates to 2 + 1

MyLazyVar1 := MyLazyVar1 + 1;

MyVar2 := MyLazyVar1; // causes an error as MyLazyVar1 references itself

## 11.2 Template variables

A TTCN-3 template variable stores templates. They are declared by the **var** **template** keyword followed by a type identifier and a variable identifier. An initial content can be assigned at declaration. In addition to values, template variables may also store matching mechanisms (see clause 15.7).

Template variables may be used on the right hand side as well as on the left hand side of assignments, following the **return** keyword in bodies of functions defining a template-type return value in their headers and may be passed as actual parameters to template-type formal parameters. It is also allowed to assign a template instance to a template variable or a template variable field.

***Syntactical Structure***

**var template** [ **@lazy** | **@fuzzy** ] [ *restriction* ] *Type* *VarIdentifier* [ *ArrayDef* ] ":=" *TemplateBody*

{ [ "," ] *VarIdentifier* [ *ArrayDef* ] ":=" *TemplateBody* } [ ";" ]

***Semantic Description***

A template variable associates a name with the location of a template or a value (as every value is also a template).   
A template variable may change its template during test execution several times. A template or value can be assigned several times to a template variable. The template variable can be referenced multiple times in a TTCN-3 module.

The content of a template variable can be restricted to the matching mechanisms specific value and omit in the same way as formal template parameters, see clause 5.4.1.2. The restriction **template (omit)** can be replaced by the shorthand notation **omit**.

NOTE 1: String and list type templates can be concatenated, see clause 15.11.

***Restrictions***

In addition to the general static rules of TTCN‑3 given in clause 5, the following restrictions apply:

a) Template variables shall not be declared or used in a module definitions part (i.e. global variables are not supported in TTCN‑3).

b) When used on the right hand side of assignments template variables shall not be operands of TTCN‑3 operators (see clause 7.1) and the variable on the left hand side shall be a template variable too.

c) When accessing element of template variables either on the left hand side or on the right hand side of assignments, the rules given in clause 15.6 shall apply.

NOTE 2: While it is not allowed to directly apply TTCN‑3 operations to template variables, it is allowed to use the dot notation and the index notation to inspect and modify template variable fields.

d) Use of uninitialized template variables at other places than the left hand side of assignments, in return statements, or as actual parameters passed to formal parameters shall cause an error.

e) Void

f) If the template variable is restricted, then the template used to initialize it shall contain only the matching mechanisms as described in clause 15.8.

g) Template variables, similarly to global and local templates, shall be fully specified in order to be used in sending and receiving operations.

h) Restrictions on templates in clause 15 shall apply.

i) The initialization or assignment of a fuzzy or lazy variable shall not contain function calls of functions with inout or out parameters. The called functions may use other functions with inout or out parameters internally.

j) If lazy or fuzzy template variables are used in deterministic contexts (i.e. during the evaluation of a snapshot or initialization of global non-fuzzy templates), the same restrictions apply to all functions used in the template body assigned to the variable as for functions described in clause 16.1.4.

k) Using the dot notation (see clauses 6.2.1.1, 6.2.2.1 and 6.2.5.1) and index notation (see clauses 6.2.3 and 6.2.7) for referencing a field, alternative or element of an **address** value, which actual value is **null** shall cause an error.

***Examples***

**var** **template** **integer** MyVarTemp1 := ?;

**var** **template** MyRecord MyVarTemp2 := { field1 := **true**, field2 := \* },  
MyVarTemp3 := { field1 := **?**, field2 := MyVarTemp1 };

**var** **template** @**fuzzy** **float** FuzzTemp1 := rnd(); // evaluated on every usage

**var** **template** @**fuzzy** MyRecord FuzzTemp2 := { rnd() < 0.5, float2int(rnd()) }

**var** **template** @**lazy** **float** LazyTemp1 := FuzzTemp1; // evaluates FuzzTemp1

**var** **template** @lazy MyRecord LazyTemp2 :=

{ LazyTemp1 < 0.5, float2int(FuzzTemp1) } // evaluates LazyTemp1 and FuzzTemp1

LazyTemp2.field1 := true; // evaluates LazyTemp2 and overwrites field1 with true

# 12 Declaring timers

TTCN-3 provides a timer mechanism. Timers can be declared and used in the module control part, test cases, functions and altsteps. Additionally, timers can be declared in component type definitions. These timers can be used in test cases, functions and altsteps which are running on the given component type.

A timer declaration may have an optional default duration value assigned to it. The timer shall be started with this value if no other value is specified. The timer value shall be a non-negative **float** value (i.e. greater than or equal to 0.0) where the base unit is seconds.

In addition to single timer instances, timer arrays can also be declared. Default duration(s) of the elements of a timer array shall be assigned using a value array. Default duration(s) assignment shall use the array value notation as specified in clause 6.2.7. If the default duration assignment is wished to be skipped for some element(s) of the timer array, it shall explicitly be declared by using the not used symbol ("-").

***Syntactical Structure***

**timer** { *TimerIdentifier* [ *ArrayDef* ] ":=" *TimerValue* [ "," ] } [ ";" ]

***Semantic Description***

Timers are local to components. A component can start and stop a timer, check if a timer is running, read the elapsed time of a running timer and process timeout events after timer expiration. The timer value is interpreted with a base unit of seconds.

NOTE 1: Timers declared and started in scope units such as functions cease to exist when the scope unit is left. They do not contribute to the test behaviour once the scope unit is left.

NOTE 2: It is not possible to define a timer array as type.

***Restrictions***

In addition to the general static rules of TTCN‑3 given in clause 5, the following restrictions apply:

1. In case of a single timer, the default duration value shall resolve to a non-negative numerical float value   
   (i.e. the value shall be greater or equal 0.0, infinity and not\_a\_number are disallowed).
2. In case of a timer array, it shall resolve to an array of float values obeying to restriction a) above of the same size as the size of the timer array.

***Examples***

EXAMPLE 1: Single timer

**timer** MyTimer1 := 5**E-3**;

// declaration of the timer MyTimer1 with the default value of 5ms

**timer** MyTimer2; // declaration of MyTimer2 without a default timer value i.e. a value has

// to be assigned when the timer is started

EXAMPLE 2: Timer array

**timer** t\_Mytimer1[5] := { 1.0, 2.0, 3.0, 4.0, 5.0 }

// all elements of the timer array get a default duration.

**timer** t\_Mytimer2[5] := { 1.0, -, 3.0, 4.0, 5.0 }

// the second timer (t\_Mytimer2[1]) is left without a default duration.

# 13 Declaring messages

One of the key elements of TTCN‑3 is the ability to send and receive simple or complex messages over message-based ports defined by the test configuration (see clauses 9 and 21). These messages may be those explicitly concerned with testing the SUT or with the internal co-ordination and control messages specific to the relevant test configuration.

Messages are instances of types declared in the in/out/inout clauses of message port type definition.

Any type can be declared as type of a message in a message port type definition, i.e. values of any basic or structured type (see clauses 6.1 and 6.2) can be sent or received. Received messages can also be declared as a combination of value and matching mechanisms (see clause 15.5). Instances of messages can be declared by global, local or in-line templates (see clause 15) or being constructed and passed via variables or template variables (see clause 11) and parameters or template parameters (see clause 5.4).

***Syntactical Structure***

See syntactical structure of types (see clause 6).

***Semantic Description***

See semantic description of types (see clause 6).

***Restrictions***

No specific restrictions in addition to the general static rules of TTCN‑3 given in clause 5.

***Examples***

// a structured, ordered message with two fields

**type** **record** ARecord { **integer** i, **float** f }

# 14 Declaring procedure signatures

Procedure signatures (or signatures for short) are needed for procedure-based communication. Procedure-based communication may be used for the communication within the test system, i.e. among test components, or for the communication between the test system and the SUT. In the latter case, a procedure may either be invoked in the SUT (i.e. the test system performs the call) or in the test system (i.e. the SUT performs the call).

***Syntactical Structure***

**signature** *SignatureIdentifier*

"(" { [ **in** | **inout** | **out** ] *Type* *ValueParIdentifier* [ ","] } ")"

[ ( **return** *Type* ) | **noblock** ]

[ **exception** "(" *ExceptionTypeList* ")" ]

***Semantic Description***

For all used procedures, i.e. procedures used for the communication among test components, procedures called from the SUT and procedures called from the test system, a procedure **signature** shall be defined in the TTCN‑3 module.

TTCN‑3 supports *blocking* and *non-blocking* procedure-based communication. By default, signature definitions without the **noblock** keyword are assumed to be used for blocking procedure-based communication.

Signature definitions may have parameters. Parameters shall be of data type only, i.e. of a basic type, a structured type thereof or a subtype thereof. Within a **signature** definition the parameter list may include parameter identifiers, parameter types and their direction, i.e. **in**, **out**, or **inout**. The direction **inout** and **out** indicate that these parameters are used to retrieve information from the remote procedure.

NOTE 1: The direction of the parameters is as seen by the *called* party rather than the *calling* party.

A remote procedure may return a value after its termination. The type of the return value shall be specified by means of a **return** clause in the corresponding signature definition.

Exceptions that may be raised by remote procedures are represented in TTCN‑3 as values of a specific type. Therefore templates and matching mechanisms can be used to specify or check return values of remote procedures.

NOTE 2: The conversion of exceptions generated by or sent to the SUT into the corresponding TTCN‑3 type or SUT representation is tool and system specific and therefore beyond the scope of the present document.

The exceptions are defined in the form of an exception list included in the **signature** definition. This list defines all the possible different types associated with the set of possible exceptions (the meaning of exceptions themselves will usually only be distinguished by specific values of these types).

***Restrictions***

In addition to the general static rules of TTCN‑3 given in clause 5, the following restrictions apply:

1. Signature definitions for non-blocking communication shall use the **noblock** keyword, shall only have **in** parameters and shall have no return value but may raise exceptions.
2. Signature parameters shall not be of port, component, timer or default type or of structured types having fields of port, component, timer or default type.

***Examples***

**signature** MyRemoteProcOne (); // MyRemoteProcOne will be used for blocking

// procedure-based communication. It has neither

// parameters nor a return value.

**signature** MyRemoteProcTwo () **noblock**; // MyRemoteProcTwo will be used for non blocking

// procedure-based communication. It has neither

// parameters nor a return value.

**signature** MyRemoteProcThree (**in** **integer** Par1, **out** **float** Par2, **inout** **integer** Par3);

// MyRemoteProcThree will be used for blocking procedure-based communication. The procedure

// has three parameters: Par1 an in parameter of type integer, Par2 an out parameter of

// type float and Par3 an inout parameter of type integer.

**signature** MyRemoteProcFour (**in** **integer** Par1) **return** **integer**;

// MyRemoteProcFour will be used for blocking procedure-based communication. The procedure

// has the in parameter Par1 of type integer and returns a value of type integer after its

// termination

**signature** MyRemoteProcFive (**inout** **float** Par1) **return** **integer**

**exception** (ExceptionType1, ExceptionType2);

// MyRemoteProcFive will be used for blocking procedure-based communication. It returns a

// float value in the inout parameter Par1 and an integer value, or may raise exceptions of

// type ExceptionType1 or ExceptionType2

**signature** MyRemoteProcSix (**in** **integer** Par1) **noblock**

**exception** (**integer**, **float**);

// MyRemoteProcSix will be used for non-blocking procedure-based communication. In case of

// an unsuccessful termination, MyRemoteProcSix raises exceptions of type integer or float.

# 15 Declaring templates

Templates are used to either transmit a set of distinct values or to test whether a set of received values matches the template specification. Templates can be defined globally or locally.

Templates provide the following possibilities:

1. they are a way to organize and to re-use test data, including a simple form of inheritance;
2. they can be parameterized;
3. they allow matching mechanisms;
4. they can be used with either message-based or procedure-based communications.

Within a template values, ranges and matching attributes can be specified and then used in both message-based and procedure-based communications. Templates may be specified for any TTCN‑3 type or procedure signature. The type‑based templates are used for message-based communications and the signature templates are used in procedure‑based communications.

A template can be declared fuzzy using the @fuzzy modifier.

NOTE 1: Using a fuzzy template from a non-fuzzy template causes evaluation of the fuzzy template. Thus, for unparameterized non-fuzzy templates, the result of the used fuzzy templates will stay the same for every usage.

A modified template declaration (see clause 15.5) specifies only the fields to be changed from the base template, i.e. it is a partial specification.

***Restrictions***

In addition to the general static rules of TTCN‑3 given in clause 5, the following restrictions apply:

1. Templates shall not be of **default** or port type.
2. Templates shall not be of a structured type that contains fields of **default** or port type on any level of nesting.

NOTE 2: The **anytype** type does not include the **default** type nor port types (see clause 6.2.6), so that restriction b) does not apply to anytype templates.

1. The body of a fuzzy template shall not contain function calls of functions with inout or out parameters. The called functions may use other functions with inout or out parameters internally.
2. Fuzzy features are valid only in the scope, where the templates' names are visible. For example, if a fuzzy template is passed to a formal template parameter declared without a modifier, it loses its fuzzy feature inside the called function.

***Examples***

**type** **record** MyRecord {

**default** def

}

**type** **union** MyUnion {

**integer** choice1,

MyRecord choice2

}

**template** MyUnion t\_integerChosen := { choice1 := 5 }

// shall cause an error as the type MyUnion contains MyRecord, which includes

// a field of default type.

**external** **function** garble(**charstring** str) **return** str;

**template @fuzzy charstring t\_fuzzy := garble("foobar"); // every usage of t\_fuzzy re-evaluates**

**// the function call**

## 15.1 Declaring message templates

Instances of messages with actual values may be specified using templates. A template can be thought of as being a set of instructions to build a message for sending or to match a received message.

***Syntactical Structure***

See syntactical structure of global and local templates (see clause 15.3) and of in-line templates (see clause 15.4).

***Semantic Description***

A template used in a **send** operation defines a complete set of field values comprising the message to be transmitted over a port.

NOTE: For sending templates, omitting an optional field is considered to be a value notation rather than a matching mechanism.

A template used in a **receive**, **trigger** or **check** operation defines a data template against which an incoming message is to be matched. Matching mechanisms, as defined in clauses 15.7 and 15.8 and in annex B, may be used in receive templates. No binding of the incoming values to the template shall occur.

***Restrictions***

In addition to restrictions in clause 15, the following restrictions apply:

a) At the time of a **send** operation, the used template shall be completely initialized and all fields shall resolve to actual values or to omit and no other matching mechanisms shall be used in the template fields, neither directly nor indirectly.

At the time of a **receiving** operation, the matching template shall be completely initialized.

b) Optional fields of record and set templates or template fields can be initialized explicitly or implicitly. For implicit initialization of the optional fields of a template or a template field, an **optional** attribute with the value **"implicit omit"** (see clause 27.7) shall be associated with it either directly or via the attribute distribution (scoping) mechanism (see clause 27.1.1).

***Examples***

EXAMPLE 1: Template for sending messages

// Given the message definition

**type record** MyMessageType

{

**integer** field1 **optional**,

**charstring** field2,

**boolean** field3

}

// a message template could be

**template** MyMessageType MyTemplate:=

{

field1 := **omit**,

field2 := "My string",

field3 := **true**

}

// and a corresponding send operation could be

MyPCO.**send**(MyTemplate);

EXAMPLE 2: Template for receiving messages

// Given the message definition

**type record** MyMessageType

{

**integer** field1 **optional**,

**charstring** field2,

**boolean** field3

}

// a message template might be

**template** MyMessageType MyTemplate:=

{

field1 := ?,

field2 := **pattern** "abc\*xyz",

field3 := **true**

}

// and a corresponding receive operation could be

MyPCO.**receive**(MyTemplate);

EXAMPLE 3: Template for receiving messages

// When used in a receiving operation this template will match any integer value

**template** **integer** Mytemplate := ?;

// This template will match only the integer values 1, 2 or 3

**template** **integer** Mytemplate := (1, 2, 3);

## 15.2 Declaring signature templates

Instances of procedure parameter lists with actual values may be specified using templates. Templates may be defined for any procedure by referencing the associated signature definition.

***Syntactical Structure***

See syntactical structure of global and local templates (see clause 15.3) and of in-line templates (see clause 15.4).

***Semantic Description***

A signature template defines the values and matching mechanisms of the procedure parameters only, but not the return value. The values or matching mechanisms for a return have to be defined within the reply (see clause 22.3.3) or getreply operation (see clause 22.3.4).

A template used in a **call** or **reply** operation defines a complete set of field values for all **in** and **inout** parameters. At the time of the **call** operation, all **in** and **inout** parameters in the template shall resolve to actual values, no matching mechanisms shall be used in these fields, either directly or indirectly. Any template specification for **out** parameters is simply ignored, therefore it is allowed to specify matching mechanisms for these fields, or to omit them (see annex B).

A template used in a **getcall** operation defines a data template against which the incoming parameter fields are matched. Matching mechanisms, as defined in annex B, may be used in any templates used by this operation. No binding of incoming values to the template shall occur. Any **out** parameters shall be ignored in the matching process.

***Restrictions***

In addition to restrictions in clause 15, the following restrictions apply:

1. At the time of a **call**, **reply** and **raise** operation, the used template shall be completely initialized and all **in**/**inout** parameters in a **call**, all **out**/**inout** parameters in a **reply** or **raise** operation shall resolve to specific values or to omit and no other matching mechanisms shall be used for these parameters, neither directly nor indirectly.
2. The NotUsedSymbol shall only be used in signature templates for parameters which are not relevant and in modified template declarations and modified in-line templates to indicate no change for the specified field or element.

At the time of a **getcall**, **getreply** and **catch** operation, the matching template shall be completely initialized.

1. Optional fields of record and set parameters or parameter fields can be initialized explicitly or implicitly. For implicit initialization of a parameter or a parameter field, an **optional** attribute with the value **"implicit omit"** (see clause 27.7) shall be associated with it either directly or via the attribute distribution (scoping) mechanism (see clause 27.1.1).

***Examples***

EXAMPLE 1: Templates for invoking and accepting procedures

// signature definition for a remote procedure

**signature** RemoteProc(**in integer** Par1, **out integer** Par2, **inout integer** Par3) **return** **integer**;

// example templates associated to defined procedure signature

**template** RemoteProc Template1:=

{

Par1 := 1,

Par2 := 2,

Par3 := 3

}

**template** RemoteProc Template2:=

{

Par1 := 1,

Par2 := ?,

Par3 := 3

}

**template** RemoteProc Template3:=

{

Par1 := 1,

Par2 := ?,

Par3 := ?

}

template RemoteProc Template4:=?;

EXAMPLE 2: In-line templates for invoking procedures

// Given example 1 in this clause

// Valid invocation since all in and inout parameters have a distinct value

MyPCO.**call(**RemoteProc:Template1);

// Valid invocation since all in and inout parameters have a distinct value

MyPCO.**call(**RemoteProc:Template2);

// Invalid invocation causing an error

// since the inout parameter Par3 has a matching attribute not a value

MyPCO.**call(**RemoteProc:Template3);

// Templates never return values. In the case of Par2 and Par3 the values returned by the

// call operation shall be retrieved using an assignment clause at the end of the call statement

EXAMPLE 3: In-line templates for accepting procedure invocations

// Given example 1 in this clause

// Valid getcall, it will match if Par1 == 1 and Par3 == 3

MyPCO.**getcall**(RemoteProc:Template1);

// Valid getcall, it will match if Par1 == 1 and Par3 == 3

MyPCO.**getcall**(RemoteProc:Template2);

// Valid getcall, it will match on Par1 == 1 and Any value of Par3

MyPCO.**getcall**(RemoteProc:Template3);

EXAMPLE 4: In-line templates for accepting procedure replies

// Given example 1 in this clause

// Valid getreply, in parameters will be ignored, matches if return value is 4

MyPCO.**getreply**(RemoteProc:Template2 value 4);

// Valid getreply, accepting any reply for RemoteProc

MyPCO.**getreply**(RemoteProc:?);

// Valid getreply, also accepting any reply for RemoteProc

MyPCO.**getcall**(RemoteProc:Template4 value ?);

## 15.3 Global and local templates

TTCN-3 allows defining global templates and local templates.

***Syntactical Structure***

**template** [ *restriction* ] [ **@fuzzy** ] *Type* *TemplateIdentifier* ["(" *TemplateFormalParList* ")"]

[ **modifies** *TemplateRef* ] ":=" *TemplateBody*

NOTE: The optional restriction part is covered by clause 15.8.

***Semantic Description***

Global templates shall be defined in the module definitions part. Local templates shall be defined in module control, testcases, functions, altsteps or statement blocks. Both global and local templates shall adhere to the scoping rules specified in clause 5.

Both global and local templates can be parameterized. The actual parameters of a template can include values and templates. The rules for formal and actual parameter lists shall be followed as defined in clause 5.2.

Both global and local templates are initialized at the place of their declaration. This means, all template fields which are not affected by parameterization shall receive a value or matching mechanism. Template fields affected by parameterization are initialized at the time of template use.

If functions are used for the initialization of module parameters, it is strongly advised to adhere to the rules defined in clause 16.1.4. Not following these rules may cause non-deterministic test executions.

At the time of their use (e.g. in communication operations **send**, **receive**, **call**, **getcall,** etc.), it is allowed to change template fields by in-line modified templates, to pass in values via value parameters as well as to pass in templates via template parameters. The effects of these changes on the values of the template fields do not persist in the template subsequent to the corresponding communication event.

***Restrictions***

In addition to restrictions in clause 15, the following restrictions apply:

a) The dot notation such as *MyTemplateId.FieldId* shall not be used to set or retrieve values in templates in communication events. The "->" symbol shall be used for this purpose (see clause 23).

b) Restrictions on referencing elements of templates or template fields are described in clause 15.6.

c) There exist a number of restrictions on the functions used in expressions when specifying templates or template fields; these are specified in clause 16.1.4.

***Examples***

// The template

**template** MyMessageType MyTemplate (**integer** MyFormalParam):=

{

field1 := MyFormalParam,

field2 := **pattern** "abc\*xyz",

field3 := **true**

}

// could be used as follows

pco1.**send**(MyTemplate(123));

## 15.4 In-line Templates

Templates can be specified directly at the place they are used. Such templates are called in-line templates.

***Syntactical Structure***

[ *Type* ":" ] [ **modifies** *TemplateRefWithParList* ":=" ] *TemplateBody*

NOTE 1: An in-line template is an argument of a communication operation or an actual parameter of a testcase, function or altstep call, i.e. it is always placed within parenthesis and potentially separated with a comma.

***Semantic Description***

In‑line templates can be defined directly at the place of its use.

In‑line templates do not have names, therefore they cannot be referenced or reused. The lifetime of in‑line templates is the TTCN-3 statement (an assignment, a testcase/function/alstep invocation, a return from a function, a communication operation), where they are defined.

***Restrictions***

In addition to restrictions in clause 15, the following restrictions apply:

a) Templates may be specified for any TTCN‑3 type defined in table 3 and for any procedure signature except for **port** and **default** types.

b) The type field may only be omitted when the type is implicitly unambiguous.

NOTE 2: For literal in‑line templates, the following types may be omitted: **integer**, **float**, **boolean**, **bitstring**, **hexstring**, **octetstring**.

NOTE 3: Types of constants, parameters and variables of the actual scope are always unambiguous and can hence always be omitted.

c) In-line templates containing instead of values or inside values matching mechanisms (see clause 15.7) can only be defined in arguments of receiving communication operations (i.e. **receive, trigger, check, getcall**, **getreply** and **catch**), in arguments of the **match** and **select case** operations, in actual template parameters, at the right hand side of assignments (when there is a template variable at the left hand side of the assignment) and in return statements of template returning functions. In-line templates not containing matching mechanisms can be defined wherever values are allowed.

d) When used in communication operations, the type of the in-line template shall be in the port list over which the template is sent or received. In the case where there is an ambiguity between the listed type and the type of the value provided (e.g. through subtyping) then the type name of the in-line template shall be included in the communication operation.

e) There exist a number of restrictions on the functions used in expressions when specifying templates or template fields; these are specified in clause 16.1.4.

***Examples***

MyPCO.**receive**(**charstring**:"abcxyz");

## 15.5 Modified templates

Normally, a template specifies a set of base or default values or matching symbols for each and every field defined in the appropriate type or signature definition. In cases where small changes are needed to specify a new template, it is possible to specify a modified template. A modified template specifies modifications to particular fields of the original template, either directly or indirectly. As well as creating explicitly named modified templates, TTCN‑3 allows the definition of in-line modified templates.

***Syntactical Structure***

Global or local modified template:

**template** [*restriction*] [ **@fuzzy** ] *Type* *TemplateIdentifier* ["(" *TemplateFormalParList* ")"]

**modifies** *TemplateRef* ":=" *TemplateBody*

NOTE 1: The optional restriction part is covered by clause 15.8.

In-line modified template:

[ *Type* ":" ] **modifies** *TemplateRefWithParList* ":=" *TemplateBody*

***Semantic Description***

The **modifies** keyword denotes the parent template from which the new, or modified template shall be derived. This parent template may be either an original template or a modified template.

The modifications occur in a linked fashion, eventually tracing back to the original template.

(a) In case of templates, template fields or list elements of simple types, **union** and **enumerated** types, the matching mechanism specified in the modified template is simply replacing its corresponding content in its parent.

(b) For templates, template fields and elements of **record** and **set** types, if a **record** or **set** field and its corresponding matching mechanism is specified in the modified template, then the specified matching mechanism replaces the one specified in the corresponding field of the parent template. If a **record** or **set** field or its corresponding matching mechanism is – implicitly or explicitly by using the not used symbol "‑" - left unspecified in the modified template, then the matching mechanism in the corresponding field of the parent template shall be used. When the field to be modified is nested within a template field which is a structured field itself, no other field of the structured field is changed apart from the explicitly denoted one(s).

(c) For templates, template fields and elements of **record of** and **set of** types, the above rules specified for **records** and **sets** apply with the following deviations:

* if the value list notation is used, only the number of elements listed in the modified template is inherited from the parent (i.e. the list is truncated at the last element of the list notation in the modified template);
* when individual values of a modified template or a modified template field of **record of** or **set of** type wished to be changed, and only in these cases, the index assignment notation may also be used, where the left hand side of the assignment is the index of the element to be altered.

In case of **record of** and **set of** types first apply rule (c) to the complete structure (e.g. truncation) than apply further rules for the remaining individual type structure elements (see EXAMPLE 3).

Formal value or template parameters of modified templates inherit the default value or respectively template of the corresponding parameter of their parent templates only, if this is denoted by the dash (don't change) symbol at the place of the parameters' default value or respectively template.

Modified templates may also be restricted. Template restrictions are specified in clause 15.8.

A modified template may also be declared fuzzy using the @fuzzy modifier.

NOTE 2: If a fuzzy modified template modifies a non-fuzzy unparameterized template, the inherited fields before modification will be the same for every evaluation of the fuzzy template.

***Restrictions***

In addition to the general static rules of TTCN‑3 given in clause 5, the following restrictions apply:

a) A modified template shall not refer to itself, either directly or indirectly, i.e. recursive derivation is not allowed.

b) If a base template has a formal parameter list, the following rules apply to all modified templates derived from that base template, whether or not they are derived in one or several modification steps:

1) the derived template shall not omit parameters and change types or names of parameters defined at any of the modification steps between the base template and the actual modified template;

2) a template parameter restriction of a derived template specified at any of the modification steps between the base template and the actual modified template can be changed to a stricter one (see clause 15.8);

3) a derived template can have additional (appended) parameters if wished;

4) if the dash (don't change) symbol is used at the place of a default value or default template, the corresponding parameter of the parent template shall have a valid default value or default template, either assigned directly or inherited. If not, this shall cause an error.

c) Restrictions on referencing elements of templates or template fields are described in clause 15.6: for modified templates the rules for the left hand side of assignments apply.

d) Limitations on template restrictions described in clause 15.8 shall apply.

***Examples***

EXAMPLE 1: Modifying record templates (non-embedded case)

// Modifying records

**type record** MyRecordType

{

**integer** field1 optional,

**charstring** field2,

**boolean** field3

}

**template** MyRecordType MyRecTemplate1 :=

{

field1 := 123,

field2 := "A string",

field3 := **true**

}

// then writing

**template** MyRecordType MyRecTemplate2 **modifies** MyRecTemplate1 :=

{

field1 := **omit,** // field1 is optional but present in MyTemplate1

field2 := "A modified string"

// field3 is unchanged

}

// is the same as writing

// **template** MyRecordType MyRecTemplate2 :=

// {

// field1 := **omit**,

// field2 := "A modified string",

// field3 := **true**

// }

**template** MyRecordType MyRecTemplate3 **modifies** MyRecTemplate1 := { **omit,** "A modified string" }

//field3 is implicitly left unchanged;

//MyRecTemplate3 has the same content as MyRecTemplate2

**template** MyRecordType MyRecTemplate4 **modifies** MyRecTemplate1 := { **omit,** "A modified string", - }

//field3 is explicitly left unchanged;

//MyRecTemplate4 has the same content as MyRecTemplate2 and MyRecTemplate3

EXAMPLE 2: Modifying record of templates (non-embedded case)

**type record of integer** MyRecordOfType;

**template** MyRecordOfType MyBaseTemplate := { 0, 1, 2, 3, 4, 5, 6, 7, 8, 9 };

**template** MyRecordOfType MyRecOfTemplate1 **modifies** MyBaseTemplate := { -, -, 3, 2, -, -, -, -, -, - };  
 // MyRecOfTemplate1 contains { 0, 1, 3, 2, 4, 5, 6, 7, 8, 9 }

**template** MyRecordOfType MyRecOfTemplate2 **modifies** MyBaseTemplate := { -, -, 3, 2 };  
 // MyRecOfTemplate2 replaces MyBaseTemplate with: { 0, 1, 3, 2 };

//elements 5 to 10 of MyBaseTemplate are truncated

**template** MyRecordOfType MyRecOfTemplate3 **modifies** MyBaseTemplate := { [2] := 3, [3] := 2 };  
 // MyRecOfTemplate3 has the same content as MyMod1Template: { 0, 1, 3, 2, 4, 5, 6, 7, 8, 9 }

EXAMPLE 3: Modifying embedded record and record of templates

//Modifying a record embedded in a record of

**type record of record** **{**  
 integer a,  
 integer b  
 **}** MyListType

**template** MyListType MyBaseListTemplate := { ?, { a := 1, b := 2 }, ?, { a := 3, b := 4 } }

**template** MyListType MyListTemplate1 **modifies** MyBaseListTemplate := { [1] := { a := 42 } }  
 //Content of field ″a″ of the second element is modified,

//the content of MyListTemplate1 is: { ?, { a := 42, b := 2 }, ?, { a := 3, b := 4 } }

**template** MyListType MyListTemplate2 **modifies** MyBaseListTemplate := { -, { a := 42 } ,- }  
 //Content of field ″a″ of the second element is modified, and the

//record of is truncated after the third element: { ?, { a := 42, b := 2 }, ? }

EXAMPLE 4: Modified in-line template

// Given

**template** MyRecordType Setup :=

{

field1 := 75,

field2 := "abc",

field3 := **true**

}

// Could be used to define an in-line modified template of Setup

// pco1.**send** (**modifies** Setup := {field1:= 76});

EXAMPLE 5: Modified parameterized template

// Given

**template** MyRecordType MyTemplate1(**integer** MyPar):=

{

field1 := MyPar,

field2 := "A string",

field3 := **true**

}

// then a modification could be

**template** MyRecordType MyTemplate2(**integer** MyPar) **modifies** MyRecTemplate1 :=

// field1 is parameterized in Template1 and remains also parameterized in Template2

{

field2 := "A modified string"

}

EXAMPLE 6: Default values of modified parameterized templates

// Given

**template** MyRecordType MyTemplate11 (**integer** p\_int := 5 ):=

// p\_int has the default value 5

{

field1 := p\_int,

field2 := "A string",

field3 := **true**

}

// then possible template modifications are

**template** MyRecordType MyTemplate12(**integer** p\_int) **modifies** MyTemplate11 :=

// p\_int had a default value in MyTemplate11 but has none in this template

{

field2 := "B string"

}

**template** MyRecordType MyTemplate13(**integer** p\_int := 0) **modifies** MyTemplate12 := { }

// p\_int has the default value 0

// no change is made to the template's content, but only to the default value of p\_int

**template** MyRecordType MyTemplate14(**integer** p\_int := - ) **modifies** MyTemplate13 :=

// p\_int inherits the default value 0 from its parent MyTemplate13

{

field2 := "C string"

}

**template** MyRecordType MyTemplate15(**integer** p\_int := - ) **modifies** MyTemplate14 :=

// p\_int inherits the default value 0 from MyTemplate13 via MyTemplate14

{

field2 := "D string"

}

**template** MyRecordType MyTemplate16(**integer** p\_int) **modifies** MyTemplate15 := { }

// p\_int has no default value; no change in the template’s content

**template** MyRecordType MyTemplate17(**integer** p\_int := - ) **modifies** MyTemplate16 :=

// causes an error as p\_int has no default value in the parent template MyTemplate16

{

field2 := "E string"

}

## 15.6 Referencing elements of templates or template fields

This clause defines rules and restrictions for referencing elements of templates or template fields in case of unrestricted templates or templates with the present restriction. When referencing elements of templates or templates fields with the value or omit restriction, the rules for referencing elements of values are used.

### 15.6.1 Referencing individual string elements

It is not allowed to reference individual string elements inside templates or template fields. Instead, the **substr** function (see clause C.4.24.2) shall be used.

EXAMPLE:

**var template** **charstring** t\_Char1 := "MYCHAR";

**var template** **charstring** t\_Char2;

t\_Char2 := t\_Char1[1];

// shall cause an error as referencing individual string elements is not allowed

### 15.6.2 Referencing **record** and **set** fields

Both templates and template variables allow referencing sub-fields inside a template definition using the dot notation. However, the referenced field may be a subfield of a structured field to which a matching mechanism is assigned. This clause provides rules for such cases.

a) Omit, AnyValueOrNone, template lists and complemented lists: referencing a subfield within a structured field to which Omit, AnyValueOrNone, a template list or a complemented list is assigned, at the right hand side of an assignment, shall cause an error.  
When referencing a subfield within a structured field to which AnyValueOrNone or omit is assigned, at the left hand side of an assignment, the structured field is implicitly set to be present, it is expanded recursively up to and including the depth of the referenced subfield. During this expansion an AnyValue shall be assigned to mandatory subfields and AnyValueOrNone shall be assigned to optional subfields. After this expansion the value or matching mechanism at the right hand side of the assignment shall be assigned to the referenced subfield.  
When referencing a subfield within a structured field to which template lists or complemented template lists are assigned, at the left hand side of an assignment, shall cause an error.

EXAMPLE 1:

**type record** R1 {

**integer** f1 **optional**,

R2 f2 **optional**

}

**type record** R2 {

**integer** g1,

R2 g2 **optional**

}

:

**var template** R1 t\_R1 := {

f1 := 5,

f2 := **omit**

}

**var template** R2 t\_R2 := t\_R1.f2.g2;

// causes an error as **omit** is assigned to t\_R1.f2

t\_R1. f2 := \*;

t\_R2 := t\_R1.f2.g2;

// causes an error as **\*** is assigned to t\_R1.f2

t\_R1 := ({f1:=**omit**, f2:={g1:=0, g2:=**omit**}},{f1:=5, f2:={g1:=1, g2:={g1:=2, g2:=**omit**}}});

t\_R2 := t\_R1.f2;

t\_R2 := t\_R1.f2.g2;

t\_R2 := t\_R1.f2.g2.g2;

// all these assignments cause error as a template list is assigned to t\_R1

t\_R1 :=

**complement**({f1:=**omit**, f2:={g1:=0, g2:=**omit**}},{f1:=5, f2:={g1:=1, g2:={g1:=2, g2:=**omit**}}});

t\_R2 := t\_R1.f2;

t\_R2 := t\_R1.f2.g2;

t\_R2 := t\_R1.f2.g2.g2;

// all these assignments cause errors as a complemented list is assigned to t\_R1

b) AnyValue: when referencing a subfield within a structured field to which AnyValue is assigned, at the right hand side of an assignment, AnyValue shall be returned for mandatory subfields and AnyValueOrNone shall be returned for optional subfields.  
When referencing a subfield within a structured field to which AnyValue is assigned, at the left hand side of an assignment, the structured field is implicitly expanded recursively up to and including, the depth of the referenced subfield. During this expansion an AnyValue shall be assigned to mandatory subfields and AnyValueOrNone shall be assigned to optional subfields. After this expansion the value or matching mechanism at the right hand side of the assignment shall be assigned to the referenced subfield.

EXAMPLE 2:

t\_R1 := {f1:=0, f2:=?}

t\_R2 := t\_R1.f2.g2;

// after the assignment t\_R2 will be {g1:=?, g2:=\*}

t\_R1.f2.g2.g2 := ({g1:=1, g2:=**omit**},{g1:=2, g2:=**omit**});

// first the field t\_R1.f2 has hypothetically be expanded to {g1:=?,g2:={g1:=?,g2:=\*}}  
 // thus after the assignment t\_R1 will be:  
 // {f1:=0, f2:={g1:=?,g2:={g1:=?,g2:=({g1:=1, g2:=**omit**},{g1:=2, g2:=**omit**})}}}

c) Ifpresent attribute: referencing a subfield within a structured field to which the ifpresent attribute is attached, shall cause an error (irrespective of the value or the matching mechanism to which **ifpresent** is appended).

d) Special value **null**: referencing a field of an **address** type, which actual value is **null** shall cause an error.

### 15.6.3 Referencing **record** **of** and **set** **of** elements

Both templates and template variables allow referencing elements of a **record of**, array or **set of** template or field using the index notation. However, a matching mechanism may be assigned to the template or field within which the element is referenced. This clause provides rules on handling such cases.

a) Omit: referencing an element within a record of, set of or array field to which omit is assigned shall follow the rules specified in 6.2.3.

b) Template lists, complemented lists, subset and superset: referencing an element within a record of or set of field to which a complemented list, a subset or a superset is assigned, shall cause an error.

EXAMPLE 1:

**type record** **of integer** RoI;

:

**var template** RoI t\_RoI;

**var template integer** t\_Int;

t\_RoI := ({},{0},{0,0},{0,0,0});

t\_Int := t\_RoI[0];

// shall cause an error as template list is assigned to t\_RoI

c) AnyValue: when referencing an element of a **record of** or **set of** template or field to which AnyValue is assigned (without a length attribute), at the right hand side of an assignment, AnyValue shall be returned. If a length attribute is attached to the AnyValue , the index of the reference shall not violate the length attribute.  
When referencing an element within a **record of** or **set of** template or field to which AnyValue is assigned (without a length attribute), at the left hand side of an assignment, the value or matching mechanism at the right hand side of the assignment shall be assigned to the referenced element, AnyElement shall be assigned to all elements before the referenced one (if any) and a single AnyElementsOrNone shall be added at the end. When a length attribute is attached to AnyValue, the attribute shall be conveyed to the new template or field transparently. The index shall not violate type restrictions in any of the above cases.

EXAMPLE 2:

**type record** **of integer** RoI;

**type record** **of** RoI RoRoI;

:

**var template** RoI t\_RoI;

**var template** RoRoI t\_RoRoI;

**var template integer** t\_Int;

:

t\_RoI := ?;

t\_Int := t\_RoI[5];

// after the assignment t\_Int will be AnyValue(?);

t\_RoRoI := ?;

t\_RoI := t\_RoRoI[5];

// after the assignment t\_RoI will be AnyValue(?);

t\_Int := t\_RoRoI[5].[3];

// after the assignment t\_Int will be AnyValue(?);

t\_RoI := ? **length** (2..5);

t\_Int := t\_RoI[3];

// after the assignment t\_Int will be AnyValue(?);

t\_Int := t\_RoI[5];

// shall cause an error as the referenced index is outside the length attribute  
 // (note that index 5 would refer to the 6th element);

t\_RoRoI[2] := {0,0};

// after the assignment t\_RoRoI will be {?,?,{0,0},\*};

t\_RoRoI[4] := {1,1};

// after the assignment t\_RoRoI will be {?,?,{0,0},?,{1,1},\*};

t\_RoI[0] := -5;

// after the assignment t\_RoI will be {-5,\*} **length**(2..5);

t\_RoI := ? **length** (2..5);

t\_RoI[1] := 1;

// after the assignment t\_RoI will be {?,1,\*} **length**(2..5);

t\_RoI[3] := ?;

// after the assignment t\_RoI will be {?,1,?,?,\*} **length**(2..5);

t\_RoI[5] := 5;

// after the assignment t\_RoI will be {?,1,?,?,?,5,\*} **length**(2..5); note that t\_RoI

// becomes an empty set but that shall cause no error;

d) AnyValueOrNone: referencing an element within a record of, set of or array field to which AnyValueOrNone with or without a length attribute is assigned on the right hand side of an assignment shall cause an error. When referencing an element within a record of, set of or array field to which AnyValueOrNone is assigned on the left hand side of an assignment, the rules for AnyValue shall apply (see item c) for more details).

EXAMPLE 3:

**type record** **of integer** RoI;

**type record** **R**

**{**

**RoI field1 optional**

**}**

:

**var template** R mw\_t1 := { field1 := \* };

**var template** **integer**\_mw\_t2;

mw\_t1.field1[2] := 2; // after the assignment, mw\_t1 will be { field1 := { ?, ?, 2, \* } }

mw\_t1.field1 := \*;

mw\_t2 := mw\_t1.field1[0];

// shall cause an error as mw\_t1.field1 contains AnyValueOrNone

e) Permutation: when referencing an element of a **record of** template or field, which is located inside a permutation (based on its index), this shall cause an error. Indexes of elements sheltered by a permutation shall be determined based on the number of permutation elements. AnyElementsOrNone as a permutation element causes that the permutation shelters all record of element indexes.

EXAMPLE 4:

t\_RoI := {**permutation**(0,1,3,?),2,?};

t\_Int := t\_RoI[5];

// after the assignment t\_Int will be AnyValue(?)

t\_RoI := {**permutation**(0,1,3,?),2,\*};

t\_Int := t\_RoI[5];

// after the assignment t\_Int will be \* (AnyValueOrNone)

t\_Int := t\_RoI[2];

// causes error as the third element (with index 2) is inside permutation

t\_RoI := {**permutation**(0,1,3,\*),2,?};

t\_Int := t\_RoI[5];

// causes error as the permutation contains AnyValueOrNone(\*) that is able to

// cover any record of indexes

f) Ifpresent attribute: referencing an element within a **record of** or **set of** field to which the **ifpresent** attribute is attached, shall cause an error (irrespective of the value or the matching mechanism to which **ifpresent** is appended).

g) AnyElementsOrNone: when referencing an element of a record of or set of template or field that contains AnyElementsOrNone, the result of an operation is dependent on the position of AnyElementsOrNone, the referenced index and length attributes attached to AnyElementsOrNone.  
  
When resolving the reference, a transformed form of the record of or set of template is used. The transformed form is equal to the original value where all occurrences of AnyElementsOrNone with a length restriction are replaced with a sequence of AnyElements of the same size as the lower bound. If the lower bound is greater than the upper bound, the sequence shall be followed by a single AnyElementsOrNone symbol with a length restriction. The lower bound of this restriction is zero and the upper bound is the difference between the lower and upper bound of the original restriction.

EXAMPLE 5:

**type record of interger** RoI;  
**template** RoI t\_RoI := {1, \* **length**(2), 5}; // transformed form: {1, ?, ?, 5}  
**template** RoI t\_RoI := {1, \* **length**(1..3), 5};// transformed form: {1, ?, \* length(0..2), 5}

h) Special value **null**: referencing an element of an **address** type, which actual value is **null** shall cause an error.

When the reference is used at the right hand side of the assignment, the following applies:

* If positions of all AnyElementsOrNone matching symbols in the transformed form are greater than the position of the referenced item, rules from the clause 6.2.3.2 are used for resolving the reference.

EXAMPLE 6:

**type record of interger** RoI;  
:  
**var template** RoI t\_RoI := {1, 2, \* length(2), 5};   
 // transformed form: {1, 2, ?, ?, 5}  
**var template integer** t\_Int;  
t\_Int := t\_RoI[1]; // after the assignment, t\_Int will be 2  
t\_Int := t\_RoI[2]; // after the assignment, t\_Int will be ?

* If the position of the referenced item is greater or equal to the position of any AnyElementsOrNone symbol in the transformed template, an error is generated.

EXAMPLE 7:

**type record of interger** RoI;  
:  
**var template** RoI t\_RoI := {1, 2, \*, 5};   
**var template integer** t\_Int := t\_RoI[3]; // produces an error  
  
t\_RoI := {1, 2, \*};   
t\_Int := t\_RoI[2]; // produces an error

When the reference is used at the left hand side of the assignment, the following applies:

* If positions of all AnyElementsOrNone matching symbols in the transformed form are greater than the position of the referenced item the following rules are used. If the referenced item is not a result of transformation, the value or matching symbol at the right hand side of the assignment shall replace the referenced symbol in the original template. If the referenced element was a result of transformation, then the AnyValueOrNone symbol in the original template is replaced with its transformed form and the assignment is performed afterwards.

EXAMPLE 8:

**type record of interger** RoI;  
:  
**var template** RoI t\_RoI := {1, 2, \* length(2), 5};   
 // transformed form: {1, 2, ?, ?, 5}  
t\_RoI[1] := 10; // after the assignment, t\_RoI will be {1, 10, \* length(2), 5}  
t\_RoI[2] := 3; // after the assignment, t\_RoI will be {1, 10, 3, ?, 5}

* If the position of the referenced item is greater or equal to the position of any AnyElementsOrNone symbol in the transformed form and this AnyElementsOrNone symbol is not the last element in the template, an error is generated.

EXAMPLE 9:

**type record of interger** RoI;  
:  
**var template** RoI t\_RoI := {1, 2, \*, 5};   
t\_RoI[3] := 4; // produces an error

* If the position of the referenced item is greater or equal to the position of an AnyElementsOrNone symbol in the transformed form and this AnyElementsOrNone is the last symbol in the template, the value or matching symbol at the right hand side of the assignment shall be assigned to the referenced element. Then the AnyElementsOrNone symbol and all unbound values between it and the referenced symbol shall be replaced with AnyElement symbols. If the AnyElementsOrNone symbol had a length restriction, only as many AnyElement symbols can be added as is the value of the upper bound of the restriction. As the last step, an AnyElementsOrNone symbol can be appended to the end of the template. The symbol is always appended if the original AnyElementsOrNone symbol was unrestricted. If the original AnyElementsOrNone had a length restriction, the symbol is appended only if the restriction included items beyond the referenced item. In such a case, the appended symbol contains the original length restriction adjusted by the difference between the size of the template before and after assignment.

EXAMPLE 10:

**type record of interger** RoI;  
:  
**var template** RoI t\_RoI := {1, 2, \* };  
t\_RoI[4] := 5; // {1, 2, ?, ?, 5, \*};   
  
t\_RoI := {1, \* **length**(1..2)};  
t\_RoI[4] := 5; // {1, ?, ?, -, 5};  
 // short length restriction: only two ? symbols added and no \* at the end  
  
t\_RoI := {1, \* **length**(1..5)};  
t\_RoI[2] := 3; // {1, ?, 3, \* length(0..3)};  
 // adjusted length restriction at the end

The index of the referenced item shall not violate type restrictions in any of the above cases.

### 15.6.4 Referencing signature parameters

While signature templates do not allow referencing their parameters directly (e.g. using dot notation), such a reference is possible when modifying a signature template. However, there can be a matching mechanism assigned to the signature template. This clause provides rules for such cases.

a) Value lists and complemented lists: referencing a parameter of a signature template to which a value list or a complemented list is assigned, at the left hand side of an assignment, shall cause an error.

EXAMPLE 1:

**signature** MySignature(**in** **integer** par1, **in** **integer** par2);  
**template** MySignature t\_mySign1 := ({ par1 := 1, par2 := 2 }, { par1 := 2, par2 := 1 });  
**template** MySignature t\_mySign2 **modifies** t\_mySign1 := { par1 := ? };

// shall cause an error as t\_mySign1 contains a value list template

b) AnyValue: when referencing a parameter within a signature to which AnyValue is assigned, at the left hand side of an assignment, the signature template is implicitly expanded to the parameter level. During this expansion an AnyValue shall be assigned to all parameters of the template. After this expansion the value or matching mechanism at the right hand side of the assignment shall be assigned to the referenced parameter.

EXAMPLE 2:

**template** MySignature t\_mySign3 := ?;  
**template** MySignature t\_mySign4 **modifies** t\_mySign3 := { par1 := 3 };   
// t\_mySign3 is expanded to { par1 := ?, par2 := ? }, then 3 is assigned to par1,  
// thus t\_mySign4 will be { par1 := 3, par2 := ? }

### 15.6.5 Referencing **union** alternatives

Both templates and template variables allow referencing alternatives inside a union template definition using the dot notation. However, the referenced alternative may belong to template field containing a matching mechanism. This clause provides rules for such cases.

a) Omit, AnyValueOrNone, template lists and complemented lists: referencing an alternative of a union template or template field to which Omit, AnyValueOrNone, a template list or a complemented list is assigned, at the right hand side of an assignment, shall cause an error.  
When referencing an alternative of a union template or template field to which AnyValueOrNone or omit is assigned, at the left hand side of an assignment, the template field is implicitly set to be present and the referenced alternative becomes the chosen one. If the referenced alternative is not the last element of the dot notation, rules in clause 15.6.2 valid for AnyValue shall apply recursively for further expansion. After this expansion the value or matching mechanism at the right hand side of the assignment shall be assigned to the referenced subfield.  
Referencing an alternative of a union template field to which template lists or complemented template lists are assigned, at the left hand side of an assignment, shall cause an error.

EXAMPLE 1:

**type record** R1 {

**integer** f1,

**integer** f2

}

**type union** U {

**integer** c1,

R1 c2

}

**type record** R2 {

**integer** g1,

U g2 **optional**

}

:

**var template** R2 mw\_t1 := {

g1 := 5,

g2 := **\***

}

**var template integer** mw\_t2;

mw\_t1.g2.f1 := 1;

// after the assignment mw\_t2.g2 is { g2 := { f1 := 1, f2 := ? } }

mw\_t1.g2 := omit;

mw\_t2 := mw\_1.g2.c1;

// causes an error as **omit** is assigned to mw\_1.g2

b) AnyValue: when referencing an alternative of a union template or template field to which AnyValue is assigned, at the right hand side of an assignment, AnyValue shall be returned.  
When referencing an alternative of a union template or template field to which AnyValue is assigned, at the left hand side of an assignment, the referenced alternative becomes the chosen one. If the referenced alternative is not the last element of the dot notation, rules in clause 15.6.2 valid for AnyValue shall apply recursively for further expansion. After this expansion the value or matching mechanism at the right hand side of the assignment shall be assigned to the referenced subfield.

EXAMPLE 2:

**var template** U mw\_t3 := ?;

mw\_t2 := mw\_t3.c1;

// after the assignment mw\_t2 will be ?

mw\_t3.c1.f1 := 1;

// after the assignment mw\_t3 will be { c1 := { f1 := 1, f2 := ? } }

c) Ifpresent attribute: referencing an alternative of a union template field to which the ifpresent attribute is attached, shall cause an error (irrespective of the value or the matching mechanism to which **ifpresent** is appended).

d) Special value **null**: referencing an alternative of an **address** type, which actual value is **null** shall cause an error.

## 15.7 Template matching mechanisms

Generally, matching mechanisms are used to replace values of single template fields or to replace even the entire contents of a template. Matching mechanisms may also be used in-line (see clause 15.4)*.*

Matching mechanisms are arranged in four groups:

* specific values;
* special symbols that can be used *instead* of values;
* special symbols that can be used *inside* values;
* special symbols which describe *attributes* of values;

Some of the mechanisms may be used in combination.

The supported matching mechanisms and their associated symbols (if any) and the scope of their application are shown in table 11. The left-hand column of this table lists all the TTCN‑3 types to which these matching mechanisms apply. A full description of each matching mechanism can be found in annex B.

***Restrictions***

In addition to the general static rules of TTCN‑3 given in clause 5, the following restrictions apply:

1. All other applications of matching mechanisms than the ones allowed in table 11 are forbidden.

Table 11: TTCN‑3 Matching Mechanisms

| **Used with values of** | **Value** | **Instead of values** | | | | | | | | | | | **Inside values** | | | **Attributes** | |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | S  p  e  c  i  f  i  c  V  a  l  u  e | | O  m  i  t | C  o  m  p  l  e  m  e  n  t  e  d  L  i  s  t | T e m p l a  t e  L  i  s  t | A  n  y  V  a  l  u  e  (?) | A  n  y  V  a  l  u  e  O  r  N  o  n  e  (\*) | R  a  n  g  e | S  u  p  e  r  s  e  t | S  u  b  s  e  t | P  a  t  t  e  r  n | M  a  t  c  h  d  e  c  o  d  e  d  c  o  n  t  e  n  t | A  n  y  E  l  e  m  e  n  t  (?) | A  n  y  E  l  e  m  e  n  t  s  O  r  N  o  n  e  (\*) | P  e  r  m  u  t  a  t  i  o  n | L  e  n  g  t  h  R  e  s  t  r  i  c  t  i  o  n | I  f  P  r  e  s  e  n  t | |
| **boolean** | Yes | | Yes**1** | Yes | Yes | Yes | Yes**1** |  |  |  |  |  |  |  |  |  | Yes**1** | |
| **integer** | Yes | | Yes**1** | Yes | Yes | Yes | Yes**1** | Yes |  |  |  |  |  |  |  |  | Yes**1** | |
| **float** | Yes | | Yes**1** | Yes | Yes | Yes | Yes**1** | Yes |  |  |  |  |  |  |  |  | Yes**1** | |
| **bitstring** | Yes | | Yes**1** | Yes | Yes | Yes | Yes**1** |  |  |  |  | Yes | Yes | Yes |  | Yes | Yes**1** | |
| **octetstring** | Yes | | Yes**1** | Yes | Yes | Yes | Yes**1** |  |  |  |  | Yes | Yes | Yes |  | Yes | Yes**1** | |
| **hexstring** | Yes | | Yes**1** | Yes | Yes | Yes | Yes**1** |  |  |  |  | Yes | Yes | Yes |  | Yes | Yes**1** | |
| **character strings** | Yes | | Yes**1** | Yes | Yes | Yes | Yes**1** | Yes |  |  | Yes | Yes | Yes2 | Yes2 |  | Yes | Yes**1** | |
| **record** | Yes | | Yes**1** | Yes | Yes | Yes | Yes**1** |  |  |  |  |  |  |  |  |  | Yes**1** | |
| **record of** | Yes | | Yes**1** | Yes | Yes | Yes | Yes**1** |  |  |  |  |  | Yes | Yes | Yes | Yes | Yes**1** | |
| **array** | Yes | | Yes**1** | Yes | Yes | Yes | Yes**1** |  |  |  |  |  | Yes | Yes | Yes | Yes | Yes**1** | |
| **set** | Yes | | Yes**1** | Yes | Yes | Yes | Yes**1** |  |  |  |  |  |  |  |  |  | Yes**1** | |
| **set of** | Yes | | Yes**1** | Yes | Yes | Yes | Yes |  | Yes | Yes |  |  | Yes | Yes |  | Yes | Yes**1** | |
| **enumerated** | Yes | | Yes**1** | Yes | Yes | Yes | Yes**1** |  |  |  |  |  |  |  |  |  | Yes**1** | |
| **union** | Yes | | Yes**1** | Yes | Yes | Yes | Yes**1** |  |  |  |  |  |  |  |  |  | Yes**1** | |
| **anytype** | Yes | | Yes**1** | Yes | Yes | Yes | Yes**1** |  |  |  |  |  |  |  |  |  | Yes**1** | |
| NOTE 1: Can be assigned to templates of any type as a whole or to optional fields of record and set templates. However when matching, it shall be applied to optional fields of record and set types only (without restriction on the type of that field).  NOTE 2: Have matching mechanism meaning within character patterns only. | | | | | | | | | | | | | | | | | | |

### 15.7.1 Specific values

Specific values are the basic matching mechanism of TTCN-3 templates. Specific values in templates are expressions which do not contain any matching mechanisms.

***Syntactical Structure***

*SingleExpression*

***Semantic Description***

The matching mechanism for a specific value is an expression that evaluates to a specific value.

For further details please refer to clause 6 and to annex B.

***Restrictions***

In addition to the general static rules of TTCN‑3 given in clause 5, the following restrictions apply:

1. See the restrictions given in table 11 and in annex B.

***Examples***

MyPCO.**receive**(**charstring**:"abcxyz");

MyPCO.**receive**('AAAA'O);

### 15.7.2 Special symbols that can be used instead of values

These matching mechanisms can be used to characterize a set of values.

***Syntactical Structure***

**omit** |

"(" { (*TemplateInstance* | **all from** *TemplateInstance*)[","] } ")" |

**complement** "(" { (*TemplateInstance* | **all from** *TemplateInstance*)[","] } ")" |

"?" |

" \*" |

"(" ( *ConstantExpression |* **-infinity** ) ".." ( *ConstantExpression |* **infinity** ) ")" |

**superset** "(" { (*TemplateInstance* | **all from** *TemplateInstance*)[","] } ")" |

**subset** "(" { (*TemplateInstance* | **all from** *TemplateInstance*)[","] } ")" |

**pattern [@nocase]** *Cstring*

**decmatch** ["(" *Expression* ]")" ] *InlineTemplate*

***Semantic Description***

The matching mechanisms for special symbols that can be used *instead* of values are:

* **omit:** the optional field, in which it is used, is not present;

NOTE 1: **omit** can be assigned to templates of any type as a whole or to optional fields of record and set types. **omit** can only be used for matching optional fields.

* **(…):** a list of values or templates;
* **complement (…):** complement of a list of values or templates;
* **?:** wildcard for any value;
* **\*:** wildcard for any value or no value at all, i.e. the field is not present;

NOTE 2: **\*** can be assigned to templates of any type as a whole or to optional fields of record and set types. **\*** can only be used for matching optional fields.

* **(***lowerBound* **..** *upperBound***):** a range of integer or float values between and including the lower- and upper bounds;
* **superset:** at least all of the elements listed, i.e. possibly more;
* **subset:** at most the elements listed, i.e. possibly less;
* **pattern:** a charstring or universal charstring that matches this format;
* **decmatch:** used for matching of encoded payload fields.

The matching mechanisms list, complemented list, subset, and superset can use the elements of a template using the **all from** clause.

For further details please refer to annex B.

***Restrictions***

In addition to the general static rules of TTCN‑3 given in clause 5, the following restrictions apply:

1. See the restrictions given in table 11 and in annex B.
2. All templates and values used in the matching mechanisms above (including the referenced ones, e.g. within a pattern) shall be completely initialized.

***Examples***

MyPCO.**receive** (**integer**:**complement**(1, 2, 3));

### 15.7.3 Special symbols that can be used inside values

These matching mechanisms allow to characterize value sets by varying values inside.

***Syntactical Structure***

… "?"… |

… "\*"… |

… **permutation** "(" { ( *TemplateBody* | "?" | "\*" | **all from** *TemplateInstance* )[","] } ")" …

***Semantic Description***

The matching mechanisms for special symbols that can be used *inside* values are:

* **?**: wildcard for any single element in a string, array, **record of** or **set of;**
* **\***: wildcard for any number of consecutive elements in a string, array, **record of** or **set of**, or no element at all (i.e. an omitted element);
* **permutation**: all of the elements listed but in an arbitrary order (note, that ? and \* are also allowed as elements of the permutation list and all elements of a template can be added to permutation using the **all from** clause).

For further details please refer to annex B.

***Restrictions***

In addition to the general static rules of TTCN‑3 given in clause 5, the following restrictions apply:

1. See the restrictions given in table 11 and in annex B.
2. All templates or values used in the permutation matching mechanism shall be completely initialized.

***Examples***

**template** **bitstring** b := '10???'B; // where each "?" may either be 0 or 1

**type** **record** **of** **integer** RI;

**template** RI ri := {1, ?, 3} // where ? may be any integer value

### 15.7.4 Special symbols which describe attributes of values

These matching mechanisms define properties of values.

***Syntactical Structure***

**length** "(" *ConstantExpression* [ ".." ( *ConstantExpression |* **infinity** ) ] ")" [ **ifpresent** ] |

**ifpresent**

***Semantic Description***

The matching mechanisms which describe *attributes* of values are:

* **length**:restrictions for string length of string types and the number of elements for **record of**, **set of** and arrays;
* **ifpresent**: for matching of optional field values (if not omitted).

NOTE 1: **ifpresent** can be assigned to templates of any type as a whole or to optional fields of record and set types. **ifpresent** can only be used for matching optional fields.

NOTE 2: Assigning **ifpresent** to a template that already matches the special value omit (i.e. it is either **omit**, an **ifpresent** template or AnyValueOrNone) has no effect; the resulting template will match the same set of values and the special value **omit** as the template the **ifpresent** is assigned to.

For further details please refer to annex B.

***Restrictions***

In addition to the general static rules of TTCN‑3 given in clause 5, the following restrictions apply:

1. See the restrictions given in table 11 and in annex B.
2. All values used in the length matching attribute shall be completely initialized.

***Examples***

**type** **record** R {

**record** **of** **integer** ri **optional**

}

**template** R r:=

{

ri := \* **length** (1 .. 6) **ifpresent** // any value containing 1, 2, 3, 4,

// 5 or 6 elements, provided it is present

}

## 15.8 Template Restrictions

Template restrictions allow to restrict the matching mechanisms that can be used with a template. Template restrictions are applicable to template definitions and template variables, formal template parameters, and return template types of functions. Template restrictions can be applied equally to message and signature templates.

***Syntactical Structure***

**template** "(" ( **omit** | **present** | **value** ) ")" *Type*

***Semantic Description***

The restrictions mean in case of:

* **(omit)** the template shall resolve to a value matching mechanism (i.e. the fields of it shall resolve to a specific value or omit, and the whole template may also resolve to omit). Such a template can be used to define a field of a record and set template and the latter one could still be used in a **send** statement.
* **(value)** the template shall resolve to a specific value (i.e. the fields of it shall resolve to a specific value or omit, but the whole template shall not resolve to omit). It can be used to define a mandatory field of a record or set template and the latter one could still be used in a **send** statement.
* **(present)** the template as a whole shall not resolve to matching mechanisms that match omit (i.e. its fields may contain any of the matching mechanisms or matching attributes). Such a template can be used to define a mandatory field of a record or set template.

NOTE: Template restrictions allow TTCN-3 tools to check more easily at compile time whether templates and matching expressions are used correctly. Whether the checks are performed at compile time and invalid code is rejected or whether the checks are performed at execution time and dynamic errors are raised, is outside the scope of the present document.

***Restrictions***

In addition to the general static rules of TTCN‑3 given in clause 5, the following restrictions apply:

1. Matching mechanisms can be used within restricted templates according to table 12.

Table 12: Using matching mechanisms with restricted templates

| Used with template restriction | Value | | Instead of values | | | | | | | | | | Inside values | | | | Attributes | | | |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | S  p  e  c  i  f  i  c  V  a  l  u  e | O  m  i  t | | C  o  m  p  l  e  m  e  n  t  e  d  L  i  s  t | T e m p l a  t e L  i  s  t | A  n  y  V  a  l  u  e  (?) | A  n  y  V  a  l  u  e  O  r  N  o  n  e  (\*) | R  a  n  g  e | S  u  p  e  r  s  e  t | S  u  b  s  e  t | P  a  t  t  e  r  n | M  a  t  c  h  d  e  c  o  d  e  d  c  o  n  t  e  n  t | | A  n  y  E  l  e  m  e  n  t  (?) | A  n  y  E  l  e  m  e  n  t  s  O  r  N  o  n  e  (\*) | P  e  r  m  u  t  a  t  i  o  n | | L  e  n  g  t  h  R  e  s  t  r  i  c  t  i  o  n | I  f  P  r  e  s  e  n  t | | |
| **omit** | Yes | Yes | |  |  |  |  |  |  |  |  |  | |  |  |  | |  |  | | |
| **value** | Yes | Note1 | |  |  |  |  |  |  |  |  |  | |  |  |  | |  |  | | |
| **present** | Yes | Note1 | | Yes | Yes | Yes | Note1 | Yes | Yes | Yes | Yes | Note2 | | Yes | Yes | Yes | | Yes | Note1 | | |
| NOTE 1: It is allowed to use the matching mechanism in fields of the template, but the template as a whole shall not resolve to this matching mechanism.  NOTE 2: The matching mechanism is allowed only if the template following the **decmatch** keyword is fulfilling the given restriction. | | | | | | | | | | | | | | | | | | | |

1. Restricted and unrestricted templates can be used as actual parameters of formal template parameters or assigned to template variables according to table 13.

Table 13: Restrictions of formal and actual template parameters

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
|  | Actual parameter/right hand side of an expression | value | template (omit) | template (value) | template (present) | template |
| Formal parameter/­left hand side of an expression |  |
| template(omit) | | Yes | Yes | Yes | (see note) | (see note) |
| template(value) | | Yes | (see note) | Yes | (see note) | (see note) |
| template(present) | | Yes | (see note) | Yes | Yes | (see note) |
| template | | Yes | Yes | Yes | Yes | Yes |
| NOTE: These restrictions are related to the content of the actual parameter or right hand side expression and not to the definition of the entities used. Which cases are checked at compile time and which ones at runtime is a tool implementation issue. | | | | | | |

***Examples***

// definitions of restricted templates

**type** **record** ExampleType {

integer a,

boolean b optional

}

**template**(**omit**) ExampleType exampleOmit := **omit**;

**template**(**omit**) ExampleType exampleOmitValue:= { 1, **true** };  
 **template**(**omit**) ExampleType exampleOmitAny := **?**; // incorrect  
  
 **template**(**value**) ExampleType exampleValueomit := **omit**; // incorrect  
 **template**(**value**) ExampleType exampleValue := { 1, **true** };  
 **template**(**value**) ExampleType exampleValueOptional := { 1, **omit** };

// omit assigned to a field is correct  
  
 **template**(**present**) ExampleType examplePresent := {1, **?**};

**template**(**present**) ExampleType examplePresentIfpresent := { 1, **true** } **ifpresent**;

// incorrect

**template**(**present**) ExampleType examplePresentAny := **?**;

// restricted template usage  
 **var** **template** (**omit**)ExampleType v\_omit;  
 **var** **template** (**present**) ExampleType v\_present;  
 **var** **template** (**value**)ExampleType v\_value;

v\_omit := exampleOmit;  
 v\_omit := exampleValueOptional;  
 v\_omit := examplePresentAny; // incorrect, not a specific value  
  
 v\_present := exampleOmit; // incorrect, shall not be omit  
 v\_present := examplePresent;  
  
 v\_value := exampleOmit; // incorrect, shall not be omit  
 v\_value := examplePresentAny; // incorrect, shall be a single value

## 15.9 Match Operation

The **match** operation allows to compare a value (specified in form of an expression) with a template.

***Syntactical Structure***

**match** "(" *Expression* "," *TemplateInstance* ")"

***Semantic Description***

The **match** operation returns a boolean value. If the types of the template and the value (specified in form of an expression) are not compatible (see clause 6.3) the operation returns **false**. If the types are compatible, the return value of the **match** operation indicates whether the value matches the specified template.

***Restrictions***

In addition to the general static rules of TTCN‑3 given in clause 5, the following restrictions apply:

1. The expression-parameter of the **match** operation shall evaluate to a value, i.e. the **match** operation cannot be used to compare two templates.
2. The operands of the **match** operation shall be completely initialized.

***Examples***

**template integer** LessThan10 := (-infinity..9);

:

MyPort.**receive**(**integer**:?) -> **value** RxValue;

**if**( **match**( RxValue, LessThan10)) { … }

// true if the actual value of Rxvalue is less than 10 and false otherwise

:

## 15.10 Valueof Operation

The **valueof** operation allows to return the value specified within a template. The returned value can be assigned to a variable, may be used in expressions, as an actual value parameter, etc.

***Syntactical Structure***

**valueof** "(" *TemplateInstance* ")"

***Semantic Description***

The **valueof** operation returns the value of a template instance.

***Restrictions***

In addition to the general static rules of TTCN‑3 given in clause 5, the following restrictions apply:

a) The template shall be completely initialized and resolve to a specific value.

***Examples***

EXAMPLE 1:

**type** **record** ExampleType

{

**integer** field1,

**boolean** field2

}

**template** ExampleType SetupTemplate :=

{

field1 := 1,

field2 := **true**

}

:

**var** ExampleType RxValue := **valueof**(SetupTemplate);

EXAMPLE 2:

**function** MyFunc() {  
 **var** **template** **integer** vt\_int := **omit**;

//is ok, but to be used for optional record or set fields only

**var** **integer** v\_int := **valueof**(vt\_int)

//causes an error as omit is not a value and shall not be an argument of valueof  
 :  
 }

## 15.11 Concatenating templates of string and list types

Templates of string and list types (bitstring, octetstring, hexstring, charstring, universal charstring, record of, set of, and array) can be concatenated from several single (in-line) templates using the concatenation operation. With the exception of charstring and universal charstring templates, each single template shall have the same root type. The single templates of binary string and list types shall contain only the matching mechanisms specific values, AnyValue without a length modifier, AnyValue or AnyValueOrNone, both constrained to a fixed length, AnyElement or AnyElementsOrNone possibly constrained with a length attribute for list types. The length matching attribute shall not follow a template or template field produced by concatenation directly, but in this case the concatenation shall be placed within a pair of parentheses.

Single templates of charstring and universal charstring types shall contain specific values only. When concatenating templates of charstring and universal charstring types, each single template shall be either of the charstring or universal charstring type. When templates of charstring and universal charstring type are both present in the concatenation, the charstring values are implicitly converted to universal charstring values according to the rules specified in 6.3.1 before concatenation and the resulting template is of the universal charstring type.

The concatenation results in the sequential concatenation of the single templates from left to right, with two exceptions: matching symbol AnyValue without a length modifier shall be replaced by a single AnyElementsOrNone matching symbol before concatenation and matching symbols AnyValue and AnyValueOrNone that are each constrained to a fixed length N shall be replaced by N AnyElement matching symbols before concatenation. The concatenation shall be performed completely before using the resulting template (e.g. for assignment or matching) and the result shall be type-compatible with the place of its use.

NOTE 1: See also concatenation of character string patterns in clause B.1.5.

***Restrictions***

In addition to the general static rules of TTCN‑3 given in clause 5, the following restrictions apply:

a) All operands of the concatenation operation shall be at least partially initialized.

EXAMPLE 1: Composing templates of string types

**template charstring** t\_Mychar1 := "ABC" & "DE\*" & "F?";

// results in the template "ABCDE\*F?"

// please note that "\*" and "?" denote the characters "\*" and "?"

**template charstring** t\_Mychar2 := "ABC" & \* **length**(2) & "EF";

// causes an error as for character string types only

// specific values are allowed

**template bitstring** t\_Mybit := '010'B & ? & '1'B & ? length(1) & '1'B;

// results in the template '010\*1?1'B

// note that & ? & turns to \* within the resulting bitstring as the original ?

// stands for a bitstring of any length

**template octetstring** t\_Myoct1 := 'ABCD'O & 'EF'O & ? & ? length(1) & 'EF'O;

// results in the template 'ABCDEF\*?EF'O

// note that & ? & turns to \* within the resulting octetstring as the original ?

// stands for an octetstring of any length

**template octetstring** t\_Myoct2 := 'ABCD'O & ? length (2) & 'EF'O;

// results in the template 'ABCD??EF'O

// (i.e. a 5 octets i.e. 10 hexadecimal digits long value)

**template octetstring** t\_MyoctWrong := 'ABCD'O & ? **length**(2) length (4);

// causes an error, no length matching attribute shall directly follow a concatenation

**template octetstring** t\_Myoct3 := ('ABCD'O & ? **length**(2)) length (1..3);

// However, this is correct but will not match any value;

**template hexstring** t\_MyhexPar (**integer** N):=

'ABC'H & ? **length**(N) & 'E'H & ? **length**(1) & 'F'H;

**function** MyFunc() **runs on** MyCompType {

**var integer** v\_int := 3;

**var template hexstring** vt\_hstring;

:

vt\_hstring := 'ABC'H & ? **length**(v\_int) & 'E'H & ? length(1) & 'F'H;

//results in the template 'ABC???E?F'H

P.**receive** (t\_MyhexPar(4));

//actual content of t\_MyhexPar is 'ABC????E?F'H

}

EXAMPLE 2: Composing templates of list types

**type record of charstring RecofChar;**

**type set of integer SetofInt;**

**template RecofChar** t\_MyRecofChar := {"ABC"} & {"D?", "EF"};

// results in the template {"ABC", "D?", "EF" }

**template SetofInt** t\_MySetofInt := { 1, 2 } & ? **length**(2) & { 3, 4 };

// results in the template {1, 2, ?, ?, 3, 4 }

**template RecofInt** t\_MyRecofInt := { 1, 2 } & { \* **length**(2), 3, 4 };

// results in the template {1, 2, ?, ?, 3, 4 }

**template RecofChar** t\_MyRecofCharWrong:= {"ABC"} & ? **length**(1..2) & {"EF"};

// causes an error, the length attribute shall denote a fixed length

**template RecofChar** t\_MyRecofCharPar (**integer** N):= { "ABC" } & ? & \* **length**(N) & { "EF" };

**function** MyFunc() **runs on** MyCompType{

**var integer** v\_int := 3;

**var template RecofChar** vt\_recofChar;

:

vt\_recofChar := { "ABC" } & ? **length**(v\_int) & { "EF" };

//results in the template { "ABC", ?, ?, ?, "EF" }

P.**receive** ( t\_MyRecofCharPar(3) );

//actual content of t\_MyRecofCharPar is { "ABC", ?, ?, ?, ?, "EF" }

}

# 16 Functions, altsteps and testcases

In TTCN‑3, functions, altsteps and testcases are used to specify and structure test behaviour, define default behaviour and to structure computation in a module, etc. as described in the following clauses.

## 16.1 Functions

Functions are used in TTCN‑3 to express test behaviour, to organize test execution or to structure computation in a module, for example, to calculate a single value, to initialize a set of variables or to check some condition.

***Syntactical Structure***

**function** [ **@deterministic** ] *FunctionIdentifier*

"(" [ { ( *FormalValuePar* | *FormalTimerPar* | *FormalTemplatePar* | *FormalPortPar* ) [","] } ] ")"

[ **runs** **on** *ComponentType* ]

[ **mtc** *ComponentType* ]

[ **system** *ComponentType* ]

[ **return** [ **template** ] *Type* ]

*StatementBlock*

***Semantic Description***

Functions are portions of TTCN-3 behaviour, which perform a specific task and are relatively independent of the remaining behaviour.

Functions may return a value or a template. Value return is denoted by the **return** keyword followed by a type expression. Template return is denoted by the **return template** keywords followed by an optional restriction and a type expression. Execution of a **return** statement in the body of the function causes evaluation of the return value or template, the function to terminate and to return the result to the location of the call of the function.

The behaviour of a function can be defined by using statements and operations described in clauses 18 to 26.

Functions may be parameterized.

Functions may have an **mtc** clause. If a function has an **mtc** clause, the type referenced by this clause shall be mtc-compatible (see clause 6.3.3) with the type of the **mtc** component reference. If the mtc clause is not present, the type of the **mtc** component reference is unknown in the scope of this function.

Functions may have a **system** clause. If a function has a **system** clause, the type referenced by this clause shall be system-compatible (see clause 6.3.3) with the type of the **system** component reference**.** If the system clause is not present, the type of the **system** component reference is unknown in the scope of this function.

Using the @deterministic modifier, a function can be declared to be deterministic. Deterministic functions are safe to be used when called from specific places where non-determinism could lead to unexpected side effects (see clause 16.1.4)

NOTE 0: The determination of determinism of a function is a semi-decidable problem and as such can and will not be exhaustively checked. As such, the annotation deterministic is mainly used for informational purposes and for allowing certain functions to be used during snapshot evaluation. Principally, a function can be seen as deterministic if it does not violate any of the restrictions from clause 16.1.4 which does not mean that violation of these restriction automatically leads to non-determinism.

***Restrictions***

In addition to the general static rules of TTCN‑3 given in clause 5, the following restrictions apply:

1. A function without **runs on** clause shall never invoke a function or altstep or activate an altstep as default with a **runs on** clause locally.
2. Functions started by using the **start** test component operation shall always have a **runs on** clause (see clause 22.5) and are considered to be invoked in the component to be started, i.e. not locally. However, the **start** test component operation may be invoked in functions without a **runs on** clause.

NOTE 1: The restrictions concerning the **runs on** clause are only related to functions and altsteps and not to test cases.

1. Functions used in the control part of a TTCN‑3 module shall have no **runs on**, **mtc** or **system** clause.

NOTE 2: Nevertheless, functions used in the control part are allowed to execute test cases.

1. The rules for formal parameter lists shall be followed as defined in clause 5.4.
2. For **return template** statements the restrictions specified in clause 15 shall apply.
3. Template **return** can be restricted to the matching mechanisms specific value and **omit**, see clause 5.4.1.2.
4. A **return** statement in a value returning function shall always have a value expression compatible to the type specified in the function header return clause.
5. A **return** statement in a template returning function shall always have a template reference (including calling a value or template returning function)or template instance compatible to the type specified in the function header return clause. If the **return** clause has a template restriction, this restriction shall be adhered to by the returned template. The return statement shall return a template that is at least partially initialized.
6. If the function header includes a **return** clause the function, when terminating, shall do so by executing a **return** statement. The function will cause a test case error if it terminates (i.e. reaches the end of the function body) without executing a **return** statement.
7. If a function references the names of definitions that are defined inside a component type definition, the component type shall be referenced using the **runs on** keywords in the function header. The one exception to this rule is if all the necessary component-wide information is passed in the function as parameters.

***Examples***

EXAMPLE 1: Function with return

// Definition of MyFunction which has no parameters

**function** MyFunction() **return** **integer**

{

**return** 7; // returns the integer value 7 when the function terminates

}

EXAMPLE 2: Function with template return

// Definition of functions which may return matching symbols or templates

**function** MyFunction2() **return** **template** **integer**

{

:

**return** ?; // returns the matching mechanism AnyValue

}

**function** MyFunction3() **return** **template** **octetstring**

{

:

**return** 'FF??FF'O; // returns an octetstring with AnyValue inside it

}

EXAMPLE 3: Function with runs on clause

**function** MyFunction3() **runs on** MyPTCType {

lo // MyFunction3 does not return a value, but

**var integer** MyVar := 5; // does make use of the port operation

PCO1.**send**(MyVar); // send and therefore requires a runs on

// clause to resolve the port identifiers

} // by referencing a component type

EXAMPLE 4: Parameterized function

**function** MyFunction2(**inout integer** MyPar1) {

// MyFunction2 does not return a value

MyPar1 := 10 \* MyPar1; // but changes the value of MyPar1 which

} // is passed in by reference

EXAMPLE 5: Function without return statement

**function** MyFunction5(**inout integer** MyPar1) return integer {

if (MyPar1 > 5) {

MyPar1 := 5;

return MyPar1;

}

// in case of MyPar1 <= 5, MyFunction5 does not terminate in a return statement

// and will cause a test case error

}

EXAMPLE 6: Function with system and mtc

**type component** MtcType { ... }

**type component** SystemType **{ ... }**

**function** MyFunction6() **runs** **on** MyPtcType **mtc** MtcType **system** SystemType {

**var** MtcType v\_mtc := **mtc**;

**var** SystemType v\_system := **system**;

MyFunction3(); // allowed, MyFunction3() has no mtc and system clause

MyFunction6(); // allowed, MyFunction6() has compatible mtc and system clause

}

**function** MyFunction7() runs **on** MyPtcType **system** SystemType {

**var** MtcType v\_mtc := **mtc**; // not allowed, mtc type unknown

MyFunction6(); // possible runtime error, no mtc clause

}

**function** MyFunction8() **runs** on MyPtcType **mtc** MtcType {

var SystemType v\_system := **system**; // not allowed, system type unknown

MyFunction6(); // possible runtime error, no system clause

}

### 16.1.1 Invoking functions

A function is invoked by referring to its name and providing the actual list of parameters.

***Syntactical Structure***

*FunctionRef* "(" [ { *ActualPar* [","] } ] ")"

***Semantic Description***

A function invocation results in the execution of the statement block of the invoked function. The invoked function is performed by the test component invoking it. Actual parameters are passed into the statement block. If the function returns (upon termination and potentially with a return value), the test components continues its behaviour right after the function invocation.

***Restrictions***

In addition to the general static rules of TTCN‑3 given in clause 5, the following restrictions apply:

a) Functions that do not return values shall be invoked directly. Functions that return values may be invoked directly or inside expressions.

b) The rules for actual parameter lists shall be followed as defined in clause 5.4.

c) Special restrictions apply to functions bound to test components using the **start** test component operation. These restrictions are described in clause 21.3.2.

d) When invoking a function, the compatibility to the test component type of the invoking test component as described in clause 6.3.3 need to be fulfilled.

e) Restrictions on invoking functions from specific places are described in clause 16.1.4.

f) When invoking a function, the mtc and system compatibility of the mtc and system components of the invoked function with the actual mtc and system types of the running test case as described in clause 6.3.3 need to be fulfilled.

***Examples***

MyVar := MyFunction4(); // The value returned by MyFunction4 is assigned to MyVar.

// The types of the returned value and MyVar have to be compatible

MyFunction2(MyVar2); // MyFunction2 does not return a value and is called with the

// actual parameter MyVar2, which may be passed in by reference

MyVar3 := MyFunction6(4) + MyFunction7(MyVar3); // Functions used in expressions

### 16.1.2 Predefined functions

TTCN‑3 contains a number of predefined (built-in) functions that need not be declared before use. These are summarized in table 14.

Table 14: List of TTCN‑3 predefined functions

| Category | Function | Keyword |
| --- | --- | --- |
| **Conversion functions** | Convert **integer** value to **charstring** value | **[int2char](#annex_PredefinedFunctions_int2char)** |
| Convert **integer** value to **universal** **charstring** value | **[int2unichar](#annex_PredefinedFunctions_int2unichar)** |
| Convert **integer** value to **bitstring** value | **[int2bit](#annex_PredefinedFunctions_int2bit)** |
| Convert **integer** value to enumerated value | **[int2enum](#annex_PredefinedFunctions_int2enum)** |
| Convert **integer** value to **hexstring** value | **[int2hex](#annex_PredefinedFunctions_int2hex)** |
| Convert **integer** value to **octetstring** value | **[int2oct](#annex_PredefinedFunctions_int2oct)** |
| Convert **integer** value to **charstring** value | **[int2str](#annex_PredefinedFunctions_int2str)** |
| Convert **integer** value to **float** value | **[int2float](#annex_PredefinedFunctions_int2float)** |
| Convert **float** value to **integer** value | **[float2int](#annex_PredefinedFunctions_float2int)** |
| Convert **charstring** value to **integer** value | **[char2int](#annex_PredefinedFunctions_char2int)** |
| Convert **charstring** value to **octetstring** value | **[char2oct](#annex_PredefinedFunctions_char2oct)** |
| Convert **universal charstring** value to **octetstring** value | **[unichar2oct](#annex_PredefinedFunctions_unichar2oct)** |
| Convert **universal** **charstring** value to **integer** value | **[unichar2int](#annex_PredefinedFunctions_unichar2int)** |
| Convert **bitstring** value to **integer** value | **[bit2int](#annex_PredefinedFunctions_bit2int)** |
| Convert **bitstring** value to **hexstring** value | **[bit2hex](#annex_PredefinedFunctions_bit2hex)** |
| Convert **bitstring** value to **octetstring** value | **[bit2oct](#annex_PredefinedFunctions_bit2oct)** |
| Convert **bitstring** value to **charstring** value | **[bit2str](#annex_PredefinedFunctions_bit2str)** |
| Convert **hexstring** value to **integer** value | **[hex2int](#annex_PredefinedFunctions_bit2int)** |
| Convert **hexstring** value to **bitstring** value | **[hex2bit](#annex_PredefinedFunctions_hex2bit)** |
| Convert **hexstring** value to **octetstring** value | **[hex2oct](#annex_PredefinedFunctions_hex2oct)** |
| Convert **hexstring** value to **charstring** value | **[hex2str](#annex_PredefinedFunctions_hex2str)** |
| Convert **octetstring** value to **integer** value | **[oct2int](#annex_PredefinedFunctions_oct2int)** |
| Convert **octetstring** value to **bitstring** value | **[oct2bit](#annex_PredefinedFunctions_oct2bit)** |
| Convert **octetstring** value to **hexstring** value | **[oct2hex](#annex_PredefinedFunctions_oct2hex)** |
| Convert **octetstring** value to **charstring** value | **[oct2str](#annex_PredefinedFunctions_oct2str)** |
| Convert **octetstring** value to **charstring** value, version II | **[oct2char](#annex_PredefinedFunctions_oct2char)** |
| Convert **octetstring** value to **universal charstring** value | **[oct2unichar](#annex_PredefinedFunctions_oct2unichar)** |
| Convert **charstring** value to **integer** value | **[str2int](#annex_PredefinedFunctions_str2int)** |
| Convert **charstring** value to **hexstring** value | **[str2hex](#annex_PredefinedFunctions_str2hex)** |
| Convert **charstring** value to **octetstring** value | **[str2oct](#annex_PredefinedFunctions_str2oct)** |
| Convert **charstring** value to **float** value | **[str2float](#annex_PredefinedFunctions_str2float)** |
| Convert enumerated value to **integer** value | **[enum2int](#annex_PredefinedFunctions_enum2int)** |
| Convert value or template to **universal charstring** value | **[any2unistr](#annex_PredefinedFunctions_any2unistr)** |
| **Length/size functions** | Return the length of a value or template of any string type, **record of**, **set of** or **array** | **[lengthof](#annex_PredefinedFunctions_lengthof)** |
| Return the number of elements in a value or a template of a **record** or **set** | **[sizeof](#annex_PredefinedFunctions_sizeof)** |
| **Presence checking functions** | Determine if an optional field in a **record** or **set** value or template is present | **[ispresent](#annex_PredefinedFunctions_ispresent)** |
| Determine which choice has been selected in a **union** value or template | **[ischosen](#annex_PredefinedFunctions_ischosen)** |
| Determine if a template evaluates to a concrete value | **[isvalue](#annex_PredefinedFunctions_isvalue)** |
| Determine if a template is uninitialized or not | **[isbound](#annex_PredefinedFunctions_isbound)** |
| Determine if a template contains certain matching mechanism | **[istemplatekind](#annex_PredefinedFunctions_isTemplateKind)** |
| **String/list handling functions** | Returns part of the input string matching the specified pattern group within a character pattern | **[regexp](#annex_PredefinedFunctions_regexp)** |
| Returns the specified portion of the input string/list value or template | **[substr](#annex_PredefinedFunctions_substr)** |
| Replaces a substring of a string with or inserts the input string into a string, and similarly for lists | **[replace](#annex_PredefinedFunctions_replace)** |
| **Codec functions** | Encode a value into a bitstring | **[encvalue](#annex_PredefinedFunctions_encvalue)** |
| Decode a bitstring into a value | **[decvalue](#annex_PredefinedFunctions_decvalue)** |
| Encode a value into a universal charstring | **[encvalue\_unichar](#annex_PredefinedFunctions_encvalueUchar)** |
| Decode a universal charstring into a value | **[decvalue\_unichar](#annex_PredefinedFunctions_decvalueUchar)** |
| Retrieve the type of string encoding | **[get\_stringencoding](#annex_PredefinedFunctions_getStringenc)** |
| Remove BOMs of UCS encoding schemes | **[remove\_bom](#annex_PredefinedFunctions_removeBOM)** |
| **Other functions** | Generate a random float number | **[rnd](#annex_PredefinedFunctions_rnd)** |
| Returns the name of the currently executing test case | **[testcasename](#annex_PredefinedFunctions_testcasename)** |
| Returns the host id of the test component or module | **[hostid](#annex_PredefinedFunctions_hostid)** |

***Syntactical Structure***

**int2char** "(" *SingleExpression* ")" |

**int2unichar** "(" *SingleExpression* ")" |

**int2bit** "(" *SingleExpression* "," *SingleExpression* ")" |

**int2enum** "(" *SingleExpression* "," *SingleExpression* ")" |

**int2hex** "(" *SingleExpression* "," *SingleExpression* ")" |

**int2oct** "(" *SingleExpression* "," *SingleExpression* ")" |

**int2str** "(" *SingleExpression* ")" |

**int2float** "(" *SingleExpression* ")" |

**float2int** "(" *SingleExpression* ")" |

**char2int** "(" *SingleExpression* ")" |

**char2oct** "(" *SingleExpression* ")" |

**unichar2int** "(" *SingleExpression* ")" |

**unichar2oct** "(" *SingleExpression* [, *SingleExpression*] ")" |

**bit2int** "(" *SingleExpression* ")" |

**bit2hex** "(" *SingleExpression* ")" |

**bit2oct** "(" *SingleExpression* ")" |

**bit2str** "(" *SingleExpression* ")" |

**hex2int** "(" *SingleExpression* ")" |

**hex2bit** "(" *SingleExpression* ")" |

**hex2oct** "(" *SingleExpression* ")" |

**hex2str** "(" *SingleExpression* ")" |

**oct2int** "(" *SingleExpression* ")" |

**oct2bit** "(" *SingleExpression* ")" |

**oct2hex** "(" *SingleExpression* ")" |

**oct2str** "(" *SingleExpression* ")" |

**oct2char** "(" *SingleExpression* ")" |

**oct2unichar** "(" *SingleExpression* [, *SingleExpression*] ")" |

**str2int** "(" *SingleExpression* ")" |

**str2hex** "(" *SingleExpression* ")" |

**str2oct** "(" *SingleExpression* ")" |

**str2float** "(" *SingleExpression* ")" |

**enum2int** "(" *SingleExpression* ")" |

**any2unistr** "(" *SingleExpression* ")" |

**lengthof** "(" *TemplateInstance* ")" |

**sizeof** "(" *TemplateInstance* ")" |

**ispresent** "(" *TemplateInstance* ")" |

**ischosen** "(" *TemplateInstance* ")" |

**isvalue** "(" *TemplateInstance* ")" |

**isbound** "(" *TemplateInstance* ")" |

**istemplatekind** "(" *TemplateInstance* "," *TemplateInstance* ")" |

**regexp** **[@nocase]** "(" *TemplateInstance*"," *TemplateInstance*"," *SingleExpression* ")" |

**substr** "(" *TemplateInstance* "," *SingleExpression* "," *SingleExpression* ")" |

**replace** "(" *SingleExpression* "," *SingleExpression* "," *SingleExpression* "," *SingleExpression* ")" |

**encvalue** "("*TemplateInstance*")" |

**decvalue** "("*SingleExpression*","*SingleExpression*")" |

**encvalue\_unichar** "("*TemplateInstance* **[,** *SingleExpression***]** ")" |

**decvalue\_unichar** "("*SingleExpression*","*SingleExpression* **[,** *SingleExpression***]**")" |

**get\_stringencoding(**"*SingleExpression*" **)**

**remove\_bom**("*SingleExpression*")

**rnd** "(" [ *SingleExpression* ] ")" |

**testcasename** "()"

**hostid** "(" [ *SingleExpression* ]")"

***Semantic Description***

The description of predefined functions is given in annex C.

***Restrictions***

In addition to the general static rules of TTCN‑3 given in clause 5, the following restrictions apply:

a) When a predefined function is invoked:

1) the number of the actual parameters shall be the same as the number of the formal parameters; and

2) each actual parameter shall evaluate to an element of its corresponding formal parameter's type; and

3) all actual in and inout parameters shall be initialized with the following exceptions:

* the actual in parameter passed to the predefined functions isvalue, ischosen, ispresent and isbound may be uninitialized or even contain non-evaluable reference expressions,
* any\_string\_or\_sequence\_type parameters of the functions lengthof, substr and replace may be partially initialized,
* the invalue parameter of the any2unistr function may be uninitialized or partially initialized.
* the encoded\_value parameter of the decvalue and decvalue\_unichar function may be uninitialized.

b) Restrictions on invoking functions from specific places are described in clause 16.1.4.

***Examples***

**var hexstring** h:= **bit2hex** ('111010111'B);

**var octetstring** o:= **substr** ('01AB23CD'O, 1, 2);

### 16.1.3 External functions

A function may be defined within a module or be declared as being defined externally (i.e. **external**).

***Syntactical Structure***

**external** **function** [ **@deterministic** ] *ExtFunctionIdentifier*

"(" [ { ( *FormalValuePar* | *FormalTimerPar* | *FormalTemplatePar* | *FormalPortPar* ) [","] } ] ")"

[ **return** *Type* ]

***Semantic Description***

For an external function only the function interface has to be provided in the TTCN‑3 module. The realization of the external function is outside the scope of the present document.

Using the @deterministic modifier, an external function can be declared to be deterministic. Deterministic functions are safe to be used when called from specific places where non-determinism could lead to unexpected side effects (see clause 16.1.4).

***Restrictions***

In addition to the general static rules of TTCN‑3 given in clause 5, the following restrictions apply:

1. Void.
2. External functions are not allowed to return templates.
3. Restrictions on invoking functions from specific places are described in clause 16.1.4.

NOTE: External functions should only exchange information with the test system via return values and parameter passing. Side-effects that change the status of the test system and may influence the test outcome should be avoided. Such side-effects can occur if an external function contains default handling, configuration, communication or timer operations.

***Examples***

**external** **function** MyFunction4() **return** **integer**; // External function without parameters

// which returns an integer value

**external** **function** InitTestDevices(); // An external function which only has an

// effect outside the TTCN‑3 module

### 16.1.4 Invoking functions from specific places

If value returning functions are called in receiving communication operations (in templates, template fields, in-line templates, or as actual parameters), in guards or events of alt statements or altsteps (see clause 20.2), or in initializations of altstep local definitions (see clause 16.2), the following operations shall not be used in functions called in the cases specified above, in order to avoid side effects that cause changing the state of the component or the actual snapshot and to prevent different results of subsequent evaluations on an unchanged snapshot:

1. All component operations, i.e. **create**, **start**(component), **stop**(component), **kill**, **running**(component), **alive,** **done** and **killed** (see notes 1, 3, 4 and 6).
2. All port operations, i.e. **start**(port), **stop**(port), **halt**, **clear**, **send**, **receive**, **trigger**, **call**, **getcall**, **reply**, **getreply**, **raise**, **catch**, **check**, **connect**, **map** (see notes 1, 2, 3 and 6).
3. The **action** operation (see notes 2 and 6).
4. All timer operations, i.e. **start**(timer), **stop**(timer), **running**(timer), **read**, **timeout** (see notes 4 and 6).
5. Calling non-deterministic external functions, i.e. external functions where the resulting values for actual inout or out parameters or the return value may differ for different invocations with the same actual in and inout parameters (see notes 4 and 6).
6. Calling the **rnd** predefined function (see notes 4 and 6).
7. Changing of component variables, i.e. using component variables on the left-hand side of assignments, and in the instantiation of **out** and **inout** parameters (see notes 4 and 6).
8. Calling the **setverdict** operation (see notes 4 and 6).
9. Activation and deactivation of defaults, i.e. the **activate** and **deactivate** statements (see notes 5 and 6).
10. Calling functions and deterministic external functions with **out** or **inout** parameters (see notes 7 and 8).

NOTE 1: The execution of the operations **start**, **stop**, **done**, **killed**, **halt**, **clear**, **receive**, **trigger**, **getcall**, **getreply**, **catch** and **check** can cause changes to the current snapshot.

NOTE 2: The use of operations **send**, **call**, **reply**, **raise**, and **action** causes an error, i.e. all communication are to be made explicit and not as a side effect of another communication operation or the evaluation of a snapshot.

NOTE 3: The use of operations **map**, **unmap**, **connect**, **disconnect**, **create** causes an error, i.e. all configuration operations are to be made explicit, and not as a side effect of a communication operation or the evaluation of a snapshot.

NOTE 4: Calling of non-deterministic external functions, **rnd**, **running**, **alive**, **read**, **setverdict**, and writing to component variables causes an error because this may lead to different results of subsequent evaluations of the same snapshot, thus, e.g. rendering deadlock detection impossible.

NOTE 5: The use of operations **activate** and **deactivate** causes an error because they modify the set of defaults that is considered during the evaluation of the current snapshot.

NOTE 6: Restrictions except the limitation on the use of **out** or **inout** parameterization in restriction j) apply recursively, i.e. it is disallowed to use them directly, or via an arbitrary long chain of function invocations.

NOTE 7: The restriction of calling functions and deterministic external functions with **out** or **inout** parameters does not apply recursively, i.e. calling functions that themselves call functions with **out** or **inout** parameters is legal.

NOTE 8: Using **out** or **inout** parameters causes an error because this may lead to different results of subsequent evaluations of the same snapshot.

## 16.2 Altsteps

TTCN‑3 uses altsteps to specify default behaviour or to structure the alternatives of an **alt** statement.

***Syntactical Structure***

**altstep** *AltstepIdentifier*

"(" [ { ( *FormalValuePar* | *FormalTimerPar* | *FormalTemplatePar* | *FormalPortPar* ) [","] } ] ")"

[ **runs** **on** *ComponentType* ]

[ **mtc** *ComponentType* ]

[ **system** *ComponentType* ]

"{"

{ ( *VarInstance* | *TimerInstance* | *ConstDef* | *TemplateDef* ) [";"] }

*AltGuardList*

"}"

***Semantic Description***

Altsteps are scope units similar to functions. The altstep body defines an optional set of local definitions and a set of alternatives, the so-called *top alternatives*, that form the altstep body. The syntax rules of the top alternatives are identical to the syntax rules of the alternatives of **alt** statements.

The behaviour of an altstep can be defined by using the program statements and operations summarized in clause 18. Altsteps may invoke functions and altsteps or activate altsteps as defaults.

Altsteps may be parameterized as defined in clause 5.4.

Altsteps may have an **mtc** clause. If an altstep has an **mtc** clause, the type referenced by this clause shall be mtc-compatible (see clause 6.3.3) with the type of the **mtc** component reference. If the **mtc** clause is not present, the type of the **mtc** component reference is unknown in the scope of this altstep.

Altsteps may have a **system** clause. If an altstep has a **system** clause, the type referenced by this clause shall by system-compatible (see clause 6.3.3) with the type of the **system** component reference**.** If the **system** clause is not present, the type of the **system** component reference is unknown in the scope of this altstep.

***Restrictions***

In addition to the general static rules of TTCN‑3 given in clause 5, the following restrictions apply:

a) The local definitions of an altstep shall be defined before the set of alternatives.

b) The initialization of local definitions by calling value returning functions may have side effects. To avoid side effects that cause an inconsistency between the actual snapshot and the state of the component, and to prevent different results of subsequent evaluations on an unchanged snapshot, restrictions given in clause 16.1.4 shall apply to the initialization of local definitions.

c) If an altstep includes port operations or uses component variables, constants or timers the associated component type shall be referenced using the **runs on** keywords in the altstep header. The one exception to this rule is if all ports, variables, constants and timers used within the altstep are passed in as parameters.

d) An altstep without a **runs on** clause shall never invoke a function or altstep or activate an altstep as default with a **runs on** clause locally.

e) An altstep that is activated as a default shall only have **in** value or template parameters, port parameters, and timer parameters. An altstep that is only invoked as an alternative in an **alt** statement or as stand-alone statement in a TTCN‑3 behaviour description may have **in**, **out** and **inout** parameters. The rules for formal parameter lists shall be followed as defined in clause 5.4.

***Examples***

EXAMPLE 1: Parameterized altstep with runs on clause

// Given

**type** **component** MyComponentType {

**var** **integer** MyIntVar := 0;

**timer** MyTimer;

**port** MyPortTypeOne PCO1, PCO2;

**port** MyPortTypeTwo PCO3;

}

// Altstep definition using PCO1, PCO2, MyIntVar and MyTimer of MyComponentType

**altstep** AltSet\_A(**in integer** MyPar1) **runs on** MyComponentType {

[] PCO1.**receive**(MyTemplate(MyPar1, MyIntVar) {

**setverdict**(**inconc**);

}

[] PCO2.**receive** {

**if** (MyPar1 != 0) {

**repeat**

}

**else** {

**break**

}

}

[] MyTimer.**timeout** {

**setverdict**(**fail**);

**stop**

}

}

EXAMPLE 2: Altstep with local definitions

**altstep** AnotherAltStep(**in integer** MyPar1) **runs on** MyComponentType {

**var integer** MyLocalVar := MyFunction(); // local variable

**const float** MyFloat := 3.41; // local constant

[] PCO1.**receive**(MyTemplate(MyPar1, MyLocalVar) {

**setverdict**(**inconc**);

}

[] PCO2.**receive** {

**repeat**

}

}

### 16.2.1 Invoking altsteps

The invocation of an altstep is always related to an **alt** statement. The invocation may be done either implicitly by the default mechanism (see clause 20.5.) or explicitly by a direct call within an **alt** statement (see clause 20.2).

***Syntactical Structure***

*AltstepRef* "(" [ { *ActualPar* [","] } ] ")"

***Semantic Description***

The invocation of an altstep causes no new snapshot and the evaluation of the top alternatives of an altstep is done by using the actual snapshot of the **alt** statement from which the altstep was called.

NOTE 1: A new snapshot within an altstep will of course be taken, if within a selected top alternative a new **alt** statement is specified and entered.

For an implicit invocation of an altstep by means of the default mechanism, the altstep shall be activated as a default by means of an **activate** statement before the place of the invocation is reached.

An explicit call of an altstep within an **alt** statement looks syntactically like a function invocation as an alternative. When an altstep is called explicitly within an **alt** statement, the next alternative to be checked is the first alternative of the **altstep**. The alternatives of the **altstep** are checked and executed the same way as alternatives of an **alt** statement (see clause 20.1) with the exception that no new snapshot is taken when entering the **altstep**. An unsuccessful termination of the altstep (i.e. all top alternatives of the **altstep** have been checked and no matching branch is found) causes the evaluation of the next alternative or invocation of the default mechanism (if the explicit call is the last alternative of the **alt** statement). A successful termination may cause either the termination of the test component, i.e. the altstep ends with a **stop** statement, or a new snapshot and re-evaluation of the **alt** statement, i.e. the altstep ends with **repeat** (see clause 20.2) or a continuation immediately after the **alt** statement, i.e. the execution of the selected top alternative of the altstep ends with a **break** statement (see clause 19.12) or without explicit **repeat** or **stop**.

NOTE 2: Due to the possibility of defining dynamic test configurations, an alternative in an explicitly invoked altstep may refer to a disconnected or unmapped port at the time of its evaluation. In TTCN-3, ports belong to the receiving component and matching is related to the top elements in the port queues. Dynamically unmapped and disconnected ports contribute to a snapshot in the same manner as mapped and connected ports. This means, an explicitly invoked **altstep** may execute receiving operations that empty the queues of unmapped and disconnected ports without causing a test case error.

An **altstep** can also be called as a stand-alone statement in a TTCN‑3 behaviour description. In this case, the call of the **altstep** can be interpreted as shorthand for an **alt** statement with only one alternative describing the explicit call of the **altstep**.

***Restrictions***

In addition to the general static rules of TTCN‑3 given in clause 5, the following restrictions apply:

a) When invoking an altstep, the compatibility of the test component type of the invoking test component and of the altstep runs on clause (as described in clause 6.3.3) need to be fulfilled.

b) Further restrictions on invoking altsteps in the activate statement are given in clause 20.5.2.

c) When invoking an altstep, the mtc and system compatibility of the mtc and system components of the invoked altstep with the actual mtc and system types of the running test case as described in clause 6.3.3 need to be fulfilled.

***Examples***

EXAMPLE 1: Implicit invocation of an altstep via a default activation

:

**var** **default** MyDefVarTwo := **activate**(MySecondAltStep()); // Activation of an altstep as default

:

EXAMPLE 2: Explicit invocation of an altstep within an alt statement

:

**alt** {

[] PCO3.receive {

…

}

[] AnotherAltStep(); // explicit call of altstep AnotherAltStep as an alternative

// of an alt statement

[] MyTimer.**timeout** {}

}

EXAMPLE 3: Explicit, stand-alone invocation of an altstep

// The statement

AnotherAltStep(); // AnotherAltStep is assumed to be a correctly defined altstep

//is a shorthand for

**alt** {

[] AnotherAltStep();

}

## 16.3 Test cases

A test case is complete and independent specification of the actions required to achieve a specific test purpose. It typically starts in a stable testing state and ends in a stable testing state. It may involve one or more consecutive or concurrent connections to the SUT. The test case shall be complete in the sense that it is sufficient to enable a test verdict to be assigned unambiguously to each potentially observable test outcome (i.e. sequence of test events). The test case shall be independent in the sense that it shall be possible to execute the derived executable test case in isolation from other such test cases.

In TTCN-3, test cases are a special kind of function. Test cases define the behaviours, which have to be executed to check whether the SUT passes a test or not. This behaviour is performed by the MTC which is automatically created when a test case is being executed.

***Syntactical Structure***

**testcase** *TestcaseIdentifier*

"(" [ { ( *FormalValuePar* | *FormalTemplatePar*) [","] } ] ")"

**runs** **on** *ComponentType*

[ **system** *ComponentType* ]

*StatementBlock*

***Semantic Description***

A test case is considered to be a self-contained and complete specification that checks a test purpose. The result of a test case execution is a test verdict.

A test case header has two parts:

1. interface part (mandatory): denoted by the keyword **runs on** which references the required component type for the MTC and makes the associated port names visible within the MTC behaviour; and
2. test system part (optional): denoted by the keyword **system** which references the component type which defines the required ports for the test system interface. The test system part shall only be omitted if, during test execution, only the MTC is instantiated. In this case, the MTC type defines the test system interface ports implicitly.

The behaviour of a test case can be defined by using the program statements and operations described in clause 18.

Test cases may be parameterized as described in clause 5.4. Test cases can be executed in the control part of a module (see clause 26).

***Restrictions***

In addition to the general static rules of TTCN‑3 given in clause 5, the following restrictions apply:

a) The rules for formal parameter lists shall be followed as defined in clause 5.4.

b) Test cases may only be invoked with an execute statement in a module control part as defined in clause 26.

***Examples***

**testcase** MyTestCaseOne()

**runs** **on** MyMtcType1 // defines the type of the MTC

**system** MyTestSystemType // makes the port names of the TSI visible to the MTC

{

: // The behaviour defined here executes on the mtc when the test case invoked

}

// or, a test case where only the MTC is instantiated

**testcase** MyTestCaseTwo() **runs on** MyMtcType2

{

: // The behaviour defined here executes on the mtc when the test case invoked

}

# 17 Void

# 18 Overview of program statements and operations

The fundamental program elements of test cases, functions, altsteps and the control part of TTCN‑3 modules are expressions, basic program statements such as assignments, loop constructs, etc., behavioural statements such as sequential behaviour, alternative behaviour, interleaving, defaults, etc., and operations such as **send**, **receive**, **create**, etc.

Statements can be either single statements (which do not include other program statements) or compound statements (which may include other statements and statement blocks).

Statements shall be executed in the order of their appearance, i.e. sequentially, as illustrated in figure 8.



Figure 8: Illustration of sequential behaviour

The individual statements in the sequence shall be separated by the delimiter ";".

EXAMPLE:

MyPort.**send**(Mymessage); MyTimer.**start**; **log**("Done!");

The specification of an empty statement block, i.e. {}, may be found in compound statements, e.g. a branch in an **alt** statement, and implies that no actions are taken.

Table 15 gives an overview of the TTCN 3 expressions, statements and operations and restrictions on their usage.

Table 15: Overview of TTCN‑3 expressions, statements and operations

| Statement | Associated keyword or symbol | Can be directly or indirectly invoked by module control, but not by test components | Can be invoked by functions, test cases and altsteps running on test components | Can be directly or indirectly invoked from specific places (see note 1) |
| --- | --- | --- | --- | --- |
| Expressions | **(…)** | Yes | Yes | Yes |
| **Basic program statements** | | | | |
| Assignments | **:=** | Yes | Yes | Yes (see note 4) |
| If-else | **if (…) {…} else {…}** | Yes | Yes | Yes |
| Select case | **select case (…) { case (…) {…} case else {…}}** | Yes | Yes | Yes |
| For loop | **for (…) {…}** | Yes | Yes | Yes |
| While loop | **while (…) {…}** | Yes | Yes | Yes |
| Do while loop | **do {…} while (…)** | Yes | Yes | Yes |
| Label and Goto | **label / goto** | Yes | Yes | Yes |
| Stop execution | **stop** | Yes | Yes |  |
| Returning control | **return** |  | Yes (see note 5) | Yes |
| Leaving a loop, alt, altstep or interleave | **break** | Yes | Yes | Yes |
| Next iteration of a loop | **continue** | Yes | Yes | Yes |
| Logging | **log** | Yes | Yes | Yes |
| **Statements and operations for alternative behaviours** | | | | |
| Alternative behaviour | **alt {…}** | Yes (see note 2) | Yes |  |
| Re-evaluation of alternative behaviour | **repeat** | Yes | Yes |  |
| Interleaved behaviour | **interleave {…}** | Yes (see note 2) | Yes |  |
| Activate a default | **activate** | Yes | Yes |  |
| Deactivate a default | **deactivate** | Yes | Yes |  |
| **Configuration operations** | | | | |
| Create parallel test component | **create** |  | Yes |  |
| Connect component port to component port | **connect** |  | Yes |  |
| Disconnect two component ports | **disconnect** |  | Yes |  |
| Map port to test interface | **map** |  | Yes |  |
| Unmap port from test system interface | **unmap** |  | Yes |  |
| Get MTC component reference value | **mtc** |  | Yes | Yes |
| Get test system interface component reference value | **system** |  | Yes | Yes |
| Get own component reference value | **self** |  | Yes | Yes |
| Start execution of test component behaviour | **start** |  | Yes |  |
| Stop execution of test component behaviour | **stop** |  | Yes |  |
| Terminating the testcase with an error verdict | **testcase.stop** |  | Yes | Yes |
| Remove a test component from the system | **kill** |  | Yes |  |
| Check termination of a PTC behaviour | **running** |  | Yes |  |
| Check if a PTC exists in the test system | **alive** |  | Yes |  |
| Wait for termination of a PTC behaviour | **done** |  | Yes |  |
| Wait a PTC cease to exist | **killed** |  | Yes |  |
| **Communication operations** | | | | |
| Send message | **send** |  | Yes |  |
| Invoke procedure call | **call** |  | Yes |  |
| Reply to procedure call from remote entity | **reply** |  | Yes |  |
| Raise exception (to an accepted call) | **raise** |  | Yes |  |
| Receive message | **receive** |  | Yes |  |
| Trigger on message | **trigger** |  | Yes |  |
| Accept procedure call from remote entity | **getcall** |  | Yes |  |
| Handle response from a previous call | **getreply** |  | Yes |  |
| Catch exception (from called entity) | **catch** |  | Yes |  |
| Check (current) message/call received | **check** |  | Yes |  |
| Clear port queue | **clear** |  | Yes |  |
| Clear queue and enable sending & receiving at a to port | **start** |  | Yes |  |
| Disable sending and disallow receiving operations to match at a port | **stop** |  | Yes |  |
| Disable sending and disallow receiving operations to match new messages/calls | **halt** |  | Yes |  |
| Check the state of a port | **checkstate** |  | Yes |  |
| **Timer operations** | | | | |
| Start timer | **start** | Yes | Yes |  |
| Stop timer | **stop** | Yes | Yes |  |
| Read elapsed time | **read** | Yes | Yes |  |
| Check if timer running | **running** | Yes | Yes |  |
| Timeout event | **timeout** | Yes | Yes |  |
| **Verdict operations** | | | | |
| Set local verdict | **setverdict** |  | Yes |  |
| Get local verdict | **getverdict** |  | Yes | Yes |
| **External actions** | | | | |
| Stimulate an (SUT) action externally | **action** | Yes | Yes |  |
| **Execution of test cases** | | | | |
| Execute test case | **execute** | Yes | Yes (see note 3) |  |
| NOTE 1: Specific places are defined in clause 16.1.4. Only operations that do not have any potential side effects on snapshot evaluation are allowed.  NOTE 2: Can be used to control timer operations only.  NOTE 3: Can only be used in functions and altsteps that are used in module control.  NOTE 4: Changing of component variables is disallowed.  NOTE 5: Can be used in functions and altsteps but not in test cases. | | | | |

# 19 Basic program statements

Table 16 provides an overview of the TTCN‑3 basic program statements.

Table 16: Overview of TTCN‑3 basic program statements

|  |  |
| --- | --- |
| Basic program statements | |
| Statement | Associated keyword or symbol |
| Assignments | **:=** |
| If-else | **if (…) {…} else {…}** |
| Select case | **select case (…) { case (…) {…} case else {…}}** |
| For loop | **for (…) {…}** |
| While loop | **while (…) {…}** |
| Do while loop | **do {…} while (…)** |
| Label and Goto | **label / goto** |
| Stop execution | **stop** |
| Returning control | **return** |
| Leaving a loop, alt, altstep or interleave | **break** |
| Next iteration of a loop | **continue** |
| Logging | **log** |

***Restrictions***

In addition to the general static rules of TTCN‑3 given in clause 5, the following restrictions apply:

a) Unless specified differently in the relevant clause, all values and templates used in a basic program statement shall be completely initialized (for exemption see e.g. clause 19.1).

NOTE: Note that the restriction applies to component of statements defined in this document, like the boolean condition of **if** statements, but not to the content of statement blocks embedded into the statements.

## 19.1 Assignments

Values or templates may be assigned to variables or template variables (see clause 11). This is indicated by the symbol ":=".

***Syntactical Structure***

*VariableRef* ":=" ( *Expression* | *TemplateBody* )

***Semantic Description***

During execution of an assignment, the right-hand side of the assignment shall evaluate to a value or template. The effect of an assignment is to bind the variable to the value of the expression or to a template. The expression shall contain no unbound variables. Assignments are processed from left to right, i.e. expressions in the left hand side are evaluated before those in the right hand side. The evaluations obey the operator precedence defined in table 6. Unless the assignment is to a lazy or fuzzy variable or parameter, the right hand side is evaluated completely before the resulting value or template is bound to the evaluated left-hand side of the assignment. Whenever assignments are used within the right hand side of an assignment (due to assignment notation), these rules apply recursively.

A structured value on the right-hand side of the assignment shall be assigned completely to the variable on the left-hand side of the assignment, If a partially initialized value is assigned to a completely initialized variable, fields uninitialized at the right-hand side of the assignment shall also become uninitialized at the left-hand side.

When a direct or indirect element or field of a lazy or fuzzy variable is assigned, the variable is also evaluated as much as necessary before assignment, i.e. if an ancestor of that element or field is initialized with a function call, it shall be evaluated. Thus, if the variable is fully assigned, it does not need to be evaluated before assignment.

NOTE: If a sub-field or sub-element of a fuzzy variable is assigned that has an ancestor which was formerly assigned a function call, this function call will be evaluated once before the assignment and replaced by its result inside the variable. Thus, the other sub-fields and sub-elements of that ancestor, apart from the field or element being assigned become non-fuzzy.

***Restrictions***

In addition to the general static rules of TTCN‑3 given in clause 5 and shown in table 15, the following restrictions apply:

1. The right‑hand side of an assignment shall evaluate to a value or template, which is type compatible with the variable at the left-hand side of the assignment.
2. When the right‑hand side of the assignment evaluates to a template (global or local template, in-line template, template variable or a matching mechanism), the variable at the left hand side shall be a template variable.
3. If the left-hand side of the assignment is a reference to a non-optional value object (i.e. a value definition, a mandatory field, a record/set of/array element, a union alternative, a value parameter), the right-hand side shall not be a reference to an omitted field or the omit symbol.
4. Using a reference to an omitted field in the right-hand side of the assignment has the same effect as using the **omit** keyword.

***Examples***

EXAMPLE 1

MyVariable := (x + y - increment(z))\*3;

EXAMPLE 2

**type** **record** MyRecord {

**record** { **float** x, **float** y } c,

**integer** a

}

**var** @lazy MyRecord r := {

c := computeC(),

a := computeA()

} // not evaluated here

r.c.x := computeX(); // first replaces field c with result of computeC(),

// then replaces field c.x with unevaluated computeX()

// field while c.y remains fixed; field a remains unevaluated

EXAMPLE 3

**type** **record** MyRecord {

**charstring** field1,

**charstring** field2,

**charstring** field3

}

**var** MyRecord v\_MyList1;

**var** MyRecord v\_MyList2;

v\_MyList1 := {"value1", "value2", "value3" }; // v\_MyList1 is completely initialized

v\_MyList2.field2 := "newvalue"; // v\_MyList2 is partilly initialized

// field1 and field3 remain uninitialized

v\_MyList1 := v\_MyList2; // v\_MyList1 become partially initialized,

// field2 has the value "newvalue"

// field1 and field3 are uninitialized

## 19.2 The If-else statement

The **if-else** statement, also known as the conditional statement, is used to denote branching in the control flow.

***Syntactical Structure***

**if** "(" *BooleanExpression* ")" *StatementBlock*

{ **else** **if** "(" *BooleanExpression* ")" *StatementBlock* }

[ **else** *StatementBlock*]

NOTE: **else if** "(" *BooleanExpression* ")" *StatementBlock* [ **else** *StatementBlock*] is a shorthand notation for  
**else** "{" **if** "(" *BooleanExpression* ")" *StatementBlock* [ **else** *StatementBlock*] "}".

***Semantic Description***

The branching of the control flow is decided upon the value of the Boolean expressions - the condition. A statement block - and only one - will be executed, if its condition evaluates to true. The optional else specifies a statement block that will be executed if all the "if" and "else if" conditions before are false.

***Restrictions***

No specific restrictions in addition to the general static rules of TTCN‑3 given in clause 5 and shown in table 15.

***Examples***

**if** (date == "1.1.2005") { **return** ( **fail** ); }

**if** (MyVar < 10) { MyVar := MyVar \* 10; log ("MyVar < 10"); }

**else** { MyVar := MyVar/5; }

## 19.3 The Select statements

### 19.3.1 The Select case statement

The **select case** statement is an alternative syntactic form of the **if-else** statement.

***Syntactical Structure***

**select** "(" *SingleExpression* ")" "{"

{ **case** "(" { *SingleExpression* [","] } ")" *StatementBlock* }

[ **case** **else** *StatementBlock* ]

"}"

***Semantic Description***

The **select case** statement is an alternative to using **if** .. **else** **if** .. **else** statements when comparing a value to one or several other values. The statement contains a header part and zero or more branches. Never more than one of the branches is executed.

In the header part of the **select case** statement an expression shall be given. Each branch starts with the **case** keyword followed by a list of templateInstance (a list branch, which may also contain a single element) or the **else** keyword (an else branch) and a statement block.

All templateInstance in all list branches shall be of a type compatible with the type of the expression in the header.   
A list branch is selected and the statement block of the selected branch is executed only, if any of the templateInstance matches the value of the expression in the header of the statement. On executing the statement block of the selected branch (i.e. not jumping out by a go to statement), execution continues with the statement following the select case statement.

The statement block of an else branch is always executed if no other branch textually preceding the else branch has been selected.

Branches are evaluated in their textual order. If none of the templateInstance-s matches the value of the expression in the header and the statement contains no else branch, execution continues without executing any of the **select case** branches.

***Restrictions***

In addition to the general static rules of TTCN‑3 given in clause 5 and shown in table 15, the following restrictions apply:

1. The **select** *SingleExpression* and the **case** *SingleExpression*-s shall be type compatible.

***Examples***

**select** (MyModulePar) // where MyModulePar is of charstring type

{ **case** ("firstValue")  
 {  
 **log** ("The first branch is selected");  
 }  
 **case** (MyCharVar, MyCharConst)  
 {  
 **log** ("The second branch is selected");  
 }  
 **case** **else**  
 {  
 **log** ("The value of the module parameter MyModulePar is selected");  
 }

}

// the above select statement is equivalent to the following nested if-else statement.

// Note: the following textual replacement of the select-case statement is described in

// the operational semantics of TTCN-3.

{

**var charstring** myTempVar := MyModulePar;

**if** (**match**(myTempVar, "firstValue")  
 {  
 **log** ("The first branch is selected");  
 }  
 **else** **if** (**match**(myTempVar, MyCharVar) **or** **match**(myTempVar, MyCharConst))  
 {  
 **log** ("The second branch is selected");  
 }  
 **else**   
 {  
 **log** ("The value of the module parameter MyModulePar is selected");  
 }

}

### 19.3.2. The Select union statement

To allow easier usage of the select statement for values of union types, a special form of the select statement exists.

***Syntactical Structure***

**select union** "(" *TemplateInstance* ")" "{"

{ **case** "(" { *Identifier* [","] } ")" *StatementBlock* }

[ **case** **else** *StatementBlock* ]

"}"

***Semantic Description***

The statement contains a header part and zero or more branches. Never more than one of the branches is executed.

In the header part of the **select union** statement a template instance of union type shall be given. Each branch shall start with the **case** keyword followed by one or more identifiers of the alternatives (fields) of the union type (a list branch) or the **else** keyword (an else branch) and a statement block. The StatementBlock of the list branch containing the identifier of the chosen alternative is executed. If no case exists for the chosen alternative, the StatementBlock of the else branch, if it is present, is executed. Otherwise, the **select union** statement has no effect.

***Restrictions***

1. The *TemplateInstance* in the header of the **select union** statement shall be of a **union** type. It shall be at least partially initialized.
2. Every *Identifier* in a **case** of the **select union** statement shall be an identifier of an alternative of the **union** type of the template instance given to the statement’s header.
3. No two cases in a **select union** statement shall have the same case *Identifier*.

***Examples***

EXAMPLE:

**type** **union** Messages {

MyMessageType1 msg1,

MyMessageType2 msg2,

MyMessageType3 msg3,

MyMessageType4 msg4,

MyMessageType5 msg5

}

**function** f(**in** Messages msg) {

**select** **union** (msg) {

**case** (msg1) { **log**(msg.msg1); }

**case** (msg2) { **log**(msg.msg2); }

**case** (msg3, msg4) { **log**("either msg3 or msg4"); }

**case** else { **log**("unhandled variant"); }

}

## 19.4 The For statement

The **for** statement defines a counter loop.

***Syntactical Structure***

**for** "(" ( *VarInstance* | *Assignment* ) ";" *BooleanExpression* ";" *Assignment* ")"

*StatementBlock*

***Semantic Description***

The **for** statement contains two assignments and a **boolean** expression. The first assignment is necessary to initialize the index (or counter) variable of the loop. The **boolean** expression terminates the loop and the second assignment is used to manipulate the index variable.

The value of the index variable is increased, decreased or manipulated in such a manner that after a certain number of execution loops a termination criteria is reached.

The termination criterion of the loop shall be expressed by a **boolean** expression. It is checked at the beginning of each new loop iteration. If it evaluates to **true**, the execution continues with the statement block in the **for** statement, if it evaluates to **false**, the execution continues with the statement which immediately follows the **for** loop. If a **break** statement is executed that is not within the body of an enclosed loop, **alt**, alststep or **interleave**, then the loop is terminated, too.

The index variable of a **for** loop can be declared before being used in the **for** statement or can be declared and initialized in the **for** statement header. If the index variable is declared and initialized in the **for** statement header, the scope of the index variable is limited to the loop body, i.e. it is only visible inside the loop body.

***Restrictions***

No specific restrictions in addition to the general static rules of TTCN‑3 given in clause 5 and shown in table 15.

***Examples***

**var integer** j; // Declaration of integer variable j

**for** (j:=1; j<=10; j:= j+1) { … } // Usage of variable j as index variable of the for loop

**for** (**var** **float** i:=1.0; i<7.9; i:= i\*1.35) { … } // Index variable i is declared and initialized

// in the for loop header. Variable i only is

// visible in the loop body.

## 19.5 The While statement

A **while** statement defines a loop that is executed as long as the loop condition holds.

***Syntactical Structure***

**while** "(" *BooleanExpression* ")" *StatementBlock*

***Semantic Description***

The loop condition shall be checked at the beginning of each new loop iteration. If the loop condition does not hold, then the loop is exited and execution shall continue with the statement, which immediately follows the **while** loop. If a **break** statement is executed that is not within the body of an enclosed loop, **alt**, alststep or **interleave**, then the loop is terminated, too.

***Restrictions***

No specific restrictions in addition to the general static rules of TTCN‑3 given in clause 5 and shown in table 15.

***Examples***

**while** (j<10){ … }

## 19.6 The Do-while statement

A **do-while** statement defines a loop that is executed up until the loop condition does not hold.

***Syntactical Structure***

**do** *StatementBlock* **while** "(" *BooleanExpression* ")"

***Semantic Description***

The **do-while** loop is identical to a **while** loop with the exception that the loop condition shall be checked at the *end* of each loop iteration. This means when using a **do-while** loop the behaviour is executed at least once before the loop condition is evaluated for the first time. If a **break** statement is executed that is not within the body of an enclosed loop, **alt**, alststep or **interleave**, then the loop is terminated, too.

***Restrictions***

No specific restrictions in addition to the general static rules of TTCN‑3 given in clause 5 and shown in table 15.

***Examples***

**do** { … } **while** (j<10);

## 19.7 The Label statement

The **label** statement allows the specification of labels in test cases, functions, altsteps and the control part of a module.

***Syntactical Structure***

**label** *LabelIdentifier*

***Semantic Description***

A **label** marks a statement. The label is used by the **goto** statement (see clause 19.8) to transfer control to a labelled statement.

***Restrictions***

In addition to the general static rules of TTCN‑3 given in clause 5 and shown in table 15, the following restrictions apply:

1. A **label** statement can be used freely like other TTCN‑3 behavioural program statements according to the syntax rules defined in annex A. It can be used before or after a TTCN‑3 statement but not as the first statement of an alternative or top alternative in an **alt** statement, **interleave** statement or **altstep**.
2. Labels used following the **label** keyword shall be unique among all labels defined in the same test case, function, altstep or control part.

***Examples***

**label** MyLabel; // Defines the label MyLabel

// The labels L1, L2 and L3 are defined in the following TTCN‑3 code fragment

:

**label** L1; // Definition of label L1

**alt**{

[] PCO1.**receive**(MySig1)

{ **label** L2; // Definition of label L2

PCO1.**send**(MySig2);

PCO1.**receive**(MySig3)

}

[] PCO2.**receive**(MySig4)

{ PCO2.**send**(MySig5);

PCO2.**send**(MySig6);

**label** L3; // Definition of label L3

PCO2.**receive**(MySig7);

}

}

:

## 19.8 The Goto statement

A **goto** statement performs a jump to a **label.**

***Syntactical Structure***

**goto** *LabelIdentifier*

***Semantic Description***

The **goto** statement can be used in functions, test cases, altsteps and the control part of a TTCN‑3 module to transfer control to a labelled statement.

The **goto** statement provides the possibility to jump freely, i.e. forwards and backwards, within a sequence of statements, to jump out of a single compound statement (e.g. a **while** loop) and to jump over several levels out of nested compound statements (e.g. nested alternatives).

***Restrictions***

In addition to the general static rules of TTCN‑3 given in clause 5 and shown in table 15, the following restrictions apply:

a) It is not allowed to jump out of or into functions, test cases, altsteps and the control part of a TTCN‑3 module.

b) It is not allowed to jump into a sequence of statements defined in a compound statement (i.e. **alt** statement, **while** loop, **for** loop, **if-else** statement, **do**- **while** loop and the **interleave** statement).

c) It is not allowed to use the **goto** statement within an **interleave** statement.

***Examples***

// The following TTCN‑3 code fragment includes

:

**label** L1; // … the definition of label L1,

MyVar := 2 \* MyVar;

**if** (MyVar < 2000) { **goto** L1; } // … a jump backward to L1,

MyVar2 := Myfunction(MyVar);

**if** (MyVar2 > MyVar) { **goto** L2; } // … a jump forward to L2,

PCO1.**send**(MyVar);

PCO1.**receive**;

**label** L2; // … the definition of label L2,

PCO2.**send**(**integer:** 21);

**alt** {

[] PCO1.**receive** { }

[] PCO2.**receive**(**integer:** 67) {

**label** L3; // … the definition of label L3,

PCO2.**send**(MyVar);

**alt** {

[] PCO1.**receive** { }

[] PCO2.**receive**(**integer:** 90) {

PCO2.**send**(**integer:** 33);

PCO2.**receive**(**integer**: 13);

**goto** L4; // … a jump forward out of two nested alt statements,

}

[] PCO2.**receive**(MyError) {

**goto** L3; // … a jump backward out of the current alt statement,

}

[] **any port**.**receive** {

**goto** L2; // … a jump backward out of two nested alt statements,

}

}

}

[] **any port**.**receive** {

**goto** L2; // … and a long jump backward out of an alt statement.

}

}

**label** L4;

:

## 19.9 The Stop execution statement

The **stop** statement terminates execution of test components, a test case or a test control.

***Syntactical Structure***

**stop**

***Semantic Description***

The **stop** statement terminates execution in different ways depending on the context in which it is executed. When executed in the control part of a module or in a function called by the control part of a module, it terminates the execution of the module control part. When invoked in a test case, altstep or function that are executed on a test component, it terminates the relevant test component.

NOTE: The semantics of a **stop** statement that terminates a test component is identical to the stop component operation **self**.**stop** (see clause 21.3.3).

***Restrictions***

No specific restrictions in addition to the general static rules of TTCN‑3 given in clause 5 and shown in table 15.

***Examples***

**module** MyModule {

: // Module definitions

**testcase** MyTestCase() **runs on** MyMTCType **system** MySystemType{

**var** MyPTCType ptc:= MyPTCType.**create**; // PTC creation

ptc.**start**(MyFunction()); // start PTC execution

: // test case behaviour continued

**stop** // stops the MTC, all PTCs and the whole test case

}

**function** MyFunction() **runs on** MyPTCType {

:

**stop** // stops the PTC only, the test case continues

}

**control** {

: // test execution

**stop** // stops the test campaign

} // end control

} // end module

## 19.10 The Return statement

The **return** statement terminates execution of functions or altsteps.

***Syntactical Structure***

**return** [ *Expression* | *TemplateInstance* ]

***Semantic Description***

The **return** statement terminates execution of a function or altstep and returns control to the point from which the function or altstep was called. When used in functions, a **return** statement may be optionally associated with a return value or template.

TTCN-3 allows optional statement blocks that may follow altstep calls within **alt** statements. If there is a statement block, the **return** statement returns control to the beginning of this statement block and the statement block is executed before the **alt** statement is left. If there is no statement block, test execution continues with the first statement following the **alt** statement.

The return value or template is first evaluated before returning.

***Restrictions***

In addition to the general static rules of TTCN‑3 given in clause 5 and shown in table 15, the following restrictions apply:

1. The return statement shall not be used in testcase definitions.

***Examples***

**function** MyFunction() **return** **boolean** {

:

**if** (date == "1.1.2005") {

**return** **false**; // execution stops on the 1.1.2000 and returns the boolean false

}

:

**return** **true**; // true is returned

}

**function** MyTemplateFunction() **return** **template charstring** {

:

**if** (date == "1.1.2005") {

**return** **"2005**"; // the string of the year is returned

}

:

**return** **?**; // the any template is returned

}

**function** MyBehaviour() **return** **verdicttype** {

:

**if** (MyFunction()) {

**setverdict**(**pass**); // use of MyFunction in an if statement

}

**else** {

**setverdict**(**inconc**);

}

:

**return** **getverdict**; // explicit return of the verdict

}

## 19.11 The Log statement

The **log** statement provides the means to write logging information to some logging device. The information that can be logged is summarized in table 17.

Table 17: TTCN‑3 language elements that can be logged

| Used in a log statement | What is logged | Comment |
| --- | --- | --- |
| module parameter identifier | actual value |  |
| literal value | value | This includes also free text. |
| data constant identifier | actual value |  |
| template instance | actual template or field values and matching symbols |  |
| data type variable identifier | actual value or "UNINITIALIZED" | See notes 3 and 4. |
| **self, mtc,** **system** or component type variable identifier | actual value and if assigned the component instance name or "UNINITIALIZED" | On logging actual values see notes 2 to 4. Actual component states shall be logged according to note 5. |
| running operation (component or timer) | return value | **true** or **false**. In case of component or timer arrays, array element specification shall be included. |
| alive operation (component) | return value | **true** or **false**. In case of arrays, array element specifications shall be included. |
| port instance | actual state | Port states shall be logged according to note 6. |
| default type variable identifier | actual state or "UNINITIALIZED" | Default states shall be logged according to note 7. See also notes 2 to 4. |
| timer name | actual state | Timer states shall be logged according to note 8. |
| read operation | return value | See clause 24.3. |
| match operation | return value |  |
| getverdict operation | return value | **none**, **pass**, **inconc**, or **fail** |
| predefined functions | return value | See annex C. |
| function instance | return value | Only functions with return clause are allowed. |
| external function instance | return value | Only external functions with return clause are allowed. |
| formal parameter identifier | see comment column | Logging of actual parameters shall follow rules specified for the language elements they are substituting. In case of value parameters the actual parameter value, in case of template-type parameters the actual template or field values and matching symbols, in case of component type parameters the actual component reference, etc. shall be logged. For timer parameters also the use of the read operation and for component type and timer parameters the use of the running operation are allowed. |
| NOTE 1: Actual value/actual template is the value/template at the moment of the execution of the log statement.  NOTE 2: The type of the logged value is tool dependent.  NOTE 3: In case of array identifiers without array element specification, actual values and for component references names of all array elements shall be logged.  NOTE 4: The string "UNINITIALIZED" is logged only if the log item is unbound (uninitialized).  NOTE 5: Component states that can be logged are: Inactive, Running, Stopped and Killed (for further details see annex F).  NOTE 6: Port states that can be logged are: Started and Stopped (for further details see annex F).  NOTE 7: Default states that can be logged are: Activated and Deactivated.  NOTE 8: Timer states that can be logged are: Inactive, Running and Expired (for further details see annex F). | | |

***Syntactical Structure***

**log** "(" { ( *FreeText* | *TemplateInstance* ) [","] } ")"

***Semantic Description***

The **log** statement provides the means to write one or more log items to some logging device associated with the test control or the test component in which the statement is used. Items to be logged shall be identified by a comma‑separated list in the argument of the log statement. Log items may be individual language elements specified in table 17 or expressions composed of such log items.

It is strongly recommended that the execution of the **log** statement has no effect on the test behaviour. In particular, functions used in a log statement should not (explicitly or implicitly) change component variable values, port or timer status, and should not change the value of any of its inout or out parameters.

NOTE: It is outside the scope of the present document to define complex logging and trace capabilities which may be tool dependent.

***Restrictions***

No specific restrictions in addition to the general static rules of TTCN‑3 given in clause 5 and shown in table 15.

***Examples***

**var** integer myVar:= 1;

**log**("Line 248 in PTC\_A: ", myVar, " (actual value of myVar)");

// The string "Line 248 in PTC\_A: 1 (actual value of myVar)" is written to some log device

// of the test system

## 19.12 The Break statement

A **break** statement causes the exit from a loop, from an altstep or from an **alt** or **interleave** statement.

***Syntactical Structure***

**break**

***Semantic Description***

On executing a **break** statement the innermost, currently executed loop, **alt** statement or **interleave** statement is left. Execution continues with the statement following the construct which is left. Using **break** outside the body of a loop (**for**, **while**, **do-while**) or an alternative of an **alt** or **interleave** statement shall cause an error.

Altsteps are always executed within a surrounding **alt** statement. If the execution of a top alternative of an altstep (see clause 16.2) ends with a **break** statement, the altstep and the surrounding **alt** statement are left. Execution continues with the statement following the surrounding **alt** statement.

NOTE: TTCN-3 allows optional statement blocks that may follow altstep calls within **alt** statements. These statement blocks are not executed when the altstep is left by executing a **break** statement. A **return** statement has to be used, if such an optional statement block has to be executed (see clause 19.10).

***Restrictions***

No specific restrictions in addition to the general static rules of TTCN‑3 given in clause 5 and shown in table 15.

***Examples***

**do** {

…

**if** (cond1) {

**break**; // the do-while loop is left

}

…

**for** (**var** **integer** j:=1; j<=10; j:= j+1) {

…

**if** (cond2) {

**break**; // the for-loop is left but the do-while loop is continued

}

…

}

…

}

**while** (j<10);

## 19.13 The Continue statement

A **continue** statement causes the start of the next iteration of a loop.

***Syntactical Structure***

**continue**

***Semantic Description***

On executing a **continue** statement, the subsequent statements of the body of the innermost, currently executed loop are skipped and the next iteration starts. Using **continue** outside the body of a loop (**for**, **while**, **do**-**while**) shall cause an error.

***Restrictions***

No specific restrictions in addition to the general static rules of TTCN‑3 given in clause 5 and shown in table 15.

***Examples***

**do** {

…

**if** (cond) {

**continue**; // execution continues with the next iteration of the do-while-loop

}

…

…

**for** (**var** **integer** j:=1; j<=10; j:= j+1) {

…

**if** (cond2) {

**continue**; // continues with the next iteration of the for-loop

}

…

}

…

}

**while** (j<10);

## 19.14 Statement block

Statement blocks can be used like basic program statements to introduce a local scope in the flow of control of TTCN-3 behaviour. The declarations and statements in a statement block are executed in the order of their appearance, i.e. sequentially.

***Syntactical Structure***

"{" { *LocalDefinition* | *Statement* } "}"

***Semantic Description***

A statement block defines a local scope unit. Scoping rules for TTCN-3 are defined in clause 5.2.

***Restrictions***

No specific restrictions in addition to the general static rules of TTCN‑3 given in clause 5 and shown in table 15.

***Examples***

**var** **integer** aVar:= 0; // aVar is declared

{ // start of a statement block

**var** **integer** myVar:= 2; // myVar is declared

aVar := 5 + myVar; // myVar is used in an assignment

} // end of statement block

// after leaving the statement block aVar is still known, but myVar is not known anymore.

# 20 Statement and operations for alternative behaviours

Test behaviour cannot only be expressed sequentially, but also as a set of alternatives or combinations of both. An interleaving operator allows the specification of interleaved sequences or alternatives. Table 18 summarizes the statements and operations for alternative behaviours.

Table 18: Overview of TTCN‑3 statements and operations for alternative behaviours

|  |  |
| --- | --- |
| Statements and operations for alternative behaviours | |
| Statement/Operation | Associated keyword or symbol |
| Alternative behaviour | **alt { … }** |
| Re-evaluation of alt statements | **repeat** |
| Interleaved behaviour | **interleave { … }** |
| Activate a default | **activate** |
| Deactivate a default | **deactivate** |

## 20.1 The snapshot mechanism

A more complex form of behaviour is where sequences of statements are expressed as sets of possible alternatives to form a tree of execution paths, as illustrated in figure 9.



Figure 9: Illustration of alternative behaviour

This is done with the **alt** statement.

When entering an **alt** statement, a snapshot is taken. A snapshot is considered to be a partial state of a test component that includes all information necessary to evaluate the Boolean conditions that guard alternative branches, all relevant stopped test components, all relevant timeout events and the top messages, calls, replies and exceptions in the relevant incoming port queues. Any test component, timer and port which is referenced in at least one alternative in the **alt** statement, or in a top alternative of an altstep that is invoked as an alternative in the **alt** statement or activated as default is considered to be relevant. A detailed description of the snapshot semantics is given in the operational semantics of TTCN‑3 (part 4 of the TTCN‑3 standard - ES 201 873-4 [1]).

NOTE 1: Snapshots are only a conceptual means for describing the behaviour of the **alt** statement. The concrete algorithms for the snapshot handling can be found in part 4 of the TTCN‑3 standard (ES 201 873-4 [1]).

NOTE 2: The TTCN‑3 semantics assumes that taking a snapshot is instantaneous, i.e. has no duration. In a real implementation, taking a snapshot may take some time and race conditions may occur. The handling of such race conditions is outside the scope of the present document.

## 20.2 The Alt statement

An alt statement expresses sets of possible alternatives that form a tree of possible execution paths.

***Syntactical Structure***

**alt** "{"

{

"[" [ *BooleanExpression* ] "]"

( ( *TimeoutStatement* |

*ReceiveStatement* |

*TriggerStatement* |

*GetCallStatement* |

*CatchStatement* |

*CheckStatement* |

*GetReplyStatement* |

*DoneStatement* |

*KilledStatement* ) *StatementBlock* )

|

( *AltstepInstance* [ *StatementBlock* ] )

}

[ "[" **else** "]" *StatementBlock* ]

"}"

***Semantic Description***

The **alt** statement denotes branching of test behaviour due to the reception and handling of communication and/or timer events and/or the termination of parallel test components, i.e. it is related to the use of the TTCN‑3 operations **receive**, **trigger**, **getcall**, **getreply**, **catch**, **check**, **timeout, done** and **killed**. The **alt** statement denotes a set of possible events that are to be matched against a particular snapshot.

**Execution of alternative behaviour:**

When entering an **alt** statement, a snapshot is taken.

The alternative branches in the **alt** statement and the top alternatives of invoked altsteps and altsteps that are activated as defaults are processed in the order of their appearance. If several defaults are active, the reverse order of their activation determines the evaluation order of the top alternatives in the defaults. The alternative branches in active defaults are reached by the default mechanism described in clause 20.5.

The individual alternative branches are either branches that may be guarded by a Boolean expression or else-branches, i.e. alternative branches starting with [**else**].

Else-branches are always chosen and executed when they are reached (see below).

Branches that may be guarded by a Boolean expressions either invoke an altstep (*altstep-branch*), or start with a **done** operation (*done-branch*), a **killed** operation (*killed-branch*), **timeout** operation (*timeout-branch*) or a receiving operation (*receiving-branch*), i.e. **receive**, **trigger**, **getcall**, **getreply,** **catch** or a **check** operation. The evaluation of the Boolean guards shall be based on the snapshot. The Boolean guard is considered to be *fulfilled* if no Boolean guard is defined, or if the Boolean guard evaluates to **true**. The branches are processed and executed in the following manner.

An *altstep-branch* is selected if the Boolean guard is fulfilled. The selection of an *altstep-branch* causes the invocation of the referenced altstep, i.e. the altstep is invoked and the evaluation of the snapshot continues within the altstep. Altstep-branches may contain an optional statement block. The optional statement block shall be executed only, if an alternative of the altstep referenced in the altstep-branch has been selected and executed.

A *done-branch* is selected if the Boolean guard is fulfilled and if the specified test component is in the list of stopped components of the snapshot. The selection causes the execution of the statement block following the **done** operation. The **done** operation itself has no further effect.

A *killed-branch* is selected if the Boolean guard is fulfilled and if the specified test component is in the list of killed components of the snapshot. The selection causes the execution of the statement block following the **killed** operation. The **killed** operation itself has no further effect.

A *timeout-branch* is selected if the Boolean guard is fulfilled and if the specified timeout event is in the timeout-list of the snapshot. The selection causes execution of the specified **timeout** operation, i.e. removal of the timeout event from the timeout-list, and the execution of the statement block following the **timeout** operation.

A *receiving-branch* is selected if the Boolean guard is fulfilled and if the matching criteria of receiving operation is fulfilled by one of the messages, calls, replies or exceptions in the snapshot. The selection causes execution of the receiving operation, i.e. removal of the matching message, call, reply or exception from the port queue, maybe an assignment of the received information to a variable and the execution of the statement block following the receiving operation. In the case of the **trigger** operation the top message of the queue is also removed if the Boolean guard is fulfilled but the matching criteria is not. In this case the statement block of the given alternative is not executed.

NOTE 1: The TTCN‑3 semantics describe the evaluation of a snapshot as a series of indivisible actions of a test component. The semantics do not assume that the evaluation of a snapshot has no duration. During the evaluation of a snapshot, test components may stop, timers may timeout and new messages, calls, replies or exceptions may enter the port queues of the component However, these events do not change the actual snapshot and thus, are not considered for the snapshot evaluation.

NOTE 2: Due to the possibility of defining dynamic test configurations, a receiving branch may refer to a disconnected or unmapped port at the time of its evaluation. In TTCN-3, ports belong to the receiving component and matching is related to the top elements in the port queues. Dynamically unmapped and disconnected ports contribute to a snapshot in the same manner as mapped and connected ports. This means, the execution of receiving operations may empty the queues of unmapped and disconnected ports without causing a test case error.

If none of the alternative branches in the **alt** statement and top alternatives in the invoked altsteps and active defaults can be selected and executed, the **alt** statement shall be executed again, i.e. a new snapshot is taken and the evaluation of the alternative branches is repeated with the new snapshot. This repetitive procedure shall continue until either an alternative branch is selected and executed, or the test case is stopped by another component or by the test system (e.g. because the MTC is stopped) or with a dynamic error.

The test case shall stop and indicate a dynamic error if a test component is completely blocked. This means none of the alternatives can be chosen, no relevant test component is running, no relevant timer is running and all relevant ports contain at least one message, call, reply or exception that do not match.

NOTE 3: The repetitive procedure of taking a complete snapshot and re-evaluate all alternatives is only a conceptual means for describing the semantics of the **alt** statement. The concrete algorithm that implements this semantics is outside the scope of the present document.

**Selecting/deselecting an alternative:**

If necessary, it is possible to enable/disable an alternative by means of a Boolean expression placed between the ("[…]") brackets of the alternative.

**Else branch in alternatives:**

Any branch in an **alt** statement can be defined as an else branch by including the **else** keyword between the opening and closing brackets at the beginning of the alternative. The statement block of the else branch is always executed if no other alternative textually preceding the else branch has proceeded.

**Default mechanism:**

It should be noted that the default mechanism (see clause 20.5) is always invoked at the end of all alternatives. If an **else** branch is defined, the default mechanism will never be called, i.e. active defaults will never be entered.

NOTE 4: It is also possible to use **else** in altsteps.

NOTE 5: It is allowed to use a **repeat** statement within an **else** branch.

NOTE 6: It is allowed to define more than one else branch in an alt statement or in an altstep, however always only the first else branch is executed.

**Re-evaluation of alt statements:**

The re-evaluation of an **alt** statement can be specified by using a **repeat** statement (see clause 20.3).

**Invocation of altsteps as alternatives:**

TTCN‑3 allows the invocation of altsteps as alternatives in **alt** statements (see clause 16.2.1). When an altstep is explicitly invoked as an alternative, the optional statement block following the altstep call shall also be executed.

**Continue execution after the alt statement:**

Behaviour execution continues with the statement following the **alt** statement when one of the branches of the **alt** or invoked defaults is selected and completely executed, or a branch of an **altstep** used in an altsteps-branch is selected and the branch and the optional statement block following the invoked altstep are completely executed.

Execution also continues with the statement following the **alt** statement if a **break** statement is reached in the statement block of the selected branch of an **alt** statement, of an **altstep** used in an altstep-branch, or of an **altstep** invoked as default.

The **alt** statement can also be left by using a **goto** statement in the selected branch of the **alt** (i.e. no branches of altsteps and defaults can be considered in this case), and execution continues with the statement following the label, **goto** is pointing to.

***Restrictions***

In addition to the general static rules of TTCN‑3 given in clause 5 and shown in table 15, the following restrictions apply:

1. The open and close square brackets ("[…]") shall be present at the start of each alternative, even if they are empty. This not only aids readability but also is necessary to syntactically distinguish one alternative from another.
2. The evaluation of a Boolean expression guarding an alternative shall not have side effects. To avoid side effects that cause an inconsistency between the actual snapshot and the state of the component, the same restrictions as the restrictions for the initialization of local definitions within altsteps shall apply (clause 16.2). Also, the guard expression shall not use of the operations create, running, alive and activate.
3. The evaluation of the event of an alt branch shall not have side effects. To avoid side effects that cause an inconsistency between the actual snapshot and the state of the component or introduce indeterminism in the evaluation of the following alt branches or the re-evalutaion of the same alt branch, the same restrictions as for function calls as in clause 16.1.4 shall apply to all function calls in the event part. Also, the event operation shall not use the operations create, running, alive and activate.
4. The evaluation of an altstep invoked from an alt branch, if none of the alternatives in the altstep is chosen, shall not have side effects. To avoid side effects the same restrictions as for function calls as in clause 16.1.4 shall apply to all function calls used in the actual parameters of the invoked altstep. Also, the altstep invocation parameters shall not use the operations create, running, alive and activate.
5. The else branch shall not contain any of the actions allowed in branches guarded by a boolean expression (i.e. an **altstep** call or a **done**, a **killed**, a **timeout** or a receiving operation).
6. An **alt** statement used within the module control part shall only contain **timeout** statements.

***Examples***

EXAMPLE 1: Nested alternatives

**alt** {

[] MyPort.**receive** (MyMessage) {

**setverdict** (**pass**);

MyTimer.**start**;

**alt** {

[] MyPort.**receive** (MySecondMessage) {

MyTimer.**stop**;

**setverdict** (**pass**);

}

[] MyTimer.**timeout** {

MyPort.**send** (MyRepeat);

MyTimer.**start**;

a**l**t {

[] MyPort.**receive** (MySecondMessage) {

MyTimer.**stop**;

**setverdict** (**pass**)

}

[] MyTimer.**timeout** { **setverdict** (**inconc**) }

[] MyPort.**receive** { **setverdict** (**fail**) }

}

}

[] MyPort.**receive** { **setverdict** (**fail**) }

}

}

[] MyTimer.**timeout** { **setverdict** (**inconc**) }

[] MyPort.**receive** { **setverdict** (**fail**) }

}

EXAMPLE 2: Alt statement with guards

**alt** {

[x>1] L2.**receive** { // Boolean guard/expression

**setverdict**(**pass**);

}

[x<=1] L2.**receive** { // Boolean guard/expression

**setverdict**(**inconc**);

}

}

EXAMPLE 3: Alt statement with else branch

// Use of alternative with Boolean expressions (or guard) and else branch

**alt** {

:

[**else**] { // else branch

MyErrorHandling();

**setverdict**(**fail**);

**stop;**

}

}

EXAMPLE 4: Re-evaluation with repeat

**alt** {

[] PCO3.**receive** {

count := count + 1;

**repeat** // usage of repeat

}

[] T1.**timeout** { }

[] **any** **port**.**receive** {

**setverdict**(**fail**);

**stop**;

}

}

EXAMPLE 5: Alt statement with explicitly invoked altstep

**alt** {

[] PCO3.**receive** { }

[] AnotherAltStep() { // Explicit call of altstep AnotherAltStep as alternative.

**setverdict**(**inconc**) // Statement block executed if an alternative within

// altstep AnotherAltStep has been selected and executed.

}

[] MyTimer.**timeout** { }

}

EXAMPLE 6: Alt statement with forbidden function calls

**alt** {

[] getPort().**receive**(t(p())) { } // forbidden if getPort, t or p has side effects

[] AnotherAltStep(f()); // forbidden if f has side effects

[] MyTimer[i(p())].**timeout** { } // forbidden if i or p has side effects

[g()] getComponent(p()).**done** {} // forbidden if g, getComponent or p has side effects

}

## 20.3 The Repeat statement

The **repeat** statement is used for a re-evaluation of an **alt** statement.

***Syntactical Structure***

**repeat**

***Semantic Description***

The **repeat** statement, when used in the statement block of alternatives of **alt** statements, causes the re-evaluation of the **alt** statement, i.e. a new snapshot is taken and the alternatives of the **alt** statement are evaluated in the order of their specification.

When used in statement blocks of the response and exception handling parts of blocking procedure calls, the repeat statement causes the re-evaluation of the response and exception handling part of the call (see clause 22.3.1).

If a **repeat** statement is used in a top alternative in an altstep definition, it causes a new snapshot and the re‑evaluation of the **alt** statement from which the altstep has been called. The call of the altstep may either be done implicitly by the default mechanism (see clause 20.5.1) or explicitly in the **alt** statement (see clause 20.2).

***Restrictions***

In addition to the general static rules of TTCN‑3 given in clause 5 and shown in table 15, the following restrictions apply:

1. The **repeat** statement shall only be used within **alt** statements, **call** statements or altsteps.

***Examples***

EXAMPLE 1: Usage of repeat in an alt statement

**alt** {

[] PCO3.**receive** {

count := count + 1;

**repeat** // usage of repeat

}

[] T1.**timeout** { }

[] **any** **port**.**receive** {

**setverdict**(**fail**);

**stop**;

}

}

EXAMPLE 2: Usage of repeat in an altstep

**altstep** AnotherAltStep() **runs on** MyComponentType {

[] PCO1.**receive**{

**setverdict**(**inconc**);

**repeat** // usage of repeat

}

[] PCO2.**receive** {}

}

## 20.4 The Interleave statement

The **interleave** statement allows to specify the interleaved occurrence and handling of receiving events including **done**, **killed**, **timeout**, **receive**, **trigger**, **getcall**, **getreply**, **catch** and **check.**

***Syntactical Structure***

**interleave** "{"

{ "[]" ( *TimeoutStatement* |

*ReceiveStatement* |

*TriggerStatement* |

*GetCallStatement* |

*CatchStatement* |

*CheckStatement* |

*GetReplyStatement* |

*DoneStatement* |

*KilledStatement* ) *StatementBlock*

}

"}"

***Semantic Description***

The **interleave** statement allows to specify the interleaved occurrence and handling of the statements **done**, **killed**, **timeout**, **receive**, **trigger**, **getcall**, **getreply**, **catch** and **check**.

Interleaved behaviour can always be replaced by an equivalent set of nested **alt** statements. The procedures for this replacement and the operational semantics of interleaving are described in part 4 of the TTCN‑3 standard (ES 201 873‑4 [1]).

The rules for the evaluation of an interleaving statement are the following:

1. Whenever a reception statement is executed, the following non-reception statements are subsequently executed until the next reception statement is reached, a **break** statement is reached, or the interleaved sequence ends.

NOTE 1: Reception statements are TTCN‑3 statements which may occur in sets of alternatives, i.e. **receive**, **check**, **trigger**, **getcall**, **getreply**, **catch**, **done,** **killed** and **timeout**. Non-reception statements denote all other non-control-transfer statements which can be used within the **interleave** statement.

1. If none of the alternatives of the **interleave** statement can be executed, the default mechanism will be invoked. This means, according to the semantics of the default mechanism, the actual snapshot will be used to evaluate those altsteps that have been activated before entering the **interleave** statement.

NOTE 2: The complete semantics of the default mechanism within an **interleave** statement is given by replacing the **interleave** statement by an equivalent set of nested **alt** statements. The default mechanism applies for each of these **alt** statements.

1. The evaluation then continues by taking the next snapshot if no **break** statement was encountered.
2. The evaluation of the **interleave** statement is terminated if a **break** statement is executed.

The operational semantics of interleaving are fully defined in part 4 of the TTCN‑3 standard (ES 201 873-4 [1]).

***Restrictions***

In addition to the general static rules of TTCN‑3 given in clause 5 and shown in table 15, the following restrictions apply:

1. Control transfer statements **for**, **while**, **do-while**, **goto**, **activate**, **deactivate**, **stop**, **repeat**, **return**, direct call of altsteps as alternatives and (direct and indirect) calls of user-defined functions, which include reception statements, shall not be used in **interleave** statements.
2. In addition, it is not allowed to guard branches of an **interleave** statement with Boolean expressions (i.e. the '[ ]' shall always be empty). It is also not allowed to specify **else** branches in interleaved behaviour.
3. An **interleave** statement used within the module control part shall only contain **timeout** statements.

***Examples***

// The following TTCN‑3 code fragment

**interleave** {

[] PCO1.**receive**(MySig1) {

PCO1.**send**(MySig2);

PCO1.**receive**(MySig3);

}

[] PCO2.**receive**(MySig4) {

PCO2.**send**(MySig5);

PCO2.**send**(MySig6);

PCO2.**receive**(MySig7);

}

}

// is a shorthand for

**alt** {

[] PCO1.**receive**(MySig1) {

PCO1.**send**(MySig2);

**alt** {

[] PCO1.**receive**(MySig3) {

alt {

[] PCO2.**receive**(MySig4) {

PCO2.**send**(MySig5);

PCO2.**send**(MySig6);

PCO2.**receive**(MySig7)

}

}

}

[] PCO2.**receive**(MySig4) {

PCO2.**send**(MySig5);

PCO2.**send**(MySig6);

**alt** {

[] PCO1.**receive**(MySig3) {

PCO2.**receive**(MySig7);

}

[] PCO2.**receive**(MySig7) {

PCO1.**receive**(MySig3);

}

}

}

}

}

[] PCO2.**receive**(MySig4) {

PCO2.**send**(MySig5);

PCO2.**send**(MySig6);

**alt** {

[] PCO1.**receive**(MySig1) {

PCO1.**send**(MySig2);

**alt** {

[] PCO1.**receive**(MySig3) {

PCO2.**receive**(MySig7);

}

[] PCO2.**receive**(MySig7) {

PCO1.**receive**(MySig3);

}

}

}

[] PCO2.**receive**(MySig7) {

**alt** {

[] PCO1.**receive**(MySig1) {

PCO1.**send**(MySig2);

PCO1.**receive**(MySig3);

}

}

}

}

}

}

## 20.5 Default Handling

TTCN‑3 allows the activation of altsteps (see clause 16.2) as defaults. For each test component the defaults, i.e. activated altsteps, are stored as an ordered list. The defaults are listed in the reversed order of their activation i.e. the last activated default is the first element in the list of active defaults. The TTCN‑3 operations **activate** (see clause 20.5.2) and **deactivate** (see clause 20.5.3) operate on the list of defaults. An **activate** puts a new default as the first element into the list and a **deactivate** removes a default from the list. A default in the default list can be identified by means of default reference that is generated as a result of the corresponding **activate** operation.

### 20.5.1 The default mechanism

The default mechanism is evoked at the end of each **alt** statement, if due to the actual snapshot none of the specified alternatives could be executed. An evoked default mechanism invokes the first altstep in the list of defaults, i.e. the last activated default, and waits for the result of its termination. The termination can be successful or unsuccessful. Unsuccessful means that none of the top alternatives of the **altstep** (see clause 16.2) defining the default behaviour could be selected, successful means that one of the top alternatives of the default has been selected and executed.

NOTE 1: An **interleave** statement is semantically equivalent to a nested set of **alt** statements and the default mechanism also applies to each of these **alt** statements. This means, the default mechanism also applies to **interleave** statements. Furthermore, the restrictions imposed on interleave statements in clause 20.4 do not apply to altsteps that are activated as default behaviour for interleave statements.

NOTE 2: Due to the possibility of defining dynamic test configurations, an alternative in an altstep activated as default may refer to a disconnected or unmapped port at the time of its evaluation. In TTCN-3, ports belong to the receiving component and matching is related to the top elements in the port queues. Dynamically unmapped and disconnected ports contribute to a snapshot in the same manner as mapped and connected ports. This means, an **altstep** invoked as default may execute receiving operations that empty the queues of unmapped and disconnected ports without causing a test case error.

In the case of an unsuccessful termination, the default mechanism invokes the next default in the list. If the last default in the list has terminated unsuccessfully, the default mechanism will return to the place in the **alt** statement in which it has been invoked, i.e. at the end of the **alt** statement, and indicate an unsuccessful default execution. An unsuccessful default execution will also be indicated if the list of defaults is empty.

An unsuccessful default execution may cause a new snapshot or a dynamic error if the test component is blocked (see clause 20.1).

In the case of a successful termination, the default may either stop the test component by means of a **stop** statement, or the main control flow of the test component will continue immediately after the **alt** statement from which the default mechanism was called or the test component will take new snapshot and re-evaluate the **alt** statement. The latter has to be specified by means of a **repeat** statement (see clause 20.3). If the execution of the selected top alternative of the default ends with a **break** statement or without a **repeat** statement the control flow of the test component will continue immediately after the **alt** statement.

NOTE 3: TTCN‑3 does not restrict the implementation of the default mechanism. It may for example be implemented in form of a process that is implicitly called at the end of each **alt** statement or in form of a separate thread that is only responsible for the default handling. The only requirement is that defaults are called in the reverse order of their activation when the default mechanism has been invoked.

### 20.5.2 The Activate operation

The **activate** operation is used to activate altsteps as defaults.

***Syntactical Structure***

**activate** "(" *AltstepRef* "(" [ { *ActualPar* [","] } ] ")" ")"

***Semantic Description***

An **activate** operation will put the referenced altstep as the first element into the list of defaults and return a default reference. The default reference is a unique identifier for the default and may be used in a **deactivate** operation for the deactivation of the default.

The effect of an **activate** operation is local to the test component in which it is called. This means, a test component cannot activate a default in another test component.

The **activate** operation can be called without saving the returned default reference. This form is useful in test cases which do not require explicit deactivation of the activated default, i.e. deactivation of a default is done implicitly at MTC termination.

The actual parameters of a parameterized altstep (see clause 16.2.1) that should be activated as a default, shall be provided in the corresponding **activate** statement. This means the actual parameters are bound to the default at the time of its activation (and not e.g. at the time of its invocation by the default mechanism).

***Restrictions***

In addition to the general static rules of TTCN‑3 given in clause 5 and shown in table 15, the following restrictions apply:

1. For altsteps activated on test components, all timer instances in the actual parameter list shall be declared as component type local timers (see clause 6.2.10.1).
2. For altsteps activated in module control or in functions or altsteps invoked directly or indirectly from module control, all timer instances in the actual parameter list shall be declared in the highest scope of the module control part (see clause 26.2). Timers from lower scopes of the module control part (i.e. from the nested statement blocks) are not allowed to occur in the actual parameter list.
3. An altstep that is activated as a default shall only have **in** parameters, port parameters, or timer parameters.

***Examples***

EXAMPLE 1: Activation where the default reference is kept

// Declaration of a variable for the handling of defaults

**var default** MyDefaultVar := **null**;

:

// Declaration of a default reference variable and activation of an altstep as default

**var** **default** MyDefVarTwo := **activate**(MySecondAltStep());

:

// Activation of altstep MyAltStep as a default

MyDefaultVar := **activate**(MyAltStep()); // MyAltStep is activated as default

:

// Usage of MyDefaultVar for the deactivation of default MyDefAltStep

**deactivate**(MyDefaultVar);

EXAMPLE 2: Simple activation

// Activation of an altstep as a default, without assignment of default reference

**activate**(MyCommonDefault());

EXAMPLE 3: Activation of a parameterized altstep

**altstep** MyAltStep2 ( **integer** par\_value1, MyType par\_value2,   
 MyPortType par\_port, **timer** par\_timer )  
 {  
 :  
 }

**function** MyFunc () **runs on** MyCompType

{ :

**var default** MyDefaultVar := **null**;

MyDefaultVar := **activate**(MyAltStep2(5, myVar, myCompPort, myCompTimer);

// MyAltStep2 is activated as default with the actual parameters 5 and

// the value of myVar. A change of myVar before a call of MyAltStep2 by

// the default mechanism will not change the actual parameters of the call.

:

}

### 20.5.3 The Deactivate operation

The **deactivate** operation is used to deactivate defaults, i.e. previously activated altsteps.

***Syntactical Structure***

**deactivate** [ "(" *VariableRef | FunctionInstance* ")" ]

***Semantic Description***

A **deactivate** operation will remove the referenced default from the list of defaults.

The effect of a **deactivate** operation is local to the test component in which it is called. This means, a test component cannot deactivate a default in another test component.

A **deactivate** operation without parameter deactivates all defaults of a test component.

Calling a **deactivate** operation with the special value **null** has no effect. Calling a **deactivate** operation with an undefined default reference, e.g. an old reference to a default that has already been deactivated or an uninitialized default reference variable, shall cause a runtime error.

***Restrictions***

In addition to the general static rules of TTCN‑3 given in clause 5 and shown in table 15, the following restrictions apply:

1. The variable associated with *VariableRef* (being a component type variable, a component type parameter, etc.) or the return type associated with *FunctionInstance* shall be of default type.

***Examples***

**var default** MyDefaultVar := **null**;

**var** **default** MyDefVarTwo := **activate**(MySecondAltStep());

**var** **default** MyDefVarThree := **activate**(MyThirdAltStep());

:

MyDefaultVar := **activate**(MyAltStep());

:

**deactivate**(MyDefaultVar); // deactivates MyAltStep

:

**deactivate**; // deactivates all other defaults, i.e. in this case MySecondAltStep

// and MyThirdAltStep

# 21 Configuration Operations

Configuration operations are used to set up and control test components and their connections. They are summarized in table 19.

***Restrictions***

In addition to the general static rules of TTCN‑3 given in clause 5, the following restrictions apply:

1. These operations shall only be used in:

* TTCN‑3 test cases;
* functions invoked directly or indirectly from a test case or from the function started on a ptc; and
* altsteps invoked directly or indirectly from a test case or from the function started on a ptc.

1. They shall not be used in:

* the module control part;
* functions or altsteps invoked directly or indirectly from the module control part;
* declarations inside component type definitions; or
* functions invoked directly or indirectly from declarations inside component type definitions.

Table 19: Overview of TTCN‑3 configuration operations

| Operation | Explanation | Syntax Examples |
| --- | --- | --- |
| **Connection Operations** | | |
| connect | Connects the port of one test component to the port of another test component | **connect**(ptc1:p1, ptc2:p2); |
| disconnect | Disconnects two or more connected ports | **disconnect**(ptc1:p1, ptc2:p2); |
| map | Maps the port of one test component to the port of the test system interface | **map**(ptc1:q, **system**:sutPort1); |
| unmap | Unmaps two or more mapped ports | **unmap**(ptc1:q, **system**:sutPort1); |
| **Test Component Operations** | | |
| create | Creation of a normal or alive test component, the distinction between normal and alive test components is made during creation (MTC behaves as a normal test component) | Non-alive test components:  **var** PTCType c := PTCType.**create**;  Alive test components:  **var** PTCType c := PTCType.**create** **alive**; |
| start | Starting test behaviour on a test component, starting a behaviour does not affect the status of component variables, timers or ports | c.**start**(PTCBehaviour()); |
| stop | Stopping test behaviour on a test component | c.**stop**; |
| kill | Causes a test component to cease to exist | c.**kill**; |
| alive | Returns true if the test component has been created and is ready to execute or is executing already a behaviour; otherwise returns false | **if** (c.**alive**) … |
| running | Returns true as long as the test component is executing a behaviour; otherwise returns false | if (c.**running**) … |
| done | Checks whether the function running on a test component has terminated | c.**done**; |
| killed | Checks whether a test component has ceased to exist | c.**killed** { … } |
| **Test Case Operations** | | |
| stop | Terminates the test case with the test verdict **error** | **testcase**.**stop** ( … ); |
| **Reference Operations** | | |
| mtc | Gets the reference to the MTC | **connect**(**mtc**:p, ptc:p); |
| system | Gets the reference to the test system interface | **map**(c:p, **system**:sutPort); |
| self | Gets the reference to the test component that executes this operation | **self**.**stop**; |

## 21.1 Connection Operations

The ports of a test component can be connected to other components or to the ports of the test system interface (see figure 10). In the case of connections between two test components, the **connect** operation shall be used. When connecting a test component to a test system interface the **map** operation shall be used. The **connect** operation directly connects one port to another with the **in** side connected to the **out** side and vice versa. The **map** operation on the other hand can be seen purely as a name translation defining how communications streams can be referenced.



Figure 10: Illustration of the connect and map operations

### 21.1.1 The Connect and Map operations

The **connect** operation and the **map** operation are used to setup connections to the SUT or between test components.

***Syntactical Structure***

**connect** "(" *ComponentRef* ":" *Port* "," *ComponentRef* ":" *Port* ")"

**map** "(" *ComponentRef* ":" *Port* "," *ComponentRef* ":" *Port* ")"

[ **param** "(" [ { *ActualPar* [","] }+ ] ")" ]

***Semantic Description***

With both the **connect** operation and the **map** operation, the ports to be connected are identified by the component references of the components to be connected and the names of the ports to be connected.

The operation **mtc** identifies the MTC, the operation **system** identifies the test system interface and the operation **self** identifies the test component in which **self** has been called (see clause 6.2.11). All these operations can be used for identifying and connecting ports.

Both the **connect** and **map** operations can be called from any behaviour definition except for the control part of a module. However before either operation is called, the components to be connected shall have been created and their component references shall be known together with the names of the relevant ports.

Both the **map** and **connect** operations allow the connection of a port to more than one other port. It is not allowed to connect to a mapped port or to map to a connected port.

Applying a **map** or **connect** operation to ports which are already mapped or connected has no effect on the test behaviour or test configuration, i.e. test execution continues as if the operation has not been invoked.

NOTE: Please note that also triMap or tciConnect respectively will not be invoked in such a case.

The **map** operation provides an optional parameter list for configuration purposes. This allows to pass values needed for dynamic runtime configuration. If a parameter list is present, the actual parameters shall conform to the **map** **param** clause of the port type declaration of the system port used.

***Restrictions***

In addition to the general static rules of TTCN‑3 given in clauses 5 and 21 and shown in table 15, the following restrictions apply:

a) For both the **connect** and **map** operations, only consistent connections are allowed.

Assuming the following:

1) ports PORT1 and PORT2 are the ports to be connected;

2) inlist-PORT1 defines the messages or procedures of the in-direction of PORT1;

3) outlist-PORT1defines the messages or procedures of the out-direction of PORT1;

4) inlist-PORT2 defines the messages or procedures of the in-direction of PORT2; and

5) outlist-PORT2 defines the messages or procedures of the out-direction of PORT2.

b) The **connect** operation is allowed if and only if:

outlist-PORT1 ⊆ inlist-PORT2 and outlist-PORT2 ⊆ inlist-PORT1.

c) The **map** operation (assuming PORT2 is the test system interface port) is allowed if and only if:

outlist-PORT1 ⊆ outlist-PORT2 *and* inlist-PORT2 ⊆ inlist-PORT1.

d) In all other cases, the operations shall not be allowed.

e) Since TTCN‑3 allows dynamic configurations and addresses, not all of these consistency checks can be made statically at compile-time. All checks, which could not be made at compile-time, shall be made at runtime and shall lead to a test case error when failing.

f) In addition, the restrictions on allowed and disallowed connections described in clause 9.1 apply.

g) In **map** operations, **param** clauses are optional. If in a **map** operation a **param** clause is present, exactly one of the components referenced by the operation shall be the **system** component reference, the type of the system component shall be known in the context of the operation either via a **system** clause or via a **runs on** clause in a **testcase** without **system** clause, the type of the system port to which the operation is applied shall include a **map param** declaration, and the actual parameters shall conform to the **map** **param** clause of the port type declaration of the system port used.

h) If the type of the component referenced in a connection operation is known (either when the component reference is a variable or value returned from a function or the type is defined in the runs on, mtc or system clause of the calling function), the referenced port declaration shall be present in this component type.

***Examples***

EXAMPLE 1: Simple map and connect

// It is assumed that the ports Port1, Port2, Port3 and PCO1 are properly defined and declared

// in the corresponding port type and component type definitions

:

**var** MyComponentType MyNewPTC;

MyNewPTC := MyComponentType.**create**;

:

**connect**(MyNewPTC:Port1, **mtc**:Port3);

**map**(MyNewPTC:Port2, **system**:PCO1);

:

// In this example a new component of type MyComponentType is created and its reference stored

// in variable MyNewPTC. Afterwards in the connect operation, Port1 of this new component

// is connected with Port3 of the MTC. By means of the map operation, Port2 of the new component

// is then connected to port PCO1 of the test system interface

EXAMPLE 2: Parameterized map

:

**var** MyConfigType MyConfig := { option := 1, lock := false};

:

**map**(**mtc**:Port4, **system**:PCO2) param (MyConfig);

:

// In this example by means of the map operation, Port4 of the MTC is connected to the port PCO2

// of the test system interface, and additionally a parameter containing configuration options

// for the connection is passed.

EXAMPLE 3: Port visibility

**type** **port** P **message** { **inout** **integer**; }

**type** **component** C1 { **port** P p1; }

**type** **component** C2 { **port** P p1, p2; }

**testcase** TC **runs on** C1 **system** C1

{

**var** C1 v\_ptc := C2.**create**; // valid assignment, instance of C2 is compatible with C1 type

**connect** (**self**:p1, v\_ptc:p1); // valid, p1 is present in C1 type definition

**disconnect** (**self**:p1, v\_ptc:p1);

**connect** (**self**:p1, v\_ptc:p2); // invalid, although the real instance in v\_ptc is of the

// C2 type, the variable itself is of the C1 type making the p2 port invisible to the

// connection operation  
 }

### 21.1.2 The Disconnect and Unmap operations

The **disconnect** and **unmap** operations are the opposite operations of **connect** and **map**.

***Syntactical Structure***

**disconnect** [ ( "(" *ComponentRef* ":" *Port* "," *ComponentRef* ":" *Port* ")" ) |

( "(" *PortRef* ")" ) |

( "(" *ComponentRef* ":" **all** **port** ")" ) |

( "(" **all** **component** ":" **all** **port** ")" ) ]

**unmap** [ ( "(" *ComponentRef* ":" *Port* "," *ComponentRef* ":" *Port* ")"

[ **param** "(" [ { *ActualPar* [","] }+ ] ")" ] ) |

( "(" *PortRef* ")" [ **param** "(" [ { *ActualPar* [","] }+ ] ")" ] ) |

( "(" *ComponentRef* ":" **all** **port** ")" ) |

( "(" **all** **component** ":" **all** **port** ")" ) ]

***Semantic Description***

The **disconnect** and **unmap** operations perform the disconnection (of previously connected) ports of test components and the unmapping of (previously mapped) ports of test components and ports in the test system interface.

Both, the **disconnect** and **unmap** operations can be called from any component if the relevant component references together with the names of the relevant ports are known. A **disconnect** or **unmap** operation has only an effect if the connection or mapping to be removed has been created beforehand.

To ease **disconnect** and **unmap** operations related to all connections and mappings of a component or a port, it is allowed to use **disconnect** and **unmap** operations with one argument only. This one argument specifies one side of the connections to be disconnected or unmapped. The **all port** keyword can be used to denote all ports of a component.

The usage of a **disconnect** or **unmap** operation without any parameters is a shorthand form for using the operation with the parameter **self**:**all port**. It disconnects or unmaps all ports of the component that calls the operation.

The **all component** keyword shall only be used in combination with the **all port** keyword, i.e. **all** **component**:**all** **port**, and shall only be used by the MTC. Furthermore, the **all component**:**all port** argument shall be used as the one and only argument of a **disconnect** or **unmap** operation and it allows to release all connections and mappings of the test configuration.

Similar to the **map** operation, **unmap** provides an optional parameter list for configuration purposes. If a parameter list is present, the actual parameters shall conform to the **unmap** **param** clause of the port type declaration of the system port used. It allows to pass values needed for dynamic runtime configuration.

***Restrictions***

In addition to the general static rules of TTCN‑3 given in clauses 5 and 21 and shown in table 15, the following restrictions apply:

a) In an **unmap** operation, a **param** clause shall only be present if the system port to which the **param** clause belongs to is explicitly referenced.

b) In **unmap** operations, **param** clauses are optional. If in an **unmap** operation a **param** clause is present, exactly one of the components referenced by the operation shall be the **system** component reference, the type of the system component shall be known in the context of the operation either via a **system** clause or via a **runs on** clause in a **testcase** without **system** clause, the type of the system port to which the operation is applied shall include an **unmap param** declaration and the actual parameters shall conform to the **unmap** **param** clause of the port type declaration of the system port used.

c) If the type of the component referenced in a connection operation is known (either when the component reference is a variable or value returned from a function or the type is defined the runs on, mtc or system clause of the calling function), the referenced port declaration shall be present in this component type.

***Examples***

EXAMPLE 1: Disconnect/unmap for specific connections

**connect**(MyNewComponent:Port1, **mtc**:Port3);

**map**(MyNewComponent:Port2, **system**:PCO1);

:

**disconnect**(MyNewComponent:Port1, **mtc**:Port3); // disconnect previously made connection

**unmap**(MyNewComponent:Port2, **system**:PCO1); // unmap previously made mapping

EXAMPLE 2: Disconnect/unmap for a component

**disconnect**(MyNewComponent:Port1); // disconnects all connections of Port1, which  
 // is owned by component MyNewComponent.

**unmap**(MyNewComponent:**all port**); // unmaps all ports of component MyNewComponent

EXAMPLE 3: Disconnect/unmap for "self"

**disconnect**; // is a shorthand form for …

**disconnect**(**self**:**all** **port**); // which disconnects all ports of the component

// that called the operation

:

**unmap**; // is a shorthand form for …

**unmap**(**self**:**all** **port**); // which unmaps all ports of the component

// that called the operation

EXAMPLE 4: Disconnect/unmap for "all component"

**disconnect**(**all component**:**all** **port**); // the MTC disconnects all ports of all

// components in the test configuration.

:

**unmap**(**all component**:**all** **port**); // the MTC unmaps all ports of all

// components in the test configuration.

## 21.2 Test case operations

Test case operations address the entire test case by using the keyword testcase. Currently, the test case stop operation is the only test case operation. It specifies an immediate stop of the test case behaviour with an error verdict.

### 21.2.1 Test case stop operation

The testcase stop operation defines a user defined immediate termination of a test case with the test verdict **error** and an (optional) associated reason for the termination. Such an immediate stop of a test case is required for cases where a user defined behaviour that does not contribute to the test outcome behaves in an unexpected manner which leads to a situation where the continuation of the test case makes no more sense.

***Syntactical Structure***

**testcase** "." **stop** [ "(" { ( *FreeText* | *TemplateInstance* ) [","] } ")" ]

***Semantic Description***

The test case stop operation causes an immediate stop of the entire test case behaviour with the verdict **error**. In addition, the test case stop operation provides the means to specify the reason for the immediate termination of a test case by writing one or more items to some logging device associated with the test control or the test component in which the operation is used. Items to be logged shall be identified by a comma‑separated list in the argument of the test case stop operation. The argument of the test case stop operation shall follow the same restrictions as the argument of the log statement (see clause 19.11).

***Restrictions***

No specific restrictions in addition to the general static rules of TTCN‑3 given in clause 5 and shown in table 15.

***Examples***

**testcase.stop**("Unexpected Termination");

// The test case stops the an error verdict and the string "Unexpected Termination"

// is written to some log device of the test system

## 21.3 Test Component Operations

Test component operations are used to create, start, stop and kill test components. They can also be used to check if test components are alive, running, done or killed.

### 21.3.1 The Create operation

The **create** operation is used to create test components.

***Syntactical Structure***

*ComponentType* "." **create** [ "(" *Expression* ["," *Expression*] ")" ] [ **alive** ]

***Semantic Description***

The MTC is the only test component, which is automatically created when a test case starts. All other test components (the PTCs) shall be created explicitly during test execution by **create** operations. A component is created with its full set of ports of which the input queues are empty and with its full set of constants, variables and timers. Furthermore, if a port is defined to be of the type **in** or **inout** it shall be in a listening state ready to receive traffic over the connection.

All component variables and timers are reset to their initial value (if any) and all component constants are reset to their assigned values when the component is explicitly or implicitly created.

Two types of PTCs are distinguished: a PTC that can execute a behaviour function only once and a PTC that is kept alive after termination of a behaviour function and can be therefore reused to execute another function. The latter is created using the additional **alive** keyword. An alive-type PTC shall be destroyed explicitly using the **kill** operation (see clause 21.3.4), whereas a non-alive PTC is destroyed implicitly after its behaviour function terminates. Termination of a test case, i.e. the MTC, terminates all PTCs that still exist, if any.

Since all test components and ports are implicitly destroyed at the termination of each test case, each test case shall completely create its required configuration of components and connections when it is invoked.

The **create** operation shall return the unique component reference of the newly created instance. The unique reference to the component will typically be stored in a variable (see clause 6.2.10.1) and can be used for connecting instances and for communication purposes such as sending and receiving.

Optionally, a name can be associated with the newly created component instance. The test system shall associate the names 'MTC' to the MTC and 'SYSTEM' to the test system interface automatically at creation. Associated component names are not required to be unique.

The component instance name is used for logging purposes (see clause 19.11) only and shall not be used to refer to the component instance (the component reference shall be used for this purpose) and has no effect on matching.

Also optionally, a host id can be associated with the newly created component instance. If a host id is provided, the **create** operation shall cause a test case error, if the component cannot be deployed on the specified host.

Components can be created at any point in a behaviour definition providing full flexibility with regard to dynamic configurations (i.e. any component can create any other PTC). The visibility of component references shall follow the same scope rules as that of variables and in order to reference components outside their scope of creation the component reference shall be passed as a parameter or as a field in a message.

***Restrictions***

In addition to the general static rules of TTCN‑3 given in clauses 5 and 21 and shown in table 15, the following restrictions apply:

a) The name given by the first *Expression* shall be a **charstring** value and when assigned it shall appear as the first argument of the **create** function.

b) The host id given by the second *Expression* shall be a **charstring** value and, when assigned, it shall appear as the second argument of the **create** function.

***Examples***

// This example declares variables of type MyComponentType, which is used to store the

// references of newly created component instances of type MyComponentType which is the

// result of the create operations. An associated name is allocated to some of the created

// component instances.

:

**var** MyComponentType MyNewComponent;

**var** MyComponentType MyNewestComponent;

**var** MyComponentType MyAliveComponent;

**var** MyComponentType MyAnotherAliveComponent;

**var** MyComponentType MyDeployedComponent;

:

MyNewComponent := MyComponentType.**create**;

MyNewestComponent := MyComponentType.**create**("Newest");

MyAliveComponent := MyComponentType.**create alive**;

MyAnotherAliveComponent := MyComponentType.**create**("Another Alive") **alive**;

MyDeployedComponent := MyComponentType.**create**(-, "Host4");

### 21.3.2 The Start test component operation

The start operation is used to associate a test behaviour to a test component, which is then being executed by that test component.

***Syntactical Structure***

( *VariableRef* | *FunctionInstance* ) "." **start** "(" *FunctionInstance* ")"

***Semantic Description***

Once a PTC has been created and connected, behaviour has to be bound to this PTC and the execution of its behaviour has to be started. This is done by using the **start** operation (as PTC creation does not start execution of the component behaviour). The reason for the distinction between **create** and **start** is to allow connection operations to be done before actually running the test component.

The **start** operation shall bind the required behaviour to the test component. This behaviour is defined by reference to an already defined function.

An alive-type PTC may perform several behaviour functions in sequential order. Starting a second behaviour function on a non-alive PTC or starting a function on a PTC that is still running results in a test case error. If a function is started on an alive-type PTC after termination of a previous function, it uses variable values, timers, ports, and the local verdict as they were left after termination of the previous function. In particular, if a timer was started in the previous function, the subsequent function should be enabled to handle a possible timeout event. In contrast to that, all active defaults are deactivated when the behaviour of an alive-type PTC is stopped. This means no default is activated when a new behaviour is started on an alive-type PTC.

NOTE 1: The lifetime of variables and timers is bound to the scope in which they are declared. When an alive-type component is stopped, only the component scope is left. This means only variable values and timers declared in the component type definition of an alive-type PTC can be accessed by a function with a corresponding **runs on**-clause that is started on an alive-type PTC.

***Restrictions***

In addition to the general static rules of TTCN‑3 given in clauses 5 and 21 and shown in table 15, the following restrictions apply:

1. The variable associated with *VariableRef* (being a component type variable, a component type parameter, etc.) or the return type associated with *FunctionInstance* shall be of component type.
2. The function invoked in a **start** test component operation shall have a **runs on** definition referencing a component type that is compatible with the newly created component (see clause 6.3.3).
3. Ports, defaults and timers shall not be passed into a function invoked in a **start** test component operation. All formal parameter types of the function shall neither be of port or default type or should contain a direct or indirect element or field of port or default type..

NOTE 2: Possible return values of a function invoked in a **start** test component operation, i.e. templates denoted by **return** keyword or **inout** and **out** parameters, have no effect when the started test component terminates.

NOTE 3: As **in** and **inout** ports starts listening when the component is created, at the moment, when it starts execution there may be messages in the incoming queues of such ports already waiting to be processed.

***Examples***

**function** MyFirstBehaviour() **runs on** MyComponentType { … }

**function** MySecondBehaviour() **runs on** MyComponentType { … }

:

**var** MyComponentType MyNewPTC;

var MyComponentType MyAlivePTC;

:

MyNewPTC := MyComponentType.**create**; // Creation of a new non-alive test component.

MyAlivePTC := MyComponentType.**create alive**; // Creation of a new alive-type test component

:

MyNewPTC.**start**(MyFirstBehaviour()); // Start of the non-alive component.

MyNewPTC.**done**; // Wait for termination

MyNewPTC.**start**(MySecondBehaviour()); // Test case error

:

MyAlivePTC.**start**(MyFirstBehaviour()); // Start of the alive-type component

MyAlivePTC.**done**; // Wait for termination

MyAlivePTC.**start**(MySecondBehaviour()); // Start of the next function on the same component

### 21.3.3 The Stop test behaviour operation

The stop test behaviour operation is used to stop the execution of a test component by itself or by another test component.

***Syntactical Structure***

**stop** |

( ( *VariableRef* | *FunctionInstance* | **mtc** | **self** ) "." **stop** ) |

( **all** **component** "." **stop** )

***Semantic Description***

By using the **stop** test component statement a test component can stop the execution of its own currently running test behaviour or the execution of the test behaviour running on another test component. If a component does not stop its own behaviour, but the behaviour running on another test component in the test system, the component to be stopped has to be identified by using its component reference. A component can stop its own behaviour by using a simple **stop** execution statement (see clause 19.9) or by addressing itself in the **stop** operation, e.g. by using the **self** operation.

NOTE 1: While the **create**, **start**, **running,** **done** and **killed** operations can be used for PTC(s) only, the **stop** operation can also be applied to the MTC.

Stopping a test component is the explicit form of terminating the execution of the currently running behaviour. A test component behaviour terminates also by completing its execution upon reaching the end of the testcase or function that is started on this component or by an explicit **return** statement. This termination is also called implicit stop. The implicit stop has the same effects as an explicit stop, i.e. the global verdict is updated with the local verdict of the stopped test component (see clause 24).

If the stopped test component is the MTC, resources of all existing PTCs shall be released, the PTCs shall be removed from the test system and the test case shall terminate (see clause 26.1).

Stopping a non-alive-type test component (implicitly or explicitly) shall destroy it and all resources associated with the test component shall be released.

Stopping an alive-type component shall stop the currently running behaviour only but the component continues to exist and can execute new behaviour (started on it using the **start** operation). Stopping an alive-type component means that all variables, timers and ports declared in the component type definition of the alive-type component keep their value, contents or state. Furthermore, the local verdict of the component keeps its value. In contrast to that, all active defaults are automatically deactivated when the alive-type component is stopped. The component shall be left in a consistent state after stopping its behaviour.

For example, if the behaviour of an alive-type component is stopped during assigning a new value to an already bound variable, the variable shall remain bound after the component is stopped (with the old or the new value). Similarly, if the component is stopped during re-starting an already running timer, the timer shall be left in the running state after termination of the behaviour.

The **all** keyword can be used by the MTC only in order to stop all running PTCs but the MTC itself.

NOTE 2: A PTC can stop the test case execution by stopping the MTC.

NOTE 3: The concrete mechanism for stopping PTCs is outside the scope of the present document.

***Restrictions***

In addition to the general static rules of TTCN‑3 given in clauses 5 and 21 and shown in table 15, the following restrictions apply:

1. The variable associated with *VariableRef* (being a component type variable, a component type parameter, etc.) or the return type associated with *FunctionInstance* shall be of component type.

***Examples***

EXAMPLE 1: Stopping another test component and a test component by itself

**var** MyComponentType MyComp := MyComponentType.**create**; // A new test component is created

MyComp.**start**(CompBehaviour()); // The new component is started

:

**if** (date == "1.1.2005") {

MyComp.**stop;** // The component "MyComp" is stopped

}

:

**if** (a < b ) {

:

**self**.**stop;** // The test component that is currently executing stops its own behaviour

}

:

**stop** // The test component stops its own behaviour

EXAMPLE 2: Stopping all PTCs by the MTC

**all component**.**stop** // The MTC stops all PTCs of the test case but not itself.

### 21.3.4 The Kill test component operation

The **kill** test component operation is used to destroy a test component by itself or by another test component. Kill and stop on a non-alive component have the same results, while they differ for alive components: stopping an alive components stops the test behaviour only, the test component continues to exist. Killing a test component destroys the test component.

***Syntactical Structure***

**kill** |

( ( *VariableRef* | *FunctionInstance* | **mtc** | **self** ) "." **kill** ) |

( **all** **component** "." **kill** )

***Semantic Description***

The **kill** operation applied on a test component stops the execution of the currently running behaviour - if any - of that component and frees all resources associated to it (including all port connections of the killed component) and removes the component from the test system. The **kill** operation can be applied on the current test component itself by a simple **kill** statement or by addressing itself using the **self** operation in conjunction with the kill operation. The **kill** operation can also be applied to another test component. In this case the component to be killed shall be addressed using its component reference. If the **kill** operation is applied on the MTC, e.g. **mtc.kill**, it terminates the test case.

The **all** keyword can be used by the MTC only in order to stop and kill all running PTCs but the MTC itself.

***Restrictions***

In addition to the general static rules of TTCN‑3 given in clause 5 and 21 and shown in table 15, the following restrictions apply:

1. The variable associated with *VariableRef* (being a component type variable, a component type parameter, etc.) or the return type associated with *FunctionInstance* shall be of component type.

***Examples***

EXAMPLE 1: Killing another test component and a test component by itself

**var** PTCType MyAliveComp := PTCType.**create alive**; // Create an alive-type test component

MyAliveComp.**start**(MyFirstBehaviour()); // The new component is started

MyAliveComp.**done**; // Wait for termination

MyAliveComp.**start**(MySecondBehavior()); // Start the component a 2nd time

MyAliveComp.**done**; // Wait for termination

MyAliveComp.**kill**; // Free its resources

EXAMPLE 2: Killing all PTCs by the MTC

**all component**.**kill**; // The MTC stops all (alive-type and normal) PTCs of the test case first  
 // and frees their resources.

### 21.3.5 The Alive operation

The **alive** operation is a Boolean operation that checks whether a test component has been created and is ready to execute or is executing already a behaviour function.

***Syntactical Structure***

( *VariableRef* |

*FunctionInstance* |

**any** **component** |

**all** **component** |

**any from** ComponentArrayRef ) "." **alive**

[ **"->" @index value** VariableRef]

***Semantic Description***

Applied on a normal test component, the **alive** operation returns true if the component is inactive or running a function and false otherwise. Applied on an alive-type test component, the operation returns true if the component is inactive, running or stopped. It returns false if the component has been killed.

The **alive** operation can be used similar to the **running** operation on PTCSs only (see clause 21.3.6). In particular, in combination with the **all** keyword it returns true if all (alive-type or normal) PTCs are alive.

The **alive** operation used in combination with the **any** keyword returns true if at least one PTC is alive.

When the **any from** component array notation is used, the components from the referenced array are iterated over and individually checked for being inactive or running a function from innermost to outermost dimension from lowest to highest index for each dimension. The first component to be found being inactive or running a function causes the alive operation to return the **true** value. The index of the first component found alive can optionally be assigned to an integer variable for single-dimensional component arrays or to an integer array or record of integer variable for multi‑dimensional component arrays.

***Restrictions***

In addition to the general static rules of TTCN‑3 given in clauses 5 and 21 and shown in table 15, the following restrictions apply:

1. The variable associated with *VariableRef* (being a component type variable, a component type parameter, etc.) or the return type associated with *FunctionInstance* shall be of component type.
2. The *ComponentArrayRef* shall be a reference to a completely initialized component array.
3. The index redirection shall only be used when the operation is used on an **any from** component array construct.
4. If the index redirection is used for single-dimensional component arrays, the type of the integer variable shall allow storing the highest index of the respective array.
5. If the index redirection is used for multi-dimensional component arrays, the size of the integer array or record of integer type shall exactly be the same as the dimension of the respective array, and its type shall allow storing the highest index (from all dimensions) of the array.
6. If a variable referenced in the **@index** clause is a lazy or fuzzy variable, the expression assigned to this variable is equal to the result produced by the **alive** operation, i.e. later evaluation of the lazy or fuzzy variable does not lead to repeated invocation of the **alive** operation.

***Examples***

PTC1.**done**; // Waits for termination of the component

**if** (PTC1.**alive**) { // If the component is still alive …

PTC1.**start**(AnotherFunction()); // … execute another function on it.

}

### 21.3.6 The Running operation

The **running** operation is a Boolean operation that checks whether a test component is executing already a behaviour function.

***Syntactical Structure***

( *VariableRef* |

*FunctionInstance* |

**any** **component** |

**all** **component** |

**any from** ComponentArrayRef ) "." **running**

[ "->" **@index value** VariableRef ]

***Semantic Description***

The **running** operation allows behaviour executing on a test component to ascertain whether behaviour running on a different test component has completed. The **running** operation can be used for PTCs only. The running operation returns **true** for PTCs that have been started but not yet terminated or stopped. It returns **false** otherwise. The **running** operation is considered to be a **boolean** expression and, thus, returns a **boolean** value to indicate whether the specified test component (or all test components) has terminated. In contrast to the **done** operation, the **running** operation can be used freely in **boolean** expressions.

When the **all** keyword is used with the **running** operation, it will return **true** if all PTCs started but not stopped explicitly by another component are executing their behaviour. Otherwise it returns **false**.

NOTE: The difference between the **running** operation applied to a single ptc and the usage of the **all** keyword leads to the situation that **ptc.running** is **false** if the ptc has never been started but **all component.running** is **true** at the same time as it considers only those components that ever have been started.

When the **any** keyword is used with the **running** operation, it will return **true** if at least one PTC is executing its behaviour. Otherwise it returns **false**.

When the **any from** component array notation is used, the components from the referenced array are iterated over and individually checked for executing currently from innermost to outermost dimension from lowest to highest index for each dimension. The first component to be found executing causes the running operation to succeed. The index of the matched component can optionally be assigned to an integer variable for single-dimensional arrays or to an integer array or record of integer variable for multi-dimensional component arrays.

***Restrictions***

In addition to the general static rules of TTCN‑3 given in clauses 5 and 21 and shown in table 15, the following restrictions apply:

1. The variable associated with *VariableRef* (being a component type variable, a component type parameter, etc.) or the return type associated with *FunctionInstance* shall be of component type.
2. The *ComponentArrayRef* shall be a reference to a completely initialized component array.
3. The index redirection shall only be used when the operation is used on an **any from** component array construct.
4. If the index redirection is used for single-dimensional component arrays, the type of the integer variable shall allow storing the highest index of the respective array.
5. If the index redirection is used for multi-dimensional component arrays, the size of the integer array or record of integer type shall exactly be the same as the dimension of the respective array, and its type shall allow storing the highest index (from all dimensions) of the array.
6. If a variable referenced in the **@index** clause is a lazy or fuzzy variable, the expression assigned to this variable is equal to the result produced by the **running** operation. Later evaluation of the lazy or fuzzy variable does not lead to repeated invocation of the **running** operation.

***Examples***

**if** (PTC1.**running**) // usage of running in an if statement

{

// do something!

}

**while** (**all** **component**.**running** != **true**) { // usage of running in a loop condition

MySpecialFunction()

}

### 21.3.7 The Done operation

The **done** operation allows behaviour executing on a test component to ascertain whether the behaviour running on a different test component has completed. In addition, the **done** operation allows to retrieve the final local verdict of completed test components, i.e., the value of the local verdict at the time of test component completion.

***Syntactical Structure***

( *VariableRef* |

*FunctionInstance* |

**any** **component** |

**all** **component** |

**any from** ComponentArrayRef ) "." **done**[ "->"[ **value** *VariableRef* ] [ **@index value** VariableRef ] ]

***Semantic Description***

The **done** operation shall be used in the same manner as a receiving operation or a **timeout** operation. This means it shall not be used in a **boolean** expression, but it can be used to determine an alternative in an **alt** statement or as stand-alone statement in a behaviour description. In the latter case a **done** operation is considered to be a shorthand for an **alt** statement with the **done** operation as the only alternative.

When the **done** operation is applied to a PTC, it matches only if the behaviour of that PTC has been stopped (implicitly or explicitly) or the PTC has been killed. Otherwise, the match is unsuccessful.

NOTE 1: The execution of a **done** operation does not change the state of the test component. Consecutive **done** operations applied to the same test component will give the same result as long as the test component does not change its state (see clause F.1.2).

When the **done** operation is applied to a PTC and matches, the final local verdict of the PTC can be retrieved and stored in variable of the type **verdicttype**. This is denoted by the symbol '**->**' the keyword **value** followed by the name of the variable into which the verdict is stored.

When the **all** keyword is used with the **done** operation, it matches if no one PTC is executing its behaviour. It also matches if no PTC has been created.

NOTE 2: The difference between the **done** operation applied to a single ptc and the usage of the **all** keyword leads to the situation that **ptc.done** does not match if the ptc has never been started but **all component.done** matches at the same time as it considers only those components that ever have been started.

When the **any** keyword is used with the **done** operation, it matches if at least the behaviour of one PTC has been stopped or killed. Otherwise, the match is unsuccessful.

NOTE 3: Stopping the behaviour of a non-alive component also results in removing that component from the test system, while stopping an alive-type component leaves the component alive in the test system. In both cases the **done** operation matches.

When the **any from** component array notation is used, the components from the referenced array are iterated over and individually checked for being stopped or killed from innermost to outermost dimension from lowest to highest index for each dimension. The first component to be found stopped or killed causes done operation to succeed. The index of the matched component can optionally be assigned to an integer variable for single-dimensional arrays or to an integer array or record of integer variable for multi-dimensional component arrays.

***Restrictions***

In addition to the general static rules of TTCN‑3 given in clauses 5 and 21 and shown in table 15, the following restrictions apply:

1. The **done** operation can be used for PTCs only.
2. The variable or the return type associated with *FunctionInstance* followed by the **done** keyword, i.e. used for identifying a specific PTC, shall be of component type.
3. The *ComponentArrayRef* shall be a reference to a completely initialized component array.
4. The variable used in the (optional) **value** clause for storing the final local verdict of a PTC shall be of the type **verdicttype**.
5. The (optional) **value** clause for storing the final local verdict of a PTC shall not be used in combination with **all component** or **any component**.
6. The index redirection shall only be used when the operation is used on an **any from** component array construct.
7. If the index redirection is used for single-dimensional component arrays, the type of the integer variable shall allow storing the highest index of the respective array.
8. If the index redirection is used for multi-dimensional component arrays, the size of the integer array or record of integer type shall exactly be the same as the dimension of the respective array, and its type shall allow storing the highest index (from all dimensions) of the array.
9. If a variable referenced in the **@index** clause is a lazy or fuzzy variable, the expression assigned to this variable is equal to the result produced by the **done** operation. Later evaluation of the lazy or fuzzy variable does not lead to repeated invocation of the **done** operation.

***Examples***

// Use of done in alternatives

**alt** {

[] MyPTC.**done** {

**setverdict**(**pass**)

}

[] **any port**.**receive** {

**repeat**

}

}

**var** MyComp c := MyComp.**create** **alive**;

c.**start**(MyPTCBehaviour());

:

c.**done**;

// matches as soon as the function MyPTCBehaviour (or function/altstep called by it) stops

c.**done**;

// matches the end of MyPTCBehaviour (or function/altstep called by it) too

if(c.**running**) {c.**done**}

// done here matches the end of the next behaviour only

// the following done as stand-alone statement:

**all component**.**done**;

// has the following meaning:

**alt** {

[] **all component**.**done** {}

}

// and thus, blocks the execution until all parallel test components have terminated

// Retrieving and using the final local verdict of a completed PTC

**var** MyComp MyPTC := MyPTC.**create** **alive**;

**var verdicttype** MyPTCverdict := **none**;

MyPTC.**start**(MyPTCBehaviour());

:

**alt** {

[] MyPTC.**done** -> **value** MyPTCverdict{

**if** (MyPTCverdict == **fail**) {

**setverdict**(**fail**);

**stop**;

}

**else** {

**setverdict** (**pass**);

}

}

[] **any port**.**receive** {

**repeat**

}

}

### 21.3.8 The Killed operation

The **killed** operation allows to ascertain whether a different test component is alive or has been removed from the test system. In addition, the **killed** operation allows to retrieve the final local verdict of killed test components, i.e., the value of the local verdict at the time when the test component was killed.

***Syntactical Structure***

( *VariableRef* |

*FunctionInstance* |

**any** **component** |

**all** **component** |

**any from** ComponentArrayRef ) "." **killed**

[ "->"[ **value** *VariableRef* ] [ **@index value** VariableRef ] ]

***Semantic Description***

The **killed** operation shall be used in the same manner as receiving operations. This means it shall not be used in **boolean** expressions, but it can be used to determine an alternative in an **alt** statement or as a stand-alone statement in a behaviour description. In the latter case a **killed** operation is considered to be a shorthand for an **alt** statement with the **killed** operation as the only alternative.

NOTE 1: When checking normal test components a killed operation matches if it stopped (implicitly or explicitly) the execution of its behaviour or has been **killed** explicitly, i.e. the operation is equivalent to the **done** operation (see clause 21.3.7). When checking alive-type test components, however, the **killed** operation matches only if the component has been killed using the **kill** operation. Otherwise the **killed** operation is unsuccessful.

NOTE 2: The execution of a **killed** operation does not change the state of the test component. Consecutive **killed** operations applied to the same test component will give the same result as long as the test component does not change its state (see clause F.1.2).

When the **all** keyword is used with the **killed** operation, it matches if all PTCs of the test case have ceased to exist. It also matches if no PTC has been created.

When the **killed** operation is applied to a PTC and matches, the final local verdict of the PTC can be retrieved and stored in a variable of the type **verdicttype**. This is denoted by the symbol '**->**' the keyword **value** followed by the name of the variable into which the verdict is stored.

When the **any** keyword is used with the **killed** operation, it matches if at least one PTC ceased to exist. Otherwise, the match is unsuccessful.

When the **any from** component array notation is used, the components from the referenced array are iterated over and individually checked for being killed from innermost to outermost dimension from lowest to highest index for each dimension. The first component to be found killed causes the killed operation to succeed. The index of the matched component can optionally be assigned to an integer variable for single-dimensional component arrays or to an integer array or record of integer variable for multi-dimensional component arrays.

***Restrictions***

In addition to the general static rules of TTCN‑3 given in clauses 5 and 21 and shown in table 15, the following restrictions apply:

1. The **killed** operation can be used for PTCs only.
2. The variable or the return type associated with *FunctionInstance* followed by the **killed** keyword, i.e. used for identifying a specific PTC, shall be of a component type.
3. The *ComponentArrayRef* shall be a reference to a completely initialized component array.
4. The variable used in the (optional) **value** clause for storing the final local verdict of a PTC shall be of the type **verdicttype**.
5. The (optional) **value** clause for storing the final local verdict of a PTC shall not be used in combination with **all component** or **any component**.
6. The index redirection shall only be used when the operation is used on an **any from** component array construct.
7. If the index redirection is used for single-dimensional component arrays, the type of the integer variable shall allow storing the highest index of the respective array.
8. If the index redirection is used for multi-dimensional component arrays, the size of the integer array or record of integer type shall exactly be the same as the dimension of the respective array, and its type shall allow storing the highest index (from all dimensions) of the array.
9. If a variable referenced in the **@index** clause is a lazy or fuzzy variable, the expression assigned to this variable is equal to the result produced by the **killed** operation i.e. later evaluation of the lazy or fuzzy variable does not lead to repeated invocation of the **killed** operation.

***Examples***

**var** MyPTCType ptc := MyPTCType.**create** **alive**; // create an alive-type test component

**timer** T:= 10.0; // create a timer

T.**start**; // start the timer

ptc.**start**(MyTestBehavior()); // start executing a function on the PTC

**alt** {

[] ptc.**killed** { // if the PTC was killed during execution …

T.**stop**; // … stop the timer and …

**setverdict**(**inconc**); // … set the verdict to 'inconclusive'

}

[] ptc.**done** { // if the PTC terminated regularly …

T.**stop**; // … stop the timer and …

ptc.**start**(AnotherFunction()); // … start another function on the PTC

}

[] T.**timeout** { // if the timeout occurs before the PTC stopped

ptc.**kill**; // … kill the PTC and …

**setverdict**(**fail**); // … set the verdict to 'fail'

}

}

// Retrieving and using the final local verdict of a killed PTC

**var** MyComp MyPTC := MyPTC.**create** **alive**;

**var** **verdicttype** MyPTCverdict := **none**;

MyPTC.**start**(MyPTCBehaviour());

:

**alt** {

[] MyPTC.**done** { // expected termination

**setverdict** (**pass**);

}

}

[] MyPTC.**killed** -> **value** MyPTCverdict{

**if** (MyPTCverdict == **none**) { // MyPTC killed before verdict assingment

**setverdict**(**fail**);

**stop**;

}

**else** {

**setverdict** (**inconc**); // further analysis is needed

**stop**;

}

}

[] **any port**.**receive** {

**repeat**

}

}

### 21.3.9 Summary of the use of any and all with components

The keywords **any** and **all** may be used with configuration operations as indicated in table 20.

Table 20: Any and All with components

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Operation | Allowed | | Example | Comment |
|  | **any (see note)** | all (see note) |  |  |
| **create** |  |  |  |  |
| **start** |  |  |  |  |
| **running** | Yes but from MTC only | Yes but from MTC only | **any component.running;**  **all component.running;** | Is there any PTC performing test behaviour?  Are all PTCs performing test behaviour? |
| **alive** | Yes but from MTC only | Yes but from MTC only | **any component.alive;**  **all component.alive;** | Is there any alive PTC?  Are all PTCs alive? |
| **done** | Yes but from MTC only | Yes but from MTC only | **any component.done;**  **all component.done;** | Is there any PTC that completed execution?  Did all PTCs complete their execution? |
| **killed** | Yes but from MTC only | Yes but from MTC only | **any component.killed;**  **all component.killed;** | Is there any PTC that ceased to exist?  Did all PTCs cease to exist? |
| **stop** |  | Yes but from MTC only | **all component.stop;** | Stop the behaviour on all PTCs. |
| **kill** |  | Yes but from MTC only | **all component.kill;** | Kill all PTCs, i.e. they cease to exist. |
| NOTE: **any** and **all** refer to PTCs only, i.e. the MTC is not considered. | | | | |

# 22 Communication operations

TTCN‑3 supports *message-based* and *procedure-based* *unicast*, *multicast* and *broadcast* communication. Furthermore, TTCN‑3 allows to examine the top element of incoming port queues and to control the access to ports by means of *controlling operations*. The communication operations and restrictions on their usage are summarized in table 21.

Table 21: Overview of TTCN‑3 communication operations

|  |  |  |  |
| --- | --- | --- | --- |
| Communication operations | | | |
| Communication operation | Keyword | Can be used at message-based ports | Can be used at procedure-based ports |
| Message-based communication | | | |
| Send message | **send** | Yes |  |
| Receive message | **receive** | Yes |  |
| Trigger on message | **trigger** | Yes |  |
| Procedure-based communication | | | |
| Invoke procedure call | **call** |  | Yes |
| Accept procedure call from remote entity | **getcall** |  | Yes |
| Reply to procedure call from remote entity | **reply** |  | Yes |
| Raise exception (to an accepted call) | **raise** |  | Yes |
| Handle response from a previous call | **getreply** |  | Yes |
| Catch exception (from called entity) | **catch** |  | Yes |
| Examine top element of incoming port queues | | | |
| Check msg/call/exception/reply received | **check** | Yes | Yes |
| **Controlling operations** | | | |
| Clear port queue | **clear** | Yes | Yes |
| Clear queue and enable sending and receiving at a port | **start** | Yes | Yes |
| Disable sending and disallow receiving operations to match at a port | **stop** | Yes | Yes |
| Disable sending and disallow receiving operations to match new messages/calls | **halt** | Yes | Yes |
| Check the state of a port | **checkstate** | Yes | Yes |

## 22.1 The communication mechanisms

This clause explains the principles of TTCN‑3 communication for message-based communication (see clause 22.1.1), for procedure-based communication (see clause 22.1.2), for unicast, multicast, and broadcast communication (see clause 22.1.3), as well as the general format of sending and receiving operations (see clause 22.1.4).

### 22.1.1 Principles of message-based communication

Message-based communication is communication based on an asynchronous message exchange. Message-based communication is non-blocking on the **send** operation, as illustrated in figure 11, where processing in the SENDER continues immediately after the **send** operation occurs. The RECEIVER is blocked on the **receive** operation until it processes the received message.

In addition to the **receive** operation, TTCN‑3 provides a **trigger** operation that filters messages with certain matching criteria from a stream of received messages on a given incoming port. Messages at the top of the queue that do not fulfil the matching criteria are removed from the port without any further action.



Figure 11: Illustration of the asynchronous send and receive

### 22.1.2 Principles of procedure-based communication

The principle of procedure-based communication is to call procedures in remote entities. TTCN‑3 supports *blocking* and *non-blocking* procedure-based communication. Blocking procedure-based communication is blocking on the calling and the called side, whereas non-blocking procedure-based communication is only blocking on the called side. Signatures of procedures that are used for non-blocking procedure-based communication shall be specified according to the rules in clause 13.

The communication scheme of blocking procedure-based communication is shown in figure 12. The CALLER calls a remote procedure in the CALLEE by using the **call** operation. The CALLEE accepts the call by means of a **getcall** operation and reacts by either using a **reply** operation to answer the call or by raising (**raise** operation) an exception. The CALLER handles the reply or exception by using **getreply** or **catch** operations. In figure 12, the blocking of CALLER and CALLEE is indicated by means of dashed lines.



Figure 12: Illustration of blocking procedure-based communication

The communication scheme of non-blocking procedure-based communication is shown in figure 13. The CALLER calls a remote procedure in the CALLEE by using the **call** operation and continues its execution, i.e. does not wait for a reply or exception. The CALLEE accepts the call by means of a **getcall** operation and executes the requested procedure. If the execution is not successful, the CALLEE may raise an exception to inform the CALLER. The CALLER may handle the exception by using a **catch** operation in an **alt** statement. In figure 13, the blocking of the CALLEE until the end of the call handling and possible raise of an exception is indicated by means of a dashed line.



Figure 13: Illustration of non-blocking procedure-based communication

### 22.1.3 Principles of unicast, multicast and broadcast communication

TTCN‑3 supports unicast, multicast and broadcast communication:

* Unicast communication means one sender to one receiver.
* Multicast communication is from one sender to a list of receivers.
* Broadcast communication is from one sender to all receivers (being connected or mapped to the sender).

The terms unicast, multicast and broadcast communication are related to port communication. This means, it is only possible to address one, several or all test components that are connected to the specified port. Unicast, multicast and broadcast can also be used for mapped ports. In this case, one, several or all entities within the SUT can be reached via the specified mapped port.

### 22.1.4 General format of communication operations

Operations such as **send** and **call** are used for the exchange of information among test components and between an SUT and test components. For explaining the general format of these operations, they can be structured into two groups:

a) a test component sends a message (**send** operation), calls a procedure (**call** operation), or replies to an accepted call (**reply** operation) or raises an exception (**raise** operation). These actions are collectively referred to as *sending operations*;

b) a component receives a message (**receive** operation), awaits a message (**trigger** operation),accepts a procedure call (**getcall** operation), receives a reply for a previously called procedure (**getreply** operation) or catches an exception (**catch** operation). These actions are collectively referred to as *receiving operations*.

#### 22.1.4.1 General format of the sending operations

Sending operations consist of a *send* part and, in the case of a blocking procedure-based **call** operation, a *response* and *exception handling* part.

The send part:

* specifies the port at which the specified operation shall take place;
* defines the message or procedure call to be transmitted;
* gives an (optional) address part that uniquely identifies one or more communication partners to which a message, call, reply or exception shall be send.

The port name, operation name and value shall be present in all sending operations. The address part (denoted by the **to** keyword) is optional and need only be specified in cases of one-to-many connections where:

* unicast communication is used and one receiving entity shall be explicitly identified;
* multicast communication is used and a set of receiving entities has to be explicitly identified;
* broadcast communication is used and all entities connected to the specified port have to be addressed.

EXAMPLE 1:

|  |  |  |  |
| --- | --- | --- | --- |
| **Send part** | | | **(Optional) response and exception** |
| Port and operation | Value part | (Optional) address part | handling part |
| MyP1.**send** | (MyVariable + YourVariable - 2) | **to** MyPartner; |  |

Response and exception handling is only needed in cases of procedure-based communication. The response and exception handling part of the **call** operation is optional and is required for cases where the called procedure returns a value or has **out** or **inout** parameters whose values are needed within the calling component and for cases where the called procedure may raise exceptions which need to be handled by the calling component.

The response and exception handling part of the call operation makes use of **getreply** and **catch** operations to provide the required functionality.

EXAMPLE 2:

|  |  |  |  |
| --- | --- | --- | --- |
| Send part | | | (Optional) response and exception handling part |
| Port and operation | Value part | (Optional) address part |  |
| MyP1.**call** | (MyProc:{MyVar1}) |  | {  [] MyP1.**getreply**(MyProc:{MyVar2}) {}  [] MyP1.**catch**(MyProc, ExceptionOne) {} } |

#### 22.1.4.2 General format of the receiving operations

A receiving operation consists of a *receive* part and an (optional) *assignment* part.

The receive part:

a) specifies the port at which the operation shall take place;

b) defines a matching part which specifies the acceptable input which will match the statement;

c) gives an (optional) address expression that uniquely identifies the communication partner (in case of one‑to‑many connections).

The port name, operation name and value part of all receiving operations shall be present. The identification of the communication partner (denoted by the **from** keyword) is optional and need only be specified in cases of one‑to‑many connections where the receiving entity needs to be explicitly identified.

The assignment part in a receiving operation is optional. For message-based ports it is used when it is required to store received messages. In the case of procedure-based ports it is used for storing the **in** and **inout** parameters of an accepted call, for storing the return value or for storing exceptions. For the assignment part strong typing is required, e.g. the variable used for storing a message shall have the same type as the incoming message.

In addition, the assignment part may also be used to assign the **sender** address of a message, exception, **reply** or **call** to a variable. This is useful for one-to-many connections where, for example, the same message or call can be received from different components, but the message, reply or exception shall be sent back to the original sending component.

For receiving operations using the any port from a port array construction (see clause 22.2.2), the assignment part may also be used to store the indices that identify the specific port instance where the receiving operation matched.

EXAMPLE:

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| Receive part | | |  | (Optional) assignment part | | |
| Port and operation | Matching part | (Optional) address expression |  | (Optional) value assignment | (Optional) parameter value assignment | (Optional) sender value assignment |
| MyP1.getreply | (AProc:{?} value 5) |  | -> |  | param (V1) | sender APeer |

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| Receive part | | |  | (Optional) assignment part | | |
| Port and operation | Matching part | (Optional) address expression |  | (Optional) value assignment | (Optional) parameter value assignment | (Optional) sender value assignment |
| MyP2.receive | (MyTemplate(5,7)) | from APeer | -> | value MyVar |  |  |

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| Receive part | | |  | (Optional) assignment part | | | |
| Port and operation | Matching part | (Optional) address expression |  | (Optional) value assignment | (Optional) parameter value assignment | (Optional) sender value assignment | (Optional)  port index assignment |
| any from P.receive | (MyTemplate(5,7)) |  | -> |  |  |  | @index **value** I |

## 22.2 Message-based communication

The operations for message-based communication via asynchronous ports are summarized in table 22.

Table 22: Overview of TTCN‑3 message-based communication

|  |  |
| --- | --- |
| Communication operation | Keyword |
| Send message | **send** |
| Receive message | **receive** |
| Trigger on message | **trigger** |
| Check message received | **check** |

### 22.2.1 The Send operation

The **send** operation is used to place a message on an outgoing message port.

***Syntactical Structure***

*Port* "." **send** "(" *TemplateInstance* ")"

[ **to** *Address* ]

NOTE: *Address* may be an *AddressRef*, a list of *AddressRef*-s or "**all component**".

***Semantic Description***

The **send** operation places a message on an outgoing message port. The message may be specified by referencing a defined template or can be defined as an in-line template.

**Sending unicast, multicast or broadcast**

Unicast, multicast and broadcast communication can be determined by the optional **to** clause in the **send** operation. A **to** clause can be omitted in case of a one-to-one connection where unicast communication is used and the message receiver is uniquely determined by the test system structure.

Unicast communication is specified, if the **to** clause addresses one communication partner only. Multicast communication is used, if the **to** clause includes a list of communication partners. Broadcast is defined by using the **to** clause with **all component** keyword.

***Restrictions***

In addition to the general static rules of TTCN‑3 given in clause 5 and shown in table 15, the following restrictions apply:

a) The TemplateInstance (and all parts of it) shall have a specific value i.e. the use of matching mechanisms such as *AnyValue* is not allowed.

b) When defining the message in-line, the optional type part shall be used if there is ambiguity of the type of the message being sent.

c) The **send** operation shall only be used on message-based ports and the type of the template to be sent shall be in the list of outgoing types of the port type definition.

d) A **to** clause shall be present in case of one-to-many connections.

e) *AddressRef* shall be of type **address**, **component** or of the type provided in the address declaration of the port type of the port instance referenced in the **send** operation. No *AddressRef* shall contain the special value **null** at the time of the operation.

f) Applying a **send** operation to an unmapped or disconnected port shall cause a test case error.

***Examples***

EXAMPLE 1: Simple send (receiver is determined from the test configuration)

MyPort.**send**(MyTemplate(5,MyVar)); // Sends the template MyTemplate with the actual

// parameters 5 and MyVar via MyPort.

MyPort.**send**(5); // Sends the integer value 5 (which is an in-line template)

EXAMPLE 2: Sending with explicit to clause

MyPort.**send**(**charstring**:"My string") **to** MyPartner;

// Sends the string "My string" to a component with a

// component reference stored in variable MyPartner

MyPCO.**send**(MyVariable + YourVariable - 2) **to** MyPartner;

// Sends the result of the arithmetic expression to MyPartner.

MyPCO2.**send**(MyTemplate) **to** (MyPeerOne, MyPeerTwo);

// Specifies a multicast communication, where the value of

// MyTemplate is sent to the two component references stored

// in the variables MyPeerOne and MyPeerTwo.

MyPCO3.**send**(MyTemplate) **to all component**;

// Broadcast communication: the value of Mytemplate is send to

// all components which can be addressed via this port. If

// MyPCO3 is a mapped port, the components may reside inside

// the SUT.

### 22.2.2 The Receive operation

The **receive** operation is used to receive a message from an incoming message port queue.

***Syntactical Structure***

( *Port* | **any** **port** | **any from** PortArrayRef ) "." **receive**

[ "(" *TemplateInstance* ")" ]

[ **from** *Address* ]

[ "->" [ **value** ( *VariableRef* |

( "(" { *VariableRef* [ ":=" [ **@decoded** [ "(" *Expression* ")" ] ]

*FieldOrTypeReference* ][","] } ")" )

) ]

[ **sender** *VariableRef* ]

[ @**index** **value** *VariableRef* ] ]

NOTE 1: *Address* may be an *AddressRef*, a list of *AddressRef*-s or "**any component**".

***Semantic Description***

The **receive** operation is used to receive a message from an incoming message port queue. The message may be specified by referencing a defined template or can be defined as an in-line template.

The **receive** operation removes the top message from the associated incoming port queue if, and only if, that top message satisfies all the matching criteria associated with the **receive** operation.

If the match is not successful, the top message shall not be removed from the port queue i.e. if the **receive** operation is used as an alternative of an **alt** statement and it is not successful, the execution of the test case shall continue with the next alternative of the **alt** statement.

**Matching criteria**

The matching criteria are related to the type and value of the message to be received. The type and value of the message to be received are determined by the argument of the **receive** operation, i.e. may either be derived from the defined template or be specified in-line. An optional type field in the matching criteria to the **receive** operation shall be used to avoid any ambiguity of the type of the value being received.

NOTE 2: Encoding attributes also participate in matching in an implicit way, by preventing the decoder to produce an abstract value from the received message encoded in a different way than specified by the attributes.

**Receiving from a specific sender**

In the case of one-to-many connections the **receive** operation may be restricted to a certain communication partner. This restriction shall be denoted using the **from** keyword.

**Storing the received message and parts of the received message**

If the match is successful, the value removed from the port queue and/or parts of this value can be stored in variables or formal parameters. This is denoted by the symbol '->' and the keyword **value**.

When the keyword **value** is followed by a name of a variable or formal parameter, the whole received message shall be stored in the variable or formal parameter. The variable or formal parameter shall be type compatible with the received message.

When the keyword **value** is followed by an assignment list enframed by a pair of parentheses, the whole received message and/or one or more parts of it can be stored. In a single assignment within the list, on the left hand side of the assignment symbol (":=") a field of the template type shall be referenced, on the right hand side the name of the variable or a formal parameter, in which the value shall be stored. The variable or formal parameter shall be type compatible with the type on the left hand side of the assignment symbol. As a special case the field reference can be absent to indicate that the whole message shall be stored in a variable.

When assigning individual fields of a message, encoded payload fields can be decoded prior to assignment using the **@decoded** modifier. In this case, the referenced field on the right hand sided of the assignment shall be one of the **bitstring**, **hexstring**, **octetstring**, **charstring** or **universal** **charstring** types. It shall be decoded into a value of the same type as the variable on the left hand side of the assignment. Failure of this decoding shall cause a test case error. In case the referenced field is of the **universal** **charstring** type, the **@decoded** clause can contain an optional parameter defining the encoding format. The parameter shall be of the **charstring** type and it shall contain one of the strings allowed for the **decvalue\_unichar** function (specified in clause C.5.4). Any other value shall cause an error. In case the referenced field is not a **universal** **charstring**, the optional parameter shall not be present.

NOTE 1: The model of the behaviour of this implicit decoding is defined in clause B.1.2.9.

NOTE 2: The **@decoded** clause is typically used together with the **decmatch** matching mechanism in the matching part of the receive statement. Since the decoding procedures for assignment and matching are virtually the same, TTCN-3 tools can be optimized in such a way that only one call to the decoder is made when the receiving statement contains both **decmatch** matching mechanism and **@decoded** assignment for the same payload field.

**Storing the sender**

It is also possible to retrieve and store the component reference or address of the sender of a message. This is denoted by the keyword **sender**.

When the message is received on a connected port, only the component reference is stored in the following the **sender** keyword, but the test system shall internally store the component name too, if any (to be used in logging).

**Receive any message**

A **receive** operation with no argument list for the type and value matching criteria of the message to be received shall remove the message on the top of the incoming port queue (if any) if all other matching criteria are fulfilled.

**Receive on any port**

To **receive** a message on any port, use the **any port** keywords.

**Receive on any port from a port array**

To **receive** a message on any port from a specific port array, use the **any from** *PortArrayRef*syntax where PortArrayRefshallbe areference to a port array identifier**.** It is also possible to store the index of a port in a single-dimensional port array at which the operation was successful to a variable of type integer or, in case of multi-dimensional port arrays the index of the successful port to an integer array or record of integer variable. When checking the port array for matching messages, the port indices to be checked are iterated from lowest to highest. If the port array is multi-dimensional, then the ports are iterated over from innermost to outermost array dimension from lowest to highest index for each dimension, e.g. [0][0], [0][1], [1][0], [1][1]. The first port which matches all the criteria will cause the operation to be successful even if other ports in the array would also meet the criteria.

**Stand-alone receive**

The **receive** operation can be used as a stand-alone statement in a behaviour description. In this latter case the **receive** operation is considered to be shorthand for an **alt** statement with the **receive** operation as the only alternative.

***Restrictions***

In addition to the general static rules of TTCN‑3 given in clause 5 and shown in table 15, the following restrictions apply:

a) When defining the message in-line, the optional type part shall be present whenever the type of the message being received is ambiguous.

b) The **receive** operation shall only be used on message-based ports and the type of the value to be received shall be included in the list of incoming types of the port type definition.

c) No binding of the incoming values to the terms of the expression or to the template shall occur.

d) A message received by *receive any message* shall not be stored, i.e. the **value** clause shall not be present.

e) Type mismatch at storing the received value or parts of the received value and storing the sender shall cause an error.

f) *AddressRef* for retrieving the sending entity shall be of type **address**, **component** or of the type provided in the address declaration of the port type of the port instance referenced in the **receive** operation. No *AddressRef* shall contain the special value **null** at the time of the operation.

g) The *PortArrayRef* shall be a reference to a completely initialized port array.

h) The index redirection shall only be used when the operation is used on an any from port array construct.

i) If the index redirection is used for single-dimensional port arrays, the type of the integer variable shall allow storing the highest index of the respective array.

j) If the index redirection is used for multi-dimensional port arrays, the size of the integer array or record of integer type shall exactly be the same as the dimension of the respective array, and its type shall allow storing the highest index (from all dimensions) of the array.

k) If a variable referenced in the **value**, **sender** or **@index** clause is a lazy or fuzzy variable, the expression assigned to this variable is equal to the result produced by the **receive** operation i.e. later evaluation of the lazy or fuzzy variable does not lead to repeated invocation of the **receive** operation.

l) If the **receive** operation contains both **from** and **sender** clause, the variable or parameter referenced in the **sender** clause shall be type compatible with the template in the **from** clause.

m) When assigning implicitly decoded message fields (by using the **@decoded** modifier) in cases where the value or template to be matched uses the *MatchDecodedContent* (**decmatch**) matching for the field to be stored, the type of the template in the *MatchDecodedContent* matching shall be type-compatible to the type of the variable the decoded field is stored into.

***Examples***

EXAMPLE 1: Basic receive

MyPort.**receive**(MyTemplate(5, MyVar)); // Matches a message that fulfils the conditions

// defined by template MyTemplate at port MyPort.

MyPort.**receive**(A<B); // Matches a Boolean value that depends on the outcome of A<B

MyPort.**receive**(**integer**:MyVar); // Matches an integer value with the value of MyVar

// at port MyPort

MyPort.**receive**(MyVar); // Is an alternative to the previous example

EXAMPLE 2: Receiving from a sender, storing the message, parts of the message or the sender

**type** MyPayloadType **record** {

**integer** messageId,

ContentType content

}

**type** MyType2 **record** {

Header header,

**octetstring** payload

}

**template** MyType MyTemplate := {

messageId := 42,

content := ?

}

...

**var** MyPayloadType MyVar;

**var** **integer** MyMessageIdVar, MyIntegerVar;

**var** **charstring** MyCharstringVar;

**var** **address** MyPeer;

**var** **octetstring** MyVarOne := '00ff'O;

MyPort.**receive**(**charstring**:"Hello")**from** MyPeer; // Matches charstring "Hello" from MyPeer

MyPort.**receive**(MyType:?) -> **value** MyVar; // The value of the received message is

// assigned to MyVar.

MyPort.**receive**(MyType:?) -> **value** (MyVar, MyMessageIdVar:= MyType.messageId)

// The value of the received message is stored in the variable

// MyVar and the value of the messageId field of the received

// message is stored in the variable MyMessageIdVar.

MyPort.**receive**(anytype:?) -> **value** (MyIntegerVar := integer)

// If the received value is an integer, it is stored in the variable

// MyIntegerVar, a test case error otherwise.

MyPort.**receive**(charstring:?) -> **value** (MyCharstringVar)

// The received value is stored in the variable MyCharstringVar;

// Note that it is the same as to write "**value** MyCharstringVar"

MyPort.**receive**(A<B) -> **sender** MyPeer; // The address of the sender is assigned to MyPeer

MyPort.**receive**(MyType:{5, MyVarOne}) -> **value** MyVar **sender** MyPeer;

// The received message value is stored in MyVarTwo and the sender address is stored in MyPeer.

MyPort.**receive**(MyType2:{header := ?, payload := **decmatch** MyTemplate }) -> **value** (MyVar := **@decoded** payload);

// The encoded payload field of the received message is decoded and matched with

// MyTemplate; if the matching is successful the decoded payload is stored in MyVar.

EXAMPLE 3: Receive any message

MyPort.**receive**; // Removes the top value from MyPort.

MyPort.**receive** **from** MyPeer; // Removes the top message from MyPort if its sender is   
 MyPeer

MyPort.**receive** -> **sender** MySenderVar; // Removes the top message from MyPort and assigns

// the sender address to MySenderVar

EXAMPLE 4: Receive on any port

**any port**.**receive**(MyMessage);

EXAMPLE 5: Receive on any port from a port array

**type** **port** MyPort **message** { **inout** **integer** }

**type** **component** MyComponent {

**port** MyPort p[10][10];

}

**var** **integer** i[2];

**any** **from** p.**receive**(MyMessage) -> **@index value** i;

// checking receiving MyMessage on any port of the port array p and storing the index of the

// port on which the matching was successful first; if, for example MyMessage is matched first

// on p[4,2], the content of i will be {4,2}

### 22.2.3 The Trigger operation

The **trigger** operation is used to await a specific message on an incoming port queue.

***Syntactical Structure***

( *Port* | **any** **port** | **any from** PortArrayRef ) "." **trigger**

[ "(" *TemplateInstance* ")" ]

[ **from** *Address* ]

[ "->" [ **value** ( *VariableRef* |

( "(" { *VariableRef* [ ":=" [ @decoded [ "(" *Expression* ")" ] ]

*FieldOrTypeReference* ][","] } ")" )

) ]

[ **sender** *VariableRef* ]

[ @**index** **value** *VariableRef* ] ]

NOTE: *Address* may be an *AddressRef*, a list of *AddressRef*-s or "**any component**".

***Semantic Description***

The **trigger** operation removes the top message from the associated incoming port queue. If that top message meets the matching criteria, the **trigger** operation behaves in the same manner as a **receive** operation. If that top message does not fulfil the matching criteria, it shall be removed from the queue without any further action.

The **trigger** operation requires the port name, matching criteria for type and value, an optional **from** restriction (i.e. selection of communication partner) and an optional assignment of the matching message and sender component to variables.

**Matching criteria**

The matching criteria as defined in clause 22.2.2 apply also to the **trigger** operation.

**Trigger on any message**

A **trigger** operation with no argument list shall trigger on the receipt of any message. Thus, its meaning is identical to the meaning of receive any message.

**Trigger on any port**

To **trigger** on a message at any port, use the **any port** keywords.

**Trigger on any port from a port array**

To trigger on a message at any port from a specific port array, use the **any from** *PortArrayRef*syntax where PortArrayRefshallbe areference to a port array identifier**.** It is also possible to store the index of a port in a single‑dimensional port array at which the operation was successful to a variable of type integer or, in case of multi‑dimensional port arrays the index of the successful port to an integer array or record of integer variable. When checking the port array for matching messages, the port indices to be checked are iterated from lowest to highest. If the port array is multi-dimensional, then the ports are iterated over from innermost to outermost array dimension from lowest to highest index for each dimension, e.g. [0][0], [0][1], [1][0], [1][1]. The first port which matches all the criteria will cause the operation to be successful even if other ports in the array would also meet the criteria.

If any port in the port array which is checked for matching contains a message that does not match, this message is removed and the containing **alt** statement is re-evalutated, regardless of whether or not other ports in the port array would meet the trigger criteria.

**Stand-alone trigger**

The **trigger** operation can be used as a stand-alone statement in a behaviour description. In this latter case the **trigger** operation is considered to be shorthand for an **alt** statement with two alternatives (one alternative expecting the message and another alternative consuming all other messages and repeating the alt statement, see ES 201 873‑4 [1]).

**Storing the received message, parts of the received message or the sender**

Rules in clause 22.2.2 shall apply.

***Restrictions***

In addition to the general static rules of TTCN‑3 given in clause 5 and shown in table 15, the following restrictions apply:

a) The **trigger** operation shall only be used on message-based ports and the type of the value to be received shall be included in the list of incoming types of the port type definition.

b) A message received by *TriggerOnAnyMessage* shall not be assigned to a variable.

c) Type mismatch at storing the received value or parts of the received value and storing the sender shall cause an error.

d) *AddressRef* for retrieving the sending entity shall be of type **address**, **component** or of the type provided in the address declaration of the port type of the port instance referenced in the **trigger** operation. No *AddressRef* shall contain the special value **null** at the time of the operation.

e) The *PortArrayRef* shall be a reference to a completely initialized port array .

f) The index redirection shall only be used when the operation is used on an any from port array construct.

g) If the index redirection is used for single-dimensional port arrays, the type of the integer variable shall allow storing the highest index of the respective array.

h) If the index redirection is used for multi-dimensional port arrays, the size of the integer array or record of integer type shall exactly be the same as the dimension of the respective array, and its type shall allow storing the highest index (from all dimensions) of the array.

i) If a variable referenced in the **value**, **sender** or **@index** clause is a lazy or fuzzy variable, the expression assigned to this variable is equal to the result produced by the **trigger** operation, i.e. later evaluation of the lazy or fuzzy variable does not lead to repeated invocation of the **trigger** operation.

j) If the **trigger** operation contains both **from** and **sender** clause, the variable or parameter referenced in the **sender** clause shall be type compatible with the template in the **from** clause.

***Examples***

EXAMPLE 1: Basic trigger

MyPort.**trigger**(MyType:?);

// Specifies that the operation will trigger on the reception of the first message observed of

// the type MyType with an arbitrary value at port MyPort.

EXAMPLE 2: Trigger from a sender and with storing message or sender

MyPort.**trigger**(MyType:?) **from** MyPartner;

// Triggers on the reception of the first message of type MyType at port MyPort

// received from MyPartner.

MyPort.**trigger**(MyType:?) **from** MyPartner -> **value** MyRecMessage;

// This example is almost identical to the previous example. In addition, the message which

// triggers i.e. all matching criteria are met, is stored in the variable MyRecMessage.

MyPort.**trigger**(MyType:?) -> **sender** MyPartner;

// This example is almost identical to the first example. In addition, the reference of the

// sender component will be retrieved and stored in variable MyPartner.

MyPort.**trigger**(integer:?) -> **value** MyVar **sender** MyPartner;

// Trigger on the reception of an arbitrary integer value which afterwards is stored in

// variable MyVar. The reference of the sender component will be stored in variable MyPartner.

EXAMPLE 3: Trigger on any message

MyPort.**trigger**;

MyPort.**trigger** **from** MyPartner;

MyPort.**trigger** -> **sender** MySenderVar;

EXAMPLE 4: Trigger on any port

**any port**.**trigger**

EXAMPLE 5: Trigger on any port from port array

**type** **port** MyPort **message** { **inout** **integer** }

**type** **component** MyComponent {

**port** MyPort p[10][10];

}

**var** **integer** i[2];

**any** **from** p.**trigger**(MyMessage) -> @**index** **value** i;

// Checking if MyMessage has been received on any port of the port array p; if yes, the index

// of the port on which the matching was first successful is stored in the array i; if no port

// succeeds, the top messages are removed and the port array is re-checked.

## 22.3 Procedure-based communication

The operations for procedure-based communication via synchronous ports are summarized in table 23.

Table 23: Overview of procedure-based communication

|  |  |
| --- | --- |
| Communication operation | Keyword |
| Invoke procedure call | **call** |
| Accept procedure call from remote entity | **getcall** |
| Reply to procedure call from remote entity | **reply** |
| Raise exception (to an accepted call) | **raise** |
| Handle response from a previous call | **getreply** |
| Catch exception (from called entity) | **catch** |
| Check call/exception/reply received | **check** |

### 22.3.1 The Call operation

The **call** operation specifies the call of a remote operation on another test component or within the SUT.

***Syntactical Structure***

*Port* "." **call** "(" *TemplateInstance* [ "," *CallTimerValue* ]")"

[ **to** *Address* ]

NOTE 1: *Address* may be an *AddressRef*, a list of *AddressRef*-s or "**all component**".

***Semantic Description***

The **call** operation is used to specify that a test component calls a procedure in the SUT or in another test component.

The information to be transmitted in the send part of the **call** operation is a signature that may either be defined in the form of a signature template or be defined in-line.

**Handling responses and exceptions to a call**

In case of non-blocking procedure-based communication the handling of exceptions to **call** operations is done by using **catch** (see clause 22.3.6) operations as alternatives in **alt** statements.

If the **nowait** option is used, the handling of responses or exceptions to **call** operations is done by using **getreply** (see clause 22.3.4) and **catch** (see clause 22.3.6) operations as alternatives in **alt** statements.

In case of blocking procedure-based communication, the handling of responses or exceptions to a call is done in the response and exception handling part of the **call** operation by means of **getreply** (see clause 22.3.4) and **catch** (see clause 22.3.6) operations.

The response and exception handling part of a **call** operation looks similar to the body of an **alt** statement. It defines a set of alternatives, describing the possible responses and exceptions to the call.

If necessary, it is possible to enable/disable an alternative by means of a **boolean** expression placed between the "[ ]" brackets of the alternative.

The response and exception handling part of a call operation is executed like an **alt** statement without any active default. This means a corresponding snapshot includes all information necessary to evaluate the (optional) Boolean guards, may include the top element (if any) of the port over which the procedure has been called and may include a timeout exception generated by the (optional) timer that supervises the call.

**Handling timeout exceptions to a call**

The **call** operation may optionally include a timeout. This is defined as an explicit value or constant of **float** type and defines the length of time after the **call** operation has started that a **timeout** exception shall be generated by the test system. If no timeout value part is present in the **call** operation, no **timeout** exception shall be generated.

**Nowait calls of blocking procedures**

Using the keyword **nowait** instead of a timeout exception value in a **call** operation allows calling a procedure to continue without waiting either for a response or an exception raised by the called procedure or a timeout exception.

If the **nowait** keyword is used, a possible response or exception of the called procedure has to be removed from the port queue by using a **getreply** or a **catch** operation in a subsequent **alt** statement.

**Calling blocking procedures without return value, out parameters, inout parameters and exceptions**

A blocking procedure may have no return values, no out and inout parameters and may raise no exception. The call operation for such a procedure shall also have a response and exception handling part to handle the blocking in a uniform manner.

**Calling non-blocking procedures**

A non-blocking procedure has no out and inout parameters, no return value and the non-blocking property is indicated in the corresponding signature definition by means of a **noblock** keyword.

Possible exceptions raised by non-blocking procedures have to be removed from the port queue by using **catch** operations in subsequent **alt** or **interleave** statements.

**Unicast, multicast and broadcast calls of procedures**

Like for the **send** operation, TTCN‑3 also supports unicast, multicast and broadcast calls of procedures. This can be done in the same manner as described in clause 22.2.1, i.e. the argument of the **to** clause of a **call** operation is for unicast calls the address of one receiving entity (or can be omitted in case of one-to-one connections), for multicast calls a list of addresses of a set of receivers and for broadcast calls the **all component** keyword. In case of one-to-one connections, the **to** clause may be omitted, because the receiving entity is uniquely identified by the system structure.

The handling of responses and exceptions for a blocking or non-blocking unicast **call** operation has been explained in this clause under "Handling timeout exceptions to a call". A multicast or broadcast **call** operation may cause several responses and exceptions from different communication partners.

In case of a multicast or broadcast **call** operation of a non-blocking procedure, all exceptions which may be raised from the different communication partners can be handled in subsequent **catch**, **alt** or **interleave** statements.

In case of a multicast or broadcast **call** operation of a blocking procedure, two options exist. Either, only one response or exception is handled in the response and exception handling part of the **call** operation. Then, further responses and exceptions can be handled in subsequent **alt** or **interleave** statements. Or, several responses or exceptions are handled by the use of repeat statements in one or more of the statement blocks of the response and exception handling part of the call operation: the execution of a repeat statement causes the re-evaluation of the call body.

NOTE 2: In the second case, the user needs to handle the number of repetitions.

***Restrictions***

In addition to the general static rules of TTCN‑3 given in clause 5 and shown in table 15, the following restrictions apply:

a) The **call** operation shall only be used on procedure-based ports. The type definition of the port at which the call operation takes place shall include the procedure name in its **out** or **inout** list i.e. it shall be allowed to call this procedure at this port.

b) All **in** and **inout** parameters of the signature shall have a specific value i.e. the use of matching mechanisms such as *AnyValue* is not allowed.

c) Only out parameters may be omitted or specified with a matching attribute.

d) The signature arguments of the **call** operation are not used to retrieve variable names for **out** and **inout** parameters. The actual assignment of the procedure return value and **out** and **inout** parameter values to variables shall explicitly be made in the response and exception handling part of the **call** operation by means of **getreply** and **catch** operations. This allows the use of signature templates in **call** operations in the same manner as templates can be used for types.

e) A **to** clause shall be present in case of one-to-many connections.

f) *AddressRef* shall be of type **address**, **component** or of the type provided in the address declaration of the port type of the port instance referenced in the **call** operation. No *AddressRef* shall contain the special value **null** at the time of the operation.

g) *CallTimerValue* shall be of type float.

h) The selection of the alternatives to a call shall only be based on **getreply** and **catch** operations for the called procedure. Unqualified **getreply** and **catch** operations shall only treat replies from and exceptions raised by the called procedure. The use of **else** branches and the invocation of altsteps is not allowed.

i) The evaluation of the Boolean expressions guarding the alternatives in the response and exception handling part may have side effects. In order to avoid unexpected side effects, the same rules as for the Boolean guards in **alt** statements shall be applied (see clause 20.2).

j) The call operation for a blocking procedures without return value, out parameters, inout parameters and exceptions shall also have a response and exception handling part to handle the blocking in a uniform manner.

k) In case of a multicast or broadcast **call** operation of a blocking procedure, where the **nowait** keyword is used, all responses and exceptions have to be handled in subsequent **alt** or **interleave** statements.

l) The **call** operation for a non-blocking procedure shall have no response and exception handling part, shall raise no timeout exception and shall not use the **nowait** keyword.

m) Applying a **call** operation to an unmapped or disconnected port shall cause a test case error.

***Examples***

EXAMPLE 1: Blocking call with getreply

// Given …

**signature** MyProc (**out** integer MyPar1, **inout** boolean MyPar2);

:

// a call of MyProc

MyPort.**call**(MyProc:{ -, MyVar2}) { // in-line signature template for the call of MyProc

[] MyPort.**getreply**(MyProc:{?, ?}) { }

}

// … and another call of MyProc

MyPort.**call**(MyProcTemplate) { // using signature template for the call of MyProc

[] MyPort.**getreply**(MyProc:{?, ?}) { }

}

MyPort.**call**(MyProcTemplate) **to** MyPeer { // calling MyProc at MyPeer

[] MyPort.**getreply**(MyProc:{?, ?}) { }

}

EXAMPLE 2: Blocking call with getreply and catch

// Given

**signature** MyProc3 (**out** **integer** MyPar1, **inout** **boolean** MyPar2) **return** MyResultType

**exception** (ExceptionTypeOne, ExceptionTypeTwo);

:

// Call of MyProc3

MyPort.**call**(MyProc3:{ -, **true** }) **to** MyPartner {

[] MyPort.**getreply**(MyProc3:{?, ?}) -> **value** MyResult **param** (MyPar1Var,MyPar2Var) { }

[] MyPort.**catch**(MyProc3, MyExceptionOne) {

**setverdict**(**fail**);

**stop**;

}

[] MyPort.**catch**(MyProc3, ExceptionTypeTwo : ?) {

**setverdict**(**inconc**);

}

[MyCondition] MyPort.**catch**(MyProc3, MyExceptionThree) { }

}

EXAMPLE 3: Blocking call with timeout exception

MyPort.call(MyProc:{5,MyVar}, 20E-3) {

[] MyPort.**getreply**(MyProc:{?, ?}) { }

[] MyPort.**catch**(**timeout**) { // timeout exception after 20ms

**setverdict**(**fail**);

**stop**;

}

}

EXAMPLE 4: Nowait call

MyPort.**call**(MyProc:{5, MyVar}, **nowait**); // The calling test component will continue

// its execution without waiting for the

// termination of MyProc

EXAMPLE 5: Blocking call without return value, out parameters, inout parameters and exceptions

// Given …

**signature** MyBlockingProc (**in** integer MyPar1, **in** boolean MyPar2);

:

// a call of MyBlockingProc

MyPort.**call**(MyBlockingProc:{ 7, **false** }) {

[] MyPort.**getreply**( MyBlockingProc:{ -, - } ) { }

}

EXAMPLE 6: Broadcast call

**var** **boolean** first:= **true**;

MyPort.**call**(MyProc:{5,MyVar}, 20E-3) **to all** **component** { // Broadcast call of MyProc

// Handles the response from MyPeerOne

[first] MyPort.**getreply**(MyProc:{?, ?}) **from** MyPeerOne {

**if** (first) { first := **false**; **repeat**; }

:

}

// Handles the response from MyPeerTwo

[first] MyPort.**getreply**(MyProc:{?, ?}) **from** MyPeerTwo {

**if** (first) { first := **false**; **repeat**; }

:

}

[] MyPort.**catch**(**timeout**) { // timeout exception after 20ms

**setverdict**(**fail**);

**stop**;

}

}

**alt** {

[] MyPort.**getreply**(MyProc:{?, ?}) { // Handles all other responses to the broadcast call

**repeat**

}

}

EXAMPLE 7: Multicast call

MyPort.**call**(MyProc:{5,MyVar}, nowait) **to** (MyPeer1, MyPeer2); // Multicast call of MyProc

**interleave** {

[] MyPort.**getreply**(MyProc:{?, ?}) **from** MyPeer1 { } // Handles the response of MyPeer1

[] MyPort.**getreply**(MyProc:{?, ?}) **from** MyPeer2 { } // Handles the response of MyPeer2

}

### 22.3.2 The Getcall operation

The **getcall** operation is used to accept calls.

***Syntactical Structure***

( *Port* | **any** **port** | **any from** PortArrayRef ) "." **getcall**

[ "(" *TemplateInstance* ")" ]

[ **from** *Address* ]

[ "->" [ **param** "(" { ( *VariableRef* ":=" [ @decoded [ "(" *Expression* ")" ] ] *ParameterIdentifier* ) "," } *|*

{ ( *VariableRef* | "-" ) "," }

")" ]

[ **sender** *VariableRef* ]

[ @**index** **value** *VariableRef* ] ]

NOTE: *Address* may be an *AddressRef*, a list of *AddressRef*-s or "**any component**".

***Semantic Description***

The **getcall** operation is used to specify that a test component accepts a call from the SUT, or another test component.

The **getcall** operation shall remove the top call from the incoming port queue, if, and only if, the matching criteria associated to the **getcall** operation are fulfilled. These matching criteria are related to the signature of the call to be processed and the communication partner. The matching criteria for the signature may either be specified in-line or be derived from a signature template.

The assignment of **in** and **inout** parameter values to variables shall be made in the assignment part of the **getcall** operation. This allows the use of signature templates in **getcall** operations in the same manner as templates are used for types.

A **getcall** operation may be restricted to a certain communication partner in case of one-to-many connections. This restriction shall be denoted by using the **from** keyword.

The (optional) assignment part of the **getcall** operation comprises the assignment of **in** and **inout** parameter values to variables and the retrieval of the address of the calling component. The keyword **param** is used to retrieve the parameter values of a call.

When assigning individual parameters of a call, encoded parameters can be decoded prior to assignment using the **@decoded** modifier. In this case, the referenced parameter on the right hand sided of the assignment shall be one of the **bitstring**, **hexstring**, **octetstring**, **charstring** or **universal** **charstring** types. It shall be decoded into a value of the same type as the variable on the left hand side of the assignment. Failure of this decoding shall cause a test case error. In case the referenced field is of the **universal** **charstring** type, the **@decoded** clause can contain an optional parameter defining the encoding format. The parameter shall be of the **charstring** type and it shall contain one of the strings allowed for the **decvalue\_unichar** function (specified in clause C.5.4). Any other value shall cause an error. In case the referenced field is not a **universal** **charstring**, the optional parameter shall not be present.

The keyword **sender** is used when it is required to retrieve the address of the sender (e.g. for addressing a **reply** or exception to the calling party in a one-to-many configuration).

**Accepting any call**

A **getcall** operation with no argument list for the signature matching criteria will remove the call on the top of the incoming port queue (if any) if all other matching criteria are fulfilled.

**Getcall on any port**

To **getcall** on any port is denoted by the **any** keyword.

**Getcall on any port from a port array**

To **getcall** on any port from a specific port array, use the **any from** *PortArrayRef*syntax where PortArrayRefshallbe areference to a port array identifier**.** It is also possible to store the index of a port in a single-dimensional port array at which the operation was successful to a variable of type integer or, in case of multi-dimensional port arrays the index of the successful port to an integer array or record of integer variable. When checking the port array for matching calls, the port indices to be checked are iterated from lowest to highest. If the port array is multi-dimensional, then the ports are iterated over from innermost to outermost array dimension from lowest to highest index for each dimension, e.g. [0][0], [0][1], [1][0], [1][1]. The first port which matches all the criteria will cause the operation to be successful even if other ports in the array would also meet the criteria.

***Restrictions***

In addition to the general static rules of TTCN‑3 given in clause 5 and shown in table 15, the following restrictions apply:

a) The **getcall** operation shall only be used on procedure-based ports and the signature of the procedure call to be accepted shall be included in the list of allowed incoming procedures of the port type definition.

b) The signature argument of the **getcall** operation shall not be used to pass in variable names for **in** and **inout** parameters.

c) The *ParameterIdentifier*s shall be from the corresponding signature definition.

d) The value assignment part shall not be used with the getcall operation.

e) Parameters of calls accepted by *accepting any call* shall not be assigned to a variable, i.e. the **param** clause shall not be present.

f) *AddressRef* for retrieving the sending entity shall be of type **address**, **component** or of the type provided in the address declaration of the port type of the port instance referenced in the **getcall** operation. No *AddressRef* shall contain the special value **null** at the time of the operation.

g) The *PortArrayRef* shall be a reference to a completely initialized port array.

h) The index redirection shall only be used when the operation is used on an any from port array construct.

i) If the index redirection is used for single-dimensional port arrays, the type of the integer variable shall allow storing the highest index of the respective array.

j) If the index redirection is used for multi-dimensional port arrays, the size of the integer array or record of integer type shall exactly be the same as the dimension of the respective array, and its type shall allow storing the highest index (from all dimensions) of the array.

k) If a variable referenced in the **param**, **sender** or **@index** clause is a lazy or fuzzy variable, the expression assigned to this variable is equal to the result produced by the **getcall** operation, i.e. later evaluation of the lazy or fuzzy variable does not lead to repeated invocation of the **getcall** operation.

l) If the **getcall** operation contains both **from** and **sender** clause, the variable or parameter referenced in the **sender** clause shall be type compatible with the template in the **from** clause.

m) When assigning implicitly decoded parameters (by using the **@decoded** modifier) in cases where the value or template to be matched uses the *MatchDecodedContent* (**decmatch**) matching for the parameter to be stored, the type of the template in the *MatchDecodedContent* matching shall be type-compatible to the type of the variable the decoded field is stored into.

***Examples***

EXAMPLE 1: Basic getcall

MyPort.**getcall**(MyProc: MyProcTemplate(5, MyVar)); // accepts a call of MyProc at MyPort

MyPort.**getcall**(MyProc:{5, MyVar}) **from** MyPeer; // accepts a call of MyProc at MyPort from MyPeer

EXAMPLE 2: Getcall with matching and assignments of parameter values to variables

MyPort.**getcall**(MyProc:{?, ?}) **from** MyPartner -> **param** (MyPar1Var, MyPar2Var);

// The in or inout parameter values of MyProc are assigned to MyPar1Var and MyPar2Var.

MyPort.**getcall**(MyProc:{5, MyVar}) -> **sender** MySenderVar;

// Accepts a call of MyProc at MyPort with the in or inout parameters 5 and MyVar.

// The address of the calling party is retrieved and stored in MySenderVar.

// The following getcall examples show the possibilities to use matching attributes

// and omit optional parts, which may be of no importance for the test specification.

MyPort.**getcall**(MyProc:{5, MyVar}) -> **param**(MyVar1, MyVar2) **sender** MySenderVar;

MyPort.**getcall**(MyProc:{5, ?}) -> **param**(MyVar1, MyVar2);

MyPort.**getcall**(MyProc:{?, MyVar}) -> **param**( - , MyVar2);

// The value of the first inout parameter is not important or not used

// The following examples shall explain the possibilities to assign in and inout parameter

// values to variables. The following signature is assumed for the procedure to be called:

**signature** MyProc2(**in** **integer** A, **integer** B, **integer** C, **out** **integer** D, **inout** **integer** E);

MyPort.**getcall**(MyProc2:{?, ?, 3, - , ?}) -> **param** (MyVarA, MyVarB, - , -, MyVarE);

// The parameters A, B, and E are assigned to the variables MyVarA, MyVarB, and

// MyVarE. The out parameter D needs not to be considered.

MyPort.**getcall**(MyProc2:{?, ?, 3, -, ?}) -> **param** (MyVarA:= A, MyVarB:= B, MyVarE:= E);

// Alternative notation for the value assignment of in and inout parameter to variables. Note,

// the names in the assignment list refer to the names used in the signature of MyProc2

MyPort.**getcall**(MyProc2:{1, 2, 3, -, \*}) -> **param** (MyVarE:= E);

// Only the inout parameter value is needed for the further test case execution

// The following example demonstrates the use of encoded parameters:

**signature** MyProc3(**in** **integer** paramType, **octetstring** encodedParam);

**template integer** m\_int := ?;

…

**var integer** v\_myVarX;

MyPort.**getcall**(MyProc3:{1, **decmatch** m\_int}) -> **param** (v\_myVarX := **@decoded** encodedParam);

// The parameters encodedParam is decoded into an integer and assigned to v\_myVarX.

EXAMPLE 3: Accepting any call

MyPort.**getcall**; // Removes the top call from MyPort.

MyPort.**getcall** **from** MyPartner; // Removes a call from MyPartner from port MyPort

MyPort.**getcall** -> **sender** MySenderVar; // Removes a call from MyPort and retrieves

// the address of the calling entity

EXAMPLE 4: Getcall on any port

**any** **port**.**getcall**(MyProc:?)

EXAMPLE 5: Getcall on any port from port array

**type** **port** MyPort **procedure** { **inout** MyProc }

**type** **component** MyComponent {

**port** **MyPort** p[10][10];

}

**var** **integer** i[2];

**any** **from** p.**getcall**(MyProc:?) -> @**index** **value** i;

// checking for an incoming call of the type MyProc on any port of the port array p and storing

// the index of the port on which the matching was successful first

### 22.3.3 The Reply operation

The **reply** operation is used to reply to a call.

***Syntactical Structure***

*Port* "." **reply** "(" *TemplateInstance* [ **value** *Expression* ] ")"

[ **to** *Address* ]

NOTE 1: *Address* may be an *AddressRef*, a list of *AddressRef*-s or "**all component**".

***Semantic Description***

The **reply** operation is used to reply to a previously accepted call according to the procedure signature.

NOTE 2: The relation between an accepted call and a **reply** operation cannot always be checked statically. For testing it is allowed to specify a **reply** operation without an associated **getcall** operation.

The value part of the **reply** operation consists of a signature reference with an associated actual parameter list and (optional) return value. The signature may either be defined in the form of a signature template or it may be defined in‑line.

Responses to one or more **call** operations may be sent to one, several or all peer entities connected to the addressed port. This can be specified in the same manner as described in clause 22.2.1. This means, the argument of the **to** clause of a **reply** operation is for unicast responses the address of one receiving entity, for multicast responses a list of addresses of a set of receivers and for broadcast responses the **all component** keywords.

In case of one-to-one connections, the **to** clause may be omitted, because the receiving entity is uniquely identified by the system structure.

A return value shall be explicitly stated with the **value** keyword.

***Restrictions***

In addition to the general static rules of TTCN‑3 given in clause 5 and shown in table 15, the following restrictions apply:

a) A **reply** operation shall only be used at a procedure-based port. The type definition of the port shall include the name of the procedure to which the **reply** operation belongs.

b) All **out** and **inout** parameters of the signature shall have a specific value i.e. the use of matching mechanisms such as *AnyValue* is not allowed.

c) A **to** clause shall be present in case of one-to-many connections.

d) *AddressRef* shall be of type **address**, **component** or of the type provided in the address declaration of the port type of the port instance referenced in the **reply** operation. No *AddressRef* shall contain the special value **null** at the time of the operation.

e) If a value is to be returned to the calling party, this shall be explicitly stated using the **value** keyword.

f) Applying a **reply** operation to an unmapped or disconnected port shall cause a test case error.

***Examples***

MyPort.**reply**(MyProc2:{ - ,5}); // Replies to an accepted call of MyProc2.

MyPort.**reply**(MyProc2:{ - ,5}) **to** MyPeer; // Replies to an accepted call of MyProc2 from MyPeer

MyPort.**reply**(MyProc2:{ - ,5}) **to** (MyPeer1, MyPeer2); // Multicast reply to MyPeer1 and MyPeer2

MyPort.**reply**(MyProc2:{ - ,5}) **to** **all component**; // Broadcast reply to all entities connected

// to MyPort

MyPort.**reply**(MyProc3:{5,MyVar} **value** 20); // Replies to an accepted call of MyProc3.

### 22.3.4 The Getreply operation

The **getreply** operation is used to handle replies from a previously called procedure.

***Syntactical Structure***

( *Port* | **any** **port** | **any from** PortArrayRef ) "." **getreply**

[ "(" *TemplateInstance* [ **value** *TemplateInstance* ]")" ]

[ **from** *Address* ]

[ "->" [ **value** (*VariableRef* |

( "(" { *VariableRef* [ ":=" [ @decoded [ "(" *Expression* ")" ] ]  
 *FieldOrTypeReference* ][","] } ")" )

)]

[ **param** "(" { ( *VariableRef* ":=" [ @decoded [ "(" *Expression* ")" ] ]  
 *ParameterIdentifier* ) "," } *|*

{ ( *VariableRef* | "-" ) "," }

")" ]

[ **sender** *VariableRef* ]

[ @**index** **value** *VariableRef* ] ]

NOTE: *Address* may be an *AddressRef*, a list of *AddressRef*-s or "**any component**".

***Semantic Description***

The **getreply** operation is used to handle replies from a previously called procedure.

The **getreply** operation shall remove the top reply from the incoming port queue, if, and only if, the matching criteria associated to the **getreply** operation are fulfilled. These matching criteria are related to the signature of the procedure to be processed and the communication partner. The matching criteria for the signature may either be specified in-line or be derived from a signature template.

Matching against a received return value can be specified by using the **value** keyword.

A **getreply** operation may be restricted to a certain communication partner in case of one-to-many connections. This restriction shall be denoted by using the **from** keyword.

The assignment of **out** and **inout** parameter values to variables shall be made in the assignment part of the **getreply** operation. This allows the use of signature templates in **getreply** operations in the same manner as templates are used for types.

The (optional) assignment part of the **getreply** operation comprises the assignment of **out** and **inout** parameter values to variables and the retrieval of the address of the sender of the reply. The keyword **value** is used to retrieve return values and the keyword **param** is used to retrieve the parameter values of a reply. The keyword **sender** is used when it is required to retrieve the address of the sender.

When assigning individual parameters of a reply, encoded parameters can be decoded prior to assignment using the **@decoded** modifier. In this case, the referenced parameter on the right hand sided of the assignment shall be one of the **bitstring**, **hexstring**, **octetstring**, **charstring** or **universal** **charstring** types. It shall be decoded into a value of the same type as the variable on the left hand side of the assignment. Failure of this decoding shall cause a test case error. In case the referenced field is of the **universal** **charstring** type, the **@decoded** clause can contain an optional parameter defining the encoding format. The parameter shall be of the **charstring** type and it shall contain one of the strings allowed for the **decvalue\_unichar** function (specified in clause C.5.4). Any other value shall cause an error. In case the referenced field is not a **universal** **char string**, the optional parameter shall not be present.

**Get any reply**

A **getreply** operation with no argument list for the signature matching criteria shall remove the reply message on the top of the incoming port queue (if any) if all other matching criteria are fulfilled.

If *GetAnyReply* is used in the response and exception handling part of a **call** operation, it shall only treat replies from the procedure invoked by the **call** operation.

**Get a reply on any port**

To get a reply on any port, use the **any port** keywords.

**Get a reply on any port from a port array**

To get a reply on any port from a specific port array, use the **any from** *PortArrayRef*syntax where PortArrayRefshallbe areference to a port array identifier**.** It is also possible to store the index of a port in a single‑dimensional port array at which the operation was successful to a variable of type integer or, in case of multi‑dimensional port arrays the index of the successful port to an integer array or record of integer variable. When checking the port array for matching replies, the port indices to be checked are iterated from lowest to highest. If the port array is multi-dimensional, then the ports are iterated over from innermost to outermost array dimension from lowest to highest index for each dimension, e.g. [0][0], [0][1], [1][0], [1][1]. The first port which matches all the criteria will cause the operation to be successful even if other ports in the array would also meet the criteria.

***Restrictions***

In addition to the general static rules of TTCN‑3 given in clause 5 and shown in table 15, the following restrictions apply:

a) A **getreply** operation shall only be used at a procedure-based port. The type definition of the port shall include the name of the procedure to which the **getreply** operation belongs.

b) The signature argument of the **getreply** operation shall not be used to pass in variable names for **out** and **inout** parameters.

c) Parameters or return values of responses accepted by *get any reply* shall not be assigned to a variable, i.e. the **param** and **value** clause shall not be present.

d) *AddressRef* for retrieving the sending entity shall be of type **address**, **component** or of the type provided in the address declaration of the port type of the port instance referenced in the **getreply** operation. No *AddressRef* shall contain the special value **null** at the time of the operation.

e) The *PortArrayRef* shall be a reference to a completely initialized port array .

f) The index redirection shall only be used when the operation is used on an any from port array construct.

g) If the index redirection is used for single-dimensional arrays, the type of the integer variable shall allow storing the highest index of the respective port array.

h) If the index redirection is used for multi-dimensional arrays, the size of the integer array or record of integer type shall exactly be the same as the dimension of the respective port array, and the its type shall allow storing the highest index (from all dimensions) of the port array.

i) If a variable referenced in the **value**, **param**, **sender** or **@index** clause is a lazy or fuzzy variable, the expression assigned to this variable is equal to the result produced by the **getreply** operation, i.e. later evaluation of the lazy or fuzzy variable does not lead to repeated invocation of the **getreply** operation.

j) If the **getreply** operation contains both **from** and **sender** clause, the variable or parameter referenced in the **sender** clause shall be type compatible with the template in the **from** clause.

k) When assigning implicitly decoded parameters (by using the **@decoded** modifier) in cases where the value or template to be matched uses the *MatchDecodedContent* (**decmatch**) matching for the parameter to be stored, the type of the template in the *MatchDecodedContent* matching shall be type-compatible to the type of the variable the decoded field is stored into.

***Examples***

EXAMPLE 1: Basic getreply

MyPort.**getreply**(MyProc:{5, ?} **value** 20); // Accepts a reply of MyProc with two out or

// inout parameters and a return value of 20

MyPort.**getreply**(MyProc2:{ - ,5}) **from** MyPeer; // Accepts a reply of MyProc2 from MyPeer

EXAMPLE 2: Getreply with storing inout/out parameters and return values in variables

MyPort.**getreply**(MyProc1:{?, ?} **value** ?) -> **value** MyRetValue **param**(MyPar1,MyPar2);

// The returned value is assigned to variable MyRetValue and the value

// of the two out or inout parameters are assigned to the variables MyPar1 and MyPar2.

MyPort.**getreply**(MyProc1:{?, ?} **value** ?) -> **value** MyRetValue **param**( - , MyPar2) **sender** MySender;

// The value of the first parameter is not considered for the further test execution and

// the address of the sender component is retrieved and stored in the variable MySender.

// The following examples describe some possibilities to assign out and inout parameter values

// to variables. The following signature is assumed for the procedure which has been called

**signature** MyProc2(**in** **integer** A, **integer** B, **integer** C, **out** **integer** D, **inout** **integer** E);

MyPort.**getreply**(ATemplate) -> **param**( - , - , - , MyVarOut1, MyVarInout1);

MyPort.**getreply**(ATemplate) -> **param**(MyVarOut1:=D, MyVarOut2:=E);

MyPort.**getreply**(MyProc2:{ - , - , - , 3, ?}) -> **param**(MyVarInout1:=E);

// The following example demonstrates the use of encoded parameters:

**signature** MyProc3(**out** **integer** paramType, **out** **octetstring** encodedParam);

**template integer** m\_int := ?;

…

**var integer** v\_myVarX;

MyPort.**getreply**(MyProc3:{1, **decmatch** m\_int}) -> **param** (v\_myVarX := **@decoded** encodedParam);

// The parameters encodedParam is decoded into an integer and assigned to v\_myVarX.

EXAMPLE 3: Get any reply

MyPort.**getreply**; // Removes the top reply from MyPort.

MyPort.**getreply** **from** MyPeer; // Removes the top reply received from MyPeer from MyPort.

MyPort.**getreply** -> **sender** MySenderVar; // Removes the top reply from MyPort and retrieves the

// address of the sender entity

EXAMPLE 4: Get a reply on any port

**any** **port**.**getreply**(Myproc:?)

EXAMPLE 5: Get a reply on any port from port array

**type** **port** MyPort **procedure** { **inout** MyProc }

**type** **component** MyComponent {

**port** MyPort p[10][10];

}

**var** **integer** i[2];

**any** **from** p.**getreply**(MyProc:?) -> @**index** **value** i;

// Getting a reply of the type MyProc on any port of the port array p and

// storing the index of the port on which the matching was successful first

### 22.3.5 The Raise operation

Exceptions are raised with the **raise** operation.

***Syntactical Structure***

*Port* "." **raise** "(" *Signature* "," *TemplateInstance* ")"

[ **to** *Address* ]

NOTE 1: *Address* may be an *AddressRef*, a list of *AddressRef*-s or "**all component**".

***Semantic Description***

The **raise** operation is used to raise an exception.

NOTE 2: The relation between an accepted call and a **raise** operation cannot always be checked statically. For testing it is allowed to specify a **raise** operation without an associated **getcall** operation.

The value part of the **raise** operation consists of the signature reference followed by the exception value.

Exceptions are specified as types. Therefore the exception value may either be derived from a template or be the value resulting from an expression (which of course can be an explicit value). The optional type field in the value specification to the **raise** operation shall be used in cases where it is necessary to avoid any ambiguity of the type of the value being sent.

Exceptions to one or more **call** operations may be sent to one, several or all peer entities connected to the addressed port. This can be specified in the same manner as described in clause 22.2.1. This means, the argument of the **to** clause of a **raise** operation is for unicast exceptions the address of one receiving entity, for multicast exceptions a list of addresses of a set of receivers and for broadcast exceptions the **all component** keywords.

In case of one-to-one connections, the **to** clause may be omitted, because the receiving entity is uniquely identified by the system structure.

***Restrictions***

In addition to the general static rules of TTCN‑3 given in clause 5 and shown in table 15, the following restrictions apply:

a) An exception shall only be raised at a procedure-based port. An exception is a reaction to an accepted procedure call the result of which leads to an exceptional event.

b) The type of the exception shall be specified in the signature of the called procedure. The type definition of the port shall include in its list of accepted procedure calls the name of the procedure to which the exception belongs.

c) A **to** clause shall be present in case of one-to-many connections.

d) *AddressRef* shall be of type **address**, **component** or of the type provided in the address declaration of the port type of the port instance referenced in the **raise** operation. No *AddressRef* shall contain the special value **null** at the time of the operation.

e) Applying a **raise** operation to an unmapped or disconnected port shall cause a test case error.

***Examples***

MyPort.**raise**(MySignature, MyVariable + YourVariable - 2);

// Raises an exception with a value which is the result of the arithmetic expression

// at MyPort

MyPort.**raise**(MyProc, **integer**:5}); // Raises an exception with the integer value 5 for MyProc

MyPort**.raise**(MySignature, "My string") **to** MyPartner;

// Raises an exception with the value "My string" at MyPort for MySignature and

// send it to MyPartner

MyPort**.raise**(MySignature, "My string") **to** (MyPartnerOne, MyPartnerTwo);

// Raises an exception with the value "My string" at MyPort and sends it to MyPartnerOne and

// MyPartnerTwo (i.e. multicast communication)

MyPort**.raise**(MySignature, "My string") **to** **all component**;

// Raises an exception with the value "My string" at MyPort for MySignature and sends it

// to all entites connected to MyPort (i.e. broadcast communication)

### 22.3.6 The Catch operation

The **catch** operation is used to catch exceptions.

***Syntactical Structure***

( *Port* | **any** **port** | **any from** PortArrayRef ) "." **catch**

[ "(" ( *Signature* "," *TemplateInstance* ) | *TimeoutKeyword* ")" ]

[ **from** *Address* ]

[ "->" [ **value** ( *VariableRef* |

( "(" { *VariableRef* [ ":=" [ @decoded [ "(" *Expression* ")" ] ] *FieldOrTypeReference* ][","] } ")" )

) ]

[ **sender** *VariableRef* ]

[ @**index** **value** *VariableRef* ] ]

NOTE: *Address* may be an *AddressRef*, a list of *AddressRef*-s or "**any component**".

***Semantic Description***

The **catch** operation is used to catch exceptions raised by a test component or the SUT as a reaction to a procedure call. Exceptions are specified as types and thus, can be treated like messages, e.g. templates can be used to distinguish between different values of the same exception type.

The **catch** operation removes the top exception from the associated incoming port queue if, and only if, that top exception satisfies all the matching criteria associated with the **catch** operation.

A **catch** operation may be restricted to a certain communication partner in case of one-to-many connections. This restriction shall be denoted by using the **from** keyword.

The (optional) redirection part of the **catch** operation comprises of storing the exception value and/or one or more parts of it and the retrieval of the address of the calling component. The keyword **value** is used to retrieve the value of an exception and/or the parts of it and the keyword **sender** is used when it is required to retrieve the address of the sender.

When assigning individual fields of an exception, encoded payload fields can be decoded prior to assignment using the **@decoded** modifier. In this case, the referenced field on the right hand sided of the assignment shall be one of the **bitstring**, **hexstring**, **octetstring**, **charstring** or **universal** **charstring** types. It shall be decoded into a value of the same type as the variable on the left hand side of the assignment. Failure of this decoding shall cause a test case error. In case the referenced field is of the **universal** **charstring** type, the **@decoded** clause can contain an optional parameter defining the encoding format. The parameter shall be of the **charstring** type and it shall contain one of the strings allowed for the **decvalue\_unichar** function (specified in clause C.5.4). Any other value shall cause an error. In case the referenced field is not a **universal** **charstring**, the optional parameter shall not be present.

The **catch** operation may be part of the response and exception handling part of a **call** operation or be used to determine an alternative in an **alt** statement. If the **catch** operation is used in the accepting part of a **call** operation, the information about port name and signature reference to indicate the procedure that raised the exception is redundant, because this information follows from the **call** operation. However, for readability reasons (e.g. in case of complex **call** statements) this information shall be repeated.

**The Timeout exception**

There is one special **timeout** exception that can be caught by the **catch** operation. The **timeout** exception is an emergency exit for cases where a called procedure neither replies nor raises an exception within a predetermined time (see clause 22.3.1).

**Catch any exception**

A **catch** operation with no argument list allows any valid exception to be caught. The most general case is without using the **from** keyword. *CatchAnyException* will also catch the **timeout** exception.

**Catch on any port**

To **catch** an exception on any port use the **any** keyword.

**Catch on any port from a port array**

To **catch** an exception on any port from a specific port array, indices use the **any from** *PortArrayRef*syntax where PortArrayRefshallbe areference to a port array identifier**.** It is also possible to store the index of a port in a single-dimensional port array at which the operation was successful to a variable of type integer or, in case of multi‑dimensional port arrays the index of the successful port to an integer array or record of integer variable. When checking the port array for matching exceptions, the port indices to be checked are iterated from lowest to highest. If the port array is multi-dimensional, then the ports are iterated over from innermost to outermost array dimension from lowest to highest index for each dimension, e.g. [0][0], [0][1], [1][0], [1][1]. The first port which matches all the criteria will cause the operation to be successful even if other ports in the array would also meet the criteria.

The catch on any port from a port array operation can not be used to catch a call timeout.

***Restrictions***

In addition to the general static rules of TTCN‑3 given in clause 5 and shown in table 15, the following restrictions apply:

1. The **catch** operation shall only be used at procedure-based ports. The type of the caught exception shall be specified in the signature of the procedure that raised the exception.
2. No binding of the incoming values to the terms of the expression or to the template shall occur. The assignment of the exception values to variables shall be made in the assignment part of the **catch** operation.
3. Catching **timeout** exceptions shall be restricted to the exception handling part of a call. No further matching criteria (including a **from** part) and no assignment part is allowed for a **catch** operation that handles a **timeout** exception.
4. Exception values accepted by *catch any exception* shall not be assigned to a variable, i.e. the **value** clause shall not be present.
5. If *CatchAnyException* is used in the response and exception handling part of a **call** operation, it shall only treat exceptions raised by the procedure invoked by the **call** operation.
6. *AddressRef* for retrieving the sending entity shall be of type **address**, **component** or of the type provided in the address declaration of the port type of the port instance referenced in the **catch** operation. No *AddressRef* shall contain the special value **null** at the time of the operation.
7. The *PortArrayRef* shall be a reference to a completely initialized port array.
8. The index redirection shall only be used when the operation is used on an any from port array construct.
9. If the index redirection is used for single-dimensional arrays, the type of the integer variable shall allow storing the highest index of the respective port array.
10. If the index redirection is used for multi-dimensional arrays, the size of the integer array or record of integer type shall exactly be the same as the dimension of the respective port array, and the its type shall allow storing the highest index (from all dimensions) of the port array.
11. If a variable referenced in the **value**, **sender** or **@index** clause is a lazy or fuzzy variable, the expression assigned to this variable is equal to the result produced by the **catch** operation, i.e. later evaluation of the lazy or fuzzy variable does not lead to repeated invocation of the **catch** operation.
12. If the **catch** operation contains both **from** and **sender** clause, the variable or parameter referenced in the **sender** clause shall be type compatible with the template in the **from** clause.
13. When assigning implicitly decoded exception fields (by using the **@decoded** modifier) in cases where the value or template to be matched uses the *MatchDecodedContent* (**decmatch**) matching for the parameter to be stored, the type of the template in the *MatchDecodedContent* matching shall be type-compatible to the type of the variable the decoded field is stored into.

***Examples***

EXAMPLE 1: Basic catch

MyPort.**catch**(MyProc, **integer:** MyVar); // Catches an integer exception of value

// MyVar raised by MyProc at port MyPort.

MyPort.**catch**(MyProc, MyVar); // Is an alternative to the previous example.

MyPort.**catch**(MyProc, A<B); // Catches a boolean exception

MyPort.**catch**(MyProc, MyType:{5, MyVar}); // In-line template definition of an exception value.

MyPort.**catch**(MyProc, **charstring**:"Hello")**from** MyPeer; // Catches "Hello" exception from MyPeer

EXAMPLE 2: Catch with storing value and/or sender in variables

MyPort.**catch**(MyProc, MyType:?) **from** MyPartner -> **value** MyVar;

// Catches an exception from MyPartner and assigns its value to MyVar.

MyPort.**catch**(MyProc, MyTemplate(5)) -> **value** MyVarTwo **sender** MyPeer;

// Catches an exception, assigns its value to MyVarTwo and retrieves the

// address of the sender.

MyPort.**catch**(MyProc, MyTemplate(5)) -> **value** (MyVarThree:= f1)

**sender** MyPeer;

// Catches an exception, assigns the value of its field f1 to MyVarThree and retrieves the

// address of the sender.

// Handling encoded exception payload:

**type** MyException **record** {

**...**

}

**type** CommonException **record** {

**integer** exceptionId,

**octetstring** payload

}

**signature** S() **exception** (CommonException);

...

**var** MyException v\_myVar;

MyPort.**catch** (S, CommonException:{exceptionId := 25, payload := **decmatch** MyException:? }) -> **value** (v\_myVar := **@decoded** payload);

// The encoded payload field of the caught exception is decoded and matched with m\_excTemplate;

// if the matching is successful the decoded payload is stored in v\_myVar.

EXAMPLE 3: The Timeout exception

MyPort.**call**(MyProc:{5,MyVar}, 20E-3) {

[] MyPort.**getreply**(MyProc:{?, ?}) { }

[] MyPort.**catch**(**timeout**) { // timeout exception after 20ms

**setverdict**(**fail**);

**stop**;

}

}

EXAMPLE 4: Catch any exception

MyPort.**catch**;

MyPort.**catch** **from** MyPartner;

MyPort.**catch** -> **sender** MySenderVar;

EXAMPLE 5: Catch on any port

**any port**.**catch;**

EXAMPLE 6: Catch on any port from port array

**type** **port** MyPort **procedure** { **inout** MyProc }

**type** **component** MyComponent {

**port** MyPort p[10][10];

}

**var** **integer** i[2];

**any** **from** p.**catch**(MyProc, MyType:?) -> @**index** **value** i;

// Catching an incoming exception of type MyType on any port in the port array p and

// storing the index of the port on which the matching was successful first

## 22.4 The Check operation

The **check** operation allows reading the top element of a message‑based or procedure‑based *incoming* port queue.

***Syntactical Structure***

( *Port* | **any** **port** | **any from** PortArrayRef ) "." **check**

[ "("

( *PortReceiveOp | PortGetCallOp | PortGetReplyOp | PortCatchOp* ) |

( [ **from** *Address* ]

[ "->" [ **sender** *VariableRef* ]

[ **@index** **value** VariableRef ] ] )

")" ]

NOTE 1: *Address* may be an *AddressRef*, a list of *AddressRef*-s or "**any component**".

***Semantic Description***

The **check** operation is a generic operation that allows read access to the top element of message‑based and procedure‑based *incoming* port queues without removing the top element from the queue. The **check** operation has to handle values of a certain type at message-based ports and to distinguish between calls to be accepted, exceptions to be caught and replies from previous calls at procedure-based ports.

The receiving operations **receive**, **getcall**, **getreply** and **catch** together with their matching and value, sender or parameter storing parts, are used by the **check** operation to define the conditions that have to be checked and the information to be optionally extracted.

It is the *top* element of an incoming port queue that shall be checked (it is not possible to look *into* the queue). If the queue is empty the **check** operation fails. If the queue is not empty, a copy of the top element is taken and the receiving operation specified in the **check** operation is performed on the copy. The **check** operation fails if the receiving operation fails i.e. the matching criteria are not fulfilled. In this case the *copy* of the top element of the queue is discarded and test execution continues in the normal manner, i.e. the statement or alternative next to the check operation is evaluated. The **check** operation is successful if the receiving operation is successful. In this case, the value, sender or parameter storing parts of the receiving operation, if any, are executed, i.e. the message and/or a part of it, the sender's address or component reference, the parameter(s) of the call or reply or the value of the exception are stored in the associated variables.

If **check** is used as a stand-alone statement, it is considered to be a shorthand for an **alt** statement with the **check** operation as the only alternative.

**Check any operation**

A **check** operation with no argument list allows checking whether something waits for processing in an incoming port queue. The **check** any operation allows to distinguish between different senders (in case of one-to-many connections) by using a **from** clause and to retrieve the sender by using a shorthand assignment part with a **sender** clause.

**Check on any port**

To **check** on any port, use the **any port** keywords.

**Check on any port from a port array**

To **check** on any port from a specific port array, indicesindices use the **any from** *PortArrayRef*syntax where PortArrayRefshallbe areference to a port array identifier**.** It is also possible to store the index of a port in a single‑dimensional port array at which the operation was successful to a variable of type integer or, in case of multi‑dimensional port arrays the index of the successful port to an integer array or record of integer variable. When checking the port array for a matching message, call, reply or exception, the port indices to be checked are iterated from lowest to highest. If the port array is multi-dimensional, then the ports are iterated over from innermost to outermost array dimension from lowest to highest index for each dimension, e.g. [0][0], [0][1], [1][0], [1][1]. The first port which matches all the criteria will cause the operation to be successful even if other ports in the array would also meet the criteria.

***Restrictions***

In addition to the general static rules of TTCN‑3 given in clause 5 and shown in table 15, the following restrictions apply:

1. Using the **check** operation in a wrong manner, e.g. check for an exception at a message-based port shall cause a test case error.
2. *AddressRef* for retrieving the sending entity shall be of type **address**, **component** or of the type provided in the address declaration of the port type of the port instance referenced in the **check** operation. No *AddressRef* shall contain the special value **null** at the time of the operation.
3. The *PortArrayRef* shall be a reference to a completely initialized port array.
4. The index redirection shall only be used when the operation is used on an any from port array construct.
5. If the index redirection is used for single-dimensional arrays, the type of the integer variable shall allow storing the highest index of the respective port array.
6. If the index redirection is used for multi-dimensional arrays, the size of the integer array or record of integer type shall exactly be the same as the dimension of the respective port array, and the its type shall allow storing the highest index (from all dimensions) of the port array.
7. If a variable referenced in the **sender** or **@index** clause is a lazy or fuzzy variable, the expression assigned to this variable is equal to the result produced by the **check** operation, i.e. later evaluation of the lazy or fuzzy variable does not lead to repeated invocation of the **check** operation.
8. If the **check** operation contains both **from** and **sender** clause, the variable or parameter referenced in the **sender** clause shall be type compatible with the template in the **from** clause.

NOTE 3: In most cases the correct usage of the check operation can be checked statically, i.e. before/during compilation.

***Examples***

EXAMPLE 1: Basic check

MyPort1.**check**(**receive**(5)); // Checks for an integer message of value 5.

MyPort1.**check**(**receive**(charstring:?) -> **value** MyCharVar);

// Checks for a charstring message and stores the message if the message type is charstring

MyPort2.**check**(**getcall**(MyProc:{5, MyVar}) **from** MyPartner);

// Checks for a call of MyProc at port MyPort2 from MyPartner

MyPort2.**check**(**getreply**(MyProc:{5, MyVar} **value** 20));

// Checks for a reply from procedure MyProc at MyPort2 where the returned value is 20 and

// the values of the two out or inout parameters are 5 and the value of MyVar.

MyPort2.**check**(**catch**(MyProc, MyTemplate(5, MyVar)));

MyPort2.**check**(**getreply**(MyProc1:{?, MyVar} **value** \*) -> **value** MyReturnValue **param**(MyPar1,-));

MyPort.**check**(**getcall**(MyProc:{5, MyVar}) **from** MyPartner -> **param** (MyPar1Var, MyPar2Var));

MyPort.**check**(**getcall**(MyProc:{5, MyVar}) -> **sender** MySenderVar);

EXAMPLE 2: Check any operation

MyPort.**check**;

MyPort.**check**(**from** MyPartner);

MyPort.**check**(-> **sender** MySenderVar);

EXAMPLE 3: Check on any port

**any port**.**check;**

EXAMPLE 4: Check on any port from port array

**type** **port** MyPort **procedure** { **inout** MyProc }

**type** **component** MyComponent {

**port** MyPort p[10][10];

}

**var** **integer** i[2];

**any** **from** p.**check**(**catch**(MyProc, MyType:?)) -> @**index** **value** i;

// Checking for an incoming exception of the type MyType on any port of the port array p and

// storing the index of the port on which the matching was successful first

## 22.5 Controlling communication ports

TTCN‑3 operations for controlling message-based and procedure-based ports are presented in table 24.

Table 24: Overview of TTCN‑3 port operations

|  |  |
| --- | --- |
| Port operations | |
| Statement | Associated keyword or symbol |
| Clear port | **clear** |
| Start port | **start** |
| Stop port | **stop** |
| Halt port | **halt** |
| Check the state of a port | **checkstate** |

### 22.5.1 The Clear port operation

The **clear** port operation empties incoming port queues.

***Syntactical Structure***

( *Port* | ( **all** **port** ) ) "." **clear**

***Semantic Description***

The **clear** operation removes the contents of the *incoming* queue of the specified port or of all ports of the test component performing the **clear** operation.

If a port queue is already empty then this operation shall have no action on that port.

***Restrictions***

No specific restrictions in addition to the general static rules of TTCN‑3 given in clause 5 and shown in table 15.

***Examples***

MyPort.**clear**; // clears port MyPort

### 22.5.2 The Start port operation

The **start** operation enables sending and receiving operations on the port(s).

***Syntactical Structure***

( *Port* | ( **all** **port** ) ) "." **start**

***Semantic Description***

If a port is defined as allowing receiving operations such as **receive**, **getcall**, etc., the **start** operation clears the incoming queue of the named port and starts listening for traffic over the port. If the port is defined to allow sending operations then the operations such as **send**, **call**, **raise**, etc., are also allowed to be performed at that port.

By default, all ports of a component shall be started implicitly when a component is created. The start port operation will cause unstopped ports to be restarted by removing all messages waiting in the incoming queue.

***Restrictions***

No specific restrictions in addition to the general static rules of TTCN‑3 given in clause 5 and shown in table 15.

***Examples***

MyPort.**start**; // starts MyPort

### 22.5.3 The Stop port operation

The **stop** operation disables sending and disallow receiving operations to match at the port(s).

***Syntactical Structure***

( *Port* | ( **all** **port** ) ) "." **stop**

***Semantic Description***

If a port is defined as allowing receiving operations such as **receive** and **getcall,** the **stop** operation causes listening at the named port to cease. If the port is defined to allow sending operations then **stop** port disallows the operations such as **send**, **call**, **raise**, etc., to be performed.

To cease listening at the port means that all receiving operations defined before the stop operation shall be completely performed before the working of the port is suspended.

***Restrictions***

No specific restrictions in addition to the general static rules of TTCN‑3 given in clause 5 and shown in table 15.

***Examples***

MyPort.**receive** (MyTemplate1) -> **value** RecPDU;

// the received value is decoded, matched against  
 // MyTemplate1 and the matching value is stored  
 // in the variable RecPDU  
 MyPort.**stop**; // No receiving operation defined following the stop  
 // operation is executed (unless the port is restarted   
 // by a subsequent start operation)  
 MyPort.**receive** (MyTemplate2); // This operation does not match and will block (assuming

// that no default is activated)

### 22.5.4 The Halt port operation

The **halt** operation is comparable to the **stop** operation, but allows entries being already in the queue to be processed with receiving operations.

***Syntactical Structure***

( *Port* | ( **all** **port** ) ) "." **halt**

***Semantic Description***

If a port allows receiving operations such as **receive**, **trigger** and **getcall,** the **halt** operation disallows receiving operations to succeed for messages and procedure call elements that enter the port queue after performing the **halt** operation at that port. Messages and procedure call elements that were already in the queue before the **halt** operation can still be processed with receiving operations. If the port allows sending operations then **halt** port immediately disallows sending operations such as **send**, **call**, **raise**, etc. to be performed. Subsequent halt operations have no effect on the state of the port or its queue.

NOTE 1: The port **halt** operation virtually puts a marker after the last entry in the queue received when the operation is performed. Entries ahead of the marker can be processed normally. After all entries in the queue ahead of the marker have been processed, the state of the port is equivalent to the stopped state.

NOTE 2: If a port **stop** operation is performed on a halted port before all entries in the queue ahead of the marker have been processed, further receive operations are disallowed immediately (i.e. the marker is virtually moved to the top of the queue).

NOTE 3: A port **start** operation on a halted port clears all entries in the queue irrespectively if they arrived before or after performing the port **halt** operation. It also removes the marker.

NOTE 4: A port **clear** operation on a halted port clears all entries in the queue irrespectively if they arrived before or after performing the port **halt** operation. It also virtually puts the marker at the top of the queue.

***Restrictions***

No specific restrictions in addition to the general static rules of TTCN‑3 given in clause 5 and shown in table 15.

***Examples***

MyPort.halt; // No sending allowed on Myport from this moment on;  
 // processing of messages in the queue still possible.  
 MyPort.receive (MyTemplate1); // If a message was already in the queue before the halt  
 // operation and it matches MyTemplate1, it is processed;  
 // otherwise the receive operation blocks.

### 22.5.5 The Checkstate port operation

The **checkstate** port operation allows to check the state of a port.

***Syntactical Structure***

( *Port* | ( **all** **port** ) | ( **any** **port** )) "." **checkstate** "(" *SingleExpression*")"

***Semantic Description***

The **checkstate** port operation allows to examine the state of a port. If a port is in the state specified by the parameter, the **checkstate** operation returns the Boolean value **true**. If the port is not in the specified state, the **checkstate** operation returns the Boolean value **false**. Calling the **checkstate** operation with an invalid argument leads to an error.

The checkstate operation allows to check for different dimensions of a port state. It allows to check if a port is Started, Halted or Stopped, but also if a port is Connected, Mapped or Linked (i.e. Connected or Mapped).

NOTE 1: The states Started, Halted and Stopped refer to the port states defined in the clauses F.3.1 and F.3.2. The states Connected, Mapped and Linked are related to the application of the connection operations **connect**, **disconnect**, **map** and **unmap** as defined in clause 21.1.

The **checkstate** port operation can be used with **all port** and **any port**. Using the **checkstate** operation with **any port** allows to test if at least one port of a test component is in the specified state. Using the **checkstate** operation with **all port** allows to check if all ports of a component are in the specified state.

***Restrictions***

In addition to the general static rules of TTCN‑3 given in clause 5 and shown in table 15, the following restrictions apply:

a) The parameter of the **checkstate** operation shall be of type **charstring** and shall have one of the following values:

a) "Started"

b) "Halted"

c) "Stopped"

d) "Connected"

e) "Mapped"

f) "Linked"

NOTE 2: Clause E.2.2.4 includes the type definition objState and the constant definitions STARTED, HALTED, STOPPED, CONNECTED, MAPPED, and LINKED. It is recommended to use the **checkstate** operation in combination with this type and these constants to ease the checking of correct usage and to improve the readability of test specs.

b) Calling the **checkstate** operation with a **charstring** parameter not listed in a) shall lead to an error.

***Examples***

**type** **component** MyMTCType // Component type definition for an MTC

{

**port** MyPortType PCO1, PCO2

}

**type component** MyTestSystemInterface // Component type definition for a test system interface

{

**port** MyPortType PCO3, PCO4, PCO5;

}

// Test case definition

**testcase** MyTestcase1 () **runs** **on** MyMTCType **system** MyTestSystemInterface {

**var boolean** myPortState;

myPortState := all port.**checkstate**("Started"); // checkstate returns true, because all

// ports of a component are started after

// component creation and start

myPortState := any port.**checkstate**("Linked"); // checkstate returns false, no port is

// either connected nor mapped

**map**(**mtc**:PCO1, **system**:PCO3);

myPortState := PCO1.**checkstate**("Linked"); // checkstate returns true, PCO1 is mapped

myPortState := PCO1.**checkstate**("Mapped"); // checkstate returns true, PCO1 is mapped

myPortState := PCO1.**checkstate**("Connected"); // checkstate returns false, PCO1 is mapped

// and not connected

myPortState := **any port**.**checkstate**("Mapped"); // checkstate returns true, PCO1 is mapped

**all port**.**stop**;

myPortState := **all port**.**checkstate**("Started"); // checkstate returns false, all ports

// are stopped

myPortState := PCO1.**checkstate**("Stopped"); // checkstate returns true, PCO1 is stopped

// further testcase behaviour

// …

}

## 22.6 Use of any and all with ports

The keywords **any** and **all** may be used with configuration and communication operations as indicated in table 25.

Table 25: Any and All with ports

|  |  |  |  |
| --- | --- | --- | --- |
| Operation | Allowed | | Example |
|  | any | all |  |
| **receive, trigger, getcall, getreply, catch, check**) | yes |  | **any port.receive** |
| **connect / map** |  |  |  |
| **disconnect / unmap** |  | yes | **unmap**(**self** : **all** **port**) |
| **start, stop, clear, halt** |  | yes | **all port.start** |
| **checkstate** | yes | yes | **any port.checkstate("Started")**  **all port.checkstate("Connected")** |

NOTE: Ports are owned by test components and instantiated when a component is created. The keywords **any port** and **all port** address all ports owned by a test component and not only the ports known in the scope of the function or altstep that is executed on the component.

# 23 Timer operations

TTCN‑3 supports a number of timer operations as given in table 26. These operations may be used in test cases, functions, altsteps and module control.

Table 26: Overview of TTCN‑3 timer operations

|  |  |
| --- | --- |
| Timer operations | |
| Statement | Associated keyword or symbol |
| Start timer | **start** |
| Stop timer | **stop** |
| Read elapsed time | **read** |
| Check if timer running | **running** |
| Timeout event | **timeout** |

## 23.1 The timer mechanism

It is assumed that each test component and the module control maintain their own *running-timers* *list* and *timeout-list*, i.e. a list of all timers that are actually running and a list of all timers that have timed out. The timeout-lists are part of the snapshots that are taken when a test case is executed. The running-timers list and timeout-list of a component or module control are updated if a timer of the component or module control is started, is stopped, times out or the component or module control executes a **timeout** operation.

NOTE 1: The running-timers list and the timeout-list are only a conceptual lists and do not restrict the implementation of timers. Other data structures like a set, where the access to timeout events is not restricted by, e.g. the order in which the timeout events have happened, may also be used.

NOTE 2: Conceptually, each test component and module control maintain one running-timers list and one timeout-list only. However, within a given scope unit only timers known in the scope unit can be accessed individually, i.e. timers that are declared in the scope unit, passed in as parameters to the scope unit or known via a runs-on clause. In some special cases (e.g. for re-establishing a test component during a test run), it can be necessary to stop timers local to other scope units or to check if timers local to other scope units are running or have already timed out. This can be done by using the keywords **all** and **any** in combination with the timer operations **stop**, **timeout** and **running**. Allowed combinations are defined in clause 23.7.

When a timer expires, the timer becomes immediately inactive. A timeout event is placed in the timeout-list and the timer is removed from the running-timer list of the test component or module control for which the timer has been declared. Only one entry for any particular timer may appear in the timeout-list and running-timer list of the test component or module control for which the timer has been declared.

All running timers shall automatically be cancelled when a test component is explicitly or implicitly stopped.

## 23.2 The Start timer operation

The **start** timer operation is used to indicate that a timer shall start running.

***Syntactical Structure***

( ( *TimerIdentifier* | *TimerParIdentifier* ) { "[" *SingleExpression* "]" } )

"." **start** [ "(" *TimerValue* ")" ]

***Semantic Description***

When a timer is started, its name is added to the list of running timers (for the given scope unit).

The optional timer value parameter shall be used if no default duration is given, or if it is desired to override the default value specified in the timer declaration. When a timer duration is overridden, the new value applies only to the current instance of the timer, any later **start** operations for this timer, which do not specify a duration, shall use the default duration.

Starting a timer with the timer value 0.0 means that the timer times out immediately. Starting a timer with a negative timer value, e.g. the timer value is the result of an expression, or without a specified timer value shall cause a runtime error.

The timer clock runs from the float value zero (0.0) up to maximum stated by the duration parameter.

The **start** operation may be applied to a running timer, in which case the timer is stopped and re-started. Any entry in a timeout-list for this timer shall be removed from the timeout-list.

***Restrictions***

In addition to the general static rules of TTCN‑3 given in clause 5 and shown in table 15, the following restrictions apply:

1. Timer value shall be a non‑negative numerical **float** number (i.e. the value shall be greater or equal 0.0, infinity and not\_a\_number are disallowed).

***Examples***

MyTimer1.**start**; // MyTimer1 is started with the default duration

MyTimer2.**start**(20E-3); // MyTimer2 is started with a duration of 20 ms

// Elements of timer arrays may also be started in a loop, for example

**timer** t\_Mytimer [5];

**var** **float** v\_timerValues [5];

**for** (**var** **integer** i := 0; i<=4; i:=i+1)

{ v\_timerValues [i] := 1.0 }

**for** (**var** **integer** i := 0; i<=4; i:=i+1)

{t\_Mytimer [i].**start** ( v\_timerValues [i])}

## 23.3 The Stop timer operation

The **stop** operation is used to stop a running timer.

***Syntactical Structure***

( ( ( *TimerIdentifier* | *TimerParIdentifier* ) { "[" *SingleExpression* "]" } ) |

**all** **timer** )

"." **stop**

***Semantic Description***

A **stop** operation removes a running timer from the list of running timers. A stopped timer becomes inactive and its elapsed time is set to the float value zero (0.0).

Stopping an inactive timer is a valid operation, although it does not have any effect. Stopping an expired timer causes the entry for this timer in the timeout-list to be removed.

The **all** keyword may be used to stop all timers that have been started on a component or module control.

***Restrictions***

No specific restrictions in addition to the general static rules of TTCN‑3 given in clause 5 and shown in table 15.

***Examples***

MyTimer1.**stop**; // stops MyTimer1

**all timer.stop**; // stops all running timers

## 23.4 The Read timer operation

The **read** operation is used to retrieve the time that has elapsed since the specified timer was started.

***Syntactical Structure***

( ( *TimerIdentifier* | *TimerParIdentifier* ) { "[" *SingleExpression* "]" } )

"." **read**

***Semantic Description***

The **read** operation returns the time that has elapsed since the specified timer was started. The returned value shall be of type **float**.

Applying the **read** operation on an inactive timer, i.e. on a timer not listed on the running-timer list, will return the float value zero (0.0).

***Restrictions***

No specific restrictions in addition to the general static rules of TTCN‑3 given in clause 5 and shown in table 15.

***Examples***

**var** **float** Myvar;

MyVar := MyTimer1.**read**; // assign to MyVar the time that has elapsed since MyTimer1 was started

## 23.5 The Running timer operation

The **running** timer operation is used to check whether a timer is in the running-timer list.

***Syntactical Structure***

( ( ( *TimerIdentifier* | *TimerParIdentifier* ) { "[" *SingleExpression* "]" } ) |

**any** **timer** |

**any from** TimerArrayRef )

"." **running**

**[**"->" **@index value** VariableRef **]**

***Semantic Description***

The **running** timer operation is used to check whether a specific timer visible in the given scope unit is listed on the running-timer list or not (i.e. that it has been started and has neither timed out nor been stopped). The operation returns the value **true** if the timer is listed on the list, **false** otherwise.

The **any** keyword may be used to check if any timer started on a component or module control is running.

When the **any from** TimerArrayRefnotation is used, where TimerArrayRef shall be a timer array identifier, the timers from the referenced array are iterated over and their states are checked individually, from innermost to outermost dimension from lowest to highest index for each dimension. The first timer to be found in the running state causes the operation returning with the **true** value. If no running timer is found in the array, the operation returns with the **false** value. The index of the first timer found running can optionally be stored in an integer variable for a single‑dimensional array, or to an integer array or record of integer variable for multi-dimensional timer arrays.

***Restrictions***

In addition to the general static rules of TTCN‑3 given in clause 5 and shown in table 15, the following restrictions apply:

1. *TimerArrayRef* shall be a reference to a completely initialized timer array.
2. The index redirection shall only be used for **any from** timer array running operations.
3. If the index redirection is used for single-dimensional timer arrays, the type of the integer variable shall allow storing the highest index of the respective timer array.
4. If the index redirection is used for multi-dimensional timer arrays, the size of the integer array or record of integer type shall exactly be the same as the dimension of the respective timer array, and its type shall allow storing the highest index (from all dimensions) of the timer array.

***Examples***

EXAMPLE 1: Checking if a specific timer is running

**if** (MyTimer1.**running**){ … }

EXAMPLE 2: Checking if an arbitrary timer is running

**if** (**any timer**.**running**){ … }

EXAMPLE 3: Checking if an arbitrary timer from a timer array is running

**timer** MyTimerArray[2][2];

**var integer** i[2];

**if (any from** MyTimerArray**.running -> @index value** i;) { … }

// checks if any timer from array is running

// assigns index of matched timer to i

## 23.6 The Timeout operation

The **timeout** operation allows to check the expiration of timers.

***Syntactical Structure***

( ( ( *TimerIdentifier* | *TimerParIdentifier* ) { "[" *SingleExpression* "]" } ) |

**any** **timer** |

**any from** TimerArrayRef )

"." **timeout**

**[**"->" **@index value** VariableRef **]**

***Semantic Description***

The **timeout** operation allows to check the expiration of a specific timer in the scope unit of a test component or module control in which the timeout operation has been called or of any timer that has been started on a test component or module control before entering the scope in which the **timeout** operation has been called.

When a **timeout** operation is processed, if a timer name is indicated, the timeout-list is searched according to the TTCN‑3 scope rules. If there is a timeout event matching the timer name, that event is removed from the timeout-list, and the **timeout** operation succeeds.

The **timeout** can be used to determine an alternative in an **alt** statement or as stand-alone statement in a behaviour description. In the latter case a **timeout** operation is considered to be shorthand for an **alt** statement with the **timeout** operation as the only alternative.

The **any** keyword used with the **timeout** operation succeeds if the timeout-list is not empty. In this case a randomly chosen timeout event is removed from the timeout-list.

When the **any from** TimerArrayRefnotation is used, where TimerArrayRef shall be a timer array identifier, the timers from the referenced array are iterated over and individually checked for timeout from innermost to outermost dimension from lowest to highest index for each dimension. The first timer to be found in the timeout-list causes that timer to be removed from the list and the timeout operation succeeds. The index of the matched timer can be optionally stored in an integer variable for single-dimensional arrays or to an integer array or record of integer variable for mult‑-dimensional timer arrays.

***Restrictions***

In addition to the general static rules of TTCN‑3 given in clause 5 and shown in table 15, the following restrictions apply:

1. The **timeout** shall not be used in a **boolean** expression.
2. *TimerArrayRef* shall be a reference to a completely initialized timer array.
3. The index redirection shall only be used for **any from** timer array timeout operations.
4. If the index redirection is used for single-dimensional timer arrays, the type of the integer variable shall allow storing the highest index of the respective timer array.
5. If the index redirection is used for multi-dimensional timer arrays, the size of the integer array or record of integer type shall exactly be the same as the dimension of the respective timer array, and its type shall allow storing the highest index (from all dimensions) of the timer array.

***Examples***

EXAMPLE 1: Timeout of a specific timer

MyTimer1.**timeout**; // checks for the timeout of the previously started timer MyTimer1

EXAMPLE 2: Timeout of an arbitrary timer

**any timer.timeout**; // checks for the timeout of any previously started timer

EXAMPLE 3: Timeout of a timer from a timer array

**timer** MyTimerArray[2][2];

**var integer** i[2];

**any from** MyTimerArray**.timeout -> @index value** i;

// checks for the timeout of any timer from array

// assigns index of matched timer to i

## 23.7 Summary of use of any and all with timers

The keywords **any** and **all** may be used with timer operations as indicated in table 27.

Table 27: Any and All with Timers

|  |  |  |  |
| --- | --- | --- | --- |
| Operation | Allowed | | Example |
|  | any | all |  |
| **start** |  |  |  |
| **stop** |  | yes | **all timer.stop** |
| **read** |  |  |  |
| **running** | yes |  | **if (any timer.running) {…}** |
| **timeout** | yes |  | **any timer.timeout** |

# 24 Test verdict operations

Verdict operations given in table 28 allow to set and retrieve verdicts. These operations shall only be used in test cases, altsteps and functions.

Table 28: Overview of TTCN‑3 test verdict operations

|  |  |
| --- | --- |
| Test verdict operations | |
| Statement | Associated keyword or symbol |
| Set local verdict | **setverdict** |
| Get local verdict | **getverdict** |

## 24.1 The Verdict mechanism

Each test component of the active configuration shall maintain its own local verdict. The local verdict is an object which is created for each test component at the time of its creation. It is used to track the individual verdict in each test component (i.e. in the MTC and in each and every PTC).

Additionally, there is a global test case verdict instantiated and handled by the test system that is updated when each test component (i.e. the MTC and each and every PTC) terminates execution (see figure 14). This verdict is not accessible to the **getverdict** and **setverdict** operations. The value of this verdict shall be returned by the test case when it terminates execution. If the returned verdict is not explicitly saved in the control part (e.g. assigned to a variable) then it is lost.



Figure 14: Illustration of the relationship between verdicts

NOTE 1: TTCN‑3 does not specify the actual mechanisms that perform the updating of the local and test case verdicts. These mechanisms are implementation dependent.

The verdict can have five different values: **pass**, **fail**, **inconc**, **none** and **error**, i.e. the distinguished values of the **verdicttype** (see clause 6.1).

NOTE 2: **inconc** means an inconclusive verdict.

When a test component is instantiated, its local verdict object is created and set to the value **none**.

When changing the value of the local verdict (i.e. using the **setverdict** operation) the effect of this change shall follow the overwriting rules listed in table 29. The test case verdict is implicitly updated on the termination of a test component. The effect of this implicit operation shall also follow the overwriting rules listed in table 29.

Table 29: Overwriting rules for the verdict

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Current value of | New verdict assignment value | | | |
| Verdict | pass | inconc | fail | none |
| **None** | **pass** | **inconc** | **fail** | **none** |
| **Pass** | **pass** | **inconc** | **fail** | **pass** |
| **Inconc** | **inconc** | **inconc** | **fail** | **inconc** |
| **Fail** | **fail** | **fail** | **fail** | **fail** |

The **error** verdict is special in that it is set by the test system to indicate that a test case (i.e. runtime) error has occurred. It shall not be set by the **setverdict** operation and will not be returned by the getverdict operation. No other verdict value can override an **error** verdict. This means that an **error** verdict can only be a result of an **execute** test case operation.

Together with the local test verdict, each test component shall also maintain an implicit **charstring** variable to store information about the reasons for assigning the verdict. The implicit **charstring** variable shall have no effect on the overwriting rules and on the calculation of the final test case verdict. On the termination of the test component, the local verdict of the test component shall be logged together with the implicit **charstring** variable. The implicit **charstring** variable cannot be retrieved and read by any TTCN-3 function, it only provides additional information for logging.

## 24.2 The Setverdict operation

The local verdict is set with the **setverdict** operation.

***Syntactical Structure***

**setverdict** "(" *SingleExpression* { "," ( *FreeText* | *TemplateInstance* ) } ")"

***Semantic Description***

The value of the local verdict is changed with the **setverdict** operation. The effect of this change shall follow the overwriting rules listed in table 29.

The optional parameters allow to provide information that explain the reasons for assigning the verdict. This information is composed to a string and stored in an implicit **charstring** variable. On termination of the test component, the actual local verdict is logged together with the implicit **charstring** variable. Since the optional parameters can be seen as log information, the same rules and restrictions as for the parameters of the log statement (clause 19.11) apply.

As the result of the setverdict operation, the implicit **charstring** variable is overwritten whenever the local verdict of a test component is overwritten. A **setverdict** operation with a verdict only that overwrites the current local verdict, will also clear the implicit **charstring** variable. This means previously stored information gets lost.

***Restrictions***

In addition to the general static rules of TTCN‑3 given in clause 5 and shown in table 15, the following restrictions apply:

a) The **setverdict** operation shall only be used with the values **pass**, **fail**, **inconc** and **none**. It shall not be used to assign the value **error**, this is set by the test system only to indicate runtime errors.

b) *SingleExpression* shall resolve to a value of type **verdict**.

c) For *FreeText* and *TemplateInstance*,the same rules and restrictions apply as forthe parameters of the **log** statement. Table 17lists all language elements that can be used in a setverdict operation.

***Examples***

EXAMPLE 1:

**setverdict**(**pass**); // the local verdict is set to pass

:

**setverdict**(**fail);** // until this line is executed, which will result in the value

// of the local verdict being overwritten to fail

// When the ptc terminates the test case verdict is set to fail

EXAMPLE 2:

**var** integer myVar:= 1;

:

MyPort.**receive**(**integer**:MyVar); // Matches an integer value with the value of MyVar

// at port MyPort

**setverdict**(**pass**, "Value received: ", myVar ); // Provided the actual test component verdict is // none: local verdict is set to pass, the implicit

// charstring variable is set to "Value received: 5"

**stop**; // The test component terminates. The local test verdict and

// implicit charstring variable are logged

## 24.3 The Getverdict operation

The value of the local verdict may be retrieved using the **getverdict** operation.

***Syntactical Structure***

**getverdict**

***Semantic Description***

The **getverdict** operation returns the actual value of the local verdict.

***Restrictions***

No specific restrictions in addition to the general static rules of TTCN‑3 given in clause 5 and shown in table 15.

***Examples***

MyResult := **getverdict**; // Where MyResult is a variable of type verdicttype

# 25 External actions

In some testing situations some interface(s) to the SUT may be missing or unknown a priori (e.g. management interface) but it may be necessary that the SUT is stimulated to carry out certain actions (e.g. send a message to the test system). Also certain actions may be required from the test executing personnel (e.g. to change the environmental conditions of testing like the temperature, voltage of the power feeding, etc.).

The required action may be described as a string expression, i.e. the use of literal strings, string typed variables and parameters, etc. and any concatenation thereof are allowed.

***Syntactical Structure***

**action** "(" { ( *FreeText* | *Expression* ) ["&"] } ")"

***Semantic Description***

External actions can be used in test cases, functions, altsteps and module control.

There is no specification of what is done to or by the SUT to trigger this action, only an informal description of the required action itself.

***Restrictions***

In addition to the general static rules of TTCN‑3 given in clause 5 and shown in table 15, the following restrictions apply:

1. *Expression* shall have the base type charstring or universal charstring.

***Examples***

**var charstring** myString:= " now."

**action**("Send MyTemplate on lower PCO" & myString); // Informal description of the  
 // external action

# 26 Module control

Test cases are defined in the module definitions part while the module control part manages their execution. The statements and operations that can be used in the module control are summarized in table 30.

Table 30: Overview of TTCN‑3 statements and operations in module control

| Statement | Associated keyword or symbol |
| --- | --- |
| Assignments | **:=** |
| If-else | **if (…) {…} else {…}** |
| Select case | **select case (…) { case (…) {…} case else {…}}** |
| For loop | **for (…) {…}** |
| While loop | **while (…) {…}** |
| Do while loop | **do {…} while (…)** |
| Label and Goto | **label / goto** |
| Stop execution | **stop** |
| Leaving a loop, alt or interleave | **break** |
| Next iteration of a loop | **continue** |
| Logging | **log** |
| Alternative behaviour (see note) | **alt {…}** |
| Re-evaluation of alternative behaviour (see note) | **repeat** |
| Interleaved behaviour (see note) | **interleave {…}** |
| Activate a default (see note) | **activate** |
| Deactivate a default (see note) | **deactivate** |
| Start timer | **start** |
| Stop timer | **stop** |
| Read elapsed time | **read** |
| Check if timer running | **running** |
| Timeout event | **timeout** |
| Stimulate an (SUT) action externally | **action** |
| Execute test case | **execute** |
| NOTE: Can be used to control timer operations only. | | |

## 26.1 The Execute statement

Test cases are executed with an **execute** statement in the module control.

***Syntactical Structure***

**execute** "(" *TestcaseRef* "(" [ { *ActualPar* [","] } ] ")" [ "," *TimerValue* [ "," *HostId* ] ] ")"

***Semantic Description***

In the module control part the **execute** statement is used to start test cases (see clause 27.1). The result of an executed test case is always a value of type **verdicttype**. Every test case shall contain one and only one MTC the type of which is referenced in the header of the test case definition. The behaviour defined in the test case body is the behaviour of the MTC.

When a test case is invoked the MTC is created, the ports of the MTC and the test system interface are instantiated and the behaviour specified in the test case definition is started on the MTC. All these actions shall be performed implicitly i.e. without explicit **create** and **start** operations.

**Test case start**

A test case is called using an **execute** statement. As the result of the execution of a test case, a test case verdict of either **none**, **pass**, **inconc**, **fail** or **error** shall be returned and may be assigned to a variable for further processing.

Optionally, the **execute** statement allows supervision of a test case by means of a timer duration.

Also optionally, the execute statement allows deployment of the MTC to a specific host before starting the execution. The host is identified by means of a host id.

**Test case parameterization and configuration**

All variables (if any) defined in the control part of a module shall be passed into the test case by parameterization if they are to be used in the behaviour definition of that test case, i.e. TTCN‑3 does not support global variables of any kind.

At the start of each test case, the test configuration shall be reset. This means that all components and ports conducted by **create**, **connect,** etc. operations in a previous test case were destroyed when that test case was stopped (hence are not "visible" to the new test case).

**Test case termination**

A test case terminates with the termination of the MTC. On termination of the MTC (explicitly or implicitly), all running parallel test components shall be removed by the test system.

NOTE 1: The concrete mechanism for stopping all PTCs is tool specific and therefore outside the scope of the present document.

The final verdict of a test case is calculated based on the final local verdicts of the different test components according to the rules defined in clause 24.1. The actual local verdict of a test component becomes its final local verdict when the test component terminates itself or is stopped by itself, another test component or by the test system.

NOTE 2: To avoid race conditions for the calculation of test verdicts due to the delayed stopping of PTCs, the MTC should ensure that all PTCs have stopped (by means of the **done** or **killed** statement) before it stops itself.

**Test case timer**

Timer may be used to supervise the execution of a test case. This may be done using an explicit timeout in the **execute** statement. If the test case does not end within this duration, the result of the test case execution shall be an error verdict and the test system shall terminate the test case. The timer used for test case supervision is a system timer and need not be declared or started.

**Host id**

A host id can be used to give a specific deployment location to the test system where the MTC shall be started and execute its behaviour. If a host id is provided, the execute statement shall end with a test case error if the MTC cannot be deployed on the specified host.

***Restrictions***

In addition to the general static rules of TTCN‑3 given in clause 5 and shown in table 15, the following restrictions apply:

a) The *TimerValue* shall resolve to a non-negative numerical float value (i.e. the value shall be greater or equal 0.0, infinity and not\_a\_number are disallowed).

b) When the corresponding formal parameter is not of template type *TemplateInstance* shall resolve to an *Expression*.

c) The execute statement shall not be called from within an existing executing testcase or function chain called from a test case, i.e. test cases can only be executed from the control part or from functions called from the control part.

d) The *HostId* parameter shall resolve to a **charstring** value.

***Examples***

EXAMPLE 1: Test case execution without keeping the test case verdict

**execute**(MyTestCase1()); // executes MyTestCase1, without storing the

// returned test verdict and without time

// supervision

EXAMPLE 2: Test case execution with keeping the test case verdict

MyVerdict := **execute**(MyTestCase2()); // executes MyTestCase2 and stores the resulting

// verdict in variable MyVerdict

EXAMPLE 3: Test case timer

MyVerdict := **execute**(MyTestCase3(),5E-3); // executes MyTestCase3 and stores the resulting

// verdict in variable MyVerdict. If the test case

// does not terminate within 5ms, MyVerdict will

// get the value 'error'

MyReturnVal := **execute** (MyTestCase(), 7E-3);

// Where the return verdict will be error if MyTestCase does not complete execution

// within 7ms

EXAMPLE 4: Host id

MyVerdict := **execute**(MyTestCase3(), -, "Host1");

// executes MyTestCase3 with unlimited time

// with MTC deployed to 'Host1'

## 26.2 The Control part

The control part defines, in which order, sequence, loop, under which preconditions, and with which parameters test cases are to be executed.

***Syntactical Structure***

**control** "{"

{ ( *ConstDef* |

*TemplateDef* |

*VarInstance* |

*TimerInstance* |

*TimerStatements* |

*BasicStatements* |

*BehaviourStatements* |

*SUTStatements* |

**stop** ) [";"] }

"}"

[ *WithStatement* ] [";"]

***Semantic Description***

**Sequence of test cases**

Program statements specify such things like the order in which test cases are to be executed or the number of times a test case should run.

If no programming statements are used then, by default, the test cases are executed in the sequential order in which they appear in the module control.

NOTE: This does not preclude the possibility that certain tools may wish to override this default ordering to allow a user or tool to select a different execution order.

Timer operations may also be used explicitly to control test case execution.

**Selection/deselection of test cases**

The selection and deselection of test cases can also be used to control the execution of test cases.

There are different ways in TTCN‑3 to select and deselect test cases. For example, boolean expressions may be used to select and deselect which test cases are to be executed. This includes, of course, the use of functions that return a **boolean** value.

Another way to execute test cases as a group is to collect them in a function and execute that function from the module control.

As a test case returns a single value of type **verdicttype**, it is also possible to control the order of test case execution depending on the outcome of a test case. The use of the TTCN‑3 verdicttype is another way to select test cases.

***Restrictions***

In addition to the general static rules of TTCN‑3 given in clause 5 and shown in table 15, the following restrictions apply:

a) Configuration statements such as connect and map (with the exception of stop execution, which is allowed), communication statements such as send and receive and verdict statements such as setverdict shall not be invoked by module control.

b) Statements for alternative behaviours shall only be used to control timer behaviours.

c) The restrictions on the use of statements in the control part are given in table 15.

***Examples***

EXAMPLE 1: Test case execution in a loop

**module** MyTestSuite () {

:

**control** {

:

// Do this test 10 times

count:=0;

**while** (count < 10)

{ **execute** (MySimpleTestCase1());

count := count+1;

}

}

}

EXAMPLE 2: Test case execution controlled by a timer and a counter

// Example of the use of the running timer operation

**while** (T1.**running** **or** x<10) // Where T1 is a previously started timer

{ **execute**(MyTestCase());

x := x+1;

}

// Example of the use of the start and timeout operations

**timer** T1 := 1.0;

:

**execute**(MyTestCase1());

T1.**start**;

T1.**timeout**; // Pause before executing the next test case

**execute**(MyTestCase2());

EXAMPLE 3: Selection/deselection of test cases with Boolean expressions

**module** MyTestSuite () {

:

**control** {

:

**if** (MySelectionExpression1()) {

**execute**(MySimpleTestCase1());

**execute**(MySimpleTestCase2());

**execute**(MySimpleTestCase3());

}

**if** (MySelectionExpression2()) {

**execute**(MySimpleTestCase4());

**execute**(MySimpleTestCase5());

**execute**(MySimpleTestCase6());

}

:

}

}

EXAMPLE 4: Selection/deselection of test cases with functions

**function** MyTestCaseGroup1()

{ **execute**(MySimpleTestCase1());

**execute**(MySimpleTestCase2());

**execute**(MySimpleTestCase3());

}

**function** MyTestCaseGroup2()

{ **execute**(MySimpleTestCase4());

**execute**(MySimpleTestCase5());

**execute**(MySimpleTestCase6());

}

:

**control**

{ **if** (MySelectionExpression1()) { MyTestCaseGroup1(); }

**if** (MySelectionExpression2()) { MyTestCaseGroup2(); }

:

}

EXAMPLE 5: Selection/deselection of test cases based on test case verdicts

**if** ( **execute** (MySimpleTestCase()) == **pass** )

{ **execute** (MyGoOnTestCase()) }

**else**

{ **execute** (MyErrorRecoveryTestCase()) };

# 27 Specifying attributes

TTCN‑3 uses attributes to give special characterization/meaning to language elements such as specific presentation format, specific encoding and encoding variants, and user-defined properties.

## 27.1 The Attribute mechanism

Attributes can be associated with TTCN‑3 language elements by means of the with statement. The with statement can be applied to modules, global module definitions and to local definitions in control, test cases, functions, altsteps, statement blocks and in component type definitions.

### 27.1.1 Scope of attributes

A **with** statement may associate attributes to a single language element or to elements or fields of structured types (in a recursive way) or to members of component or port types, the same way as specified in clauses 6.2.1.1 and 6.2.3.2. It is also possible to associate attributes to a number oflanguage elements by, e.g. listing fields of a structured type in an attribute statement associated with a single type definition or associating a **with** statement to the surrounding scope unit or **group** of language elements. A **with** statement can follow any module, any global definition inside module and group declarations as well as any local definition in component types and statement blocks inside behaviour definitions or the control part.

EXAMPLE 1: // attributes for single language elements and groups

// MyPDU1 will be displayed as PDU

**type** **record** MyPDU1 { … } **with** { **display** "PDU"}

// MyPDU2 will be displayed as PDU with the application specific extension attribute MyRule

**type** **record** MyPDU2 { … }

**with**

{

**display** "PDU";

**extension** "MyRule"

}

// The following group definition …

**group** MyPDUs {

**type** **record** MyPDU3 { … }

**type** **record** MyPDU4 { … }

}

**with** {**display** "PDU"} // All types of group MyPDUs will be displayed as PDU

// is identical to

**group** MyPDUs {

**type** **record** MyPDU3 { … } **with** { **display** "PDU"}

**type** **record** MyPDU4 { … } **with** { **display** "PDU"}

}

EXAMPLE 2: // attributes for fields and elements

**type** **record** MyRec {

**integer** field1,

**record** {

**integer** eField1,

**boolean** eField2

} field2

}

**with** { **display** (field2.eField1) "colour blue" }

// the embedded field eField1 is displayed blue

**type** **record of integer** MyRecOfInteger

**with** { **display** ([-]) "colour green"

// all integer elements are displayed green

**type** **record** of integer MyRecOfInteger2

**with** { **display** ([-]) "colour red" }

// integer elements are displayed red

**const** MyRecOfInteger c\_MyRecordOfInt := {0, 1, 2, 3}

**with** { **display** ([0]) "colour blue" }

// the first element is displayed blue, the other elements are displayed red

### 27.1.2 Overwriting rules for attributes

An attribute definition in a lower scope unit will override a general attribute definition in a higher scope. Additional overwriting rules for variant attributes are defined in clause 27.1.2.1.

EXAMPLE 1:

**type** **record** MyRecordA

{

:

} **with** { **encode** "RuleA" }

// In the following, MyRecordA is encoded according to RuleA and not according to RuleB

**type record** MyRecordB

{

:

MyRecordA field

} **with** { **encode** "RuleB" }

A **with** statement that is placed inside the scope of another **with** statement shall override the outermost **with**. This shall also apply to the use of the **with** statement with groups. Care should be taken when the overwriting scheme is used in combination with references to single definitions. The general rule is that attributes shall be assigned and overwritten according to the order of their occurrence.

// Example of the use ofthe overwriting scheme of the **with** statement

**group** MyPDUs

{

**type** **record** MyPDU1 { … }

**type** **record** MyPDU2 { … }

**group** MySpecialPDUs

{

**type** **record** MyPDU3 { … }

**type** **record** MyPDU4 { … }

}

**with** {**extension** "MySpecialRule"} // MyPDU3 and MyPDU4 will have the application

// specific extension attribute MySpecialRule

}

**with**

{

**display** "PDU"; // All types of group MyPDUs will be displayed as PDU and

**extension** "MyRule"; // (if not overwritten) have the extension attribute MyRule

}

// is identical to …

**group** MyPDUs

{

**type** **record** MyPDU1 { … } **with** {**display** "PDU"; **extension** "MyRule" }

**type** **record** MyPDU2 { … } **with** {**display** "PDU"; **extension** "MyRule" }

**group** MySpecialPDUs {

**type** **record** MyPDU3 { … } **with** {**display** "PDU"; **extension** "MySpecialRule" }

**type** **record** MyPDU4 { … } **with** {**display** "PDU"; **extension** "MySpecialRule" }

}

}

An attribute definition in a lower scope can be overwritten in a higher scope by using the **override** directive.

EXAMPLE 2:

**type** **record** MyRecordA

{

:

} **with** { **encode** "RuleA" }

// In the following, fieldA of a MyRecordB instance is encoded according to RuleB

**type record** MyRecordB

{

:

MyRecordA fieldA

} **with** { **encode** **override** (fieldA) "RuleB" }

The **override** directive forces all contained types at all lower scopes to be forced to the specified attribute.

An attribute definition for a field or element of a structured type overrides the corresponding attribute of the structured type, as regards the identified field or element. The attribute definition for a field or element of a structured type can however be overridden with the override directive in the attribute definition of the structured type.

In case of nested override directives, the override directive of the highest scope shall take precedence. Override directives of definitions at the same scope level do not effect each other.

EXAMPLE 3:

// An instance of MyRecordA is encoded according to RuleA.

**type** **record** MyRecordA

{

:

} **with** { **encode** **override** "RuleA" }

// In the following, fieldA of a MyRecordB instance is encoded according to RuleB.

**type** **record** MyRecordB

{

:

MyRecordA fieldA

} **with** { **encode** **override** (fieldA) "RuleB" }

// In the following, both rules "RuleA" and "RuleB" are overriden by "RuleC" of the group.

**group** MyGroup {

**type** **record** MyRecordA

{

:

} **with** { **encode** **override** "RuleA" }

**type** **record** MyRecordB

{

:

MyRecordA fieldA

} **with** { **encode** **override** (fieldA) "RuleB" }

} **with** { **encode** **override** "RuleC" }

#### 27.1.2.1 Additional overwriting rules for variant attributes

A **variant** attribute is always related to an **encode** attribute. Whereas a variant of an encoding may change, an encoding shall not change without overwriting all current variant attributes.

The present document defines the default rules for variant attributes. Extension packages of TTCN-3, for example specifying language mappings, may define their own overwriting rules for variant attributes. For variant attributes the following default overwriting rules apply:

* a **variant** attribute overwrites an current **variant** attribute according to the rules defined in clause 27.1.2;
* an **encoding** attribute, which overwrites a current **encoding** attribute according to the rules defined in clause 27.1.2, also overwrites a corresponding current **variant** attribute, i.e. no new **variant** attribute is provided, but the current **variant** attribute becomes inactive;
* an **encoding** attribute, which changes a current **encoding** attribute of an imported language element according to the rules defined in clause 27.1.3, also changes a corresponding current **variant** attribute, i.e. no new **variant** attribute is provided, but the current **variant** attribute becomes inactive.

EXAMPLE:

**module** MyVariantEncodingModule {

:

**type** **charstring** MyType**;** // Normally encoded according to "Encoding 1"

:

**group** MyVariantsOne {

:

**type record** MyPDUone

{

**integer** field1, // field1 will be encoded according to "Encoding 2" only.

// "Encoding 2" overwrites "Encoding 1" and variant "Variant 1"

MyType field3 // field3 will be encoded according to "Encoding 1" with

// variant "Variant 1".

}

**with** { **encoding** (field1) "Encoding 2" }

:

}

**with** { **variant** "Variant 1" }

**group** MyVariantsTwo

{ :

**type record** MyPDUtwo

{

**integer** field1, // field1 will be encoded according to "Encoding 3"

// using encoding variant "Variant 3"

MyType field3 // field3 will be encoded according to "Encoding 3"

// using encoding variant "Variant 2"

}

**with** { **variant** (field1) "Variant 3" }

:

}

**with** { **encode** "Encoding 3"; **variant** "Variant 2"}

}

**with** { **encode** "Encoding 1" }

### 27.1.3 Changing attributes of imported language elements

In general, a language element is imported together with its attributes. In some cases these attributes may have to be changed when importing the language element, e.g. a type may be displayed in one module as ASP, then it is imported by another module where it should be displayed as PDU. For such cases it is allowed to change attributes on the **import** statement.

NOTE: If a **with** statement is added to an import of a definition where a local definition also has a **with** statement, the local definition's attributes overwrite the attributes added to the import statement in the normal way. Thus, if the attributes of a local definition shall be changed via the import statement, the override directive needs to be used.

EXAMPLE:

**import from** MyModule {

**type** MyType

}

**with** { **display** "ASP" } // MyType will be displayed as ASP

**import from** MyModule {

**group** MyGroup

}

**with** {

**display** "PDU"; // By default all types will be displayed as PDU

**extension** "MyRule"

}

## 27.2 The With statement

The with statement is used to associate attributes to TTCN‑3 language elements (and sets thereof).

***Syntactical Structure***

**with** "{"

{ ( **encode** | **variant** | **display** | **extension** | **optional** )

[ **override** ]

["(" *DefinitionRef* | *FieldReference* | *AllRef* ")"]

*FreeText* [";"] }

"}"

***Semantic Description***

There are five kinds of attributes that can be associated to language elements:

a) **display:** allows the specification of display attributes related to specific presentation formats;

b) **encode:** allows references to specific encoding rules;

c) **variant:** allows references to specific encoding variants;

d) **extension:** allows the specification of user-defined attributes;

e) **optional:** allows the implicit setting of optional fields in records and sets to omit.

The syntax for the argument of the **with** statement (i.e. the actual attributes) is defined as a free text string.

***Restrictions***

In addition to the general static rules of TTCN‑3 given in clause 5, the following restrictions apply:

a) *DefinitionRef* and *FieldReference* shall refer to a definition or field respectively which is within the module, group or definition to which the with statement is associated.

***Examples***

**type** **record** MyService {

**integer** i,

**float** f

}

**with** { **display** "ServiceCall" } // MyRecord will be displayed as a ServiceCall

## 27.3 Display attributes

Display attributes allow the specification of display attributes related to specific presentation formats.

***Syntactical Structure***

**display**

***Semantic Description***

All TTCN‑3 language elements can have **display** attributes to specify how particular language elements shall be displayed in, for example, a tabular format.

Special attribute strings related to the display attributes for the graphical presentation format can be found in ES 201 873-3 [i.2].

Other **display** attributes may be defined by the user.

NOTE: Because user-defined attributes are not standardized, the interpretation of these attributes may differ between tools or even may not be supported.

***Restrictions***

No specific restrictions in addition to the general static rules of TTCN‑3 given in clause 5.

***Examples***

**type** **record** MyService {

**integer** i,

**float** f

}

**with** { **display** "ServiceCall" } // MyRecord will be displayed as a ServiceCall

## 27.4 Encoding attributes

In TTCN‑3, general or particular encoding rules can be specified by using **encode** and **variant** attributes. Encoding attributes allow references to specific encoding rules.

***Syntactical Structure***

**encode**

***Semantic Description***

Encoding rules define how a particular value, template, etc. shall be encoded and transmitted over a communication **port** and how received signals shall be decoded. TTCN‑3 does not have a default encoding mechanism. This means that encoding rules or encoding directives are defined in some external manner to TTCN‑3.

The **encode** attribute allows the association of some referenced encoding rule or encoding directive to be made to a TTCN‑3 definition.

The manner in which the actual encoding rules are defined (e.g. prose, functions, etc.) is outside the scope of the present document. If no specific rules are referenced then encoding shall be a matter for individual implementation.

In most cases encoding attributes will be used in a hierarchical manner. The top-level is the entiremodule, the next level is a group and the lowest is an individual type or definition:

a) **module:** encoding applies to all types defined in the module, including TTCN‑3 types (built-in types);

b) **group:** encoding applies to a group of user-defined type definitions;

c) **type or definition:** encoding applies to a single user-defined type or definition;

d) **field:** encoding applies to a field in a **record** or **set** type or **template**.

***Restrictions***

No specific restrictions in addition to the general static rules of TTCN‑3 given in clause 5.

***Examples***

**module** MyFirstmodule

{ :

**import from** MySecondModule {

**type** MyRecord

}

**with** { **encode** "MyRule 1" } // Instances of MyRecord will be encoded according to MyRule 1

:

**type** **charstring** MyType**;** // Normally encoded according to the 'Global encoding rule

:

**group** MyRecords

{ :

**type record** MyPDU1

{

**integer** field1, // field1 will be encoded according to "Rule 3"

**boolean** field2**,** // field2 will be encoded according to "Rule 3"

Mytype field3 // field3 will be encoded according to "Rule 2"

}

**with** { **encode** (field1, field2) "Rule 3" }

:

}

**with** { **encode** "Rule 2" }

}

**with** { **encode** "Global encoding rule" }

## 27.5 Variant attributes

In TTCN‑3, general or particular encoding rules can be specified by using **encode** and **variant** attributes. Variant attributes allow references to specific encoding variants.

***Syntactical Structure***

**variant**

***Semantic Description***

To specify a refinement of the currently specified encoding scheme instead of its replacement, the **variant** attribute shall be used. The variant attributes are different from other attributes, because they are closely related to encode attributes. Therefore, for variant attributes, additional overwriting rules apply (see clause 27.1.2.1).

**Special variant strings:**

The following strings are the predefined (standardized) **variant** attributes for simple basic types (see clause E.2.1):

a) "8 bit" and "unsigned 8 bit" mean, when applied to integer and enumerated types, that the integer value or the integer numbers associated with enumerated values shall be handled as it was represented on 8‑bits (single byte) within the system.

b) "16 bit" and "unsigned 16 bit" mean, when applied to integer and enumerated types, that the integer value or the integer numbers associated with enumerated values shall be handled as it was represented on 16‑bits (two bytes) within the system.

c) "32 bit" and "unsigned 32 bit" mean, when applied to integer and enumerated types, that the integer value or the integer numbers associated with enumerated values shall be handled as it was represented on 32‑bits (four bytes) within the system.

d) "64 bit" and "unsigned 64 bit" mean, when applied to integer and enumerated types, that the integer value or the integer numbers associated with enumerated values shall be handled as it was represented on 64‑bits (eight bytes) within the system.

e) "IEEE754 float","IEEE754 double", "IEEE754 extended float" and "IEEE754 extended double" mean, when applied to a float type, that the value shall be encoded and decoded according to the standard IEEE 754 [6] (see annex E).

The following strings are the predefined (standardized) **variant** attributes for **charstring** and **universal charstring** (see clause E.2.2):

a) "UTF-8" means, when applied to the universal charstring type, that the value shall be encoded and decoded according to the UCS encoding scheme UTF-8 as defined in clause 10.1 of ISO/IEC 10646 [2].

b) "UTF-16" means, when applied to the universal charstring type, that the value shall be encoded and decoded according to the UCS encoding scheme UTF-16 as defined in clause 10.4 of ISO/IEC 10646 [2].

c) "UTF-16LE" means, when applied to the universal charstring type, that each character of the value shall be individually encoded and decoded according to the UCS Encoding scheme UTF-16LE as defined in clause 10.3 of ISO/IEC 10646 [2].

d) "UTF-16BE" means, when applied to the universal charstring type, that the value shall be encoded and decoded according to the UCS Encoding scheme UTF-16BE as defined in clause 10.2 of ISO/IEC 10646 [2].

e) "UTF-32" means, when applied to the universal charstring type, that the value shall be encoded and decoded according to the UCS Encoding scheme UTF-32 as defined in clause 10.7 of ISO/IEC 10646 [2].

f) "UTF-32LE" means, when applied to the universal charstring type, that the value shall be encoded and decoded according to the UCS Encoding scheme UTF-32LE as defined in clause 10.6 of ISO/IEC 10646 [2].

g) "UTF-32BE" means, when applied to the universal charstring type, that the value shall be encoded and decoded according to the UCS Encoding scheme UTF-32BE as defined in clause 10.5 of ISO/IEC 10646 [2].

h) "8 bit" means, when applied to charstring and universal charstring types, that each character of the value shall be individually encoded and decoded according to the coded representation as specified in ISO/IEC 10646 [2] (an 8-bit coding).

NOTE: The UCS Encoding schemes allow an optional signature (also known as byte order mark, BOM) to be present in encoded character strings. The above UCS encoding scheme variant attributes does not specify, if signatures are present in the encoded values or not, this is an option for the encoder. It is expected that decoders are able to process signatures in the decoding process.

The following strings are the predefined (standardized) **variant** attributes for structured types (see clause E.2.2.4):

a) "IDL:fixed FORMAL/01-12-01 v.2.6" means, when applied to a record type, that the value shall be handled as an IDL fixed point decimal value (see annex E).

These variant attributes can be used in combination with the more general encode attributes specified at a higher level. For example a **universal charstring** specified with the **variant** attribute "UTF-8" within a module which itself has a global encoding attribute "BER:1997" (see clause 12.2 of ES 201 873-7 [i.5]) will cause each character of the values within the string to first be encoded following the UTF-8 rules and then this UTF-8 value will be encoded following the more global BER rules.

**Invalid encodings**

If it is desired to specify invalid encoding rules then these shall be specified in a referenceable source external to the module in the same way that valid encoding rules are referenced.

***Restrictions***

No specific restrictions in addition to the general static rules of TTCN‑3 given in clause 5.

***Examples***

EXAMPLE:

**module** MyTTCNmodule1

{ :

**type** **charstring** MyType**;** // Normally encoded according to the "Global encoding rule"

:

**group** MyRecords

{ :

**type record** MyPDU1

{

**integer** field1, // field1 will be encoded according to "Rule 2"

// using encoding variant "length form 3"

Mytype field3 // field3 will be encoded according to "Rule 2"

// using any possible length encoding format

}

**with** { **variant** (field1) "length form 3" }

:

}

**with** { **encode** "Rule 2" }

}

**with** { **encode** "Global encoding rule" }

## 27.6 Extension attributes

Extension attributes can be used for proprietary extensions to TTCN‑3.

***Syntactical Structure***

**extension**

***Semantic Description***

All TTCN‑3 language elements can have **extension** attributes specified by the user.

NOTE: Because user-defined attributes are not standardized the interpretation of these attributes between tools supplied by different vendors may differ or even not be supported.

***Restrictions***

No specific restrictions in addition to the general static rules of TTCN‑3 given in clause 5.

***Examples***

**testcase** MyTestcase() **runs** **on** MTCType {

:

}

**with** { **extension** "Test Purpose: This test case is used to check …" }

## 27.7 Optional attributes

The **optional** attribute can be used to indicate that optional fields of constants, module parameters or templates of record and set types are implicitly set to **omit**.

***Syntactical Structure***

**optional**

***Semantic Description***

TTCN‑3 constants, module parameters, and templates can have an **optional** attribute. Also, TTCN-3 language elements that contain such definitions, i.e. module, group, function, altstep, test case, control, and component type definitions can have an **optional** attribute. When an **optional** attribute is associated to a function, altstep, test case, control or component type definitions, it shall have effect on all the constants, module parameters, and templates declared within these definitions and not on the enframing definition itself.

**Special optional strings:**

The following strings are the predefined (standardized) **optional** attributes.

a) "implicit omit" means that all optional fields, that have no assigned value definition in the statement on which the attribute operates, are set to omit. This applies recursively to the optional fields of the entity and to subfields of the mandatory fields.

b) "explicit omit" means that all optional fields, that have no assigned value definition in the statement on which the attribute operates, are left undefined. This applies recursively to the optional fields of the entity and to subfields of the mandatory fields.

***Restrictions***

In addition to the general static rules of TTCN‑3 given in clause 5, the following restrictions apply:

a) Data type, port type, procedure signature and variable definitions and import statements shall not have an **optional** attribute associated to them directly. When an **optional** attribute is associated to module, group, function, altstep, test case, control or component type containing such definitions, it shall not have any effect on the included data type, port type, procedure signature, variable or import statement.

***Examples***

type record MyRecord1 { **integer** a, **boolean** b **optional**}  
**type record** MyRecord2{MyRecord1m}  
// reference templates with explicitly set fields  
**template** MyRecord1MyTemplate1:= { a := ?, b := **omit** }  
**template** MyRecord2MyTemplate2:= { m := { a := ?, b := **omit** }}// reference templates  
**template** MyRecord1MyTemplate1a:= { a := ? } // b is undefined  
**template** MyRecord1MyTemplate1b:= { a := ? } **with** {**optional** "explicit omit**"**} // b is undefined  
 **template** MyRecord2MyTemplate2a:= {} // m and its subfields are undefined

**template** MyRecord2MyTemplate2b:= { m := { a := ?}}; // m.b is undefined

// templates with attribute

**template** MyRecord1MyTemplate11 **:=** { a := ? } **with** {**optional "**implicit omit**"**}  
 // same as MyTemplate1, b is set to omit

**template** MyRecord2MyTemplate21:= { m := { a := ?}} **with** {**optional "**implicit omit**"**}  
// same as MyTemplate2, by recursive application of the attribute

**template** MyRecord2MyTemplate22:= { m := MyTemplate1a } **with** {**optional "**implicit omit**"**}  
// same as MyTemplate2, by recursive application of the attribute

**template** MyRecord2MyTemplate23:= {} **with** {**optional "**implicit omit**"**}  
 // same as MyTemplate2a, m remains undefined

**template** MyRecord2MyTemplate24 **:=** { m := MyTemplate1b } **with** {**optional "**implicit omit**"**}  
// same as MyTemplate2b, the attribute on the lower scope is not overwritten

**template** MyRecord2MyTemplate25:= { m := MyTemplate1b } **with** {**optional override "**implicit omit**"**}  
 // same as MyTemplate2, the attribute on the lower scope is overwritten

Annex A (normative):  
BNF and static semantics

# A.1 TTCN‑3 BNF

This annex defines the syntax of TTCN‑3 using extended BNF (henceforth just called BNF).

## A.1.1 Conventions for the syntax description

Table A.1 defines the metanotation used to specify the extended BNF grammar for TTCN‑3.

Table A.1: The syntactic metanotation

|  |  |  |
| --- | --- | --- |
| ::= | is defined to be | definition of non-terminal |
| abc xyz | abc followed by xyz | concatenation |
| | | alternative | alternative |
| [abc] | 0 or 1 instances of abc | optional |
| {abc} | 0 or more instances of abc | repetition 1 |
| {abc}+ | 1 or more instances of abc | repetition 2 |
| {abc}#(n, m) | n to m instances of abc | repetition 3 |
| (...) | textual grouping | grouping |
| Abc | the non-terminal symbol abc | non-terminal |
| "abc" | a terminal symbol abc | terminal |

NOTE: The metanotation defined in table A.1 is parsed from left to right. The metanotation operators have the following precedence, from highest (binding tightest) at the top, to lowest (loosest) at the bottom:

- Repetition, Optional

- Grouping

- Concatenation

- Alternative

- Definition

## A.1.2 Statement terminator symbols

In general all TTCN‑3 language constructs (i.e. definitions, declarations, statements and operations) are terminated with a semi-colon (;). The semi-colon is optional if the language construct ends with a right-hand curly brace (}) or the following symbol is a right-hand curly brace (}), i.e. the language construct is the last statement in a statement block.

## A.1.3 Identifiers

TTCN‑3 identifiers are case sensitive and may only contain lowercase letters (a-z) uppercase letters (A-Z) and numeric digits (0-9). Use of the underscore ( \_ ) symbol is also allowed. An identifier shall begin with a letter (i.e. not with a number and not an underscore).

## A.1.4 Comments

Comments written in free text may appear anywhere in a TTCN‑3 specification. Comments may contain any graphical character defined in ISO/IEC 10646 [2]. Block comments shall be opened by the symbol pair /\* and closed by the symbol pair \*/.

EXAMPLE 1:

/\* This is a block comment

spread over two lines \*/

Block comments shall not be nested.

/\* This is not /\* a legal \*/ comment \*/

Line comments shall be opened by the symbol pair // and closed by a <*newline*>.

EXAMPLE 2:

// This is a line comment

// spread over two lines

EXAMPLE 3:

// The following is not legal

**const** // This is MyConst **integer** MyConst := 1;

// A block comment should have been used instead

**const** /\* This is MyConst \*/ **integer** MyConst := 1;

// A line comment like this works as well

**const** // This is MyConst

**integer** MyConst := 1;

## A.1.5 TTCN‑3 terminals

TTCN‑3 terminal symbols and reserved words are listed in tables A.2 and A.3.

Table A.2: List of TTCN‑3 special terminal symbols

|  |  |
| --- | --- |
| Begin/end block symbols | **{ }** |
| Begin/end list symbols | **( )** |
| Element specifier symbols | **[ ]** |
| Range symbol | **..** |
| Line and block comments | **/\* \*/**  **//** |
| Statement separator symbol | **;** |
| Arithmetic operator symbols | **+ / - \*** |
| Concatenation operator symbol | **&** |
| Relational operator symbols | **!= == >= <= < >** |
| Shift operator symbols | **<< >>** |
| Rotate operator symbols | **<@ @>** |
| String enclosure symbols | **" '** |
| Wildcard/matching symbols | **? \*** |
| Assignment symbol | **:=** |
| Communication operation assignment | **->** |
| Bitstring, hexstring and Octetstring values | **B H O** |
| Float exponent | **E** |
| List element separator symbol | **,** |

The predefined function identifiers defined in table 14 and described in annex C shall also be treated as reserved words.

Table A.3: List of TTCN‑3 terminals which are reserved words

|  |  |  |  |
| --- | --- | --- | --- |
| **action**  **activate**  **address**  **alive**  **all**  **alt**  **altstep**  **and**  **and4b**  **any**  **anytype**  **bitstring**  **boolean**  **break**  **case**  **call**  **catch**  **char**  **charstring**  **check**  **clear**  **complement**  **component**  **connect**  **const**  **continue**  **control**  **create**  **deactivate**  **decmatch**  **default**  **disconnect**  **display**  **do**  **done**  **else**  **encode**  **enumerated**  **error**  **except**  **exception**  **execute**  **extends**  **extension**  **external** | **fail**  **false**  **float**  **for**  **friend**  **from**  **function**  **getverdict**  **getcall**  **getreply**  **goto**  **group**  **halt hexstring**  **if**  **ifpresent**  **import**  **in**  **inconc**  **infinity**  **inout**  **integer**  **interleave**  **kill**  **killed**  **label**  **language**  **length**  **log**  **map**  **match**  **message**  **mixed**  **mod**  **modifies**  **module**  **modulepar**  **mtc** | **noblock**  **none**  **not**  **not4b**  **nowait**  **null**  **octetstring**  **of**  **omit**  **on**  **optional**  **or**  **or4b**  **out**  **override**  **param**  **pass**  **pattern**  **permutation**  **port**  **present**  **private**  **procedure**  **public**  **raise**  **read**  **receive**  **record**  **recursive**  **rem**  **repeat**  **reply**  **return**  **running**  **runs** | **select**  **self**  **send**  **sender**  **set**  **setverdict**  **signature**  **start**  **stop**  **subset**  **superset**  **system**  **template**  **testcase**  **timeout**  **timer**  **to**  **trigger**  **true**  **type**  **union**  **universal**  **unmap**  **value**  **valueof**  **var**  **variant**  **verdicttype**  **while**  **with**  **xor**  **xor4b** |

The TTCN‑3 terminals listed in table A.3 shall not be used as identifiers in a TTCN‑3 module. These terminals shall be written in all lowercase letters.

Additionally, there are special TTCN-3 terminals consisting of an @-symbol, directly followed by an identifier. These terminals shall also be written in all lowercase letters.

NOTE: These terminals can be used in combination with the @-symbol, which results in a specific semantics for the annotated language element. They can also be used like any other identifier without any special meaning.

Table A.4: List of TTCN‑3 terminals which are modifiers

|  |  |  |  |
| --- | --- | --- | --- |
| **@decoded**  **@deterministic** | **@fuzzy** | **@index** | **@lazy**  **@nocase** |

### A.1.5.1 Use of whitespaces and newlines

The elements of the TTCN-3 syntax (reserved words, identifiers, terminal symbols and literal values) shall be separated by whitespace or by special terminal symbols listed in table A.2 according to the TTCN-3 syntax.

In representing whitespace, any one or more of the following characters of the C0 set of Recommendation ITU‑T T.50 [4] and of annex A of Recommendation ITU‑T T.50 [4] may be used in any combination:

* HT - HORIZONTAL TABULATION (9)
* LF - LINE FEED (10)
* VT -VERTICAL TABULATION (11)
* FF - FORM FEED (12)
* CR - CARRIAGE RETURN (13)
* SP - SPACE (32)

The characters of the C0 set of Recommendation ITU‑T T.50 [4] and of annex A of Recommendation ITU‑T T.50 [4] below are denoting newline (end of line). A single CR(13) character directly followed by an LF(10) character denote a single end of line (i.e. the sequence CRLFCRLFVT denotes 3 lines):

* LF - LINE FEED (10)
* VT - VERTICAL TABULATION (11)
* FF - FORM FEED (12)
* CR - CARRIAGE RETURN (13)

Any character or character sequence that is a valid newline is also a valid whitespace.

NOTE: It is recommended that for newline only the CR and LF and for whitespace only the HT, LF, CR and SP control characters are used as the VT and FF characters may cause problems with some conventional text editors.

## A.1.6 TTCN-3 syntax BNF productions

### A.1.6.0 TTCN-3 module

TTCN3Module ::= [TTCN3ModuleKeyword](#TTTCN3ModuleKeyword) [ModuleId](#TModuleId) "{" [[ModuleDefinitionsList](#TModuleDefinitionsList)]

[[ModuleControlPart](#TModuleControlPart)] "}" [[WithStatement](#TWithStatement)] [[SemiColon](#TSemiColon)]

TTCN3ModuleKeyword ::= "module"

ModuleId ::= [Identifier](#TIdentifier) [[LanguageSpec](#TLanguageSpec)]

LanguageSpec ::= [LanguageKeyword](#TLanguageKeyword) [FreeText](#TFreeText) {"," [FreeText](#TFreeText)}

LanguageKeyword ::= "language"

### A.1.6.1 Module definitions part

#### A.1.6.1.0 General

ModuleDefinitionsList ::= {[ModuleDefinition](#TModuleDefinition) [[SemiColon](#TSemiColon)]}+

ModuleDefinition ::= (([[Visibility](#TVisibility)] ([TypeDef](#TTypeDef) |

[ConstDef](#TConstDef) |

[TemplateDef](#TTemplateDef) |

[ModuleParDef](#TModuleParDef) |

[FunctionDef](#TFunctionDef) |

[SignatureDef](#TSignatureDef) |

[TestcaseDef](#TTestcaseDef) |

[AltstepDef](#TAltstepDef) |

[ImportDef](#TImportDef) |

[ExtFunctionDef](#TExtFunctionDef) |

[ExtConstDef](#TExtConstDef)

)) |

(["public"] [GroupDef](#TGroupDef)) |

(["private"] [FriendModuleDef](#TFriendModuleDef))

) [[WithStatement](#TWithStatement)]

Visibility ::= "public" |

"friend" |

"private"

#### A.1.6.1.1 Typedef definitions

TypeDef ::= [TypeDefKeyword](#TTypeDefKeyword) [TypeDefBody](#TTypeDefBody)

TypeDefBody ::= [StructuredTypeDef](#TStructuredTypeDef) | [SubTypeDef](#TSubTypeDef)

TypeDefKeyword ::= "type"

StructuredTypeDef ::= [RecordDef](#TRecordDef) |

[UnionDef](#TUnionDef) |

[SetDef](#TSetDef) |

[RecordOfDef](#TRecordOfDef) |

[SetOfDef](#TSetOfDef) |

[EnumDef](#TEnumDef) |

[PortDef](#TPortDef) |

[ComponentDef](#TComponentDef)

RecordDef ::= [RecordKeyword](#TRecordKeyword) [StructDefBody](#TStructDefBody)

RecordKeyword ::= "record"

StructDefBody ::= ([Identifier](#TIdentifier) | [AddressKeyword](#TAddressKeyword)) "{" [[StructFieldDef](#TStructFieldDef)

{"," [StructFieldDef](#TStructFieldDef)}]

"}"

StructFieldDef ::= ([Type](#TType) | [NestedTypeDef](#TNestedTypeDef)) [Identifier](#TIdentifier) [[ArrayDef](#TArrayDef)] [[SubTypeSpec](#TSubTypeSpec)]

[[OptionalKeyword](#TOptionalKeyword)]

NestedTypeDef ::= [NestedRecordDef](#TNestedRecordDef) |

[NestedUnionDef](#TNestedUnionDef) |

[NestedSetDef](#TNestedSetDef) |

[NestedRecordOfDef](#TNestedRecordOfDef) |

[NestedSetOfDef](#TNestedSetOfDef) |

[NestedEnumDef](#TNestedEnumDef)

NestedRecordDef ::= [RecordKeyword](#TRecordKeyword) "{" [[StructFieldDef](#TStructFieldDef) {"," [StructFieldDef](#TStructFieldDef)}]

"}"

NestedUnionDef ::= [UnionKeyword](#TUnionKeyword) "{" [UnionFieldDef](#TUnionFieldDef) {"," [UnionFieldDef](#TUnionFieldDef)}

"}"

NestedSetDef ::= [SetKeyword](#TSetKeyword) "{" [[StructFieldDef](#TStructFieldDef) {"," [StructFieldDef](#TStructFieldDef)}]

"}"

NestedRecordOfDef ::= [RecordKeyword](#TRecordKeyword) [[StringLength](#TStringLength)] [OfKeyword](#TOfKeyword) ([Type](#TType) |

[NestedTypeDef](#TNestedTypeDef))

NestedSetOfDef ::= [SetKeyword](#TSetKeyword) [[StringLength](#TStringLength)] [OfKeyword](#TOfKeyword) ([Type](#TType) | [NestedTypeDef](#TNestedTypeDef))

NestedEnumDef ::= [EnumKeyword](#TEnumKeyword) "{" [EnumerationList](#TEnumerationList) "}"

OptionalKeyword ::= "optional"

UnionDef ::= [UnionKeyword](#TUnionKeyword) [UnionDefBody](#TUnionDefBody)

UnionKeyword ::= "union"

UnionDefBody ::= ([Identifier](#TIdentifier) | [AddressKeyword](#TAddressKeyword)) "{" [UnionFieldDef](#TUnionFieldDef) {","

[UnionFieldDef](#TUnionFieldDef)}

"}"

UnionFieldDef ::= ([Type](#TType) | [NestedTypeDef](#TNestedTypeDef)) [Identifier](#TIdentifier) [[ArrayDef](#TArrayDef)] [[SubTypeSpec](#TSubTypeSpec)]

SetDef ::= [SetKeyword](#TSetKeyword) [StructDefBody](#TStructDefBody)

SetKeyword ::= "set"

RecordOfDef ::= [RecordKeyword](#TRecordKeyword) [[StringLength](#TStringLength)] [OfKeyword](#TOfKeyword) [StructOfDefBody](#TStructOfDefBody)

OfKeyword ::= "of"

StructOfDefBody ::= ([Type](#TType) | [NestedTypeDef](#TNestedTypeDef)) ([Identifier](#TIdentifier) | [AddressKeyword](#TAddressKeyword))

[[SubTypeSpec](#TSubTypeSpec)]

SetOfDef ::= [SetKeyword](#TSetKeyword) [[StringLength](#TStringLength)] [OfKeyword](#TOfKeyword) [StructOfDefBody](#TStructOfDefBody)

EnumDef ::= [EnumKeyword](#TEnumKeyword) ([Identifier](#TIdentifier) | [AddressKeyword](#TAddressKeyword)) "{" [EnumerationList](#TEnumerationList)

"}"

EnumKeyword ::= "enumerated"

EnumerationList ::= [Enumeration](#TEnumeration) {"," [Enumeration](#TEnumeration)}

Enumeration ::= [Identifier](#TIdentifier) ["(" [[Minus](#TMinus)] [Number](#TNumber) ")"]

SubTypeDef ::= [Type](#TType) ([Identifier](#TIdentifier) | [AddressKeyword](#TAddressKeyword)) [[ArrayDef](#TArrayDef)] [[SubTypeSpec](#TSubTypeSpec)]

SubTypeSpec ::= [AllowedValuesSpec](#TAllowedValuesSpec) [[StringLength](#TStringLength)] | [StringLength](#TStringLength)   
  
/\* STATIC SEMANTICS - AllowedValues shall be of the same type as the field being subtyped \*/

AllowedValuesSpec ::= "(" (([TemplateOrRange](#TTemplateOrRange) {"," [TemplateOrRange](#TTemplateOrRange)}) |

[CharStringMatch](#TCharStringMatch)) ")"

TemplateOrRange ::= [RangeDef](#TRangeDef) |

[TemplateBody](#TTemplateBody) |

[Type](#TType)   
  
/\* STATIC SEMANTICS - RangeDef production shall only be used with integer, charstring, universal charstring or float based types \*/   
  
  
/\* STATIC SEMANTICS - When subtyping charstring or universal charstring range and values shall not be mixed in the same SubTypeSpec \*/

RangeDef ::= [Bound](#TBound) ".." [Bound](#TBound)

StringLength ::= [LengthKeyword](#TLengthKeyword) "(" [SingleExpression](#TSingleExpression) [".."(SingleExpression | InfinityKeyword) ] ")"   
  
/\* STATIC SEMANTICS - StringLength shall only be used with String types or to limit set of and record of. SingleExpression and Bound shall evaluate to non-negative integer values (in case of Bound including infinity) \*/

LengthKeyword ::= "length"

PortDef ::= [PortKeyword](#TPortKeyword) [PortDefBody](#TPortDefBody)

PortDefBody ::= [Identifier](#TIdentifier) [PortDefAttribs](#TPortDefAttribs)

PortKeyword ::= "port"

PortDefAttribs ::= [MessageAttribs](#TMessageAttribs) |

[ProcedureAttribs](#TProcedureAttribs) |

[MixedAttribs](#TMixedAttribs)

MessageAttribs ::= [MessageKeyword](#TMessageKeyword) "{" {([AddressDecl](#TAddressDecl) |

[MessageList](#TMessageList) |

[ConfigParamDef](#TConfigParamDef)

) [[SemiColon](#TSemiColon)]}+ "}"

ConfigParamDef ::= [MapParamDef](#TMapParamDef) | [UnmapParamDef](#TUnmapParamDef)

MapParamDef ::= [MapKeyword](#TMapKeyword) [ParamKeyword](#TParamKeyword) "(" [FormalValuePar](#TFormalValuePar) {"," [FormalValuePar](#TFormalValuePar)}

")"

UnmapParamDef ::= [UnmapKeyword](#TUnmapKeyword) [ParamKeyword](#TParamKeyword) "(" [FormalValuePar](#TFormalValuePar) {","

[FormalValuePar](#TFormalValuePar)}

")"

AddressDecl ::= [AddressKeyword](#TAddressKeyword) [Type](#TType)

MessageList ::= [Direction](#TDirection) [AllOrTypeList](#TAllOrTypeList)

Direction ::= [InParKeyword](#TInParKeyword) |

[OutParKeyword](#TOutParKeyword) |

[InOutParKeyword](#TInOutParKeyword)

MessageKeyword ::= "message"

AllOrTypeList ::= [AllKeyword](#TAllKeyword) | [TypeList](#TTypeList)   
  
/\* NOTE: The use of AllKeyword in port definitions is deprecated \*/

AllKeyword ::= "all"

TypeList ::= [Type](#TType) {"," [Type](#TType)}

ProcedureAttribs ::= [ProcedureKeyword](#TProcedureKeyword) "{" {([AddressDecl](#TAddressDecl) |

[ProcedureList](#TProcedureList) |

[ConfigParamDef](#TConfigParamDef)

) [[SemiColon](#TSemiColon)]}+ "}"

ProcedureKeyword ::= "procedure"

ProcedureList ::= [Direction](#TDirection) [AllOrSignatureList](#TAllOrSignatureList)

AllOrSignatureList ::= [AllKeyword](#TAllKeyword) | [SignatureList](#TSignatureList)

SignatureList ::= [Signature](#TSignature) {"," [Signature](#TSignature)}

MixedAttribs ::= [MixedKeyword](#TMixedKeyword) "{" {([AddressDecl](#TAddressDecl) |

[MixedList](#TMixedList) |

[ConfigParamDef](#TConfigParamDef)

) [[SemiColon](#TSemiColon)]}+ "}"

MixedKeyword ::= "mixed"

MixedList ::= [Direction](#TDirection) [ProcOrTypeList](#TProcOrTypeList)

ProcOrTypeList ::= [AllKeyword](#TAllKeyword) | ([ProcOrType](#TProcOrType) {"," [ProcOrType](#TProcOrType)})

ProcOrType ::= [Signature](#TSignature) | [Type](#TType)

ComponentDef ::= [ComponentKeyword](#TComponentKeyword) [Identifier](#TIdentifier) [[ExtendsKeyword](#TExtendsKeyword) [ComponentType](#TComponentType)

{"," [ComponentType](#TComponentType)}] "{"

[[ComponentDefList](#TComponentDefList)] "}"

ComponentKeyword ::= "component"

ExtendsKeyword ::= "extends"

ComponentType ::= [ExtendedIdentifier](#TExtendedIdentifier)

ComponentDefList ::= {[ComponentElementDef](#TComponentElementDef) [[WithStatement](#TWithStatement)] [[SemiColon](#TSemiColon)]}

ComponentElementDef ::= [PortInstance](#TPortInstance) |

[VarInstance](#TVarInstance) |

[TimerInstance](#TTimerInstance) |

[ConstDef](#TConstDef) |

[TemplateDef](#TTemplateDef)

PortInstance ::= [PortKeyword](#TPortKeyword) [ExtendedIdentifier](#TExtendedIdentifier) [PortElement](#TPortElement) {"," [PortElement](#TPortElement)}

PortElement ::= [Identifier](#TIdentifier) [[ArrayDef](#TArrayDef)]

#### A.1.6.1.2 Constant definitions

ConstDef ::= [ConstKeyword](#TConstKeyword) [Type](#TType) [ConstList](#TConstList)

ConstList ::= [SingleConstDef](#TSingleConstDef) {"," [SingleConstDef](#TSingleConstDef)}

SingleConstDef ::= [Identifier](#TIdentifier) [[ArrayDef](#TArrayDef)] [AssignmentChar](#TAssignmentChar) [ConstantExpression](#TConstantExpression)

ConstKeyword ::= "const"

#### A.1.6.1.3 Template definitions

TemplateDef ::= [TemplateKeyword](#TTemplateKeyword) [[TemplateRestriction](#TTemplateRestriction)] [[FuzzyModifier](#TFuzzyModifier)]

[BaseTemplate](#TBaseTemplate) [[DerivedDef](#TDerivedDef)] [AssignmentChar](#TAssignmentChar) [TemplateBody](#TTemplateBody)

BaseTemplate ::= ([Type](#TType) | [Signature](#TSignature)) [Identifier](#TIdentifier) ["(" [TemplateOrValueFormalParList](#TTemplateOrValueFormalParList)

")"]

TemplateKeyword ::= "template"

DerivedDef ::= [ModifiesKeyword](#TModifiesKeyword) [ExtendedIdentifier](#TExtendedIdentifier)

ModifiesKeyword ::= "modifies"

TemplateOrValueFormalParList ::= [TemplateOrValueFormalPar](#TTemplateOrValueFormalPar) {"," [TemplateOrValueFormalPar](#TTemplateOrValueFormalPar)}

TemplateOrValueFormalPar ::= [FormalValuePar](#TFormalValuePar) | [FormalTemplatePar](#TFormalTemplatePar)   
  
/\* STATIC SEMANTICS - FormalValuePar shall resolve to an in parameter \*/

TemplateBody ::= ([SimpleSpec](#TSimpleSpec) |

[FieldSpecList](#TFieldSpecList) |

[ArrayValueOrAttrib](#TArrayValueOrAttrib)

) [[ExtraMatchingAttributes](#TExtraMatchingAttributes)]   
  
/\* STATIC SEMANTICS - Within TeplateBody the ArrayValueOrAttrib can be used for array, record, record of and set of types. \*/

SimpleSpec ::= ([SingleExpression](#TSingleExpression) ["&" [SimpleTemplateSpec](#TSimpleTemplateSpec)]) | [SimpleTemplateSpec](#TSimpleTemplateSpec)

SimpleTemplateSpec ::= [SingleTemplateExpression](#TSingleTemplateExpression) ["&" [SimpleSpec](#TSimpleSpec)]

SingleTemplateExpression ::= [MatchingSymbol](#TMatchingSymbol) | ([TemplateRefWithParList](#TTemplateRefWithParList)

[[ExtendedFieldReference](#TExtendedFieldReference)])

FieldSpecList ::= "{" [FieldSpec](#TFieldSpec) {"," [FieldSpec](#TFieldSpec)} "}"

FieldSpec ::= [FieldReference](#TFieldReference) [AssignmentChar](#TAssignmentChar) ([TemplateBody](#TTemplateBody) | [Minus](#TMinus))

FieldReference ::= [StructFieldRef](#TStructFieldRef) |

[ArrayOrBitRef](#TArrayOrBitRef) |

[ParRef](#TParRef)

StructFieldRef ::= [Identifier](#TIdentifier) |

[PredefinedType](#TPredefinedType) |

[TypeReference](#TTypeReference)   
  
/\* STATIC SEMANTICS - PredefinedType and TypeReference shall be used for anytype value notation only. PredefinedType shall not be AnyTypeKeyword.\*/

ParRef ::= [Identifier](#TIdentifier)   
  
/\* STATIC SEMANTICS - Identifier in ParRef shall be a formal parameter identifier from the associated signature definition \*/

ArrayOrBitRef ::= "[" [FieldOrBitNumber](#TFieldOrBitNumber) "]"   
  
/\* STATIC SEMANTICS - ArrayRef shall be optionally used for array types and TTCN-3 record of and set of. The same notation can be used for a Bit reference inside an TTCN-3 charstring, universal charstring, bitstring, octetstring and hexstring type \*/

FieldOrBitNumber ::= [SingleExpression](#TSingleExpression)   
  
/\* STATIC SEMANTICS - SingleExpression will resolve to a value of integer type \*/

ArrayValueOrAttrib ::= "{" [[ArrayElementSpecList](#TArrayElementSpecList)] "}"

ArrayElementSpecList ::= [ArrayElementSpec](#TArrayElementSpec) {"," [ArrayElementSpec](#TArrayElementSpec)}

ArrayElementSpec ::= [Minus](#TMinus) |

[PermutationMatch](#TPermutationMatch) |

[TemplateBody](#TTemplateBody)

MatchingSymbol ::= [Complement](#TComplement) |

([AnyValue](#TAnyValue) [[WildcardLengthMatch](#TWildcardLengthMatch)]) |

([AnyOrOmit](#TAnyOrOmit) [[WildcardLengthMatch](#TWildcardLengthMatch)]) |

[ListOfTemplates](#TListOfTemplates) |

[Range](#TRange) |

[BitStringMatch](#TBitStringMatch) |

[HexStringMatch](#THexStringMatch) |

[OctetStringMatch](#TOctetStringMatch) |

[CharStringMatch](#TCharStringMatch) |

[SubsetMatch](#TSubsetMatch) |

[SupersetMatch](#TSupersetMatch) |

DecodedContentMatch

DecodedContentMatch ::= DecodedMatchKeyword ["(" Expression] ")"] InlineTemplate   
DencodedMatchKeyword ::= "decmatch"

/\* STATIC SEMANTIC – WildcardLengthMatch shall be used when MatchingSymbol is used in fractions of a concatenated string or list (see clause 15.11) and shall not be used in other cases. In this case, the Complement, ListOfTemplates, Range, BitStringMatch, HexStringMatch, OctetStringMatch, CharStringMatch, SubsetMatch and SupersetMatch productions shall not be used. \*/

ExtraMatchingAttributes ::= [StringLength](#TStringLength) |

[IfPresentKeyword](#TIfPresentKeyword) |

([StringLength](#TStringLength) [IfPresentKeyword](#TIfPresentKeyword))

BitStringMatch ::= "'" {[BinOrMatch](#TBinOrMatch)} "'" "B"

BinOrMatch ::= [Bin](#TBin) |

[AnyValue](#TAnyValue) |

[AnyOrOmit](#TAnyOrOmit)

HexStringMatch ::= "'" {[HexOrMatch](#THexOrMatch)} "'" "H"

HexOrMatch ::= [Hex](#THex) |

[AnyValue](#TAnyValue) |

[AnyOrOmit](#TAnyOrOmit)

OctetStringMatch ::= "'" {[OctOrMatch](#TOctOrMatch)} "'" "O"

OctOrMatch ::= [Oct](#TOct) |

[AnyValue](#TAnyValue) |

[AnyOrOmit](#TAnyOrOmit)

CharStringMatch ::= [PatternKeyword](#TPatternKeyword) [CaseInsenModifier] [PatternParticle](#TPatternParticle) {"&" [PatternParticle](#TPatternParticle)}

PatternParticle ::= [Pattern](#TPattern) | [ReferencedValue](#TReferencedValue)

PatternKeyword ::= "pattern"

Pattern ::= """ {[PatternElement](#TPatternElement)} """

PatternElement ::= (("\" ("?" | "\*" | "\" | "[" | "]" | "{" | "}" |

""" | "|" | "(" | ")" | "#" | "+" | "d" |

"w" | "t" | "n" | "r" | "s" | "b"

)) | ("?" | "\*" | "\" | "|" | "+"

) | ("[" ["^"] [{[PatternClassChar](#TPatternClassChar) ["-"

[PatternClassChar](#TPatternClassChar)]}]

"]") |

("{" ["\"] [ReferencedValue](#TReferencedValue) "}") | ("\" "N" "{"

([ReferencedValue](#TReferencedValue) |

[Type](#TType)) "}") |

(""" """) |

("(" [PatternElement](#TPatternElement) ")") |

("#" ([Num](#TNum) |

("(" [Number](#TNumber) "," [[Number](#TNumber)] ")") |

("(" "," [Number](#TNumber) ")") |

("(" [","] ")") [Num](#TNum) ")"

))

) | [PatternChar](#TPatternChar)

PatternChar ::= [NonSpecialPatternChar](#TNonSpecialPatternChar) | [PatternQuadruple](#TPatternQuadruple)   
  
/\* STATIC SEMANTICS: Characters "?", "\*", "\", "[", "]", "{", "}", """, "|", "(", ")", "#", "+", "d", "^", "N" have special semantics – they are metacharacters for the definition of pattern elements – only if they follow the BNF as defined above, if not they are interpreted like normal characters \*/

NonSpecialPatternChar ::= [Char](#TChar)

PatternClassChar ::= [NonSpecialPatternClassChar](#TNonSpecialPatternClassChar) |

[PatternQuadruple](#TPatternQuadruple) |

"\" [EscapedPatternClassChar](#TEscapedPatternClassChar)

NonSpecialPatternClassChar ::= [Char](#TChar)   
  
/\* STATIC SEMANTICS: Characters "[", "-", "^", "]", "\", "q", ","have special semantics – they are metacharacters for the definition of pattern class characters – only if they follow the BNF as defined above, if not they are interpreted like normal characters \*/

EscapedPatternClassChar ::= "[" | "-" | "^" | "]"

PatternQuadruple ::= "\" "q" "(" [Number](#TNumber) "," [Number](#TNumber) "," [Number](#TNumber) ","

[Number](#TNumber) ")"

Complement ::= [ComplementKeyword](#TComplementKeyword) [ListOfTemplates](#TListOfTemplates)

ComplementKeyword ::= "complement"

ListOfTemplates ::= "(" [TemplateListItem](#TTemplateListItem) {"," [TemplateListItem](#TTemplateListItem)} ")"

TemplateListItem ::= [TemplateBody](#TTemplateBody) | [AllElementsFrom](#TAllElementsFrom)

AllElementsFrom ::= [AllKeyword](#TAllKeyword) [FromKeyword](#TFromKeyword) [TemplateBody](#TTemplateBody)

SubsetMatch ::= [SubsetKeyword](#TSubsetKeyword) [ListOfTemplates](#TListOfTemplates)

SubsetKeyword ::= "subset"

SupersetMatch ::= [SupersetKeyword](#TSupersetKeyword) [ListOfTemplates](#TListOfTemplates)

SupersetKeyword ::= "superset"

PermutationMatch ::= [PermutationKeyword](#TPermutationKeyword) [ListOfTemplates](#TListOfTemplates)   
  
/\* STATIC SEMANTICS: Restrictions on the content of TemplateBody within the ListOfTemplates are given in clause B.1.3.3. \*/

PermutationKeyword ::= "permutation"

AnyValue ::= "?"

AnyOrOmit ::= "\*"

WildcardLengthMatch ::= [LengthKeyword](#TLengthKeyword) "(" [SingleExpression](#TSingleExpression) ")"   
  
/\* STATIC SEMANTICS: SingleExpression shall evaluate to type integer \*/

IfPresentKeyword ::= "ifpresent"

PresentKeyword ::= "present"

Range ::= "(" [Bound](#TBound) ".." [Bound](#TBound) ")"

Bound ::= (["!"] [SingleExpression](#TSingleExpression)) | ([[Minus](#TMinus)] [InfinityKeyword](#TInfinityKeyword))   
  
/\* STATIC SEMANTICS - Bounds shall evaluate to types integer, charstring, universal charstring or float. In case they evaluate to types charstring or universal charstring, the string length shall be 1. infinity as lower bound and –infinity as upper bound are allowed for float types only. \*/

InfinityKeyword ::= "infinity"

TemplateInstanceAssignment ::= [Identifier](#TIdentifier) ":=" [InLineTemplate](#TInLineTemplate)   
  
/\* STATIC SEMANTICS – if a value parameter is used, the inlinein-line template shall evaluate to a value \*/

TemplateRefWithParList ::= [ExtendedIdentifier](#TExtendedIdentifier) [[TemplateActualParList](#TTemplateActualParList)]

InLineTemplate ::= [([Type](#TType) | [Signature](#TSignature)) [Colon](#TColon)] [[DerivedRefWithParList](#TDerivedRefWithParList)

[AssignmentChar](#TAssignmentChar)] [TemplateBody](#TTemplateBody)

DerivedRefWithParList ::= [ModifiesKeyword](#TModifiesKeyword) [TemplateRefWithParList](#TTemplateRefWithParList)

TemplateActualParList ::= "(" [([TemplateInstanceActualPar](#TTemplateInstanceActualPar) {"," [TemplateInstanceActualPar](#TTemplateInstanceActualPar)}) |

([TemplateInstanceAssignment](#TTemplateInstanceAssignment) {"," [TemplateInstanceAssignment](#TTemplateInstanceAssignment)})]

")"

TemplateInstanceActualPar ::= [InLineTemplate](#TInLineTemplate) | [Minus](#TMinus)   
  
/\* STATIC SEMANTICS - When the corresponding formal parameter is not of template type the TemplateInstance production shall resolve to one or more SingleExpressions \*/

TemplateOps ::= [MatchOp](#TMatchOp) | [ValueofOp](#TValueofOp)

MatchOp ::= [MatchKeyword](#TMatchKeyword) "(" [Expression](#TExpression) "," [InLineTemplate](#TInLineTemplate) ")"

MatchKeyword ::= "match"

ValueofOp ::= [ValueofKeyword](#TValueofKeyword) "(" [InLineTemplate](#TInLineTemplate) ")"

ValueofKeyword ::= "valueof"

#### A.1.6.1.4 Function definitions

FunctionDef ::= [FunctionKeyword](#TFunctionKeyword) [[DeterministicModifier](#TDeterministicModifier)] [Identifier](#TIdentifier)

"(" [[FunctionFormalParList](#TFunctionFormalParList)] ")" [[RunsOnSpec](#TRunsOnSpec)] [[MtcSpec](#TMtcSpec)]

[[SystemSpec](#TSystemSpec)] [[ReturnType](#TReturnType)] [StatementBlock](#TStatementBlock)

FunctionKeyword ::= "function"

FunctionFormalParList ::= [FunctionFormalPar](#TFunctionFormalPar) {"," [FunctionFormalPar](#TFunctionFormalPar)}

FunctionFormalPar ::= [FormalValuePar](#TFormalValuePar) |

[FormalTimerPar](#TFormalTimerPar) |

[FormalTemplatePar](#TFormalTemplatePar) |

[FormalPortPar](#TFormalPortPar)

ReturnType ::= [ReturnKeyword](#TReturnKeyword) [[TemplateKeyword](#TTemplateKeyword) | [RestrictedTemplate](#TRestrictedTemplate)]

[Type](#TType)

ReturnKeyword ::= "return"

RunsOnSpec ::= [RunsKeyword](#TRunsKeyword) [OnKeyword](#TOnKeyword) [ComponentType](#TComponentType)

RunsKeyword ::= "runs"

OnKeyword ::= "on"

MtcSpec ::= [MTCKeyword](#TMTCKeyword) [ComponentType](#TComponentType)

MTCKeyword ::= "mtc"

StatementBlock ::= "{" [[FunctionDefList](#TFunctionDefList)] [[FunctionStatementList](#TFunctionStatementList)] "}"

FunctionDefList ::= {([FunctionLocalDef](#TFunctionLocalDef) | [FunctionLocalInst](#TFunctionLocalInst)) [[WithStatement](#TWithStatement)]

[[SemiColon](#TSemiColon)]}+

FunctionStatementList ::= {[FunctionStatement](#TFunctionStatement) [[SemiColon](#TSemiColon)]}+

FunctionLocalInst ::= [VarInstance](#TVarInstance) | [TimerInstance](#TTimerInstance)

FunctionLocalDef ::= [ConstDef](#TConstDef) | [TemplateDef](#TTemplateDef)

FunctionStatement ::= [ConfigurationStatements](#TConfigurationStatements) |

[TimerStatements](#TTimerStatements) |

[CommunicationStatements](#TCommunicationStatements) |

[BasicStatements](#TBasicStatements) |

[BehaviourStatements](#TBehaviourStatements) |

[SetLocalVerdict](#TSetLocalVerdict) |

[SUTStatements](#TSUTStatements) |

[TestcaseOperation](#TTestcaseOperation)

FunctionInstance ::= [FunctionRef](#TFunctionRef) "(" [[FunctionActualParList](#TFunctionActualParList)] ")"

FunctionRef ::= [[Identifier](#TIdentifier) [Dot](#TDot)] ([Identifier](#TIdentifier) | [PreDefFunctionIdentifier](#TPreDefFunctionIdentifier))

PreDefFunctionIdentifier ::= [Identifier](#TIdentifier) [CaseInsenModifier]  
  
/\* STATIC SEMANTICS - The Identifier shall be one of the pre-definedpredefined TTCN-3 function identifiers from Annex C of ES 201 873-1. CaseInsenModifier shall be present only if [Identifier](" \l "TIdentifier) is "regexp". \*/

FunctionActualParList ::= ([FunctionActualPar](#TFunctionActualPar) {"," [FunctionActualPar](#TFunctionActualPar)}) |

([FunctionActualParAssignment](#TFunctionActualParAssignment) {"," [FunctionActualParAssignment](#TFunctionActualParAssignment)})

FunctionActualPar ::= [ArrayIdentifierRef](#TArrayIdentifierRef) |

[InLineTemplate](#TInLineTemplate) |

[ComponentRef](#TComponentRef) |

[Minus](#TMinus)   
  
/\* STATIC SEMANTICS - When the corresponding formal parameter is not of template type the TemplateInstance production shall resolve to one or more SingleExpressions i.e. equivalent to the Expression production \*/

FunctionActualParAssignment ::= [TemplateInstanceAssignment](#TTemplateInstanceAssignment) |

[ComponentRefAssignment](#TComponentRefAssignment) |

[ArrayIdentifierRefAssignment](#TArrayIdentifierRefAssignment)

ArrayIdentifierRefAssignment ::= [Identifier](#TIdentifier) ":=" [ArrayIdentifierRef](#TArrayIdentifierRef)

#### A.1.6.1.5 Signature definitions

SignatureDef ::= [SignatureKeyword](#TSignatureKeyword) [Identifier](#TIdentifier) "(" [[SignatureFormalParList](#TSignatureFormalParList)]

")" [[ReturnType](#TReturnType) | [NoBlockKeyword](#TNoBlockKeyword)] [[ExceptionSpec](#TExceptionSpec)]

SignatureKeyword ::= "signature"

SignatureFormalParList ::= [FormalValuePar](#TFormalValuePar) {"," [FormalValuePar](#TFormalValuePar)}

ExceptionSpec ::= [ExceptionKeyword](#TExceptionKeyword) "(" [TypeList](#TTypeList) ")"

ExceptionKeyword ::= "exception"

Signature ::= [ExtendedIdentifier](#TExtendedIdentifier)

NoBlockKeyword ::= "noblock"

#### A.1.6.1.6 Testcase definitions

TestcaseDef ::= [TestcaseKeyword](#TTestcaseKeyword) [Identifier](#TIdentifier) "(" [[TemplateOrValueFormalParList](#TTemplateOrValueFormalParList)]

")" [ConfigSpec](#TConfigSpec) [StatementBlock](#TStatementBlock)

TestcaseKeyword ::= "testcase"

ConfigSpec ::= [RunsOnSpec](#TRunsOnSpec) [[SystemSpec](#TSystemSpec)]

SystemSpec ::= [SystemKeyword](#TSystemKeyword) [ComponentType](#TComponentType)

SystemKeyword ::= "system"

TestcaseInstance ::= [ExecuteKeyword](#TExecuteKeyword) "(" [ExtendedIdentifier](#TExtendedIdentifier) "(" [[TestcaseActualParList](#TTestcaseActualParList)]

")" ["," ([Expression](#TExpression) | [Minus](#TMinus)) ["," [SingleExpression](#TSingleExpression)]]

")"

ExecuteKeyword ::= "execute"

TestcaseActualParList ::= ([TemplateInstanceActualPar](#TTemplateInstanceActualPar) {"," [TemplateInstanceActualPar](#TTemplateInstanceActualPar)}) |

([TemplateInstanceAssignment](#TTemplateInstanceAssignment) {"," [TemplateInstanceAssignment](#TTemplateInstanceAssignment)})   
  
/\* STATIC SEMANTICS - When the corresponding formal parameter is not of template type the TemplateInstance production shall resolve to one or more SingleExpressions i.e. equivalent to the Expression production \*/

#### A.1.6.1.7 Altstep definitions

AltstepDef ::= [AltstepKeyword](#TAltstepKeyword) [Identifier](#TIdentifier) "(" [[FunctionFormalParList](#TFunctionFormalParList)]

")" [[RunsOnSpec](#TRunsOnSpec)] [[MtcSpec](#TMtcSpec)] [[SystemSpec](#TSystemSpec)] "{" [AltstepLocalDefList](#TAltstepLocalDefList)

[AltGuardList](#TAltGuardList) "}"

AltstepKeyword ::= "altstep"

AltstepLocalDefList ::= {[AltstepLocalDef](#TAltstepLocalDef) [[WithStatement](#TWithStatement)] [[SemiColon](#TSemiColon)]}

AltstepLocalDef ::= [VarInstance](#TVarInstance) |

[TimerInstance](#TTimerInstance) |

[ConstDef](#TConstDef) |

[TemplateDef](#TTemplateDef)

AltstepInstance ::= [ExtendedIdentifier](#TExtendedIdentifier) "(" [[FunctionActualParList](#TFunctionActualParList)]

")"

#### A.1.6.1.8 Import definitions

ImportDef ::= [ImportKeyword](#TImportKeyword) [ImportFromSpec](#TImportFromSpec) ([AllWithExcepts](#TAllWithExcepts) | ("{"

[ImportSpec](#TImportSpec)

"}"))

ImportKeyword ::= "import"

AllWithExcepts ::= [AllKeyword](#TAllKeyword) [[ExceptsDef](#TExceptsDef)]

ExceptsDef ::= [ExceptKeyword](#TExceptKeyword) "{" [ExceptSpec](#TExceptSpec) "}"

ExceptKeyword ::= "except"

ExceptSpec ::= {[ExceptElement](#TExceptElement) [[SemiColon](#TSemiColon)]}

ExceptElement ::= [ExceptGroupSpec](#TExceptGroupSpec) |

[ExceptTypeDefSpec](#TExceptTypeDefSpec) |

[ExceptTemplateSpec](#TExceptTemplateSpec) |

[ExceptConstSpec](#TExceptConstSpec) |

[ExceptTestcaseSpec](#TExceptTestcaseSpec) |

[ExceptAltstepSpec](#TExceptAltstepSpec) |

[ExceptFunctionSpec](#TExceptFunctionSpec) |

[ExceptSignatureSpec](#TExceptSignatureSpec) |

[ExceptModuleParSpec](#TExceptModuleParSpec)

ExceptGroupSpec ::= [GroupKeyword](#TGroupKeyword) ([QualifiedIdentifierList](#TQualifiedIdentifierList) | [AllKeyword](#TAllKeyword))

IdentifierListOrAll ::= [IdentifierList](#TIdentifierList) | [AllKeyword](#TAllKeyword)

ExceptTypeDefSpec ::= [TypeDefKeyword](#TTypeDefKeyword) [IdentifierListOrAll](#TIdentifierListOrAll)

ExceptTemplateSpec ::= [TemplateKeyword](#TTemplateKeyword) [IdentifierListOrAll](#TIdentifierListOrAll)

ExceptConstSpec ::= [ConstKeyword](#TConstKeyword) [IdentifierListOrAll](#TIdentifierListOrAll)

ExceptTestcaseSpec ::= [TestcaseKeyword](#TTestcaseKeyword) [IdentifierListOrAll](#TIdentifierListOrAll)

ExceptAltstepSpec ::= [AltstepKeyword](#TAltstepKeyword) [IdentifierListOrAll](#TIdentifierListOrAll)

ExceptFunctionSpec ::= [FunctionKeyword](#TFunctionKeyword) [IdentifierListOrAll](#TIdentifierListOrAll)

ExceptSignatureSpec ::= [SignatureKeyword](#TSignatureKeyword) [IdentifierListOrAll](#TIdentifierListOrAll)

ExceptModuleParSpec ::= [ModuleParKeyword](#TModuleParKeyword) [IdentifierListOrAll](#TIdentifierListOrAll)

ImportSpec ::= {[ImportElement](#TImportElement) [[SemiColon](#TSemiColon)]}

ImportElement ::= [ImportGroupSpec](#TImportGroupSpec) |

[ImportTypeDefSpec](#TImportTypeDefSpec) |

[ImportTemplateSpec](#TImportTemplateSpec) |

[ImportConstSpec](#TImportConstSpec) |

[ImportTestcaseSpec](#TImportTestcaseSpec) |

[ImportAltstepSpec](#TImportAltstepSpec) |

[ImportFunctionSpec](#TImportFunctionSpec) |

[ImportSignatureSpec](#TImportSignatureSpec) |

[ImportModuleParSpec](#TImportModuleParSpec) |

[ImportImportSpec](#TImportImportSpec)

ImportFromSpec ::= [FromKeyword](#TFromKeyword) [ModuleId](#TModuleId) [[RecursiveKeyword](#TRecursiveKeyword)]

RecursiveKeyword ::= "recursive"

ImportGroupSpec ::= [GroupKeyword](#TGroupKeyword) ([GroupRefListWithExcept](#TGroupRefListWithExcept) | [AllGroupsWithExcept](#TAllGroupsWithExcept))

GroupRefListWithExcept ::= [QualifiedIdentifierWithExcept](#TQualifiedIdentifierWithExcept) {"," [QualifiedIdentifierWithExcept](#TQualifiedIdentifierWithExcept)}

AllGroupsWithExcept ::= [AllKeyword](#TAllKeyword) [[ExceptKeyword](#TExceptKeyword) [QualifiedIdentifierList](#TQualifiedIdentifierList)]

QualifiedIdentifierWithExcept ::= [QualifiedIdentifier](#TQualifiedIdentifier) [[ExceptsDef](#TExceptsDef)]

IdentifierListOrAllWithExcept ::= [IdentifierList](#TIdentifierList) | [AllWithExcept](#TAllWithExcept)

ImportTypeDefSpec ::= [TypeDefKeyword](#TTypeDefKeyword) [IdentifierListOrAllWithExcept](#TIdentifierListOrAllWithExcept)

AllWithExcept ::= [AllKeyword](#TAllKeyword) [[ExceptKeyword](#TExceptKeyword) [IdentifierList](#TIdentifierList)]

ImportTemplateSpec ::= [TemplateKeyword](#TTemplateKeyword) [IdentifierListOrAllWithExcept](#TIdentifierListOrAllWithExcept)

ImportConstSpec ::= [ConstKeyword](#TConstKeyword) [IdentifierListOrAllWithExcept](#TIdentifierListOrAllWithExcept)

ImportAltstepSpec ::= [AltstepKeyword](#TAltstepKeyword) [IdentifierListOrAllWithExcept](#TIdentifierListOrAllWithExcept)

ImportTestcaseSpec ::= [TestcaseKeyword](#TTestcaseKeyword) [IdentifierListOrAllWithExcept](#TIdentifierListOrAllWithExcept)

ImportFunctionSpec ::= [FunctionKeyword](#TFunctionKeyword) [IdentifierListOrAllWithExcept](#TIdentifierListOrAllWithExcept)

ImportSignatureSpec ::= [SignatureKeyword](#TSignatureKeyword) [IdentifierListOrAllWithExcept](#TIdentifierListOrAllWithExcept)

ImportModuleParSpec ::= [ModuleParKeyword](#TModuleParKeyword) [IdentifierListOrAllWithExcept](#TIdentifierListOrAllWithExcept)

ImportImportSpec ::= [ImportKeyword](#TImportKeyword) [AllKeyword](#TAllKeyword)

#### A.1.6.1.9 Group definitions

GroupDef ::= [GroupKeyword](#TGroupKeyword) [Identifier](#TIdentifier) "{" [[ModuleDefinitionsList](#TModuleDefinitionsList)] "}"

GroupKeyword ::= "group"

#### A.1.6.1.10 External function definitions

ExtFunctionDef ::= [ExtKeyword](#TExtKeyword) [FunctionKeyword](#TFunctionKeyword) [[DeterministicModifier](#TDeterministicModifier)]

[Identifier](#TIdentifier) "(" [[FunctionFormalParList](#TFunctionFormalParList)] ")" [[ReturnType](#TReturnType)]

ExtKeyword ::= "external"

#### A.1.6.1.11 External constant definitions

ExtConstDef ::= [ExtKeyword](#TExtKeyword) [ConstKeyword](#TConstKeyword) [Type](#TType) [IdentifierList](#TIdentifierList)

#### A.1.6.1.12 Module parameter definitions

ModuleParDef ::= [ModuleParKeyword](#TModuleParKeyword) ([ModulePar](#TModulePar) | ("{" [MultitypedModuleParList](#TMultitypedModuleParList)

"}"))

ModuleParKeyword ::= "modulepar"

MultitypedModuleParList ::= {[ModulePar](#TModulePar) [[SemiColon](#TSemiColon)]}

ModulePar ::= [Type](#TType) [ModuleParList](#TModuleParList)

ModuleParList ::= [Identifier](#TIdentifier) [[AssignmentChar](#TAssignmentChar) [ConstantExpression](#TConstantExpression)] {","

[Identifier](#TIdentifier)

[[AssignmentChar](#TAssignmentChar)

[ConstantExpression](#TConstantExpression)]}

#### A.1.6.1.13 Friend module definitions

FriendModuleDef ::= "friend" "module" [IdentifierList](#TIdentifierList) [[SemiColon](#TSemiColon)]

### A.1.6.2 Control part

ModuleControlPart ::= [ControlKeyword](#TControlKeyword) "{" [ModuleControlBody](#TModuleControlBody) "}" [[WithStatement](#TWithStatement)]

[[SemiColon](#TSemiColon)]

ControlKeyword ::= "control"

ModuleControlBody ::= [[ControlStatementOrDefList](#TControlStatementOrDefList)]

ControlStatementOrDefList ::= {[ControlStatementOrDef](#TControlStatementOrDef) [[SemiColon](#TSemiColon)]}+

ControlStatementOrDef ::= ([FunctionLocalDef](#TFunctionLocalDef) | [FunctionLocalInst](#TFunctionLocalInst)) [[WithStatement](#TWithStatement)] |

[ControlStatement](#TControlStatement)

ControlStatement ::= [TimerStatements](#TTimerStatements) |

[BasicStatements](#TBasicStatements) |

[BehaviourStatements](#TBehaviourStatements) |

[SUTStatements](#TSUTStatements) |

[StopKeyword](#TStopKeyword)

### A.1.6.3 Local definitions

#### A.1.6.3.1 Variable instantiation

VarInstance ::= [VarKeyword](#TVarKeyword) (([[LazyModifier](#TLazyModifier) | [FuzzyModifier](#TFuzzyModifier)] [Type](#TType) [VarList](#TVarList)) |

(([TemplateKeyword](#TTemplateKeyword) | [RestrictedTemplate](#TRestrictedTemplate))

[[LazyModifier](#TLazyModifier) | [FuzzyModifier](#TFuzzyModifier)] [Type](#TType) [TempVarList](#TTempVarList)))

VarList ::= [SingleVarInstance](#TSingleVarInstance) {"," [SingleVarInstance](#TSingleVarInstance)}

SingleVarInstance ::= [Identifier](#TIdentifier) [[ArrayDef](#TArrayDef)] [[AssignmentChar](#TAssignmentChar) [Expression](#TExpression)]

VarKeyword ::= "var"

TempVarList ::= [SingleTempVarInstance](#TSingleTempVarInstance) {"," [SingleTempVarInstance](#TSingleTempVarInstance)}

SingleTempVarInstance ::= [Identifier](#TIdentifier) [[ArrayDef](#TArrayDef)] [[AssignmentChar](#TAssignmentChar) [TemplateBody](#TTemplateBody)]

VariableRef ::= [Identifier](#TIdentifier) [[ExtendedFieldReference](#TExtendedFieldReference)]

#### A.1.6.3.2 Timer instantiation

TimerInstance ::= [TimerKeyword](#TTimerKeyword) [VarList](#TVarList)

TimerKeyword ::= "timer"

ArrayIdentifierRef ::= [Identifier](#TIdentifier) {[ArrayOrBitRef](#TArrayOrBitRef)}

### A.1.6.4 Operations

#### A.1.6.4.1 Component operations

ConfigurationStatements ::= [ConnectStatement](#TConnectStatement) |

[MapStatement](#TMapStatement) |

[DisconnectStatement](#TDisconnectStatement) |

[UnmapStatement](#TUnmapStatement) |

[DoneStatement](#TDoneStatement) |

[KilledStatement](#TKilledStatement) |

[StartTCStatement](#TStartTCStatement) |

[StopTCStatement](#TStopTCStatement) |

[KillTCStatement](#TKillTCStatement)

ConfigurationOps ::= [CreateOp](#TCreateOp) |

[SelfOp](#TSelfOp) |

[SystemKeyword](#TSystemKeyword) |

[MTCKeyword](#TMTCKeyword) |

[RunningOp](#TRunningOp) |

[AliveOp](#TAliveOp)

CreateOp ::= [ComponentType](#TComponentType) [Dot](#TDot) [CreateKeyword](#TCreateKeyword) ["(" ([SingleExpression](#TSingleExpression) |

[Minus](#TMinus)) ["," [SingleExpression](#TSingleExpression)]

")"] [[AliveKeyword](#TAliveKeyword)]

SelfOp ::= "self"

DoneStatement ::= [ComponentOrAny](#TComponentOrAny) [Dot](#TDot) [DoneKeyword](#TDoneKeyword) [ [PortRedirectSymbol](#TPortRedirectSymbol)

[ [ValueStoreSpec](#TValueStoreSpec) ] [ [IndexSpec](#TIndexSpec) ] ]

/\*STATIC SEMANTICS – If *[PortRedirectSymbol](#TPortRedirectSymbol)* is present, at least one of *ValueStoreSpec* and *[IndexSpec](#TIndexSpec)* shall be present\*/

ComponentOrAny ::= [ComponentOrDefaultReference](#TComponentOrDefaultReference) |

([AnyKeyword](#TAnyKeyword) ([ComponentKeyword](#TComponentKeyword) | [FromKeyword](#TFromKeyword) [VariableRef](#TVariableRef))) |

([AllKeyword](#TAllKeyword) [ComponentKeyword](#TComponentKeyword))

ValueStoreSpec ::= ValueKeyword VariableRef

IndexAssignment ::= [PortRedirectSymbol](#TPortRedirectSymbol) [IndexSpec](#TIndexSpec)

IndexSpec ::= [IndexModifier](#TIndexModifier) [ValueStoreSpec](#TValueStoreSpec)

KilledStatement ::= [ComponentOrAny](#TComponentOrAny) [Dot](#TDot) [KilledKeyword](#TKilledKeyword) [ [PortRedirectSymbol](#TPortRedirectSymbol)

[ [ValueStoreSpec](#TValueStoreSpec) ] [ [IndexSpec](#TIndexSpec)] ]

/\*STATIC SEMANTICS – If *[PortRedirectSymbol](#TPortRedirectSymbol)* is present, at least one of *ValueStoreSpec* and *[IndexSpec](#TIndexSpec)* shall be present\*/

DoneKeyword ::= "done"

KilledKeyword ::= "killed"

RunningOp ::= [ComponentOrAny](#TComponentOrAny) [Dot](#TDot) [RunningKeyword](#TRunningKeyword) [[IndexAssignment](#TIndexAssignment)]

RunningKeyword ::= "running"

AliveOp ::= [ComponentOrAny](#TComponentOrAny) [Dot](#TDot) [AliveKeyword](#TAliveKeyword) [[IndexAssignment](#TIndexAssignment)]

CreateKeyword ::= "create"

AliveKeyword ::= "alive"

ConnectStatement ::= [ConnectKeyword](#TConnectKeyword) [SingleConnectionSpec](#TSingleConnectionSpec)

ConnectKeyword ::= "connect"

SingleConnectionSpec ::= "(" [PortRef](#TPortRef) "," [PortRef](#TPortRef) ")"

PortRef ::= [ComponentRef](#TComponentRef) [Colon](#TColon) [ArrayIdentifierRef](#TArrayIdentifierRef)

ComponentRef ::= [ComponentOrDefaultReference](#TComponentOrDefaultReference) |

[SystemKeyword](#TSystemKeyword) |

[SelfOp](#TSelfOp) |

[MTCKeyword](#TMTCKeyword)

ComponentRefAssignment ::= [Identifier](#TIdentifier) ":=" [ComponentRef](#TComponentRef)

DisconnectStatement ::= [DisconnectKeyword](#TDisconnectKeyword) [[SingleConnectionSpec](#TSingleConnectionSpec) |

[AllConnectionsSpec](#TAllConnectionsSpec) |

[AllPortsSpec](#TAllPortsSpec) |

[AllCompsAllPortsSpec](#TAllCompsAllPortsSpec)

]

AllConnectionsSpec ::= "(" [PortRef](#TPortRef) ")"

AllPortsSpec ::= "(" [ComponentRef](#TComponentRef) ":" [AllKeyword](#TAllKeyword) [PortKeyword](#TPortKeyword) ")"

AllCompsAllPortsSpec ::= "(" [AllKeyword](#TAllKeyword) [ComponentKeyword](#TComponentKeyword) ":" [AllKeyword](#TAllKeyword)

[PortKeyword](#TPortKeyword) ")"

DisconnectKeyword ::= "disconnect"

MapStatement ::= [MapKeyword](#TMapKeyword) [SingleConnectionSpec](#TSingleConnectionSpec) [[ParamClause](#TParamClause)]

ParamClause ::= [ParamKeyword](#TParamKeyword) [FunctionActualParList](#TFunctionActualParList)

MapKeyword ::= "map"

UnmapStatement ::= [UnmapKeyword](#TUnmapKeyword) [[SingleConnectionSpec](#TSingleConnectionSpec) [[ParamClause](#TParamClause)] |

[AllConnectionsSpec](#TAllConnectionsSpec) [[ParamClause](#TParamClause)] |

[AllPortsSpec](#TAllPortsSpec) |

[AllCompsAllPortsSpec](#TAllCompsAllPortsSpec)

]

UnmapKeyword ::= "unmap"

StartTCStatement ::= [ComponentOrDefaultReference](#TComponentOrDefaultReference) [Dot](#TDot) [StartKeyword](#TStartKeyword)

"(" [FunctionInstance](#TFunctionInstance) ")"

StartKeyword ::= "start"

StopTCStatement ::= [StopKeyword](#TStopKeyword) | ([ComponentReferenceOrLiteral](#TComponentReferenceOrLiteral) | [AllKeyword](#TAllKeyword)

[ComponentKeyword](#TComponentKeyword)) [Dot](#TDot) [StopKeyword](#TStopKeyword)

ComponentReferenceOrLiteral ::= [ComponentOrDefaultReference](#TComponentOrDefaultReference) |

[MTCKeyword](#TMTCKeyword) |

[SelfOp](#TSelfOp)

KillTCStatement ::= [KillKeyword](#TKillKeyword) | (([ComponentReferenceOrLiteral](#TComponentReferenceOrLiteral) |

[AllKeyword](#TAllKeyword) [ComponentKeyword](#TComponentKeyword)) [Dot](#TDot)

[KillKeyword](#TKillKeyword))

ComponentOrDefaultReference ::= [VariableRef](#TVariableRef) | [FunctionInstance](#TFunctionInstance)

KillKeyword ::= "kill"

#### A.1.6.4.2 Port operations

CommunicationStatements ::= [SendStatement](#TSendStatement) |

[CallStatement](#TCallStatement) |

[ReplyStatement](#TReplyStatement) |

[RaiseStatement](#TRaiseStatement) |

[ReceiveStatement](#TReceiveStatement) |

[TriggerStatement](#TTriggerStatement) |

[GetCallStatement](#TGetCallStatement) |

[GetReplyStatement](#TGetReplyStatement) |

[CatchStatement](#TCatchStatement) |

[CheckStatement](#TCheckStatement) |

[ClearStatement](#TClearStatement) |

[StartStatement](#TStartStatement) |

[StopStatement](#TStopStatement) |

[HaltStatement](#THaltStatement) |

[CheckStateStatement](#TCheckStateStatement)

SendStatement ::= [ArrayIdentifierRef](#TArrayIdentifierRef) [Dot](#TDot) [PortSendOp](#TPortSendOp)

PortSendOp ::= [SendOpKeyword](#TSendOpKeyword) "(" [InLineTemplate](#TInLineTemplate) ")" [[ToClause](#TToClause)]

SendOpKeyword ::= "send"

ToClause ::= [ToKeyword](#TToKeyword) ([InLineTemplate](#TInLineTemplate) |

[AddressRefList](#TAddressRefList) |

[AllKeyword](#TAllKeyword) [ComponentKeyword](#TComponentKeyword)

)

AddressRefList ::= "(" [InLineTemplate](#TInLineTemplate) {"," [InLineTemplate](#TInLineTemplate)} ")"

ToKeyword ::= "to"

CallStatement ::= [ArrayIdentifierRef](#TArrayIdentifierRef) [Dot](#TDot) [PortCallOp](#TPortCallOp) [[PortCallBody](#TPortCallBody)]

PortCallOp ::= [CallOpKeyword](#TCallOpKeyword) "(" [CallParameters](#TCallParameters) ")" [[ToClause](#TToClause)]

CallOpKeyword ::= "call"

CallParameters ::= [InLineTemplate](#TInLineTemplate) ["," [CallTimerValue](#TCallTimerValue)]

CallTimerValue ::= [Expression](#TExpression) | [NowaitKeyword](#TNowaitKeyword)

NowaitKeyword ::= "nowait"

PortCallBody ::= "{" [CallBodyStatementList](#TCallBodyStatementList) "}"

CallBodyStatementList ::= {[CallBodyStatement](#TCallBodyStatement) [[SemiColon](#TSemiColon)]}+

CallBodyStatement ::= [CallBodyGuard](#TCallBodyGuard) [StatementBlock](#TStatementBlock)

CallBodyGuard ::= [AltGuardChar](#TAltGuardChar) [CallBodyOps](#TCallBodyOps)

CallBodyOps ::= [GetReplyStatement](#TGetReplyStatement) | [CatchStatement](#TCatchStatement)

ReplyStatement ::= [ArrayIdentifierRef](#TArrayIdentifierRef) [Dot](#TDot) [PortReplyOp](#TPortReplyOp)

PortReplyOp ::= [ReplyKeyword](#TReplyKeyword) "(" [InLineTemplate](#TInLineTemplate) [[ReplyValue](#TReplyValue)] ")" [[ToClause](#TToClause)]

ReplyKeyword ::= "reply"

ReplyValue ::= [ValueKeyword](#TValueKeyword) [Expression](#TExpression)

RaiseStatement ::= [ArrayIdentifierRef](#TArrayIdentifierRef) [Dot](#TDot) [PortRaiseOp](#TPortRaiseOp)

PortRaiseOp ::= [RaiseKeyword](#TRaiseKeyword) "(" [Signature](#TSignature) "," [InLineTemplate](#TInLineTemplate) ")"

[[ToClause](#TToClause)]

RaiseKeyword ::= "raise"

ReceiveStatement ::= [PortOrAny](#TPortOrAny) [Dot](#TDot) [PortReceiveOp](#TPortReceiveOp)

PortOrAny ::= [ArrayIdentifierRef](#TArrayIdentifierRef) | ([AnyKeyword](#TAnyKeyword) ([PortKeyword](#TPortKeyword) | [FromKeyword](#TFromKeyword)

[VariableRef](#TVariableRef)))

PortReceiveOp ::= [ReceiveOpKeyword](#TReceiveOpKeyword) ["(" [InLineTemplate](#TInLineTemplate) ")"] [[FromClause](#TFromClause)]

[[PortRedirect](#TPortRedirect)]

ReceiveOpKeyword ::= "receive"

FromClause ::= [FromKeyword](#TFromKeyword) ([InLineTemplate](#TInLineTemplate) |

[AddressRefList](#TAddressRefList) |

[AnyKeyword](#TAnyKeyword) [ComponentKeyword](#TComponentKeyword)

)

FromKeyword ::= "from"

PortRedirect ::= [PortRedirectSymbol](#TPortRedirectSymbol) (([ValueSpec](#TValueSpec) [[SenderSpec](#TSenderSpec)] [[IndexSpec](#TIndexSpec)]) |

([SenderSpec](#TSenderSpec) [[IndexSpec](#TIndexSpec)]) |

[IndexSpec](#TIndexSpec)

)

PortRedirectSymbol ::= "->"

ValueSpec ::= [ValueKeyword](#TValueKeyword) ([VariableRef](#TVariableRef) | ("(" [SingleValueSpec](#TSingleValueSpec) {"," [SingleValueSpec](#TSingleValueSpec)} ")"))

SingleValueSpec ::= [VariableRef](#TVariableRef) [[AssignmentChar](#TAssignmentChar) [ DecodedModifier ["(" Expression] ")"] ]  
 [FieldReference](#TFieldReference) [ExtendedFieldReference](#TExtendedFieldReference)]   
  
/\*STATIC SEMANTICS – FieldReference shall not be ParRef and ExtendedFieldReference shall not be TypeDefIdentifier\*/

ValueKeyword ::= "value"

SenderSpec ::= [SenderKeyword](#TSenderKeyword) [VariableRef](#TVariableRef)

SenderKeyword ::= "sender"

TriggerStatement ::= [PortOrAny](#TPortOrAny) [Dot](#TDot) [PortTriggerOp](#TPortTriggerOp)

PortTriggerOp ::= [TriggerOpKeyword](#TTriggerOpKeyword) ["(" [InLineTemplate](#TInLineTemplate) ")"] [[FromClause](#TFromClause)]

[[PortRedirect](#TPortRedirect)]

TriggerOpKeyword ::= "trigger"

GetCallStatement ::= [PortOrAny](#TPortOrAny) [Dot](#TDot) [PortGetCallOp](#TPortGetCallOp)

PortGetCallOp ::= [GetCallOpKeyword](#TGetCallOpKeyword) ["(" [InLineTemplate](#TInLineTemplate) ")"] [[FromClause](#TFromClause)]

[[PortRedirectWithParam](#TPortRedirectWithParam)]

GetCallOpKeyword ::= "getcall"

PortRedirectWithParam ::= [PortRedirectSymbol](#TPortRedirectSymbol) [RedirectWithParamSpec](#TRedirectWithParamSpec)

RedirectWithParamSpec ::= ([ParamSpec](#TParamSpec) [[SenderSpec](#TSenderSpec)] [[IndexSpec](#TIndexSpec)]) |

([SenderSpec](#TSenderSpec) [[IndexSpec](#TIndexSpec)]) |

[IndexSpec](#TIndexSpec)

ParamSpec ::= [ParamKeyword](#TParamKeyword) [ParamAssignmentList](#TParamAssignmentList)

ParamKeyword ::= "param"

ParamAssignmentList ::= "(" ([AssignmentList](#TAssignmentList) | [VariableList](#TVariableList)) ")"

AssignmentList ::= [VariableAssignment](#TVariableAssignment) {"," [VariableAssignment](#TVariableAssignment)}

VariableAssignment ::= [VariableRef](#TVariableRef) [AssignmentChar](#TAssignmentChar) [ DecodedModifier ["(" Expression] ")"]  
 [Identifier](#TIdentifier)

VariableList ::= [VariableEntry](#TVariableEntry) {"," [VariableEntry](#TVariableEntry)}

VariableEntry ::= [VariableRef](#TVariableRef) | [Minus](#TMinus)

GetReplyStatement ::= [PortOrAny](#TPortOrAny) [Dot](#TDot) [PortGetReplyOp](#TPortGetReplyOp)

PortGetReplyOp ::= [GetReplyOpKeyword](#TGetReplyOpKeyword) ["(" [InLineTemplate](#TInLineTemplate) [[ValueMatchSpec](#TValueMatchSpec)]

")"] [[FromClause](#TFromClause)] [[PortRedirectWithValueAndParam](#TPortRedirectWithValueAndParam)]

PortRedirectWithValueAndParam ::= [PortRedirectSymbol](#TPortRedirectSymbol) [RedirectWithValueAndParamSpec](#TRedirectWithValueAndParamSpec)

RedirectWithValueAndParamSpec ::= ([ValueSpec](#TValueSpec) [[ParamSpec](#TParamSpec)] [[SenderSpec](#TSenderSpec)]

[[IndexSpec](#TIndexSpec)]) | [RedirectWithParamSpec](#TRedirectWithParamSpec)

GetReplyOpKeyword ::= "getreply"

ValueMatchSpec ::= [ValueKeyword](#TValueKeyword) [InLineTemplate](#TInLineTemplate)

CheckStatement ::= [PortOrAny](#TPortOrAny) [Dot](#TDot) [PortCheckOp](#TPortCheckOp)

PortCheckOp ::= [CheckOpKeyword](#TCheckOpKeyword) ["(" [CheckParameter](#TCheckParameter) ")"]

CheckOpKeyword ::= "check"

CheckParameter ::= [CheckPortOpsPresent](#TCheckPortOpsPresent) |

[FromClausePresent](#TFromClausePresent) |

[RedirectPresent](#TRedirectPresent)

FromClausePresent ::= [FromClause](#TFromClause) [[PortRedirectSymbol](#TPortRedirectSymbol) (([SenderSpec](#TSenderSpec)

[[IndexSpec](#TIndexSpec)]) |

[IndexSpec](#TIndexSpec))]

RedirectPresent ::= [PortRedirectSymbol](#TPortRedirectSymbol) (([SenderSpec](#TSenderSpec) [[IndexSpec](#TIndexSpec)]) |

[IndexSpec](#TIndexSpec))

CheckPortOpsPresent ::= [PortReceiveOp](#TPortReceiveOp) |

[PortGetCallOp](#TPortGetCallOp) |

[PortGetReplyOp](#TPortGetReplyOp) |

[PortCatchOp](#TPortCatchOp)

CatchStatement ::= [PortOrAny](#TPortOrAny) [Dot](#TDot) [PortCatchOp](#TPortCatchOp)

PortCatchOp ::= [CatchOpKeyword](#TCatchOpKeyword) ["(" [CatchOpParameter](#TCatchOpParameter) ")"] [[FromClause](#TFromClause)]

[[PortRedirect](#TPortRedirect)]

CatchOpKeyword ::= "catch"

CatchOpParameter ::= [Signature](#TSignature) "," [InLineTemplate](#TInLineTemplate) | [TimeoutKeyword](#TTimeoutKeyword)

ClearStatement ::= [PortOrAll](#TPortOrAll) [Dot](#TDot) [ClearOpKeyword](#TClearOpKeyword)

PortOrAll ::= [ArrayIdentifierRef](#TArrayIdentifierRef) | [AllKeyword](#TAllKeyword) [PortKeyword](#TPortKeyword)

ClearOpKeyword ::= "clear"

StartStatement ::= [PortOrAll](#TPortOrAll) [Dot](#TDot) [StartKeyword](#TStartKeyword)

StopStatement ::= [PortOrAll](#TPortOrAll) [Dot](#TDot) [StopKeyword](#TStopKeyword)

StopKeyword ::= "stop"

HaltStatement ::= [PortOrAll](#TPortOrAll) [Dot](#TDot) [HaltKeyword](#THaltKeyword)

HaltKeyword ::= "halt"

AnyKeyword ::= "any"

CheckStateStatement ::= [PortOrAllAny](#TPortOrAllAny) [Dot](#TDot) [CheckStateKeyword](#TCheckStateKeyword) "(" [SingleExpression](#TSingleExpression)

")"

PortOrAllAny ::= [PortOrAll](#TPortOrAll) | [AnyKeyword](#TAnyKeyword) [PortKeyword](#TPortKeyword)

CheckStateKeyword ::= "checkstate"

#### A.1.6.4.3 Timer operations

TimerStatements ::= [StartTimerStatement](#TStartTimerStatement) |

[StopTimerStatement](#TStopTimerStatement) |

[TimeoutStatement](#TTimeoutStatement)

TimerOps ::= [ReadTimerOp](#TReadTimerOp) | [RunningTimerOp](#TRunningTimerOp)

StartTimerStatement ::= [ArrayIdentifierRef](#TArrayIdentifierRef) [Dot](#TDot) [StartKeyword](#TStartKeyword) ["(" [Expression](#TExpression)

")"]

StopTimerStatement ::= [TimerRefOrAll](#TTimerRefOrAll) [Dot](#TDot) [StopKeyword](#TStopKeyword)

TimerRefOrAll ::= [ArrayIdentifierRef](#TArrayIdentifierRef) | [AllKeyword](#TAllKeyword) [TimerKeyword](#TTimerKeyword)

ReadTimerOp ::= [ArrayIdentifierRef](#TArrayIdentifierRef) [Dot](#TDot) [ReadKeyword](#TReadKeyword)

ReadKeyword ::= "read"

RunningTimerOp ::= [TimerRefOrAny](#TTimerRefOrAny) [Dot](#TDot) [RunningKeyword](#TRunningKeyword) [[IndexAssignment](#TIndexAssignment)]

TimeoutStatement ::= [TimerRefOrAny](#TTimerRefOrAny) [Dot](#TDot) [TimeoutKeyword](#TTimeoutKeyword) [[IndexAssignment](#TIndexAssignment)]

TimerRefOrAny ::= [ArrayIdentifierRef](#TArrayIdentifierRef) |

([AnyKeyword](#TAnyKeyword) [TimerKeyword](#TTimerKeyword)) |

([AnyKeyword](#TAnyKeyword) [FromKeyword](#TFromKeyword) [Identifier](#TIdentifier))

TimeoutKeyword ::= "timeout"

#### A.1.6.4.4 Testcase operation

TestcaseOperation ::= [TestcaseKeyword](#TTestcaseKeyword) "." [StopKeyword](#TStopKeyword) ["(" {([FreeText](#TFreeText) |

[InLineTemplate](#TInLineTemplate))

[","]}

")"]

### A.1.6.5 Type

Type ::= [PredefinedType](#TPredefinedType) | [ReferencedType](#TReferencedType)

PredefinedType ::= [BitStringKeyword](#TBitStringKeyword) |

[BooleanKeyword](#TBooleanKeyword) |

[CharStringKeyword](#TCharStringKeyword) |

[UniversalCharString](#TUniversalCharString) |

[IntegerKeyword](#TIntegerKeyword) |

[OctetStringKeyword](#TOctetStringKeyword) |

[HexStringKeyword](#THexStringKeyword) |

[VerdictTypeKeyword](#TVerdictTypeKeyword) |

[FloatKeyword](#TFloatKeyword) |

[AddressKeyword](#TAddressKeyword) |

[DefaultKeyword](#TDefaultKeyword) |

[AnyTypeKeyword](#TAnyTypeKeyword)

BitStringKeyword ::= "bitstring"

BooleanKeyword ::= "boolean"

IntegerKeyword ::= "integer"

OctetStringKeyword ::= "octetstring"

HexStringKeyword ::= "hexstring"

VerdictTypeKeyword ::= "verdicttype"

FloatKeyword ::= "float"

AddressKeyword ::= "address"

DefaultKeyword ::= "default"

AnyTypeKeyword ::= "anytype"

CharStringKeyword ::= "charstring"

UniversalCharString ::= [UniversalKeyword](#TUniversalKeyword) [CharStringKeyword](#TCharStringKeyword)

UniversalKeyword ::= "universal"

ReferencedType ::= [ExtendedIdentifier](#TExtendedIdentifier) [[ExtendedFieldReference](#TExtendedFieldReference)]

TypeReference ::= [Identifier](#TIdentifier)

ArrayDef ::= {"[" [SingleExpression](#TSingleExpression) [".." [SingleExpression](#TSingleExpression)] "]"}+   
  
/\* STATIC SEMANTICS - ArrayBounds will resolve to a non negative value of integer type \*/

### A.1.6.6 Value

Value ::= [PredefinedValue](#TPredefinedValue) | [ReferencedValue](#TReferencedValue)

PredefinedValue ::= [Bstring](#TBstring) |

[BooleanValue](#TBooleanValue) |

[CharStringValue](#TCharStringValue) |

[Number](#TNumber) | /\* IntegerValue \*/

[Ostring](#TOstring) |

[Hstring](#THstring) |

[VerdictTypeValue](#TVerdictTypeValue) |

[Identifier](#TIdentifier) | /\* EnumeratedValue \*/

[FloatValue](#TFloatValue) |

[AddressValue](#TAddressValue) |

[OmitKeyword](#TOmitKeyword)

BooleanValue ::= "true" | "false"

VerdictTypeValue ::= "pass" |

"fail" |

"inconc" |

"none" |

"error"

CharStringValue ::= [Cstring](#TCstring) | [Quadruple](#TQuadruple) | USIlikeNotation

Quadruple ::= [CharKeyword](#TCharKeyword) "(" [Number](#TNumber) "," [Number](#TNumber) "," [Number](#TNumber) "," [Number](#TNumber) ")"

USIlikeNotation ::= [CharKeyword](#TCharKeyword) "(" UIDlike { "," [UID](#TNumber)like } ")"

UIDlike ::= (U|u) {"+"} {Hex}#(1,8)

CharKeyword ::= "char"

FloatValue ::= [FloatDotNotation](#TFloatDotNotation) |

[FloatENotation](#TFloatENotation) |

[NaNKeyword](#TNaNKeyword)

NaNKeyword ::= "not\_a\_number"

FloatDotNotation ::= [Number](#TNumber) [Dot](#TDot) [DecimalNumber](#TDecimalNumber)

FloatENotation ::= [Number](#TNumber) [[Dot](#TDot) [DecimalNumber](#TDecimalNumber)] [Exponential](#TExponential) [[Minus](#TMinus)]

[Number](#TNumber)

Exponential ::= "E"

ReferencedValue ::= [ExtendedIdentifier](#TExtendedIdentifier) [[ExtendedFieldReference](#TExtendedFieldReference)]

Number ::= ([NonZeroNum](#TNonZeroNum) {[Num](#TNum)}) | "0"

NonZeroNum ::= "1" | "2" | "3" | "4" | "5" | "6" | "7" | "8" | "9"

DecimalNumber ::= {[Num](#TNum)}+

Num ::= "0" | [NonZeroNum](#TNonZeroNum)

Bstring ::= "'" {[Bin](#TBin)} "'" "B"

Bin ::= "0" | "1"

Hstring ::= "'" {[Hex](#THex)} "'" "H"

Hex ::= [Num](#TNum) | "A" | "B" | "C" | "D" | "E" | "F" | "a" | "b" | "c" |

"d" | "e" | "f"

Ostring ::= "'" {[Oct](#TOct)} "'" "O"

Oct ::= [Hex](#THex) [Hex](#THex)

Cstring ::= """ {[Char](#TChar)} """

Char ::= /\* REFERENCE - A character defined by the relevant CharacterString type. For charstring a character from the character set defined in ITU-T T.50. For universal charstring a character from any character set defined in ISO/IEC 10646 \*/

Identifier ::= [Alpha](#TAlpha) {[AlphaNum](#TAlphaNum) | [Underscore](#TUnderscore)}

Alpha ::= [UpperAlpha](#TUpperAlpha) | [LowerAlpha](#TLowerAlpha)

AlphaNum ::= [Alpha](#TAlpha) | [Num](#TNum)

UpperAlpha ::= "A" | "B" | "C" | "D" | "E" | "F" | "G" | "H" | "I" |

"J" | "K" | "L" | "M" | "N" | "O" | "P" | "Q" | "R" |

"S" | "T" | "U" | "V" | "W" | "X" | "Y" | "Z"

LowerAlpha ::= "a" | "b" | "c" | "d" | "e" | "f" | "g" | "h" | "i" |

"j" | "k" | "l" | "m" | "n" | "o" | "p" | "q" | "r" |

"s" | "t" | "u" | "v" | "w" | "x" | "y" | "z"

ExtendedAlphaNum ::= /\* REFERENCE - A graphical character from the BASIC LATIN or from the LATIN-1 SUPPLEMENT character sets defined in ISO/IEC 10646 (characters from char (0,0,0,32) to char (0,0,0,126), from char (0,0,0,161) to char (0,0,0,172) and from char (0,0,0,174) to char (0,0,0,255) \*/

FreeText ::= """ {[ExtendedAlphaNum](#TExtendedAlphaNum)} """

AddressValue ::= "null"

OmitKeyword ::= "omit"

### A.1.6.7 Parameterization

InParKeyword ::= "in"

OutParKeyword ::= "out"

InOutParKeyword ::= "inout"

FormalValuePar ::= [([InParKeyword](#TInParKeyword) |

[InOutParKeyword](#TInOutParKeyword) |

[OutParKeyword](#TOutParKeyword)

)] [[LazyModifier](#TLazyModifier) | [FuzzyModifier](#TFuzzyModifier)] [Type](#TType) [Identifier](#TIdentifier)

[":=" ([Expression](#TExpression) | [Minus](#TMinus))]

FormalPortPar ::= [[InOutParKeyword](#TInOutParKeyword)] [Identifier](#TIdentifier) [Identifier](#TIdentifier)   
  
/\* The first Identifier refers to the port type. The second Identifier refers to the port parameter identifier \*/

FormalTimerPar ::= [[InOutParKeyword](#TInOutParKeyword)] [TimerKeyword](#TTimerKeyword) [Identifier](#TIdentifier)

FormalTemplatePar ::= [([InParKeyword](#TInParKeyword) |

[OutParKeyword](#TOutParKeyword) |

[InOutParKeyword](#TInOutParKeyword)

)] ([TemplateKeyword](#TTemplateKeyword) | [RestrictedTemplate](#TRestrictedTemplate)) [[LazyModifier](#TLazyModifier) |

[FuzzyModifier](#TFuzzyModifier)]

[Type](#TType) [Identifier](#TIdentifier) [":=" ([InLineTemplate](#TInLineTemplate) | [Minus](#TMinus))]

RestrictedTemplate ::= [OmitKeyword](#TOmitKeyword) | ([TemplateKeyword](#TTemplateKeyword) [TemplateRestriction](#TTemplateRestriction))

TemplateRestriction ::= "(" ([OmitKeyword](#TOmitKeyword) |

[ValueKeyword](#TValueKeyword) |

[PresentKeyword](#TPresentKeyword)

) ")"

### A.1.6.8 Statements

#### A.1.6.8.1 With statement

WithStatement ::= [WithKeyword](#TWithKeyword) [WithAttribList](#TWithAttribList)

WithKeyword ::= "with"

WithAttribList ::= "{" [MultiWithAttrib](#TMultiWithAttrib) "}"

MultiWithAttrib ::= {[SingleWithAttrib](#TSingleWithAttrib) [[SemiColon](#TSemiColon)]}

SingleWithAttrib ::= [AttribKeyword](#TAttribKeyword) [[OverrideKeyword](#TOverrideKeyword)] [[AttribQualifier](#TAttribQualifier)]

[FreeText](#TFreeText)

AttribKeyword ::= [EncodeKeyword](#TEncodeKeyword) |

[VariantKeyword](#TVariantKeyword) |

[DisplayKeyword](#TDisplayKeyword) |

[ExtensionKeyword](#TExtensionKeyword) |

[OptionalKeyword](#TOptionalKeyword)

EncodeKeyword ::= "encode"

VariantKeyword ::= "variant"

DisplayKeyword ::= "display"

ExtensionKeyword ::= "extension"

OverrideKeyword ::= "override"

AttribQualifier ::= "(" [DefOrFieldRefList](#TDefOrFieldRefList) ")"

DefOrFieldRefList ::= [DefOrFieldRef](#TDefOrFieldRef) {"," [DefOrFieldRef](#TDefOrFieldRef)}

DefOrFieldRef ::= [QualifiedIdentifier](#TQualifiedIdentifier) |

(([FieldReference](#TFieldReference) | "[" [Minus](#TMinus) "]") [[ExtendedFieldReference](#TExtendedFieldReference)]) |

[AllRef](#TAllRef)

QualifiedIdentifier ::= {[Identifier](#TIdentifier) [Dot](#TDot)} [Identifier](#TIdentifier)

AllRef ::= ([GroupKeyword](#TGroupKeyword) [AllKeyword](#TAllKeyword) [[ExceptKeyword](#TExceptKeyword) "{" [QualifiedIdentifierList](#TQualifiedIdentifierList)

"}"]) | (([TypeDefKeyword](#TTypeDefKeyword) |

[TemplateKeyword](#TTemplateKeyword) |

[ConstKeyword](#TConstKeyword) |

[AltstepKeyword](#TAltstepKeyword) |

[TestcaseKeyword](#TTestcaseKeyword) |

[FunctionKeyword](#TFunctionKeyword) |

[SignatureKeyword](#TSignatureKeyword) |

[ModuleParKeyword](#TModuleParKeyword)

) [AllKeyword](#TAllKeyword) [[ExceptKeyword](#TExceptKeyword)

"{" [IdentifierList](#TIdentifierList)

"}"])

#### A.1.6.8.2 Behaviour statements

BehaviourStatements ::= [TestcaseInstance](#TTestcaseInstance) |

[FunctionInstance](#TFunctionInstance) |

[ReturnStatement](#TReturnStatement) |

[AltConstruct](#TAltConstruct) |

[InterleavedConstruct](#TInterleavedConstruct) |

[LabelStatement](#TLabelStatement) |

[GotoStatement](#TGotoStatement) |

[RepeatStatement](#TRepeatStatement) |

[DeactivateStatement](#TDeactivateStatement) |

[AltstepInstance](#TAltstepInstance) |

[ActivateOp](#TActivateOp) |

[BreakStatement](#TBreakStatement) |

[ContinueStatement](#TContinueStatement)

SetLocalVerdict ::= [SetVerdictKeyword](#TSetVerdictKeyword) "(" [SingleExpression](#TSingleExpression) {"," [LogItem](#TLogItem)}

")"

SetVerdictKeyword ::= "setverdict"

GetLocalVerdict ::= "getverdict"

SUTStatements ::= [ActionKeyword](#TActionKeyword) "(" [ActionText](#TActionText) {[StringOp](#TStringOp) [ActionText](#TActionText)}

")"

ActionKeyword ::= "action"

ActionText ::= [FreeText](#TFreeText) | [Expression](#TExpression)

ReturnStatement ::= [ReturnKeyword](#TReturnKeyword) [[Expression](#TExpression) | [InLineTemplate](#TInLineTemplate)]   
  
/\* STATIC SEMANTICS - Expression shall evaluate to a value of a type compatible with the return type for functions returning a value. It shall evaluate to a value, template (literal or template instance), or a matching mechanism compatible with the return type for functions returning a template. \*/

AltConstruct ::= [AltKeyword](#TAltKeyword) "{" [AltGuardList](#TAltGuardList) "}"

AltKeyword ::= "alt"

AltGuardList ::= {[GuardStatement](#TGuardStatement) | [ElseStatement](#TElseStatement) [[SemiColon](#TSemiColon)]}

GuardStatement ::= [AltGuardChar](#TAltGuardChar) ([AltstepInstance](#TAltstepInstance) [[StatementBlock](#TStatementBlock)] |

[GuardOp](#TGuardOp) [StatementBlock](#TStatementBlock))

ElseStatement ::= "[" [ElseKeyword](#TElseKeyword) "]" [StatementBlock](#TStatementBlock)

AltGuardChar ::= "[" [[BooleanExpression](#TBooleanExpression)] "]"

GuardOp ::= [TimeoutStatement](#TTimeoutStatement) |

[ReceiveStatement](#TReceiveStatement) |

[TriggerStatement](#TTriggerStatement) |

[GetCallStatement](#TGetCallStatement) |

[CatchStatement](#TCatchStatement) |

[CheckStatement](#TCheckStatement) |

[GetReplyStatement](#TGetReplyStatement) |

[DoneStatement](#TDoneStatement) |

[KilledStatement](#TKilledStatement)

InterleavedConstruct ::= [InterleavedKeyword](#TInterleavedKeyword) "{" [InterleavedGuardList](#TInterleavedGuardList)

"}"

InterleavedKeyword ::= "interleave"

InterleavedGuardList ::= {[InterleavedGuardElement](#TInterleavedGuardElement) [[SemiColon](#TSemiColon)]}+

InterleavedGuardElement ::= [InterleavedGuard](#TInterleavedGuard) [StatementBlock](#TStatementBlock)

InterleavedGuard ::= "[" "]" [GuardOp](#TGuardOp)

LabelStatement ::= [LabelKeyword](#TLabelKeyword) [Identifier](#TIdentifier)

LabelKeyword ::= "label"

GotoStatement ::= [GotoKeyword](#TGotoKeyword) [Identifier](#TIdentifier)

GotoKeyword ::= "goto"

RepeatStatement ::= "repeat"

ActivateOp ::= [ActivateKeyword](#TActivateKeyword) "(" [AltstepInstance](#TAltstepInstance) ")"

ActivateKeyword ::= "activate"

DeactivateStatement ::= [DeactivateKeyword](#TDeactivateKeyword) ["(" [ComponentOrDefaultReference](#TComponentOrDefaultReference)

")"]

DeactivateKeyword ::= "deactivate"

BreakStatement ::= "break"

ContinueStatement ::= "continue"

#### A.1.6.8.3 Basic statements

BasicStatements ::= [Assignment](#TAssignment) |

[LogStatement](#TLogStatement) |

[LoopConstruct](#TLoopConstruct) |

[ConditionalConstruct](#TConditionalConstruct) |

[SelectCaseConstruct](#TSelectCaseConstruct) |

[StatementBlock](#TStatementBlock)

Expression ::= [SingleExpression](#TSingleExpression) | [CompoundExpression](#TCompoundExpression)

CompoundExpression ::= [FieldExpressionList](#TFieldExpressionList) | [ArrayExpression](#TArrayExpression)   
  
/\* STATIC SEMANTICS - Within CompoundExpression the ArrayExpression can be used for Arrays, record, record of and set of types. \*/

FieldExpressionList ::= "{" [FieldExpressionSpec](#TFieldExpressionSpec) {"," [FieldExpressionSpec](#TFieldExpressionSpec)}

"}"

FieldExpressionSpec ::= [FieldReference](#TFieldReference) [AssignmentChar](#TAssignmentChar) [NotUsedOrExpression](#TNotUsedOrExpression)

ArrayExpression ::= "{" [[ArrayElementExpressionList](#TArrayElementExpressionList)] "}"

ArrayElementExpressionList ::= [NotUsedOrExpression](#TNotUsedOrExpression) {"," [NotUsedOrExpression](#TNotUsedOrExpression)}

NotUsedOrExpression ::= [Expression](#TExpression) | [Minus](#TMinus)

ConstantExpression ::= [SingleExpression](#TSingleExpression) | [CompoundConstExpression](#TCompoundConstExpression)

BooleanExpression ::= [SingleExpression](#TSingleExpression)   
  
/\* STATIC SEMANTICS - BooleanExpression shall resolve to a Value of type Boolean \*/

CompoundConstExpression ::= [FieldConstExpressionList](#TFieldConstExpressionList) | [ArrayConstExpression](#TArrayConstExpression)   
  
/\* STATIC SEMANTICS - Within CompoundConstExpression the ArrayConstExpression can be used for arrays, record, record of and set of types. \*/

FieldConstExpressionList ::= "{" [FieldConstExpressionSpec](#TFieldConstExpressionSpec) {"," [FieldConstExpressionSpec](#TFieldConstExpressionSpec)}

"}"

FieldConstExpressionSpec ::= [FieldReference](#TFieldReference) [AssignmentChar](#TAssignmentChar) [ConstantExpression](#TConstantExpression)

ArrayConstExpression ::= "{" [[ArrayElementConstExpressionList](#TArrayElementConstExpressionList)] "}"

ArrayElementConstExpressionList ::= [ConstantExpression](#TConstantExpression) {"," [ConstantExpression](#TConstantExpression)}

Assignment ::= [VariableRef](#TVariableRef) [AssignmentChar](#TAssignmentChar) ([Expression](#TExpression) | [TemplateBody](#TTemplateBody))   
  
/\* STATIC SEMANTICS - The Expression on the right hand side of Assignment shall evaluate to an explicit value of a type compatible with the type of the left hand side for value variables and shall evaluate to an explicit value, template (literal or a template instance) or a matching mechanism compatible with the type of the left hand side for template variables. \*/

SingleExpression ::= [XorExpression](#TXorExpression) {"or" [XorExpression](#TXorExpression)}   
  
/\* STATIC SEMANTICS - If more than one XorExpression exists, then the XorExpressions shall evaluate to specific values of compatible types \*/

XorExpression ::= [AndExpression](#TAndExpression) {"xor" [AndExpression](#TAndExpression)}   
  
/\* STATIC SEMANTICS - If more than one AndExpression exists, then the AndExpressions shall evaluate to specific values of compatible types \*/

AndExpression ::= [NotExpression](#TNotExpression) {"and" [NotExpression](#TNotExpression)}   
  
/\* STATIC SEMANTICS - If more than one NotExpression exists, then the NotExpressions shall evaluate to specific values of compatible types \*/

NotExpression ::= ["not"] [EqualExpression](#TEqualExpression)   
  
/\* STATIC SEMANTICS - Operands of the not operator shall be of type boolean or derivatives of type Boolean. \*/

EqualExpression ::= [RelExpression](#TRelExpression) {[EqualOp](#TEqualOp) [RelExpression](#TRelExpression)}   
  
/\* STATIC SEMANTICS - If more than one RelExpression exists, then the RelExpressions shall evaluate to specific values of compatible types. If only one RelExpression exists, it shall not derive to a CompoundExpression. \*/

RelExpression ::= [ShiftExpression](#TShiftExpression) [[RelOp](#TRelOp) [ShiftExpression](#TShiftExpression)] | [CompoundExpression](#TCompoundExpression)   
  
/\* STATIC SEMANTICS - If both ShiftExpressions exist, then each ShiftExpression shall evaluate to a specific integer, Enumerated or float Value or derivatives of these types \*/

ShiftExpression ::= [BitOrExpression](#TBitOrExpression) {[ShiftOp](#TShiftOp) [BitOrExpression](#TBitOrExpression)}   
  
/\* STATIC SEMANTICS - Each Result shall resolve to a specific Value. If more than one Result exists the right-hand operand shall be of type integer or derivatives and if the shift op is "<<" or ">>" then the left-hand operand shall resolve to either bitstring, hexstring or octetstring type or derivatives of these types. If the shift op is " \*/

BitOrExpression ::= [BitXorExpression](#TBitXorExpression) {"or4b" [BitXorExpression](#TBitXorExpression)}   
  
/\* STATIC SEMANTICS - If more than one BitXorExpression exists, then the BitXorExpressions shall evaluate to specific values of compatible types \*/

BitXorExpression ::= [BitAndExpression](#TBitAndExpression) {"xor4b" [BitAndExpression](#TBitAndExpression)}   
  
/\* STATIC SEMANTICS - If more than one BitAndExpression exists, then the BitAndExpressions shall evaluate to specific values of compatible types \*/

BitAndExpression ::= [BitNotExpression](#TBitNotExpression) {"and4b" [BitNotExpression](#TBitNotExpression)}   
  
/\* STATIC SEMANTICS - If more than one BitNotExpression exists, then the BitNotExpressions shall evaluate to specific values of compatible types \*/

BitNotExpression ::= ["not4b"] [AddExpression](#TAddExpression)   
  
/\* STATIC SEMANTICS - If the not4b operator exists, the operand shall be of type bitstring, octetstring or hexstring or derivatives of these types. \*/

AddExpression ::= [MulExpression](#TMulExpression) {[AddOp](#TAddOp) [MulExpression](#TMulExpression)}   
  
/\* STATIC SEMANTICS - Each MulExpression shall resolve to a specific Value. If more than one MulExpression exists and the AddOp resolves to StringOp then the MulExpressions shall be valid operands for StringOp. If more than one MulExpression exists and the AddOp does not resolve to StringOp then the MulExpression shall both resolve to type integer or float or derivatives of these types. If only one MulExpression exists, it shall not derive to a CompoundExpression. \*/

MulExpression ::= [UnaryExpression](#TUnaryExpression) {[MultiplyOp](#TMultiplyOp) [UnaryExpression](#TUnaryExpression)} | [CompoundExpression](#TCompoundExpression)   
  
/\* STATIC SEMANTICS - Each UnaryExpression shall resolve to a specific Value. If more than one UnaryExpression exists then the UnaryExpressions shall resolve to type integer or float or derivatives of these types. \*/

UnaryExpression ::= [[UnaryOp](#TUnaryOp)] [Primary](#TPrimary)   
  
/\* STATIC SEMANTICS - Primary shall resolve to a specific Value of type integer or float or derivatives of these types.\*/

Primary ::= [OpCall](#TOpCall) |

[Value](#TValue) |

"(" [SingleExpression](#TSingleExpression) ")"

ExtendedFieldReference ::= {([Dot](#TDot) ([Identifier](#TIdentifier) | [PredefinedType](#TPredefinedType))) |

[ArrayOrBitRef](#TArrayOrBitRef) |

("[" [Minus](#TMinus) "]")

}+   
  
/\* STATIC SEMANTIC - The Identifier refers to a type definition if the type of the VarInstance or ReferencedValue in which the ExtendedFieldReference is used is anytype. ArrayOrBitRef shall be used when referencing elements of values or arrays. The square brackets with dash shall be used when referencing inner types of a record of or set of type. \*/

OpCall ::= [ConfigurationOps](#TConfigurationOps) |

[GetLocalVerdict](#TGetLocalVerdict) |

[TimerOps](#TTimerOps) |

[TestcaseInstance](#TTestcaseInstance) |

([FunctionInstance](#TFunctionInstance) [[ExtendedFieldReference](#TExtendedFieldReference)]) |

([TemplateOps](#TTemplateOps) [[ExtendedFieldReference](#TExtendedFieldReference)]) |

[ActivateOp](#TActivateOp)

AddOp ::= "+" |

"-" |

[StringOp](#TStringOp)   
  
/\* STATIC SEMANTICS - Operands of the "+" or "-" operators shall be of type integer or float or derivations of integer or float (i.e. subrange) \*/

MultiplyOp ::= "\*" | "/" | "mod" | "rem"   
  
/\* STATIC SEMANTICS - Operands of the "\*", "/", rem or mod operators shall be of type integer or float or derivations of integer or float (i.e. subrange) \*/

UnaryOp ::= "+" | "-"   
  
/\* STATIC SEMANTICS - Operands of the "+" or "-" operators shall be of type integer or float or derivations of integer or float (i.e. subrange) \*/

RelOp ::= "<" | ">" | ">=" | "<="   
  
/\* STATIC SEMANTICS - the precedence of the operators is defined in Table 6 \*/

EqualOp ::= "==" | "!="

StringOp ::= "&"   
  
/\* STATIC SEMANTICS - Operands of the list operator shall be bitstring, hexstring, octetstring, (universal) character string, record of, set of, or array types, or derivates of these types \*/

ShiftOp ::= "<<" | ">>" | "<@" | "@>"

LogStatement ::= [LogKeyword](#TLogKeyword) "(" [LogItem](#TLogItem) {"," [LogItem](#TLogItem)} ")"

LogKeyword ::= "log"

LogItem ::= [FreeText](#TFreeText) | [InLineTemplate](#TInLineTemplate)

LoopConstruct ::= [ForStatement](#TForStatement) |

[WhileStatement](#TWhileStatement) |

[DoWhileStatement](#TDoWhileStatement)

ForStatement ::= [ForKeyword](#TForKeyword) "(" [Initial](#TInitial) [SemiColon](#TSemiColon) [BooleanExpression](#TBooleanExpression)

[SemiColon](#TSemiColon) [Assignment](#TAssignment) ")" [StatementBlock](#TStatementBlock)

ForKeyword ::= "for"

Initial ::= [VarInstance](#TVarInstance) | [Assignment](#TAssignment)

WhileStatement ::= [WhileKeyword](#TWhileKeyword) "(" [BooleanExpression](#TBooleanExpression) ")" [StatementBlock](#TStatementBlock)

WhileKeyword ::= "while"

DoWhileStatement ::= [DoKeyword](#TDoKeyword) [StatementBlock](#TStatementBlock) [WhileKeyword](#TWhileKeyword) "(" [BooleanExpression](#TBooleanExpression)

")"

DoKeyword ::= "do"

ConditionalConstruct ::= [IfKeyword](#TIfKeyword) "(" [BooleanExpression](#TBooleanExpression) ")" [StatementBlock](#TStatementBlock)

{[ElseIfClause](#TElseIfClause)} [[ElseClause](#TElseClause)]

IfKeyword ::= "if"

ElseIfClause ::= [ElseKeyword](#TElseKeyword) [IfKeyword](#TIfKeyword) "(" [BooleanExpression](#TBooleanExpression) ")" [StatementBlock](#TStatementBlock)

ElseKeyword ::= "else"

ElseClause ::= [ElseKeyword](#TElseKeyword) [StatementBlock](#TStatementBlock)

SelectCaseConstruct ::= [SelectKeyword](#TSelectKeyword) [[UnionKeyword](#TUnionKeyword)] "(" [SingleExpression](#TSingleExpression) ")" [SelectCaseBody](#TSelectCaseBody)

SelectKeyword ::= "select"

SelectCaseBody ::= "{" {[SelectCase](#TSelectCase)}+ "}"

SelectCase ::= [CaseKeyword](#TCaseKeyword) ("(" [InLineTemplate](#TInLineTemplate) {"," [InLineTemplate](#TInLineTemplate)}

")" | [ElseKeyword](#TElseKeyword)) [StatementBlock](#TStatementBlock)

/\*\* STATIC SEMANTICS InLineTemplate-s shall be Identifier-s if the UnionKeyword is present in the surrounding SelectCaseConstruct (see clause 19.3.2. The Select union statement)\*/

CaseKeyword ::= "case"

ExtendedIdentifier ::= [[Identifier](#TIdentifier) [Dot](#TDot)] [Identifier](#TIdentifier)

IdentifierList ::= [Identifier](#TIdentifier) {"," [Identifier](#TIdentifier)}

QualifiedIdentifierList ::= [QualifiedIdentifier](#TQualifiedIdentifier) {"," [QualifiedIdentifier](#TQualifiedIdentifier)}

### A.1.6.9 Miscellaneous productions

Dot ::= "."

Minus ::= "-"

SemiColon ::= ";"

Colon ::= ":"

Underscore ::= "\_"

AssignmentChar ::= ":="

IndexModifier ::= "@index"

DeterministicModifier ::= "@deterministic"

LazyModifier ::= "@lazy"

FuzzyModifier ::= "@fuzzy"

CaseInsenModifier ::= "@nocase"

DecodedModifier ::= "@decoded"

Annex B (normative):  
Matching values

# B.1 Template matching mechanisms

This annex specifies the matching mechanisms that may be used in TTCN‑3 templates (and only in templates).

## B.1.1 Matching specific values

Specific values are the basic matching mechanism of TTCN‑3 templates. Specific values in templates are expressions which do not contain any matching mechanisms or wildcards.

Unless otherwise specified, a template field matches the corresponding field value if, and only if, the field value has exactly the same value as the value to which the expression in the template evaluates.

***Restrictions***

No specific restrictions in addition to the general static rules of TTCN‑3 given in clause 5.

***Examples***

EXAMPLE:

// Given the message type definition

**type** **record** MyMessageType

{

**integer** field1,

**charstring** field2,

**boolean** field3 **optional,**

**integer** field4[4]

}

// A message template using specific values could be

**template** MyMessageType MyTemplate:=

{

field1 := 3+2**,** // specific value of integer type

field2 := "My string"**,** // specific value of charstring type

field3 := true**,** // specific value of boolean type

field4 := {1,2,3,4} // specific value of integer array

}

## B.1.2 Matching mechanisms instead of values

The following matching mechanisms may be used in place of explicit values.

### B.1.2.1 Template list

Template lists specify lists of acceptable values. It can be used on values of all types. A template list may also contain templates.

A template field that uses a template list matches the corresponding field if, and only if, the field value matches any one of the values or templates in the template list. Each value or template in the template list shall be of the type declared for the template field in which this mechanism is used.

Besides specifying individual values, it is also possible to add all elements of an existing **record of** or **set of** template into a template list using an **all from** clause.

***Restrictions***

a) The type of the template list and the member type of the template in the **all from** clause shall be compatible.

b) The template in the **all from** clause as a whole shall not resolve into a matching mechanism (i.e. its elements may contain any of the matching mechanisms or matching attributes with the exception of those described in the following restriction).

c) Individual fields of the template in the **all from** clause shall not resolve to any of the following matching mechanisms: AnyElementsOrNone, permutation.

d) Each value or template in the template list shall be of the type declared for the template field in which this mechanism is used.

***Examples***

EXAMPLE 1:

**template** MyMessage MyTemplate:=

{

field1 := (2,4,6)**,** // list of integer values

field2 := ("String1", "String2")**,** // list of charstring values

:

:

}

EXAMPLE 2:

**type record of integer** RoI;

**template** RoIt\_RoI1 := {1, 2, (6..9)};

**template** RoIt\_RoI2 := {1, \*, 3};

**template integer** t\_i1 := (**all from** t\_RoI1, 100);

// results in (1, 2, (6..9), 100)

**template integer** t\_i2 := (0, **all from** t\_RoI2);

// causes an error because t\_RoI2 contains AnyElementsOrNone

**template** RoI t\_RoI3 := (**all from** t\_RoI1);

// causes an error because member type of t\_RoI1 (integer)

// is not compatible with the list template type (RoI)

**template** RoI t\_RoI4 := ?;

**template** RoI t\_RoI5 := (**all from** t\_RoI4);

// causes an error, because t\_RoI4 resolves into a matching mechanism

### B.1.2.2 Complemented template list

The keyword **complement** denotes a list of values that will not be accepted as values (i.e. it is the complement of a template list). It can be used on all values of all types. A complemented value list may also contain templates.

A template field that uses complement matches the corresponding field if and only if the corresponding field’s value does not match any of the values or templates listed in the template list. The template list may be a single value, of course.

Besides specifying individual values, it is possible to add all elements of an existing **record of** or **set of** template into a complement template list using an **all from** clause.

***Restrictions***

a) The type of the complemented template list and the member type of the template in the **all from** clause shall be compatible.

b) The template in the **all from** clause as a whole shall not resolve into a matching mechanism (i.e. its elements may contain any of the matching mechanisms or matching attributes with the exception of those described in the following restriction).

c) Individual fields of the template in the **all from** clause shall not resolve to any of the following matching mechanisms: AnyElementsOrNone, permutation.

d) Each value or template in the list shall be of the type declared for the template field in which the complement is used.

e) The complement of a template list shall not match **omit**.

***Examples***

EXAMPLE 1:

**template** MyMessage MyTemplate:=

{

field1 := **complement** (1,3,5)**,** // list of unacceptable integer values

:

field3 := **not**(**true)** // will match **false**

:

}

EXAMPLE 2:

**type record of integer** RoI;

**template** RoIt\_RoI1 := {1, 2, (6..9)};

**template** RoIt\_RoI2 := {1, \*, 3};

**template integer** t\_i1 := **complement**(**all from** t\_RoI1, 100);

// results in (1, 2, (6..9), 100)

**template integer** t\_i2 := **complement**(0, **all from** t\_RoI2);

// causes an error because t\_RoI2 contains AnyElementsOrNone

**template** RoI t\_RoI3 := **complement**(**all from** t\_RoI1);

// causes an error because member type of t\_RoI1 (integer) is not compatible

// with the complemented list template type (RoI)

**template** RoI t\_RoI4 := ?;

**template** RoI t\_RoI5 := **complement** (**all from** t\_RoI4);

// causes an error because t\_RoI4 resolves into a matching mechanism

### B.1.2.3 Any value

The matching symbol "?" (*AnyValue*) matches any value of the specified type. It can be used on values of all types.

A template field that uses the any value mechanism matches the corresponding field if, and only if, the field evaluates to a single element of the specified type.

***Restrictions***

No specific restrictions in addition to the general static rules of TTCN‑3 given in clause 5.

***Examples***

EXAMPLE:

**template** MyMessage MyTemplate:=

{

field1 := ?**,** // will match any integer

field2 := ?**,** // will match any non-empty charstring value

field3 := ?**,** // will match true or false

field4 := ? // will match any sequence of integers

}

### B.1.2.4 Any value or none

The matching symbol "\*" (*AnyValueOrNone*) is used to indicate that any valid value and the omission of the given optional field are acceptable. It can be assigned to templates of any type as a whole or to optional fields of **set** or **record** templates. At the time of matching, it shall be applied to optional fields of **record** and **set** templates only.

A template field that uses this symbol matches the corresponding field if, and only if, either the field evaluates to any element of the specified type, or if the field is absent.

***Restrictions***

a) It can be assigned to templates of any type as a whole or to optional fields of **set** or **record** templates.

b) At the time of matching, it shall be applied to optional fields of record and set templates only.

***Examples***

EXAMPLE:

**type** **record** MyMessage

{

**integer** field1,

MyRecordof field2 **optional**,

**boolean** field3 **optional**

}

**template** MyMessage MyMessageTemplate:=

{

:

field3 := \* // matches true or false or omitted field3

}

**template** MyMessage MyMessageTemplate2:=

{

field1 := \***,** // causes an error as field1 is mandatory

:

}

**template** MyRecordof MyRecofTemplate := \*; // this assignment is allowed

**template** boolean MyBoolTemplate := \*; // this assignment is allowed as well

**template** MyMessage MyMessageTemplate3:=

{

field1 := 42,

field2 := MyRecofTemplate,

// matches any valid value allowed by MyRecordof of absent field2

field3 := MyBoolTemplate

// matches true or false or omitted field3

}

MybooleanVar := **match** ({},MyRecofTemplate);

// causes an error as a record of template shall not be *AnyValueOrNone*

// at the time of matching

MybooleanVar := **match** ({42,**omit**,**true**},MyMessageTemplate3);

// matches and returns true

### B.1.2.5 Value range

Ranges indicate a bounded range of acceptable values, including or excluding the boundaries.

A template field that uses a range matches the corresponding field if, and only if, the field value is equal to one of the values in the range.

***Restrictions***

a) When used for values of **integer** or **float** types (and integer or float subtypes), a boundary value shall be either:

1. infinity or -infinity;
2. an expression that evaluates to a specific integer or float value.

b) The lower boundary shall be put on the left side of the range, the upper boundary at the right side. The lower boundary shall be less than the upper boundary.

c) When used in templates or template fields of charstring or universal charstring types, the boundaries shall evaluate to valid character positions according to the coded character set table(s) of the type (e.g. the given position shall not be empty).

d) Empty positions between the lower and the upper boundaries are not considered to be valid values of the specified range.

***Examples***

EXAMPLE:

**template** MyMessage MyTemplate:=

{

field1 := (1 **..** !6), // range of integer type from 1 to 5

:

:

:

}

// other entries for field1 might be (-**infinity** to 8) or (!12 to **infinity**)

### B.1.2.6 SuperSet

SuperSet is denoted by the keyword **superset**. SuperSet matches a set of values if, and only if, the set of values contains at least all of the elements defined within the SuperSet, and may contain more. The successful match shall be produced only if there exists such a one-to-one mapping from the SuperSet elements to the elements of the set of values where each SuperSet element matches the element of set of values it is mapped to. The SuperSet matching mechanism may contain templates (including template variables) and matching mechanisms with the restrictions given below. However, the length matching attribute may be attached to the SuperSet itself.

NOTE: The SuperSet matching mechanism imposes an implicit length restriction on the matched set of values: the set of values shall contain at least as many elements as the SuperSet template in order to produce a successful match.

Besides specifying individual values, it is possible to add all elements of a **record of** or **set of** template into SuperSets using an **all from** clause.

***Restrictions***

a) SuperSet is an operation for matching that shall be used only on values of **set of** types.

b) Individual members of the SuperSet's argument shall be of the type replicated by the **set of**.

c) The member type of the set of associated with the SuperSet template and the member type of the template in the **all from** clause shall be compatible.

d) The template in the **all from** clause as a whole shall not resolve into a matching mechanism (i.e. its elements may contain any of the matching mechanisms or matching attributes with the exception of those described in the following restriction).

e) The individual members of the SuperSet's argument and the elements of the template in the **all from** clause shall not be the matching mechanisms omit, SuperSet, SubSet and the matching attributes (length restriction and ifpresent). In addition, the individual members shall not resolve to AnyValueOrNone and individual elements of the template in the **all from** clause shall not resolve to AnyElementsOrNone or permutation.

f) If the length matching attribute is attached to the SuperSet, the minimal length allowed by the length attribute shall not be less than the number of the elements in the SuperSet.

***Examples***

EXAMPLE 1:

**type set of integer** MySetOfType (0 .. 10);

**template** MySetOfType MyTemplate1 := **superset** (1, 2, 3);

// matches any sequence of integers which contains at least one occurrences of the numbers

// 1, 2 and 3 in any order and position

**template** MySetOfType MyTemplate2\_AnyValue := **superset** (1, 2, ?)**;**

// matches any sequence of integers which contains at least one occurrences of the numbers

// 1, 2 and at least one more valid integer value (i.e. between 0 and 10, inclusively), in any

// order and position

**template** MySetOfType MyTemplate3 := **superset** (1, 2, (3, 4));

// matches any sequence of integers which contains at least one occurrences of the numbers

// 1, 2 and a number with the value 3 or 4, in any order and position

**template** MySetOfType MyTemplate4 := **superset** (1, 2, **complement**(3, 4));

// any sequence of integers matches which contains at least one occurrences of the numbers

// 1, 2 and a valid integer value which is not 3 or 4, in any order and position

**template** MySetOfType MyTemplate6 := **superset** (1, 2, 3) **length** (7);

// matches any sequence of 7 integers which contains at least one occurrences of the numbers

// 1, 2 and 3 in any order and position

**template** MySetOfType MyTemplate7 := **superset** (1, 2, ?) **length** (7 .. **infinity**);

// matches any sequence of at least 7 integers which contains at least one occurrences of the

// numbers 1, 2 and 3 in any order and position

**template** MySetOfType MyTemplate8 := **superset** (1, 2, 3) **length** (2 .. 7);

// causes an error, the lower bound of the length attribute contradicts to the minimum number

// of elements imposed by the superset argument

EXAMPLE 2:

**type record of integer** RoI;

**type set of integer** SoI;

**template** RoIt\_RoI1 := {1, 2, ?};

**template** SoIt\_SoI1 := **superset**(**all from** t\_RoI1);

// results in superset(1, 2, ?)

### B.1.2.7 SubSet

SubSet is denoted by the keyword **subset**. SubSet matches a set of values if, and only if, the set of values contains only elements defined within the SubSet, and may contain less. The successful match shall be produced only if there exists such a one-to-one mapping from the elements of the set of values to the SubSet elements where each element of the set of values is matched by the SubSet element it is mapped to. The SubSet matching mechanism may contain templates (including template variables) and matching mechanisms with the restrictions given below. However, the length matching attribute may be attached to the SubSet itself.

NOTE: The SubSet matching mechanism imposes an implicit length restriction on the matched set of values: the set of values shall contain at most as many elements as the SubSet template in order to produce a successful match.

Besides specifying individual values, it is possible to add all elements of a **record of** or **set of** template into SubSets using an **all from** clause.

***Restrictions***

a) SubSet is an operation for matching that can be used only on values of **set of** types.

b) Individual members of the SubSet's argument shall be of the type replicated by the **set of**.

c) The member type of the set of type associated with the SubSet and the member type of the template in the **all from** clause shall be compatible.

d) The template in the **all from** clause as a whole shall not resolve into a matching mechanism (i.e. its elements may contain any of the matching mechanisms or matching attributes with the exception of those described in the following restriction).

e) The individual members of the SubSet's argument and the elements of the template in the **all from** clause shall not be the matching mechanisms omit, SuperSet, SubSet and the matching attributes (length restriction and ifpresent). In addition, individual members shall not resolve to AnyValueOrNone and individual fields of the template in the **all from** clause shall not resolve to AnyElementsOrNone or permutation.

f) If the length matching attribute is attached to the SubSet, the maximum length allowed by the length attribute shall not exceed the number of the elements in the SubSet.

***Examples***

EXAMPLE 1:

**template** MySetOfType MyTemplate1:= **subset** (1, 2, 3);

// matches any sequence of integers which contains zero or one occurrences of the numbers

// 1, 2 and 3 in any order and position

**template** MySetOfType MyTemplate1:= **subset** (1, 2, ?);

// matches any sequence of integers which contains zero or one occurrences of the numbers

// 1, 2 and a valid integer value (i.e. between 0 and 10, inclusive) in any order and position

**template** MySetOfType MyTemplate1:= **subset** (1, 2, (3, 4));

// matches any sequence of integers which contains zero or one occurrences of the numbers

// 1, 2 and one of the numbers 3 or 4, in any order and position

**template** MySetOfType MyTemplate1:= **subset** (1, 2, **complement** (3, 4));

// matches any sequence of integers which contains zero or one occurrences of the numbers

// 1, 2 and a valid integer number which is not 3 or 4, in any order and position

**template** MySetOfType MyTemplate1:= **subset** (1, 2, 3) **length** (2);

// matches any sequence of two integers which contains zero or one occurrences of

// the numbers 1, 2 and 3, in any order and position

**template** MySetOfType MyTemplate1:= **subset** (1, 2, ?) **length** (0 .. 2);

// matches any sequence of zero, one or two integers which contains zero or one occurrences of

// the numbers 1, 2 and of a valid integer value, in any order and position

**template** MySetOfType MyTemplate1:= **subset** (1, 2, 3) **length** (0 .. 4);

// causes an error, the upper bound of length attribute contradicts to the maximum number of

// elements imposed by the subset argument

EXAMPLE 2:

**type record of integer** RoI;

**type set of integer** SoI;

**template** RoIt\_RoI1 := {1, 2, ?};

**template** SoIt\_SoI1 := **subset**(**all from** t\_RoI1);

// results in subset(1, 2, ?)

### B.1.2.8 Omitting optional fields

The keyword **omit** denotes that an optional field shall be absent. If used as a matching mechanism, it matches an optional field if and only if it is absent.

***Restrictions***

a) It can be assigned to templates of any type as a whole or to optional fields of **set** or **record** templates.

b) At the time of matching, it shall be applied to optional fields of **record** and **set** templates only.

***Examples***

EXAMPLE:

**type** **record** MyMessage

{

**integer** field1,

MyRecordof field2 **optional**,

**boolean** field3 **optional**

}

**template** MyMessage MyMessageTemplate:=

{

:

field3 := **omit** // omits the optional field field3

}

**template** MyMessage MyMessageTemplate2:=

{

field1 := **omit,** // causes an error as field1 is mandatory

:

}

**template** MyRecordof MyRecofTemplate := **omit;** // this assignment is allowed

**template** **boolean** MyBoolTemplate := **omit;** // this assignment is allowed as well

**template** MyMessage MyMessageTemplate3:=

{

field1 := 42,

field2 := MyRecofTemplate,

// matches if field2 is absent

field3 := MyBoolTemplate

// matches if field3 is absent

}

MybooleanVar := **match** ({},MyRecofTemplate)

// causes an error as a record of template shall not be "omit"at the time of matching

MybooleanVar := **match** ({42,**omit**,**omit**},MyMessageTemplate3)

// matches and returns true

### B.1.2.9 Matching decoded content

The matching symbol *MatchDecodedContent* **decmatch**is used for checking encoded payload fields. The matching symbol is composed of the **decmatch** ~~modifier~~ keyword, an optional encoding format parameter and a mandatory template instance called decoding target.

A template field that uses this symbol matches the corresponding field if, and only if, the field can be successfully decoded as an instance of the same type as the decoding target and if the decoded instance can be successfully matched by the decoding target.

The optional encoding format parameter may specify one of the UCS encoding formats (see clause C.5.4) that shall be used for the decoding trial, i.e. it overrides any variant attribute attached to the decoding target or the type of the decoding target (for example, for predefined variant attributes see clause 27.5).

***Restrictions***

a) It can be assigned to templates and template fields of **bitstring**, **hexstring**, **octetstring**, **charstring** and **universal** **charstring** types.

b) The decoding target can be a template of any data type.

c) The optional encoding format parameter can be used only for fields of r **universal** **charstring** types. The parameter value shall be of the **charstring** type and it shall contain one of the strings allowed for the **decvalue\_unichar** predefined function (specified in clause C.5.4). Any other value shall cause an error.

d) If the template field is of **charstring** type or is of **universal charstring** type and the encoding format is missing, the default value "UTF-8" shall be used.

NOTE: The model of the behaviour of this implicit decoding is the following. At first, **hexstring** and **octetstring** values are implicitly converted to a **bitstring** value using the predefined **hex2bit** and **oct2bit** functions (specified in C.1.18 and C.1.22) and **charstring** values are implicitly converted to **universal charstring** values. Prior to decoding, the **bitstring** and **universal charstring** values are stored into a temporary anonymous variable. Decoding is then performed by implicitly calling the predefined **decvalue** function (specified in C.5.2) for **bitstring** values and **decvalue\_unichar** function for **universal charstring** values. The anonymous variable containing the encoded value is passed as the first parameter to the function, the second parameter contains another temporary variable called decoded instance. The decoded instance is of the same type as the decoding target. If the optional encoding format parameter is present, it is passed as the third parameter to the **decvalue\_unichar** function. Decoding is successful only if the decoding function returns 0 and the first parameter contains an empty string (i.e. the whole encoded value has been successfully decoded). The matching mechanism will generate an unsuccessful match if decoding hasn’t succeeded.

***Examples***

EXAMPLE:

**type** **record** MyBinaryMessage

{

**...**,

**octetstring** payload

}

**type** **record** MyTextMessage

{

**...**,

**universal charstring** payload

}

**type** **record** MyPayload

{

**integer** field1,

**integer** field2

}

**template** MyBinaryMessage mw\_t1 :=

{

:

// The payload field can be matched only if it contains an encoded value of the MyPayload

// type and if the field1 of the decoded value is equal to 1.

payload := **decmatch** MyPayload:{field1 := 1, field2 := ? }

}

**template** MyTextMessage mw\_t2 :=

{

:

// The payload field can be matched only if it contains an encoded value of the MyPayload

// type in the UTF-8 format and if the field1 of the decoded value is equal to 2 or 3.

payload := **decmatch**("UTF-8") MyPayload:{field1 := (2, 3), field2 := ? }

}

## B.1.3 Matching mechanisms inside values

The following matching mechanisms may be used inside explicit values of strings, records, records of, sets, sets of and arrays.

### B.1.3.1 Any element

The matching symbol "?" (*AnyElement*) is used to indicate that it replaces single elements of a string (except character strings, see table 4 for the lengths of the units being matched by "?" in a string), a **record of**, a **set of** or an array.

***Restrictions***

a) It shall be used only within values of string types, **record of** types, **set of** types and arrays.

***Examples***

EXAMPLE:

**template** MyMessage MyTemplate:=

{ :

field2 := "abcxyz",

field3 := '10???'B, // where each "?" may either be 0 or 1

field4 := {1, ?, 3} // where ? may be any integer value

}

NOTE: The "?" in field4 can be interpreted as *AnyValue* as an integervalue, or *AnyElement* inside a **record of, set of** or array. Since both interpretations lead to the same match no problem arises.

#### B.1.3.1.1 Using single character wildcards

If it is required to express the "?" wildcard in character strings it shall be done using character patterns (see clause B.1.5). For example: "abcdxyz", "abccxyz", "abcxxyz" etc. will all match **pattern** "abc?xyz". However, "abcxyz", "abcdefxyz", etc. will not.

### B.1.3.2 Any number of elements or no element

The matching symbol "\*" (*AnyElementsOrNone*) is used to indicate that it replaces none or any number of consecutive elements of a string (except character strings), a **record of**, a **set of** or an array. The "\*" symbol matches the longest sequence of elements possible, according to the pattern as specified by the symbols surrounding the "\*".

If a "\*" appears at the highest level inside a string, a **record of**, **set of** or array, it shall be interpreted as *AnyElementsOrNone*.

NOTE: This rule prevents the otherwise possible interpretation of "\*" as *AnyValueOrNone* that replaces an element inside a string, **record of**, **set of** or array.

***Restrictions***

a) It shall be used only within values of string types, **record of** types, **set of** types and arrays and inside the permutation matching mechanism.

***Examples***

EXAMPLE:

**template** Mymessage MyTemplate:=

{ :

field2 := "abcxyz",

field3 := '10\*11'B, // where "\*" may be any sequence of bits (possibly empty)

field4 := {\*, 2, 3} // where "\*"may be any number of integer values or omitted

}

**var charstring** MyStrings[4];

MyPCO.**receive**(MyStrings:{"abyz", \*, "abc" });

#### B.1.3.2.1 Using multiple character wildcards

If it is required to expressed the "\*" wildcard in character strings it shall be done using character patterns (see clause B.1.5). For example: "abcxyz", "abcdefxyz" "abcabcxyz" etc. will all match **pattern** "abc\*xyz".

### B.1.3.3 Permutation

Permutation is an operation for matching that shall be used only on values of **record of** and array types. Permutation is denoted by the keyword **permutation**. Expressions, templates and *AnyElement* and *AnyElementsOrNone* are allowed as permutation elements. Permutation elements shall obey the restrictions given below.

A permutation without *AnyElementsOrNone* in place of a single record of element means that any series of elements is acceptable provided that there is a one to one mapping between elements in the record of and in the permutation list such that each element matches its corresponding element in the permutation list.

*AnyElementsOrNone* used inside permutation (directly or via reference) replaces none or any number of elements within the segment of the record of value matched by permutation. The permutation matching is successful, if a subset of the elements in the record of matches the permutation list without the *AnyElementsOrNone*. If both permutation and *AnyElementsOrNone* are used in a record of template, they shall be evaluated jointly.

NOTE 1: *AnyElementsOrNone* used inside permutation has a different effect as *AnyElementsOrNone* used in conjunction with permutation as in the latter *AnyElementsOrNone* replaces consecutive elements only. For example, {**permutation**(1,2,\*)} is equivalent to ({\*,1,\*,2,\*},{\*,2,\*,1,\*}), while {**permutation**(1,2),\*} is equivalent to ({1,2,\*},{2,1,\*}).

NOTE 2: When *AnyElementsOrNone* is inside a permutation, a length attribute may be applied to *AnyElementsOrNone* to restrict the number of elements matched by *AnyElementsOrNone* (see also clause B.1.4.1).

Besides specifying all individual values, it is possible to add all elements of a **record of** or **set of** template into permutations using an **all from** clause.

***Restrictions***

a) Each individual member listed in the permutation shall be of the type replicated by the **record of** or array type.

b) The member type of the permutation and the member type of the template in the **all from** clause shall be compatible.

c) The template in the **all from** clause as a whole shall not resolve into a matching mechanism other than a *SpecificValue* (see clause B.1.1), and its elements may resolve to the matching mechanisms *SpecificValue*, *AnyElement* and *AnyElementsOrNone* only.

d) Individual members of a permutation and elements of the template in the **all from** clause shall only be expressions, templates obeying to restriction c) above, and the *AnyElement* and *AnyElementsOrNone* matching mechanisms.

***Examples***

EXAMPLE 1:

**type record of integer** MySequenceOfType;

**template** MySequenceOfType MyTemplate1 := { **permutation** ( 1, 2, 3 ), 5 };

// matches any of the following sequences of 4 integers: 1,2,3,5; 1,3,2,5; 2,1,3,5;

// 2,3,1,5; 3,1,2,5; or 3,2,1,5

**template** MySequenceOfType MyTemplate2 := { **permutation** ( 1, 2, ? ), 5 };

// matches any sequence of 4 integers that ends with 5 and contains 1 and 2 at least once in

// other positions

**template** MySequenceOfType MyTemplate3 := { **permutation** ( 1, 2, 3 ), \* };

// matches any sequence of integers starting with 1,2,3; 1,3,2; 2,1,3; 2,3,1; 3,1,2 or 3,2,1

**template** MySequenceOfType MyTemplate4 := { \*, **permutation** ( 1, 2, 3 )};

// matches any sequence of integers ending with 1,2,3; 1,3,2; 2,1,3; 2,3,1; 3,1,2 or 3,2,1

**template** MySequenceOfType MyTemplate5 := { \*, **permutation** ( 1, 2, 3 ),\* };

// matches any sequence of integers containing any of the following substrings at any position:

// 1,2,3; 1,3,2; 2,1,3; 2,3,1; 3,1,2 or 3,2,1

**template** MySequenceOfType MyTemplate6 := { **permutation** ( 1, 2, \* ), 5 };

// matches any sequence of integers that ends with 5 and containing 1 and 2 at least once in

// other positions

**template** MySequenceOfType MyTemplate7 := { **permutation** ( 1, 2, 3 ), \* length (0..5)};

// matches any sequence of three to eight integers starting with 1,2,3; 1,3,2; 2,1,3; 2,3,1;

// 3,1,2 or 3,2,1

**template integer** MyInt1 := (1,2,3);

**template integer** MyInt2 := (1,2,?);

**template integer** MyInt3 := ?;

**template integer** MyInt4 := \*;

**template** MySequenceOfType MyTemplate10 := { **permutation** (MyInt1, 2, 3 ), 5 };

// matches any of the sequences of 4 integers:

// 1,3,2,5; 2,1,3,5; 2,3,1,5; 3,1,2,5; or 3,2,1,5;

// 2,3,2,5; 2,2,3,5; 2,3,2,5; 3,2,2,5; or 3,2,2,5;

// 3,3,2,5; 2,3,3,5; 2,3,3,5; 3,3,2,5; or 3,2,3,5;

**template** MySequenceOfType MyTemplate11 := { **permutation** (MyInt2, 2, 3 ), 5 };

// matches any sequence of 4 integers that ends with 5 and contains 2 and 3 at least once in

// other positions

**template** MySequenceOfType MyTemplate12 := { **permutation** (MyInt3, 2, 3 ), 5 };

// matches any sequence of 4 integers that ends with 5 and contains 2 and 3 at least once in

// other positions

**template** MySequenceOfType MyTemplate13 := { **permutation** (MyInt4, 2, 3 ), 5 };

// matches any sequence of integers that ends with 5 and containing 2 and 3 at least once in

// other positions

**template** MySequenceOfType MyTemplate14 := { **permutation** (MyInt3, 2, ? ), 5 };

// matches any sequence of 4 integers that ends with 5 and contains 2 at least once in

// other positions

**template** MySequenceOfType MyTemplate15 := { **permutation** (MyInt4, 2, \* ), 5 };

// matches any sequence of integers that ends with 5 and contains 2 at least once in

// other positions

EXAMPLE 2:

**type record of integer** RoI;

**template** RoIt\_RoI1 := {1, 2, \*};

**template** RoIt\_RoI2 := {**permutation**(0, **all from** t\_RoI1), 4, 5};

// results in {permutation(0, 1, 2, \*), 4, 5}

## B.1.4 Matching attributes of values

The following attributes may be associated with matching mechanisms.

### B.1.4.1 Length restrictions

The **length** restriction attribute is used to restrict the length of string values matching the template or the number of elements in a **set** **of**, **record** **of** or array structure.

It can also be used in conjunction with the **ifpresent** matching attribute. The syntax for **length** can be found in clauses 6.2.3.

NOTE: When the **length** attribute is used with a template list, elements of the list may be disabled by the attribute.

The units of length are to be interpreted according to table 4 in the main body of the present document in the case of string values. For **set of**, **record of** types and arrays the unit of length is the replicated type.

A template field that uses length as an attribute of a symbol matches the corresponding field if, and only if, the field matches both the symbol and its associated attribute. The length attribute matches if the length of the field is greater than or equal to the specified lower bound and less than or equal to the upper bound. In the case of a single length value the length attribute matches only if the length of the received field is exactly the specified value.

It is allowed to use a length restriction in conjunction with the special value **omit**, however in this case the length attribute has no effect (i.e. with **omit** it is redundant). With *AnyValueOrNone* and **ifpresent** it places a restriction on the value, if any.

***Restrictions***

a) The length restriction shall be used only as an attribute of the following matching mechanisms: template list, complemented template list, *AnyValue*, *AnyValueOrNone*, *AnyElement*, *AnyElementsOrNone*, superset, subset, and pattern.

b) It shall not be used directly with templates and template fields produced by concatenation (see clause 15.11). If the length of a template or template field produced by concatenation is wished to be restricted, the concatenation shall be enclosed into a pair of parentheses.

c) The boundaries of the length restriction shall be denoted by expressions which resolve to specific non-negative **integer** values. Alternatively, the keyword **infinity** can be used as a value for the upper boundary in order to indicate that there is no upper limit of length.

d) The length specifications for the template shall not conflict with the length for restrictions (if any) of the corresponding type.

e) When both the complement and the length restriction matching mechanisms are used for a template or template field, restrictions implied by them shall apply to the template or template field independently.

***Examples***

EXAMPLE:

**template** Mymessage MyTemplate:=

{

field1 := **complement** ({4,5},{1,4,8,9}) **length** (1 .. 6), // any value containing 1, 2, 3, 4, // 5 or 6 elements is accepted provided it is not {4,5} or {1,4,8,9}

field2 := "ab\*ab" **length**(5), // matches the character string "ab\*ab" only

field3 := "ab\*ab" **length**(13), // never matches as the specific value is of length 5

// and not of length 13

field4 := pattern "ab\*ab" **length**(13),

// max length of the AnyElementsOrNone string is 9 characters

:

}

### B.1.4.2 The IfPresent indicator

The **ifpresent** indicates that a match may be made if an optional field is present (i.e. not omitted).

A template field that uses **ifpresent** matches the corresponding field if, and only if, the field matches according to the associated matching mechanism, or if the field is absent.

***Restrictions***

a) This IfPresent indicator shall be used only for matching mechanisms in templates of any type as a whole or for optional fields of **set** or **record** templates.

b) At the time of matching, it shall be applied to optional fields of **record** and **set** templates only.

***Examples***

EXAMPLE:

**type** **record** MyMessage

{

**integer** field1,

MyRecordof field2 **optional**,

**boolean** field3 **optional**

}

**template** MyMessage MyMessageTemplate:=

{

:

field2 := { 1, 2, 3 } **ifpresent,** // matches { 1, 2, 3 } if not omitted

:

}

**template** MyMessage MyMessageTemplate2:=

{

field1 := 1 **ifpresent,** // causes an error as field1 is mandatory

:

}

**template** MyRecordof MyRecofTemplate := { 1, 2, 3 } **ifpresent;** // this assignment is allowed

**template** **boolean** MyBoolTemplate := **true** **ifpresent;** // this assignment is also allowed

**template** MyMessage MyMessageTemplate3:=

{

field1 := 42,

field2 := MyRecofTemplate,

// if field2 is not absent, it matches the value { 1, 2, 3 }

field3 := MyBoolTemplate

// if field3 is not absent, it matches the value **true**

}

MybooleanVar := **match** ({},MyRecofTemplate);

// causes an error as a record of template shall not contain ifpresent

// at the time of matching

MybooleanVar := **match** ({42,**omit**,**true**},MyMessageTemplate3);

// matches and returns true

NOTE: *AnyValueOrNone* has exactly the same meaning as **? ifpresent**.

## B.1.5 Matching character pattern

Character patterns can be used in templates to define the format of a required character string to be received. Character patterns can be used to match **charstring** and **universal charstring** values. In addition to literal characters, character patterns allow the use of meta-characters (e.g. ? and \* within a character pattern means matching any character and any number of any character respectively).

EXAMPLE 1:

**template** **charstring** MyTemplate:= **pattern** "ab??xyz\*0";

This template would match any character string that consists of the characters "ab", followed by any two characters, followed by the characters "xyz", followed by any number of any characters (including any number of "0"-s) before the closing character "0".

If it is required to interpret any metacharacter literally it shall be preceded with the metacharacter "\".

EXAMPLE 2:

**template** **charstring** MyTemplate:= **pattern** "ab?\?xyz\*";

This template would match any character string which consists of the characters "ab", followed by any character, followed by the characters "?xyz", followed by any number of any characters.

The list of meta characters for TTCN‑3 patterns is shown in table B.1. Metacharacters shall not contain whitespaces except a whitespace preceded by a newline character before or inside a set expression.

Table B.1: List of TTCN‑3 pattern metacharacters

| Metacharacter | Description |
| --- | --- |
| ? | Match any character (see notes 1 and 2) |
| \* | Match any character zero or more times; shall match the longest possible number of characters (see example 1 above) (see notes 1 and 2) |
| \ | Cause the following metacharacter to be interpreted as a literal (see note 3). When preceding a character without defined metacharacter meaning "\" and the character together match the character following the "\" (see note 4) |
| [ ] | Match any character within the specified set, see clause B.1.5.1 for more details |
| - | Has a metacharacter meaning in a set expression. It allows to specify a range of characters; see clause B.1.5.1 for more details |
| ^ | Has a metacharacter meaning in a set expression. It causes to match any character complementing the set of characters following this metacharacter;  see clause B.1.5.1for more details |
| \q{group,plane,row,cell} or \q{Uxxxx, Uxxx ….} | Match one or more universal character. Both the quadruple and the USI-like syntaxes specified in clause 6.1.1 can be used. |
| {reference} | Insert the referenced user defined string and interpret it as a regular expression. See clause B.1.5.2 for more details |
| {\reference} | Insert the referenced user defined string and interpret it as a set of literals. See clause B.1.5.2 for more details |
| \N{reference} | Matches a single character from the (sub)set of characters denoted; see clause B.1.5.4 for more details |
| \d | Match any numerical digit (equivalent to [0-9]) |
| \w | Match any alphanumeric character (equivalent to [0-9a-zA-Z]) |
| \t | Match the C0 control character HT(9) (see Recommendation ITU‑T T.50 [4]) |
| \n | Match any of the following C0 control characters: LF(10), VT(11), FF(12), CR(13) (see Recommendation ITU‑T T.50 [4]) (jointly called newline characters, see clause A.1.5.1) |
| \r | Match the C0 control character CR (see Recommendation ITU‑T T.50 [4]) |
| \s | Match any one of the following C0 control characters: HT(9), LF(10), VT(11), FF(12), CR(13), SP(32) (see Recommendation ITU‑T T.50 [4]) (jointly called white-space characters, see clause A.1.5.1) |
| \b | Match a word boundary (any graphical character except SP or DEL is preceded or followed by any of the whitespace or newline characters) |
| \" | Match the double quote character |
| "" | Match the double quote character |
| | | Used to denote two alternative expressions |
| ( ) | Used to group an expression |
| #(n, m) | Match the preceding expression at least n times but no more than m times (postfix). See clause B.1.5.3 for more details |
| #n | Match the previous expression exactly n times (where n is a single digit) (postfix); the same as #(n). See clause B.1.5.3 for more details |
| + | Match the preceding expression one or several times (postfix); the same as #(1,). See clause B.1.5.3 for more details |
| NOTE 1: Metacharacters ? and \* are able to match any characters of the character set of the root type of the template or template field in which they are used (i.e. not considering type constraints applied). However, it shall not be forgotten, that receiving operations require type checking of the received message before attempting to match it. Therefore received values not complying with the subtype specification of the template or template field are never provided for matching.  NOTE 2: In some other languages/notations ? and \* has different meaning as metacharacters. However in TTCN these characters are traditionally used for matching in the sense as specified in this table.  NOTE 3: Consequently the backslash character can be matched by a pair of backslash characters without space between them (\\), e.g. the pattern "\\d" will match the string "\d"; opening or closing square brackets can be matched by "\[" and "\]" respectively, etc.  NOTE 4: Such use of the metacharacter "\" is deprecated as further metacharacters can be defined later. | |

The symbols that can appear as lexical marks in metacharacter definitions are called metacharacter symbols.They include the following characters: "#", "(", ")", "\*", "+", "-", "?", "[", "\", "]", "^", "{","|","}". When any of the metacharacter symbols are present in a pattern, but do not form a valid metacharacter, they retain their literal value.

NOTE: This rule assures that no format error can occur during pattern template instantiation. However, errors caused by invalid references can still appear (see clauses B.1.5.2and B.1.5.4 for more details).

Character patterns may be composed from several fragments using the concatenation operation. The fragments of the pattern shall be concatenated before any evaluation of the pattern expression. See also the shorthand notation for referenced definitions at concatenation in clause B.1.5.2.

EXAMPLE 3:

**template** **charstring** MyTemplate:= **pattern** "ab?\?" & "xyz\*"; // results in the same pattern as

// in example2

Pattern definitions may contain references to values or templates. The referred value or template shall be of the charstring or universal charstring type and it shall contain either a specific value or pattern. When the referenced template contains a pattern, the character pattern definition of this pattern is used as a fragment for creating the new pattern.

EXAMPLE 4:

**template** **charstring** template1 := "ab?";

**template** **charstring** template2 := **pattern** "?xyz\*0";

**template** **charstring** template3 := **?;**

**template** **charstring** template4 := **pattern** template1 & template2;

// the same template as in example 1, i.e. pattern "ab??xyz\*0"

**template** **charstring** template5 := **pattern** template3

// produces as error as m\_template3 doesn’t contain a value or pattern

### B.1.5.1 Set expression

A list of characters enclosed by a pair of "[" and "]" matches any single character in that list. The set expression is delimited by the "[" "]" symbols. In addition to character literals, it is possible to specify character ranges using the hyphen "-" as separator. The range consist of the character immediately before the separator, the character immediately after it and all characters with a character code between the codes of the two bordering characters. A hyphen character "-" inside the list but without preceding or following character loses its special meaning.

The set expression can also be negated by placing the caret "^" character as the first character after the opening square bracket. Negation takes precedence over character ranges. Therefore a hyphen "-" immediately following a negating caret "^" shall be processed as a literal character.

An empty list and an empty negated list are not allowed. Therefore a closing square bracket "]" immediately following an opening square bracket "[" or a caret following the opening square bracket "[" and immediately followed by a closing square bracket "]" shall be processed as literal characters.

All metacharacters, except those listed below, lose their special meaning inside the list:

* "]" not at the first position and not immediately following a "^" at the first position;
* "-" not at the first or last positions in the list;
* "^" at the first position in the list except when immediately followed by a closing square bracket;
* "\", "\d", "\t", "\w", "\r", "\n", "\s" and "\b";
* "\q{group,plane,row,cell}";
* "**\N**{reference}".

NOTE 1: Embedded lists are not allowed. For example in pattern "[ab[r-z]]" the second "[" denotes a literal "[", the first "]" closes the list and the second "]" retains its literal value as no related opening bracket precedes it in the pattern. The pattern will match character strings containing two elements, with the first element equal to "a", "b", "[" or anything in the range "r"-"z" and the second character equal to "]".

NOTE 2: To include a literal caret character "^", place it anywhere except in the first position or precede it with a backslash. To include a literal hyphen "-", place it first or last in the list, or precede it with a backslash. To include a literal closing square bracket "]", place it first or precede it with a backslash. If the first character in the list is the caret "^", then the characters "-" and "]" also match themselves when they immediately follow that caret.

EXAMPLE:

**template** **charstring** RegExp1:= **pattern** "[a-z]"; // this will match any character from a to z

**template** **charstring** RegExp2:= **pattern** "[^a-z]"; // this will match any character except a to z

**template** **charstring** RegExp3:= **pattern** "[AC-E][0-9][0-9][0-9]YKE";

// RegExp3 will match a string which starts with the letter A or a letter between  
 // C and E (but not e.g. B) then has three digits and the letters YKE

### B.1.5.2 Reference expression

In addition to direct string values, it is also possible within the pattern to use references to templates, constants, variables, formal parameters, module parameters, or to their fields, containing either a character string value or pattern matching. The reference shall be enclosed within the "{" "}" characters and reference shall resolve a compatible character string type. The opening bracket can be optionally followed by a backslash.

If the backslash character is missing, the referenced character string or pattern shall be inserted into the pattern being constructed and shall be handled as a regular expression. Each expression shall be dereferenced only once, before the insertion (i.e. the expression dereferenced and inserted into the referencing pattern shall not be dereferenced again).

If the backslash character is present, the referenced item shall contain a character string value in this case. The character string is inserted into the pattern being constructed so that it all characters contained in it can keep their literal value   
(i.e. all metacharacter symbols are automatically escaped).

If the reference cannot be resolved or if the referenced symbol does not fulfil the requirements set by this clause, an error shall be generated.

EXAMPLE 1:

**const charstring** MyString:= "ab?";

**template** **charstring** MyTemplate:= **pattern** "{MyString}";

//matches any character string that consists of the characters "ab" followed by any character

**templatecharstring** MyTemplate2:= **pattern** "{\MyString}";

//resolves into pattern "ab\?" and matches the string"ab?" only

**template** **universal** **charstring** MyTemplate3:= **pattern** "{MyString}de\q{1, 1, 13, 7}";

//matches any character string which consists of the characters "ab", followed by any

//character, followed by the characters "de", followed by the character in ISO10646-1 with

//group=1, plane=1, row=13 and cell=7.

If a referenced definition or field of a definition contains one or more reference expressions, then these references shall recursively be dereferenced before inserting their contents into the referencing pattern.

If a fragment of a pattern contains a single reference only, it is allowed, as a shorthand notation, to reference the definition or the field of the definition directly, i.e. leave out double quotes (" ") and the pair of curly brackets ({ }).

EXAMPLE 2:

**const** **charstring** MyConst2 := "ab";

**template** **charstring** RegExp1 := **pattern** "{MyConst2}";

// matches the string "ab"

**template** **charstring** RegExp1a := **pattern** MyConst2;

// the same as above, matches the string "ab"

**template** **charstring** RegExp2 := **pattern** "{RegExp1}{RegExp1}";

// matches the string "abab"

**template** **charstring** RegExp2a := **pattern** "{RegExp1}" & "{RegExp1}";

// the same as above, matches the string "abab"

**template** **charstring** RegExp2b := **pattern** RegExp1 & RegExp1;

// the same as above, matches the string "abab"

**template** **charstring** RegExp3 := **pattern** "c{RegExp2}d";

// matches the string "cababd"

**template** **charstring** RegExp4 := **pattern** "{Reg";

**template** **charstring** RegExp5 := **pattern** "Exp1}";

**template** **charstring** RegExp6 := **pattern** "{RegExp4}{RegExp5}";

// matches the string "{RegExp1}" only (i.e. shall not be handled as a reference expression

// after insertion)

**template** **charstring** RegExp7 := **pattern** "{Reg" & "Exp1}";

// note the difference to the previous example; in this case the fragments of the  
 // pattern are joined before any evaluation, i.e. this template will match the string "ab"

EXAMPLE 3:

**template** **charstring** Ref0:= "My String";

**template** **charstring** Ref1:= "{Re";

**template** **charstring** Ref2:= "f0}";

**template** **charstring** Ref3:= "{Ref1}{Ref2}";

//this matches "{Ref0}"

//i.e. there is no further dereferencing

//as Ref1 and Ref2 do not contain a reference

**template** **charstring** Ref4:= "{Ref0}";

**template** **charstring** Ref5:= "";

**template** **charstring** Ref6:= "{Ref4}{Ref5}";

//this matches "My String" – here Ref0 is dereferenced, because Ref4 contains

//the reference expression {Ref0} with the reference Ref0

EXAMPLE 4:

**type** **record** MyRecord {

**integer** i,

**charstring** c

}

**const** MyRecord referencedRecord:= {1,"this"}

**const** **charstring** referencedConstant := referencedRecord.c;

**template** **charstring** referencingPattern := **pattern** "{referencedConstant}"

//this matches "this" as the referencedConstant is dereferenced

### B.1.5.3 Match expression n times

To specify that the preceding expression should be matched a number of times one of the following syntaxes shall be used: "#(n, m)", "#(n, )", "#( , m)", "#(n)", "#n", "#(,)", "#()" or "+".

The form "#(n, m)" specifies that the preceding expression shall be matched at least n times but not more than m times.

The metacharacter postfix "#(n, )" specifies that the preceding expression shall be matched at least n times while  
"#( , m)" indicates that the preceding expression shall be matched not more than m times.

Metacharacters (postfixes) "#(n)" and "#n" specify that the preceding expression shall be matched exactly n times (they are equivalent to "#(n, n)"). In the form "#n" n shall be a single digit.

The forms "#(,)" and "#()" are shorthand notations for "#(0,)", i.e. matches the preceding expression any number of times.

The metacharacter postfix "+" denotes that the preceding expression shall be matched at least 1 time (equivalent to "#(1,)").

EXAMPLE:

**template** **charstring** RegExp4:= **pattern** "[a-z]#(9, 11)"; // match at least 9 but no more than 11

// characters from a to z

**template** **charstring** RegExp5a:= **pattern** "[a-z]#(9)"; // match exactly 9

// characters from a to z

**template** **charstring** RegExp5b:= **pattern** "[a-z]#9"; // match exactly 9

// characters from a to z

**template** **charstring** RegExp6:= **pattern** "[a-z]#(9, )"; // match at least 9

// characters from a to z

**template** **charstring** RegExp7:= **pattern** "[a-z]#(, 11)"; // match no more than 11

// characters from a to z

**template** **charstring** RegExp8:= **pattern** "[a-z]+"; // match at least 1

// characters from a to z,

### B.1.5.4 Match a referenced character set

A notation of the form "\N{reference}", where reference is denoting a one‑character‑length template, constant, variable, formal parameter or module parameter, matches the character in the referenced value or template.

If the reference cannot be resolved or if the referenced symbol is anything else than a template, constant, variable, formal parameter or module parameter containing a character string of length 1, an error shall be generated.

A notation of the form "\N{typereference}", where "typereference" is a reference to a **charstring** or **universal charstring** type, matches any character of the character set denoted by the referenced type.

NOTE 1: Cases when the referenced set of characters is not a subset of values allowed by the type definition of the template or template field for which the character pattern is used, are not be treated as an error (but e.g. matching never can occur if the two sets do not overlap).

NOTE 2: \N{**charstring**} is equivalent to ? when the latter is applied to a template or template field of **charstring** type and \N{**universal charstring**} is equivalent to ? when the latter is applied to a template or template field of **universal charstring** type (but causes an error if applied to a template or template field of **charstring** type).

EXAMPLE:

**type** **charstring** MyCharRange ("a".."z");

**type** **charstring** MyCharList ("a", "z");

**const** MyCharRange myCharR := "r";

**template** **charstring** myTempPatt1 := **pattern** "\N{myCharR}";

// myTempPatt1 shall match the string "r" only

**template** **charstring** myTempPatt2 := **pattern** "\N{MyCharRange}";

// myTempPatt2 shall match any string containing a single character from a to z

**template** MyCharRange myTempPatt3 := **pattern** "\N{MyCharList}";

// myTempPatt3 shall match strings "a" or "z" only

### B.1.5.5 Type compatibility rules for patterns

For the purpose of referenced patterns (see clause B.1.5.2) and references character sets (see clause B.1.5.3) specific type compatibility rules apply: a referenced type, template, constant, variable or module parameter of the type **charstring** always can be used in the pattern specification of a template or template field of **universal charstring** type; a referenced type, template or value of the type **universal charstring** can be used in the pattern specification of a template or template field of **charstring** type if all characters used in the referenced template or value and the character set allowed by the referenced type has their corresponding characters in the **charstring** type (see definition of corresponding characters in clause 6.3.1).

### B.1.5.6 Case insensitive pattern matching

When the “**@nocase**” modifier is used after the pattern keyword, the matching is evaluated in a case insensitive way, i.e. at positions, where without the “**@nocase**” modifier a small letter alphabethical character would be matched, with the “**@nocase**” modifier also capital letter counterpart – but only that - shall be accepted. For example, at positions where the pattern matches the character đ (LATIN SMALL LETTER D WITH STROKE), also its counterpart Đ (LATIN CAPITAL LETTER D WITH STROKE) shall be accepted, but the similarly looking graphical characters Ð (LATIN CAPITAL LETTER ETH) and Ɖ (LATIN CAPITAL LETTER AFRICAN D) shall not.

EXAMPLE 1:

**template** **charstring** MyTemplateNoCase:= **pattern** **@nocase** "ab??xyz\*0";

//This template would match any character string that start with the characters "ab" or "Ab"

//or "aB" or "AB", followed by any two characters, followed by the characters "xyz" or "Xyz"

//or "xYz" or "xyZ" or "XYz" or "xYZ" or "XyZ" or "XYZ", followed by any number of any

//characters (including any number of "0"-s) before the closing character "0".

When referencing a pattern from inside another pattern (see clause B.1.5.2), the case sensitivity property of the referenced pattern is not inherited. I.e. - after dereferencing, possibly recursively - only the resulting string part of the referenced pattern is inserted into the referencing pattern. The whole resulting pattern is always evaluated according to the case-sensitivity of the referencing pattern.

EXAMPLE 2:

**const charstring** MyString:= "ab?";

**template** **charstring** MyTemplate:= **pattern** **@nocase** "{MyString}";

//matches any character string that consists of the characters "ab" or "Ab" or "aB" or "AB",

// followed by any character

**template** **universal** **charstring** MyTemplate3:= **pattern** "{MyTemplate}de\q{1, 1, 13, 7}";

//matches any character string which consists of the characters "ab", followed by any

//character, followed by the characters "de", followed by the character in ISO10646-1 with

//group=1, plane=1, row=13 and cell=7 (.

Annex C (normative):  
Predefined TTCN‑3 functions

This annex defines the TTCN‑3 predefined functions.

# C.0 General exception handling procedures

When the general restrictions specified in clause 16.1.2 are not met, this shall cause a compile time or runtime error. Error situations for which no explicit exception-handling rule is defined in the relevant clauses of this annex shall cause a TTCN‑3 compile-time or runtime error. Which error situation causes compile-time and which one runtime error is a tool implementation option.

# C.1 Conversion functions

## C.1.1 Integer to character

**int2char**(**in integer** invalue) **return charstring**

This function converts an **integer** value in the range of 0 to 127 (8-bit encoding) into a single-character-length **charstring** value. The integer value describes the 8-bit encoding of the character.

In addition to the general error causes in clause 16.1.2, error causes are:

* invalue is less than 0 or greater than 127.

## C.1.2 Integer to universal character

**int2unichar**(**in integer** invalue) **return universal charstring**

This function converts an **integer** value in the range of 0 to 2 147 483 647 (32-bit encoding) into a single‑character‑length **universal charstring** value. The integer value describes the 32-bit encoding of the character.

In addition to the general error causes in clause 16.1.2, error causes are:

* invalue is less than 0 or greater than 2147483647.

## C.1.3 Integer to bitstring

**int2bit**(**in integer** invalue, **in integer** length) **return bitstring**

This function converts a single **integer** value to a single **bitstring** value. The resulting string is length bits long.

For the purposes of this conversion, a **bitstring** shall be interpreted as a positive base 2 **integer** value. The rightmost bit is least significant, the leftmost bit is the most significant. The bits 0 and 1 represent the decimal values 0 and 1 respectively. If the conversion yields a value with fewer bits than specified in the length parameter, then the **bitstring** shall be padded on the left with zeros.

In addition to the general error causes in clause 16.1.2, error causes are:

* invalue is less than zero;
* the conversion yields a return value with more bits than specified by length.

## C.1.4 Integer to enumerated

**int2enum** ( **in integer** inpar**, out** Enumerated\_type outpar)

This function converts an integer value into an enumerated value of a given enumerated type. The integer value shall be provided as in parameter and the result of the conversion shall be stored in an out parameter. The type of the out parameter determines the type into which the in parameter is converted.

The general error causes in clause 16.1.2 apply.

EXAMPLE:

**type** **enumerated** MyFirstEnumType {

Monday, Tuesday, Wednesday, Thursday, Friday

};

**type** **enumerated** MySecondEnumType {

Saturday(-3), Sunday (0), Monday

};

//within a dynamic language element:

**var** MyFirstEnumType firstEnum **:=** Tuesday;

**var** MySecondEnumType secondEnum **:=** Sunday;

**int2enum**(0, firstEnum) // firstEnum == Monday

**int2enum**(1, secondEnum) // secondEnum == Monday

## C.1.5 Integer to hexstring

**int2hex**(**in integer** invalue, **in integer** length) **return hexstring**

This function converts a single **integer** value to a single **hexstring** value. The resulting string is length hexadecimal digits long.

For the purposes of this conversion, a **hexstring** shall be interpreted as a positive base 16 **integer** value. The rightmost hexadecimal digit is least significant, the leftmost hexadecimal digit is the most significant. The hexadecimal digits 0 to F represent the decimal values 0 to 15 respectively. If the conversion yields a value with fewer hexadecimal digits than specified in the length parameter, then the **hexstring** shall be padded on the left with zeros.

In addition to the general error causes in clause 16.1.2, error causes are:

* invalue is less than zero;
* the conversion yields a return value with more hexadecimal characters than specified by length.

## C.1.6 Integer to octetstring

**int2oct**(**in integer** invalue, **in integer** length) **return octetstring**

This function converts a single **integer** value to a single **octetstring** value. The resulting string is length octets long.

For the purposes of this conversion, an **octetstring** shall be interpreted as a positive base 16 **integer** value. The rightmost hexadecimal digit is least significant, the leftmost hexadecimal digit is the most significant. The number of hexadecimal digits provided shall be multiples of 2 since one octet is composed of two hexadecimal digits. The hexadecimal digits 0 to F represent the decimal values 0 to 15 respectively. If the conversion yields a value with fewer hexadecimal digits than specified in the length parameter, then the **hexstring** shall be padded on the left with zeros.

In addition to the general error causes in clause 16.1.2, error causes are:

* invalue is less than zero;
* the conversion yields a return value with more octets than specified by length.

## C.1.7 Integer to charstring

**int2str**(**in integer** invalue) **return** **charstring**

This function converts the integer value into its string equivalent (the base of the return string is always decimal).

The general error causes in clause 16.1.2 apply.

EXAMPLE:

**int2str**(66) // will return the **charstring** value "66"

**int2str**(-66) // will return the **charstring** value "-66"

**int2str**(0) // will return the **charstring** value "0"

## C.1.8 Integer to float

**int2float**(**in integer** invalue) **return float**

This function converts an **integer** value into a **float** value.

The general error causes in clause 16.1.2 apply.

EXAMPLE:

**int2floa**t(4) = 4.0

## C.1.9 Float to integer

**float2int**(**in float** invalue) **return integer**

This function converts a **float** value into an **integer** value by removing the fractional part of the argument and returning the resulting **integer**.

In addition to the general error causes in clause 16.1.2, error causes are:

* invalue is **infinity**, **-infinity** or **not\_a\_number**.

EXAMPLE:

**float2in**t(3.12345E2) = **float2in**t(312.345) = 312

## C.1.10 Character to integer

**char2int**(**in charstring** invalue) **return integer**

This function converts a single-character-length **charstring** value into an integer value in the range of 0 to 127. The integer value describes the 8-bit encoding of the character.

In addition to the general error causes in clause 16.1.2, error causes are:

* length of invalue does not equal 1.

## C.1.11 Character to octetstring

**char2oct(in charstring** invalue**) return octetstring**

This function converts a **charstring** invalue to an **octetstring**. Each octet of the **octetstring** will contain the Recommendation ITU‑T T.50 [4] codes (according to the IRV) of the appropriate characters of invalue.

The general error causes in clause 16.1.2 apply.

EXAMPLE:

**char2oct** ("Tinky-Winky") = '54696E6B792D57696E6B79'O

## C.1.12 Universal character to integer

**unichar2int**(**in universal** **charstring** invalue) **return integer**

This function converts a single-character-length **universal charstring** value into an integer value in the range of 0 to 2 147 483 647. The integer value describes the 32-bit encoding of the character.

In addition to the general error causes in clause 16.1.2, error causes are:

* length of invalue does not equal 1.

## C.1.13 Bitstring to integer

**bit2int**(**in bitstring** invalue) **return integer**

This function converts a single **bitstring** value to a single **integer** value.

For the purposes of this conversion, a **bitstring** shall be interpreted as a positive base 2 **integer** value. The rightmost bit is least significant, the leftmost bit is the most significant. The bits 0 and 1 represent the decimal values 0 and 1 respectively.

NOTE: On real test systems the integer interpretation of invalue may lead to an overflow problem that causes compile time or runtime error. However, this is out of the scope of the present document.

The general error causes in clause 16.1.2 apply.

## C.1.14 Bitstring to hexstring

**bit2hex**(**in bitstring** invalue) **return hexstring**

This function converts a single **bitstring** value to a single **hexstring**. The resulting **hexstring** represents the same value as the **bitstring**.

For the purpose of this conversion, a bitstring shall be converted into a hexstring, where the bitstring is divided into groups of four bits beginning with the rightmost bit. Each group of four bits is converted into a hex digit as follows:

'0000'B → '0'H, '0001'B → '1'H, '0010'B → '2'H, '0011'B → '3'H, '0100'B → '4'H, '0101'B → '5'H,  
'0110'B → '6'H, '0111'B → '7'H, '1000'B → '8'H, '1001'B → '9'H, '1010'B → 'A'H, '1011'B → 'B'H,  
'1100'B → 'C'H, '1101'B → 'D'H, '1110'B → 'E'H, and '1111'B → 'F'H.

When the leftmost group of bits does contain less than 4 bits, this group is filled with '0'B from the left until it contains exactly 4 bits and is converted afterwards. The consecutive order of hex digits in the resulting hexstring is the same as the order of groups of 4 bits in the bitstring.

The general error causes in clause 16.1.2 apply.

EXAMPLE:

**bit2hex** ('111010111'B)= '1D7'H

## C.1.15 Bitstring to octetstring

**bit2oct**(**in bitstring** invalue) **return octetstring**

This function converts a single **bitstring** value to a single **octetstring**. The resulting **octetstring** represents the same value as the **bitstring**.

For the conversion the following holds: bit2oct(value)=hex2oct(bit2hex(value)).

The general error causes in clause 16.1.2 apply.

EXAMPLE:

**bit2oct**('111010111'B)= '01D7'O

## C.1.16 Bitstring to charstring

**bit2str**(**in bitstring** invalue) **return charstring**

This function converts a single **bitstring** value to a single **charstrin**g. The resulting **charstring** has the same length as the **bitstring** and contains only the characters '0' and '1'.

For the purpose of this conversion, a **bitstring** shall be converted into a **charstrin**g. Each bit of the **bitstring** is converted into a character '0' or '1' depending on the value 0 or 1 of the bit. The consecutive order of characters in the resulting **charstring** is the same as the order of bits in the **bitstrin**g.

The general error causes in clause 16.1.2 apply.

EXAMPLE:

**bit2str**('1110101'B) will return "1110101"

## C.1.17 Hexstring to integer

**hex2int**(**in hexstring** invalue) **return** **integer**

This function converts a single **hexstring** value to a single **integer** value.

For the purposes of this conversion, a **hexstring** shall be interpreted as a positive base 16 **integer** value. The rightmost hexadecimal digit is least significant, the leftmost hexadecimal digit is the most significant. The hexadecimal digits 0 to F represent the decimal values 0 to 15 respectively.

NOTE: On real test systems the integer interpretation of invalue may lead to an overflow problem that causes compile time or runtime error. However, this is out of the scope of the present document.

The general error causes in clause 16.1.2 apply.

## C.1.18 Hexstring to bitstring

**hex2bit**(**in hexstring** invalue) **return bitstring**

This function converts a single **hexstring** value to a single **bitstring**. The resulting **bitstring** represents the same value as the **hexstring**.

For the purpose of this conversion, a **hexstring** shall be converted into a **bitstring**, where the hex digits of the **hexstring** are converted in groups of bits as follows:

'0'H → '0000'B, '1'H → '0001'B, '2'H → '0010'B, '3'H → '0011'B, '4'H → '0100'B, '5'H → '0101'B,  
'6'H → '0110'B, '7'H → '0111'B, '8'H → '1000'B, '9'H → '1001'B, 'A'H → '1010'B, 'B'H → '1011'B,  
'C'H → '1100'B, 'D'H → '1101'B, 'E'H → '1110'B, and 'F'H → '1111'B.

The consecutive order of the groups of 4 bits in the resulting **bitstring** is the same as the order of hex digits in the **hexstring**.

The general error causes in clause 16.1.2 apply.

EXAMPLE:

**hex2bit**('1D7'H)= '000111010111'B

## C.1.19 Hexstring to octetstring

**hex2oct**(**in hexstring** invalue) **return octetstring**

This function converts a single **hexstring** value to a single **octetstring**. The resulting **octetstring** represents the same value as the **hexstring**.

For the purpose of this conversion, a **hexstring** shall be converted into a **octetstring**, where the **octetstring** contains the same sequence of hex digits as the **hexstring** when the length of the **hexstring** modulo 2 is 0. Otherwise, the resulting **octetstring** contains 0 as leftmost hex digit followed by the same sequence of hex digits as in the **hexstring**.

The general error causes in clause 16.1.2 apply.

EXAMPLE:

**hex2oct**('1D7'H)= '01D7'O

## C.1.20 Hexstring to charstring

**hex2str**(**in hexstring** invalue) **return charstring**

This function converts a single hexstring value to a single charstring. The resulting charstring has the same length as the hexstring and contains only the characters '0' to '9'and 'A' to 'F'.

For the purpose of this conversion, a **hexstring** shall be converted into a **charstring**. Each hex digit of the **hexstring** is converted into a character '0' to '9' and 'A' to 'F' depending on the value 0 to 9 or A to F of the hex digit. The consecutive order of characters in the resulting **charstring** is the same as the order of digits in the **hexstring**.

The general error causes in clause 16.1.2 apply.

EXAMPLE:

**hex2str**('AB801'H) will return "AB801"

## C.1.21 Octetstring to integer

**oct2int**(**in octetstring** invalue) **return** **integer**

This function converts a single **octetstring** value to a single **integer** value.

For the purposes of this conversion, an **octetstring** shall be interpreted as a positive base 16 **integer** value. The rightmost hexadecimal digit is least significant, the leftmost hexadecimal digit is the most significant. The number of hexadecimal digits provided shall be multiples of 2 since one octet is composed of two hexadecimal digits. The hexadecimal digits 0 to F represent the decimal values 0 to 15 respectively.

NOTE: On real test systems the integer interpretation of invalue may lead to an overflow problem that causes compile time or runtime error. However, this is out of the scope of the present document.

The general error causes in clause 16.1.2 apply.

## C.1.22 Octetstring to bitstring

**oct2bit**(**in octetstring** invalue) **return bitstring**

This function converts a single **octetstring** value to a single **bitstring**. The resulting **bitstring** represents the same value as the **octetstring**.

For the conversion the following holds: oct2bit(value)=hex2bit(oct2hex(value)).

The general error causes in clause 16.1.2 apply.

EXAMPLE:

**oct2bit** ('01D7'O)='0000000111010111'B

## C.1.23 Octetstring to hexstring

**oct2hex**(**in octetstring** invalue) **return hexstring**

This function converts a single **octetstring** value to a single **hexstring**. The resulting **hexstring** represents the same value as the **octetstring**.

For the purpose of this conversion, a **octetstring** shall be converted into a **hexstring** containing the same sequence of hex digits as the **octetstring**.

The general error causes in clause 16.1.2 apply.

EXAMPLE:

**oct2hex**('1D74'O)= '1D74'H

## C.1.24 Octetstring to character string

**oct2str**(**in octetstring** invalue) **return charstring**

This function converts an **octetstring** invalue to an **charstring** representing the string equivalent of the input value. The resulting **charstring** shall have the same length as the incoming **octetstring**.

For the purpose of this conversion each hex digit of invalue is converted into a character '0', '1', '2', '3', '4', '5', '6', '7', '8', '9', 'A', 'B', 'C', 'D', 'E' or 'F' echoing the value of the hex digit. The consecutive order of characters in the resulting **charstring** is the same as the order of hex digits in the **octetstring**.

The general error causes in clause 16.1.2 apply.

EXAMPLE:

**oct2str**('4469707379'O) = "4469707379"

## C.1.25 Octetstring to character string, version II

**oct2char**(**in octetstring** invalue) **return charstring**

This function converts an **octetstring** invalue to a **charstring**. The input parameter invalue shall not contain octet values higher than 7F. The resulting **charstring** shall have the same length as the input **octetstring**. The octets are interpreted as Recommendation ITU‑T T.50 [4] codes (according to the IRV) and the resulting characters are appended to the returned value.

The general error causes in clause 16.1.2 apply.

EXAMPLE:

**oct2char**('4469707379'O) = "Dipsy"

NOTE: The character string returned may contain non-graphical characters, which cannot be presented between the double quotes.

## C.1.26 Charstring to integer

**str2int**(**in charstring** invalue) **return** **integer**

This function converts a **charstring** representing an **integer** value to the equivalent **integer**.

In addition to the general error causes in clause 16.1.2, error causes are:

* invalue contains characters other than "0", "1", "2", "3", "4", "5", "6", "7", "8", "9" and "-".
* invalue contains the character "-" at another position than the leftmost one.

NOTE: On real test systems the integer interpretation of invalue may lead to an overflow problem that causes compile time or runtime error. However, this is out of the scope of the present document.

EXAMPLE:

**str2int**("66") // will return the **integer** value 66

**str2int**("-66") // will return the **integer** value -66

**str2int**("6-6") // will cause an error

**str2int**("abc") // will cause an error

**str2int**("0") // will return the **integer** value 0

## C.1.27 Character string to hexstring

**str2hex**(**in charstring** invalue) **return hexstring**

This function converts a string of the type **charstring** to a **hexstring**. The string invalue shall contain the "0", "1", "2", "3", "4", "5", "6", "7", "8", "9", "a", "b", "c", "d", "e" "f", "A", "B", "C", "D", "E" or "F" graphical characters only. Each character of invalue shall be converted to the corresponding hexadecimal digit. The resulting **hexstring** will have the same length as the incoming **charstring**.

In addition to the general error causes in clause 16.1.2, error cause is:

* invalue contains characters other than specified above.

EXAMPLE:

**str2hex**("54696E6B792D57696E6B7") = '54696E6B792D57696E6B7'H

## C.1.28 Character string to octetstring

**str2oct**(**in charstring** invalue) **return octetstring**

This function converts a string of the type **charstring** to an **octetstring**. The string invalue shall contain the "0", "1", "2", "3", "4", "5", "6", "7", "8", "9", "a", "b", "c", "d", "e" "f", "A", "B", "C", "D", "E" or "F" graphical characters only. When the string invalue contains even number characters the resulting **octetstring** contains 0 as leftmost character followed by the same sequence of characters as in the **charstring**.

**lengthof** (see clause C.2.1 for the resulting **octetstring** will return half of **lengthof** of the incoming **charstring**. In addition to the general error causes in clause 16.1.2, error causes is:

* invalue contains characters other than specified above.

EXAMPLE:

**str2oct**("54696E6B792D57696E6B79") = '54696E6B792D57696E6B79'O

**str2oct**("1D7")= '01D7'O

NOTE: The semantic of the str2oct function cause asymmetric behaviour:

**oct2str(str2oct**("1D7"))// results in the charstring value "01D7"

## C.1.29 Character string to float

**str2float**(**in charstring** invalue) **return float**

This function converts a **charstring** comprising a number into a **float** value. The format of the number in the **charstring** shall follow rules in clause 6.1.0, items a) or b) with the following exceptions:

* leading zeros are allowed;
* leading "+" sign before positive values is allowed;
* "-0.0" is allowed;
* no numbers after the dot in the decimal notation are allowed.

In addition to the general error causes in clause 16.1.2, error causes are:

* the format of invalue is different than defined above.

NOTE: On real test systems the float interpretation of invalue may lead to an overflow problem that causes compile time or runtime error. However, this is out of the scope of the present document.

EXAMPLE:

str2float("12345.6") // is the same as str2float("123.456E+02")

str2float("1.6") // returns a float value equal to 1.6

str2float("+001.") // returns a float value equal to 1.0

str2float("+001") // returns a float value equal to 1.0

str2float("-0.0") // returns a float value equal to -0.0

## C.1.30 Enumerated to integer

**enum2int**(**in** Enumerated\_type inpar) **return integer**

This function accepts an enumerated value and returns the **integer** value associated to the enumerated value (see also clause 6.2.4). The actual parameter passed to inpar always shall be a typed object (see clause 6.2.4 and the definition "type context" in clause 3.1).

The general error causes in clause 16.1.2 apply.

EXAMPLE:

**type** **enumerated** MyFirstEnumType {

Monday, Tuesday, Wednesday, Thursday, Friday

};

**type** **enumerated** MySecondEnumType {

Saturday(-3), Sunday (0), Monday

};

//within a dynamic language element:

**var** MyFirstEnumType vl\_FirstEnum **:=** Monday;

**var** MySecondEnumType vl\_SecondEnum **:=** Monday;

**enum2int(**vl\_FirstEnum**)** // returns 0

**enum2int(**vl\_SecondEnum**)** // returns 1

vl\_FirstEnum **:=** Wednesday;

vl\_SecondEnum **:=** Saturday;

**enum2int(**vl\_FirstEnum**)** // returns 2

**enum2int(**vl\_SecondEnum**)** // returns -3

vl\_FirstEnum **:=** Friday;

vl\_SecondEnum **:=** Sunday;

**enum2int(**vl\_FirstEnum**)** // returns 4

**enum2int(**vl\_SecondEnum**)** // returns 0

## C.1.31 Octetstring to universal character string

**oct2unichar**(**in octetstring** invalue, in charstring string\_encoding := "UTF-8")

**return universal charstring**

This function converts an **octetstring** invalue to a **universal** **charstring** by use of the givenstring\_encoding. The octets are interpreted as mandated by the standardized mapping associated with the given string\_encoding and the resulting characters are appended to the returned value. If the optional string\_encoding parameter is omitted, the default value "UTF-8".

The following values (see ISO/IEC 10646 [2]) are allowed as string\_encoding actual parameters (for the description of the codepoints see clause 27.5):

1. "UTF-8"
2. "UTF-16"
3. "UTF-16LE"
4. "UTF-16BE
5. "UTF-32"
6. UTF-32LE"
7. "UTF-32BE"

The invalue parameter shall not include the optional signature (see clause 10 of ISO/IEC 10646 [2], also known as byte order mark).

In case of "UTF-16" and "UTF-32" big-endian ordering shall be used (as described in section 10.4 and 10.7 of ISO/IEC 10646 [2]).

The general error causes in clause 16.1.2 apply.

EXAMPLE:

**oct2unichar**('C384C396C39CC3A4C3B6C3BC'O) = "ÄÖÜäöü";

**oct2unichar**('00C400D600DC00E400F600FC'O,"UTF-16LE") = "ÄÖÜäöü";

NOTE: The character string returned may contain non-graphical characters, which cannot be presented between the double quotes.

## C.1.32 Universal character string to octetstring

**unichar2oct(in universal charstring** invalue, **in** **charstring** string\_encoding := "UTF-8"**)**

**return octetstring**

This function converts a **universal** **charstring** invalue to an **octetstring**. Each octet of the octetstring will contain the octets mandated by mapping the characters of invalue using the standardized mapping associated with the given string\_encoding in the same order as the characters appear in inpar. If the optional string\_encoding parameter is omitted, the default value "UTF-8".

The following values (see ISO/IEC 10646 [2]) are allowed as string\_encoding actual parameters (for the description of the UCS encoding scheme see clause 27.5):

1. "UTF-8"
2. "UTF-16"
3. "UTF-16LE"
4. "UTF-16BE"
5. "UTF-32"
6. "UTF-32LE"
7. "UTF-32BE"

The general error causes in clause 16.1.2 apply.

EXAMPLE:

**unichar2oct**("ÄÖÜäöü") = 'C384C396C39CC3A4C3B6C3BC'O;

**unichar2oct**("ÄÖÜäöü","UTF-16LE") = '00C400D600DC00E400F600FC'O;

## C.1.33 Value or template to universal charstring

**any2unistr**(**in template** any\_type invalue) **return universal charstring**

This function converts the content of a value or template to a single **universal charstring**. The resulting **universal charstring** is the same as the string produced by the log operation containing the same operand as the one passed to the **any2unistr** function. The value or template passed as a parameter to the **any2unichar** function may be uninitialized, partially or completely initialized.

The general error causes in clause 16.1.2 apply.

EXAMPLE:

**var integer** v\_int1 :=5, v\_int2;

**var template integer vmw\_int1** :=?;

**var template integer vmw\_int2** :=-1 ifpresent;

**var universal charstring** v\_chr1, v\_chr2, v\_chr3, v\_chr4;

v\_chr1 := **any2unistr(v\_int1)**; // after the assignment v\_chr1 will be "5"

v\_chr2 := **any2unistr(v\_int2)**; // after the assignment v\_chr2 will be "UNINITIALIZED"

v\_chr3 := **any2unistr(vmw\_int1)**; // after the assignment v\_chr3 will be "?"

v\_chr4 := **any2unistr(vmw\_int2)**; // after the assignment v\_chr3 will be "-1 ifpresent"

# C.2 Length/size functions

## C.2.1 Length of strings and lists

**lengthof**(**in template (present)** any\_string\_or\_list\_type inpar) **return integer**

This function returns the length of a value or template that is of type **bitstring**, **hexstring**, **octetstring**, **charstring, universal charstring,** **record of**, **set of**, or array. The units of length for each string type are defined in table 4 in the present document.

For values or templates of **record** **of** or **set** **of** type, the value to be returned is the maximum of the minimal length restriction value of the type, or 0 for types with no minimal length restriction, and the index of the last initialized element plus 1.

The length value returned in case of length restricted string or list type shall be at least the minimum length according to the type definition. In particular, the length of a fixed length **record of** or **set of** value will always be the fixed length according to the type definition. For array values or templates, the value to be returned is the fixed length of the corresponding **record** **of** type.

NOTE 1: As **in** formal parameters does not allow passing in uninitialized values or templates, even in these cases inpar will be at least partially initialized.

The length of an **universal charstring** shall be calculated by counting each combining character and hangul syllable character (including fillers) on its own (see ISO/IEC 10646 [2], clauses 23 and 24).

When the function **lengthof** is applied to string-type templates, inpar shall only contain the following matching mechanisms: specific value, value list, complemented value list, pattern, "?" (*AnyValue* instead of value), "\*" (*AnyValueOrNone* instead of value), "?" (*AnyElement* inside value) and "\*" (*AnyElementsOrNone* inside value) and the length restriction matching attribute. In case of string-type templates inpar shall match values of the same length only. If inpar contains uninitialized elements, each of them shall be counted as 1 element, i.e. they shall be matched as if they contained the "?" (AnyElement inside value) matching character in case of binary strings or as if they were a "?" (Match any character) character pattern for textual strings.

When the function **lengthof** is applied to templates of record of or set of types, inpar shall only contain the following matching mechanisms: specific value, value list, complemented value list, "?" (*AnyValue* instead of value), "\*" (*AnyValueOrNone* instead of value), SuperSet, SubSet, "?" (*AnyElement* inside value) and "\*" (*AnyElementsOrNone* inside value), permutation and the length restriction matching attribute. The parameter inpar shall only match values, for which the **lengthof** function would give the same result. If inpar contains uninitialized elements, each of them shall be counted as 1 element, i.e. they shall be matched as if they contained the "?" (AnyElement inside value) matching character.

NOTE 2: In case of record ofs and set ofs and arrays only elements of the TTCN‑3 object, which is the parameter of the function are calculated; i.e. no elements of nested types are taken into account when determining the return value.

In addition to the general error causes in clause 16.1.2, error causes are:

* inpar is a string-type template and it can match string values with different length or the length restriction matching attribute contradicts the number of string elements in the template body;
* inpar is a record of or set of type template and it can match values of different lengths or the length restriction matching attribute contradicts the number of elements in the template body.

NOTE 3: On real test systems the length calculation of inpar may lead to an overflow problem that causes compile time or runtime error. However, this is out of the scope of the present document.

EXAMPLE 1: Using lengthof for values

**lengthof**('010'B) // returns 3

**lengthof**('F3'H) // returns 2

**lengthof**('F2'O) // returns 1

**lengthof** (**universal charstring** : "Length\_of\_Example") // returns 17

// Given

**type** **record length**(0..10) **of integer** MyList;

**var** MyList MyListVar := { 0, 1, **-**, 2, **-** };

**lengthof**(MyListVar);

// returns 4 without respect to the fact, that the element MyListVar[2] is not initialized

EXAMPLE 2: Using lengthof for string-type templates

**lengthof**(**charstring** : "HELLO") // returns 5

**lengthof**(**octetstring** : ('12'O, '34'O)) // returns 1

**lengthof**('1??1'B) // returns 4

**lengthof**(**universal** **charstring** : ? length(8)) // returns 8

**lengthof**('1\*F'H) // shall cause an error

**lengthof**('1\*F'H **length** (8)) // returns 8

**lengthof**(bitstring : ? **length**(2..infinity)) // shall cause an error

**lengthof**('00\*FF'O **length**(1..2)) // returns 2

**lengthof**('1\*49'H **length**(1..2)) // shall cause an error

**lengthof**('1'B **length**(3)) // shall cause an error

**lengthof**('1\*1'B **length**(10..20)) // shall cause an error

EXAMPLE 3:

**type** **record** **of** **integer** RoI;

**template** RoI tr\_roI1 := { 1, permutation(2, 3), ? }

**template** RoI tr\_roI2 := {1, \*, (2, 3) }

**template** RoI tr\_roI3 := { 1, \*, 10 } length(5)

**template** RoI tr\_roI4 := { 1, 2, 3, \* } length(1..2)

**template** RoI tr\_roI5 := { 1, 2, 3, \* } length(1..3)

**lengthof** (tr\_roI1) // returns 4

**lengthof** (tr\_roI2) // shall cause an error

**lengthof** (tr\_roI3) // returns 5

**lengthof** (tr\_roI4) // shall cause an error

**lengthof** (tr\_roI5) // returns 3

## C.2.2 Number of elements in a structured value

**sizeof**(**in template** **(present)** any\_record\_set\_type inpar) **return integer**

This function returns the actual number of elements of a value or template of a **record** or **set** type (see note).

The function **sizeof** is applicable to templates of record and set types. The function is applicable only if the **sizeof** function gives the same result on all values that match the template.

NOTE: Only elements of the TTCN‑3 object, which is the parameter of the function are calculated; i.e. no elements of nested types/values are taken into account at determining the return value.

In addition to the general error causes in clause 16.1.2, error causes are:

* when inpar is a template and it can match values of different sizes.

EXAMPLE:

// Given

**type record** MyPDU

{ **boolean** field1 **optional,**

**integer** field2

};

**template** MyPDU MyTemplate :=

{ field1 := **omit**,

field2 := 5

};

**sizeof**(MyTemplate); // returns 1

**type** **set** S {

**integer** f1,

**bitstring** f2 **optional**,

**charstring** f3 **optional**

}

**template** S tr\_S1 := { f1 := (0..99), f2 := **omit**, f3 := ? }

**template** S tr\_S2 := { f3 := \*, f1 := 1, f2 := '00'B **ifpresent** }

**template** S tr\_S3 := ({ f1 := 1, f2 := **omit**, f3 := "ABC" }, { f1 := 2, f3 := **omit**, f2 := '1'B })

**template** S tr\_S4 := ?

**sizeof**(tr\_S1) // returns 2

**sizeof**(tr\_S2) // shall cause an error

**sizeof**(tr\_S3) // returns 2

**sizeof**(tr\_S4) // shall cause an error

# C.3 Presence checking functions

## C.3.1 The IsPresent function

**ispresent**(**in template** any\_ type inpar) **return boolean**

This function is allowed for templates of all data types and returns:

* the value **true** if the data object reference fulfils the (present) template restriction as described in clause 15.8;
* the value **false** otherwise.

NOTE 1: When the argument of **ispresent** is a subfield of a template field to which the "?" (*AnyValue*) matching is assigned, the extension mechanism specified in clause 15.6.2 applies.

NOTE 2: This means that whenever **ispresent**(MyTemplate) returns true:

- MyTemplate can safely be assigned to a non-optional field of the type of the template in a template variable;

- MyTemplate can safely be used as an actual template(present) parameter or assigned to a variable of kind template(present).

The application of the **ispresent** function to a semantically correct data object reference shall never result in an error, even if using the reference would normally cause a runtime error when being used e.g. in an expression.

EXAMPLE:

// Given

**type record** MyRecord

{

**record** {

**boolean** innerField1 **optional**,

**integer** innerField2 **optional,**

MyRecord innerField3 **optional**

} field1 **optional,**

**integer** field2

}

**var** MyRecord vl\_MyRecord := { field1 := {}, field2 := 5 }

// type of field1 is record with fields, therefore field1 remains uninitialized

// after this assignment (no value is assigned to any of the fields of vl\_MyRecord.field1)

**ispresent**(vl\_MyRecord.field1) // returns false

vl\_MyRecord.field1 := omit

**ispresent**(vl\_MyRecord.field1) // returns false

// and therefore, vl\_MyRecord.field1.innerField1 is an inaccessible reference

**ispresent**(vl\_MyRecord.field1.innerField3.field2) // shall return false because innerField3 is

// unintialized and therefore, vl\_MyRecord.field1.innerField3.field2 is an

// inaccessible reference

**ispresent**(vl\_MyRecord.field1.innerField1) // shall return false because field1 is omitted

**var** **template** MyRecord vlt\_MyRecord := { field1 := ?, field2 := 5 }

**ispresent**(vlt\_MyRecord.field1) // returns true

**ispresent**(vlt\_MyRecord.field1.innerField1) // returns false because field1 is AnyValue

// (pls. note, that at expansion of field1 the optional field innerField1 obtains "\*"

// that can match both a present and an omitted field

**type** **record** R { **integer** f1 **optional**, **integer** f2 **optional** }

**template** R t1 := {f1 := 1, f2 :=(2 .. 4) }

**template** R t2 := { f1 := **omit**, f2 := (5, 7) **ifpresent** }

**template** R t3 := {f1 := \*, f2 :=? }

**ispresent**(t1.f1) // returns true

**ispresent**(t1.f2) // returns true

**ispresent**(t2.f1) // returns false

**ispresent**(t2.f2) // returns false

**ispresent**(t3.f1) // returns false

**ispresent**(t3.f2) // returns true

## C.3.2 The IsChosen function

**ischosen**(**in template** any\_union\_type inpar) **return** **boolean**

This function is allowed for templates of all data types that are a union-field-reference. This function returns:

* the value **true** if and only if the data object reference specifies the variant of the **union** type that is actually selected for a given data object;
* in all other cases **false**.

The function **ischosen** is applicable to templates of union types containing a specific value or a value list. It returns **true** if all the values matched by inpar have the given field selected. The result is **false** if there is another field of the union type on which **ischosen** would return true.

The application of the **ischosen** function to a semantically correct data object reference shall never result in an error, even if using the reference would normally cause a runtime error when being used e.g. in an expression.

EXAMPLE 1:

**type** **union** U { **integer** f1, **octetstring** f2 }

**template** U t\_U1 := {f1 := 1}

**template** U t\_U2 := {f2 := ?}

**template** U t\_U3 := ?

**template** U t\_U4 := ({ f1 := 2 }, {f2 := 'AB'O })

**template** U t\_U5 := ({ f2 := '12?'O }, { f2 := '\*34'O **length**(2) })

**ischosen**(t\_U1.f1) // returns true

**ischosen**(t\_U1.f2) // returns false

**ischosen**(t\_U2.f1) // returns false

**ischosen**(t\_U2.f2) // returns true

**ischosen**(t\_U3.f1) // returns false

**ischosen**(t\_U3.f2) // returns false

**ischosen**(t\_U4.f1) // returns false

**ischosen**(t\_U4.f2) // returns false

**ischosen**(t\_U5.f1) // returns false

**ischosen**(t\_U5.f2) // returns true

**type** **record** R { U u **optional** }

**template** R t\_R1 := { **omit** }

**ischosen**(t\_R1.u.f1) // returns false

EXAMPLE 2:

// Given

**type** **union** MyUnion

{ PDU\_type1 p1,

PDU\_type2 p2,

PDU\_type p3

}

// and given that MyPDU is a template of MyUnion type

// and received\_PDU is also of MyUnion type

// then

MyPort.**receive**(MyPDU) -> **value** received\_PDU

**ischosen**(received\_PDU.p2)

// returns true if the actual instance of MyPDU carries a PDU of the type PDU\_type2

## C.3.3 The IsValue function

**isvalue**(**in** **template** any\_type inpar**) return boolean**;

This function is allowed for templates of all data types, component and address types and default values. The function shall return **true**, if inpar is completely initialized and resolves to a specific value. If inpar is of **record** or **set** type, omitted optional fields shall be considered as initialized, i.e. the function shall also return true if optional fields of inpar are set to omit. The function shall return **false** otherwise.

The **null** value assigned to default and component references shall be considered as concrete values.

The application of the **isvalue** function to a semantically correct data object reference shall never result in an error, even if using the reference would normally cause a runtime error when being used e.g. in an expression.

EXAMPLE 1: Simple types

**template** **charstring** ts\_char0 := "ABCD"; //template containing a specific value matching

**template** **charstring** tr\_char1 := "AB?D"; //template containing a specific value matching  
 //note, that "?" is not a matching symbol in this case

**template** **charstring** tr\_char2 := **pattern** "ABCD"; //a pattern matching a single value only

**template** **charstring** tr\_char3 := **pattern** "AB?D"; //pattern matching

**template** **charstring** tr\_char4 := ("ABCD"); // template containing a specific value (expression)

**template** **charstring** tr\_char5 := ("ABCD","EFGH"); //a value list matching a single value only

**isvalue**(ts\_char0); // shall return true

**isvalue**(tr\_char1); // shall return true

**isvalue**(tr\_char2); // shall return false

**isvalue**(tr\_char3); // shall return false

**isvalue**(tr\_char4); // shall return true similarly to e.g. isvalue((2)) shall return true

**isvalue**(tr\_char5); // shall return false

EXAMPLE 2: Special types

**var** **default** vl\_default := **null**;

**isvalue**(vl\_default); // shall return true

EXAMPLE 3: Record/set types

**type** **record** MyRec {

**integer** f1 **optional**,

**integer** f2 **optional**

}

**var** MyRec vl\_MyRec;

**var** **template** MyRec vlt\_MyRec;

**isvalue**(vl\_MyRec); // shall return false

**isvalue**(vlt\_MyRec); // shall return false

vl\_MyRec := { f1 := 5, f2 := **omit** }

vlt\_MyRec := { f1 := ?, f2 := 5 }

**isvalue**(vl\_MyRec); // shall return true

**isvalue**(vl\_MyRec.f2); // shall return false;

**isvalue**(vlt\_MyRec); // shall return false

**isvalue**(vlt\_MyRec.f1); // shall return false

**isvalue**(vlt\_MyRec.f2); // shall return true

vlt\_MyRec.f2 := **omit**;

**isvalue**(vlt\_MyRec.f2); // shall return false

EXAMPLE 4: Union types

**type** **union** MyUnion {

**integer** ch1,

**integer** ch2

}

**template** MyUnion ts\_MyUnion := { ch1 := 5 }

**template** MyUnion tr\_MyUnion := { ch1 := ? }

**isvalue**(ts\_MyUnion); // shall return true

**isvalue**(tr\_MyUnion); // shall return false

**isvalue**(tr\_MyUnion.ch1); // shall return false

// note, this is different from ischosen(tr\_MyUnion.ch1) as isvalue checks the content of the

// choice ch1, while ischosen is checking if ch1 has been selected or not

**isvalue**(tr\_MyUnion.ch2); // shall return false

EXAMPLE 5: Nested types

**type** **record** MyRecord {

MyUnion u optional

}

**template** MyRecord ts\_MyRecord := { u := ts\_MyUnion }

**template** MyRecord tr\_MyRecord := { u := tr\_MyUnion }

template MyRecord ts\_MyRecord2 := { u := omit }

**isvalue**(ts\_MyRecord.u.ch1); // shall return true

**isvalue**(tr\_MyRecord.u.ch1); // shall return false

**isvalue**(tr\_MyRecord.u.ch2); // shall return false

**isvalue**(ts\_MyRecord.u.ch2); // shall return false

## C.3.4 The IsBound function

**isbound**(**in** **template** any\_type inpar**) return boolean**;

This function is allowed for templates of all data types. The function shall return **true**, if inpar is at least partially initialized. If inpar is of a **record** or **set** type, omitted optional fields shall be considered as initialized, i.e. the function shall also return **true** if at least one optional field of inpar is set to **omit**. The function shall return **false** otherwise. Inaccessible fields (e.g. non-selected alternatives of **union** types, subfields of omitted record and set types or subfields of non-selected union fields) shall be considered as uninitialized, i.e. isbound shall return for them **false**.

The **null** value assigned to default and component references shall be considered as concrete values.

The application of the **isbound** function to a semantically correct template reference shall never result in an error, even if using the reference would normally cause a runtime error when being used e.g. in an expression.

EXAMPLE 1: Simple types

**var** **template** **charstring** vlt\_char;

**isbound**(vlt\_char); // shall return false as v\_char is uninitialized;

vlt\_char := "AB?D"; // template containing a specific value

**isbound**(vlt\_char); // shall return true

vlt\_char := **pattern** "AB?D"; //template containing a pattern matching

**isbound**(vlt\_char); // shall return true

EXAMPLE 2: Special types

**var** **default** vl\_default := **null**;

**isbound**(vl\_default); // shall return true

EXAMPLE 3: Record/set types

**type** **record** MyRec {

**integer** f1,

MyRec f2 **optional**

}

**var** MyRec vl\_MyRec;

**isbound**(vl\_MyRec); // shall return false

vl\_MyRec.f2 := **omit**;

**isbound**(vl\_MyRec); // shall return true as vl\_MyRec is partially initialized,

// field f2 is set to omit

vl\_MyRec := { f1 := 5, f2 := **omit** }

**isbound**(vl\_MyRec); // shall return true as vl\_MyRec is completely initialized

**isbound**(vl\_MyRec.f2.f1); // shall return false as vl\_MyRec.f2.f1 is inaccessible

**isbound**(vl\_MyRec.f1/0); // shall cause an error already during evaluating the argument

// as division by zero is not allowed

**type** **union** MyUnion {

**integer** ch1,

MyRec ch2

}

**var** **template** MyUnion vlt\_MyUnion;

**isbound**(vlt\_MyUnion); // shall return false, as vlt\_MyUnion is uninitialized

**isbound**(vlt\_MyUnion.ch1); // shall return false, as alternative ch1 is uninitialized

vlt\_MyUnion := { ch1 := 5 };

**isbound**(vlt\_MyUnion); // shall return true

**isbound**(vlt\_MyUnion.ch1); // shall return true

**isbound**(vlt\_MyUnion.ch2); // shall return false as the ch2 alternative is not selected

**isbound**(vlt\_MyUnion.ch2.f1); // shall return false as the field f1 is inaccessible

**isbound**(vlt\_MyUnion.ch1/0); // shall cause an error already during evaluating the argument

// as division by zero is not allowed

## C.3.5 Matching mechanism detection

**istemplatekind** (**in template** any\_type invalue, **in** **charstring** kind) **return boolean**

This function allows to examine if a template contains a certain kind of the matching mechanisms.

If the matching mechanism kind enquired is matching a specific value (clause B.1.1), a matching mechanism instead of values (clause B.1.2) or matching character pattern (clause B.1.5), the function shall return **true** if the content of the invalue parameter is of the same kind.

If the matching mechanism kind enquired is a matching mechanism inside values (clause B.1.3), the function shall return **true** if the template in the invalue parameter contains this kind of matching mechanism on the first level of nesting.

If the matching mechanism kind enquired is a matching attribute (clause B.1.4), the function shall return **true** if the template in the invalue parameter has this kind of matching attribute attached to it directly (i.e. it doesn’t count if the attribute is attached to a field of invalue at any level of nesting).

In all other cases the function returns **false**.

The kind parameter shall be one of the strings listed in table C.1.

Table C.1: Allowed values of kind parameter

| **Value of kind parameter** | **Searched matching mechanism** | |
| --- | --- | --- |
| **Name** | **Clause reference** |
| "value" | Specific value | B.1.1 |
| "list" | Template list | B.1.2.1 |
| "complement" | Complemented template list | B.1.2.2 |
| "AnyValue", "?" | Any value | B.1.2.3 |
| "AnyValueOrNone", "\*" | Any value or none | B.1.2.4 |
| "range" | Value range | B.1.2.5 |
| "superset" | SuperSet | B.1.2.6 |
| "subset" | SubSet | B.1.2.7 |
| "omit" | Omit | B.1.2.8 |
| "@encoded" | Encoded value | B.1.2.9 <see CR6736> |
| "AnyElement" | Any element | B.1.3.1 |
| "AnyElementsOrNone" | Any number of elements or none | B.1.3.2 |
| "permutation" | Permutation | B.1.3.3 |
| "length" | Length restriction | B.1.4.1 |
| "ifpresent" | The IfPresent indicator | B.1.4.2 |
| "pattern" | Matching character pattern | B.1.5 |

NOTE: Clause E.2.2.5 includes the type definition TemplateKind and a constant for each of the allowed values of the kind parameter. It is recommended to use the istemplatekind function in combination with this type and these constants to ease the checking of correct usage and to improve the readability of test specs.

***Restrictions***

In addition to the general error causes given in clause 16.1.2, the following restrictions apply:

1. Calling the istemplatekind function with a different second parameter than stated in table C.1 shall lead to an error.

EXAMPLE:

**type record of integer** RoI;

...

**var template integer** vt\_1 := ?, vt\_2 := (0,1,2) **ifpresent**;

**var template** RoI vt\_3:= { **permutation**(1, 2, 3), ? };  
**var boolean** v\_res;  
...  
v\_res := **istemplatekind**(vt\_1, "AnyValue"); // true  
v\_res := **istemplatekind**(vt\_1, "AnyValueOrNone"); // false  
v\_res := **istemplatekind**(vt\_2, "complement"); // false  
v\_res := **istemplatekind**(vt\_2, "list"); // true  
v\_res := **istemplatekind**(vt\_2, "ifpresent"); // true

v\_res := **istemplatekind**(vt\_3, "permutation"); // true

v\_res := **istemplatekind**(vt\_3, "AnyElement"); // true

# C.4 String/list handling functions

## C.4.1 The Regexp function

**regexp [@nocase]** (

**in** **template** **(value)** any\_character\_string\_type inpar,

**in** **template** **(present)** any\_character\_string\_type expression,

**in integer** groupno

) **return** any\_character\_string\_type

This function first matches the parameter inpar (or in case inpar is a template, its value equivalent)against the expression in the second parameter according to the pattern matching specified in clause B.1.5. If expression is not a template containing a pattern matching mechanism, it shall be processed by this predefined function as if it was a character pattern as described in clause B.1.5. If the **@nocase** modifier is present, this and all subsequent matchings shall be done in a case-insensitive way, as specified in clause B.1.5.6. If inpar is a literal (i.e. type is not explicitly given) the corresponding type shall be retrieved from the value contents

If this matching is unsuccessful, an empty string shall be returned.

If this matching is successful, the substring of inpar shall be returned, which matched the groupno-s group of expression during the matching. Group numbers are assigned by the order of occurrences of the opening bracket of a group and counted starting from 0 by step 1.

The parameters inpar and expression shall be a value or a template of **charstring** or **universal charstring** types. In case inpar is a template, it shall contain the specific value matching mechanism only. When expression is a template it shall contain the specific value or pattern matching mechanisms only. The parameter groupno shall be a non-negative integer. The type of the character string returned is the root type of inpar.

NOTE: This function differs from other well-known regular expression matching implementations in that:

a) It shall match the whole inpar string instead of only a substring.

b) It starts counting groups from 0, while in some other implementations the first group is referenced by 1 and the whole substring matched by the expression is referenced by 0.

In addition to the general error causes in clause 16.1.2, error causes are:

* when inpar is a template, it contains other matching mechanism than specific value or character pattern;
* when expression is a template, it contains other matching mechanism than specific value or character pattern;
* inpar is of charstring type and expression is of universal charstring type;
* groupno is a negative integer;
* there is no groupno -s group in expression.

EXAMPLE:

// Given

**var charstring** myInput := " simple text for a regexp example ";

**var charstring** myString;

myString := **regexp**(myInput,**charstring**:"?+(text)?+",0);

// will return "text"

myString := **regexp**(myInput,**charstring**:"?+(text)?+",1);

// causes an error as there is no group with index 1

myString := **regexp**(myInput,**charstring**:"(?+)(text)(?+)",0);

// will return " simple "

myString := **regexp**(myInput,**charstring**:"(?+)(text)(?+)",2);

// will return " for a regexp example "

myString := **regexp**(myInput,**charstring**:"((?+)(text)(?+))",0);

// will return the whole inpar, i.e. " simple text for a regexp example "

myString := **regexp**(myInput,**charstring**:"(([ ]+)(text)(?+))",0);

// will return an empty string as expression does not matches inpar

myString := **regexp**(myInput,**universal** **charstring**:"?+(text)?+",0);

// will cause an error as inpar is of type charstring, while

// expression is of type universal charstring

myInput := " date: 2001-10-20 ; msgno: 17; exp ";

**var** **template** **charstring** myPattern :=

**pattern** "([ \t]#(0,)date:[ \d\-]#(0,);[ \t]#(0,)msgno: (\d#(1,3)); (exp)#(0,1)) [ \t]#(0,)";  
 // please note, that only the very first opening bracket and the bracket before "\d#(1,3)"

// denotes groups; "#(0,)", "#(1,3)" and "#(0,1)" denotes matching the preceding expression

// several time

myString := **regexp**(myInput, myPattern,0);

// will return the input string but the whitespace at the end,

// i.e. " date: 2001-10-20 ; msgno: 17; exp"

myString := **regexp**(myInput, myPattern,1);

// will return the value "17"

//An example of a wrapper function to count groups from 1 and return the complete p\_inpar

//if p\_groupno equals 0

**function** regexp0(

**in** **template** **charstring** p\_inpar,

**in** **template** **charstring** p\_expression,

**in** **integer** p\_groupno)

**return** **charstring** {

**var** **template** **charstring** extended\_expr := **pattern** "({p expression})";

**return** **regexp**(p inpar, extended\_expr, p\_groupno )

}

## C.4.2 The Substring function

**substr**(  
 **in template** **(present)** any\_string\_or\_sequence\_type inpar,   
 **in integer** index,   
 **in integer** count  
) **return** input\_string\_or\_sequence\_type

This function returns a substring or subsequence from a value that is of a binary string type (**bitstring**, **hexstring**, **octetstring**), a character string type (**charstring**, **universal** **charstring**), or a sequence type (**record of**, **set of** or array). If inpar is a literal (i.e. type is not explicitly given) the corresponding type shall be retrieved from the value contents. The type of the substring or subsequence returned is the root type of the input parameter. The starting point of substring or subsequence to return is defined by the second parameter (index). Indexing starts from zero. The third input parameter (count) defines the length of the substring or subsequence to be returned. The units of length for string types are as defined in table 4 of the present document. For sequence types, the unit of length is element.

NOTE: Please note that the root types of arrays is **record of**, therefore if inpar is an array the returned type is **record of**. This, in some cases, may lead to different indexing in inpar and in the returned value.

When used on templates of character string types, only the inside matching mechanisms *AnyElement* and *AnyElementsOrNone* are allowed in inpar and the function shall return the character representation of the matching mechanisms, i.e. "?" for *AnyElement* and "\*" for *AnyElementsOrNone*. When inpar is a template of binary string or sequence type or is an array, only the specific value and *AnyElement* matching mechanisms are allowed and the substring or subsequence to be returned shall not contain *AnyElement.*

In addition to the general error causes in clause 16.1.2, error causes are:

* index is less than zero;
* count is less than zero;
* index+count is greater than **lengthof**(inpar);
* inpar is a template of a character string type and contains a matching mechanism other than *AnyElement* or *AnyElementsOrNone*;
* inpar is a template of a binary string or sequence type or array and it contains other matching mechanism as specific value and *AnyElement*;
* inpar is a template of a binary string or sequence type or array and the substring or subsequence to be returned contains the *AnyElement* matching mechanism.

EXAMPLE:

**substr**('00100110'B, 3, 4) // returns '0011'B

**substr**('ABCDEF'H, 2, 3) // returns 'CDE'H

**substr**('01AB23CD'O, 1, 2) // returns 'AB23'O

**substr**("My name is JJ", 11, 2) // returns "JJ"

**substr**({ 4, 5, 6 }, 1, 2) // returns {5, 6}

## C.4.3 The Replace function

**replace**(  
 **in** any\_string\_or\_sequence\_type inpar,   
 **in integer** index,  
 **in integer** len,

**in** any\_string\_or\_sequence\_type repl  
) **return** any\_string\_or\_sequence type

This function replaces the substring or subsequence of value inpar at index index of length len with the string or sequence value repl and returns the resulting string or sequence. inparshall not be modified. If len is 0 the string or sequence repl is inserted. If index is 0, repl is inserted at the beginning of inpar. If index is **lengthof**(inpar), repl is inserted at the end of inpar. If inpar is a literal (i.e. type is not explicitly given) the corresponding type shall be retrieved from the value contents. inparand repl, and the returned string or sequence shall be of the same root type. The function replace can be applied to **bitstring**, **hexstring**, **octetstring**, or any character string, **record** **of**, **set** **of**, or arrays. Note that indexing in strings starts from zero.

NOTE: Please note that the root types of arrays is **record of**, therefore if inpar or repl or both are an array, the returned type is **record of**. This, in some cases, may lead to different indexing in inpar and/or repl and in the returned value.

In addition to the general error causes in clause 16.1.2, error causes are:

* inpar or repl are not of string, **record** **of**, **set** **of**, or array type;
* inpar and repl are of different root type;
* index is less than 0 or greater than **lengthof**(inpar);
* len is less than 0 or greater than **lengthof**(inpar);
* index+len is greater than **lengthof**(inpar).

EXAMPLE:

**replace** ('00000110'B, 1, 3, '111'B) // returns '01110110'B

**replace** ('ABCDEF'H, 0, 2, '123'H) // returns '123CDEF'H

**replace** ('01AB23CD'O, 2, 1, 'FF96'O) // returns '01ABFF96CD'O

**replace** ("My name is JJ", 11, 1, "xx") // returns "My name is xxJ"

**replace** ("My name is JJ", 11, 0, "xx") // returns "My name is xxJJ"

**replace** ("My name is JJ", 2, 2, "x") // returns "Myxame is JJ",

**replace** ("My name is JJ", 12, 2, "xx") // produces test case error

**replace** ("My name is JJ", 13, 2, "xx") // produces test case error

**replace** ("My name is JJ", 13, 0, "xx") // returns "My name is JJxx"

# C.5 Codec functions

## C.5.1 The encoding function

**encvalue**(**in template (value)** any\_typeinpar) **return bitstring**

The **encvalue** function encodes a value or template into a bitstring. When the actual parameter that is passed to inpar is a template, it shall resolve to a specific value (the same restrictions apply as for the argument of the **send** statement). The returned bitstring represents the encoded value of inpar, however, the TTCN-3 test system need not make any check on its correctness.

In addition to the general error causes in clause 16.1.2, error causes are:

* Encoding fails due to a runtime system problem (i.e. no encoding function exists for the actual type of inpar).

## C.5.2 The decoding function

**decvalue**(**inout bitstring** encoded\_value**, out** any\_typedecoded\_value) **return integer**

The **decvalue** function decodes a bitstring into a value. The test system shall suppose that the bitstring encoded\_value represents an encoded instance of the actual type of decoded\_value.

If the decoding was successful, then the used bits are removed from the parameter encoded\_value, the rest is returned (in the parameter encoded\_value), and the decoded value is returned in the parameter decoded\_value. If the decoding was unsuccessful, the actual parameters for encoded\_value and decoded\_value are not changed. The function shall return an integer value to indicate success or failure of the decoding below:

* The return value 0 indicates that decoding was successful.
* The return value 1 indicates an unspecified cause of decoding failure. This value is also returned if the encoded\_value parameter contains an unitialized value.
* The return value 2 indicates that decoding could not be completed as encoded\_value did not contain enough bits.

The restrictions in clause 16.1.2 apply.

## C.5.3 The encoding to universal charstring function

**encvalue\_unichar**(**in template** (**value**)any\_typeinpar,

**in** **charstring** string\_serialization := "UTF-8")

**return universal charstring**

The **encvalue\_unichar** function encodes a value or template into a universal charstring. When the actual parameter that is passed to inpar is a template, it shall resolve to a specific value (the same restrictions apply as for the argument of the **send** statement). The returned universal charstring represents the encoded value of inpar, however, the TTCN-3 test system need not make any check on its correctness. If the optional string\_serialization parameter is omitted, the default value "UTF-8" is used.

The following values (see ISO/IEC 10646 [2]) are allowed as string\_serialization actual parameters (for the description of the UCS encoding scheme see clause 27.5):

1. "UTF-8"
2. "UTF-16"
3. "UTF-16LE"
4. "UTF-16BE"
5. "UTF-32"
6. "UTF-32LE"
7. "UTF-32BE"

The serialized bitstring shall not include the optional signature (see clause 10 of ISO/IEC 10646 [2], also known as byte order mark).

In case of "UTF-16" and "UTF-32" big-endian ordering shall be used (as described in section 10.4 and 10.7 of ISO/IEC 10646 [2]).

The specific semantics of this function are explained by the following TTCN-3 definition:

**function** encvalue\_unichar(any\_type v, **charstring** enc) **return** **universal** **charstring** {

**return** oct2unichar(bit2oct(encvalue(v)), enc);

}

The encvalue\_unichar function first invokes the encvalue function in order to encode the value passed in the inpar parameter to a bitstring. The bitstring is then converted to an octetstring by the bit2oct function and subsequently to a universal charstring using the oct2unichar function. The string\_serialization parameter defines how the encoded octets (in fact the encoded bitstring received from the codec) contain the characters. The universal charstring value is then returned as the result of the encvalue\_unichar function.

In addition to the general error causes in clause 16.1.2, error causes are:

* Encoding fails due to a runtime system problem (i.e. no encoding function exists for the actual type of inpar).
* The given string encoding is not recognized.

## C.5.4 The decoding from universal charstring function

**decvalue\_unichar**(**inout universal charstring** encoded\_value**, out** any\_typedecoded\_value,

**in charstring** string\_serialization:= "UTF-8")

**return integer**

The **decvalue\_unichar** function decodes (part of) a universal charstring into a value. The test system shall suppose that a prefix of the universal charstring encoded\_value represents an encoded instance of the actual type of decoded\_value.

If the decoding was successful, then the characters used for decoding are removed from the parameter encoded\_value, the rest is returned (in the parameter encoded\_value), and the decoded value is returned in the parameter decoded\_value. If the decoding was unsuccessful, the actual parameters for encoded\_value and decoded\_value are not changed. The function shall return an integer value to indicate success or failure of the decoding below:

* The return value 0 indicates that decoding was successful.
* The return value 1 indicates an unspecified cause of decoding failure. This value is also returned if the encoded\_value parameter contains an unitialized value.
* The return value 2 indicates that decoding could not be completed as encoded\_value did not contain enough bits.

If the optional string\_serialization parameter is omitted, the default value "UTF-8" is used.

The following values (see ISO/IEC 10646 [2]) are allowed as string\_serialization actual parameters (for the description of the UCS encoding scheme see clause 27.5):

1. "UTF-8"
2. "UTF-16"
3. "UTF-16LE"
4. "UTF-16BE"
5. "UTF-32"
6. "UTF-32LE"
7. "UTF-32BE"

The serialized bitstring shall not include the optional signature (see clause 10 of ISO/IEC 10646 [2], also known as byte order mark).

In case of "UTF-16" and "UTF-32" big-endian ordering shall be used (as described in section 10.4 and 10.7 of ISO/IEC 10646 [2]).

The semantics of the function can be explained by the following TTCN-3 function:

**function** decvalue\_unichar  
 (**inout** **universal** **charstring** encoded\_value, **out** any\_type decoded\_value,

**in** **charstring** string\_encoding := "UTF-8") **return** **integer** {

**var** **bitstring** str = oct2bit(unichar2oct(encoded\_value, string\_encoding));

**var** **integer** result := decvalue(str, decoded\_value);

**if** (result == 0) { // success

encoded\_value := oct2unichar(bit2oct(str), string\_encoding);

}

**return** result;

}

The decvalue\_unichar function first converts the universal charstring value passed in the encoded\_value parameter into an octetstring using the unichar2oct function. The string\_serialization parameter controls how the characters are converted into octets (in fact how the bitstring sent to the codec contains the characters). The octetstring is subsequently converted into a bitstring by the oct2bit function. This bitstring is then passed as a parameter to the standard decvalue function that performs the actual decoding. In case of successful decoding, the undecoded part of the message is automatically converted from bitstring to octetstring by the bit2oct function and then to universal charstring using the oct2unichar function. This universal charstring is then assigned to the encoded\_value parameter. The result of decoding is then returned to the TE, finishing the decvalue\_unichar call.

The restrictions in clause 16.1.2 apply.

## C.5.5 Retrieving the type of string encoding

**get\_stringencoding(in octetstring** encoded\_value**) return charstring**

The **get\_stringencoding** function analyses the encoded\_value and returns the UCS encoding scheme according to clause 10 of ISO/IEC 10646 [2] (see also clause 27.5 of this document). The identified encoding scheme, or the value “<unknown>”, if the type of encoding cannot be determined unanimously, shall be returned as a character string.

NOTE: The initial octet sequence (also known as byte order mark, BOM), when present, allows identifying the encoding scheme unanimously. When it is not present, other symptoms may be used to identify the encoding scheme unanimously; for example, only UTF-8 may have odd number of octets **and** bit distribution according to table 2 of clause 9.1 of ISO/IEC 10646 [2].

EXAMPLE :

**match** ( **get\_stringencoding**('6869C3BA7A'O,**charstring**:"UTF-8") ) // true  
//(the octetstring contains the UTF-8 encoding of the character sequence "hiúz")

## C.5.6 Removing BOMs of UCS encoding schemes

**remove\_bom**(**in octetstring** encoded\_value) **return octetstring**

The **remove\_bom** function removes the optional FEFF ZERO WIDTH NO-BREAK SPACE sequence that may be present at the beginning of a stream of serialized (encoded) universal character strings to indicate the order of the octets within the encoding form, as defined in clause 10 of ISO/IEC 10646 [2]. If no FEFF ZERO WIDTH NO-BREAK SPACE sequence present in the encoded\_value parameter, the function shall return the value of the parameter without change.

Table: Overview of initial octet sequences used for BOM

|  |  |  |
| --- | --- | --- |
| **Coding scheme** | **initial octet sequence** | **comments** |
| UTF-8 | EF BB BF | signature not required / no effect |
| UTF-16BE | FE FF | no signature meaning |
| UTF-16LE | FF FE | no signature meaning |
| UTF-16 | FE FF FF FE | signature (default FE FF) |
| UTF-32BE | 00 00 FE FF | no signature meaning |
| UTF-32LE | FF FE 00 00 | no signature meaning |
| UTF-32 | 00 00 FE FF FF FE 00 00 | signature (default 00 00 FE FF) |

EXAMPLE :

**remove\_bom**('FEFF0068006900FA007A'O) // returns '0068006900FA007A'O

**remove\_bom**('BC'O) ) // returns 'BC'O

// note that this octetstring doesn’t contain valid UCS character

//example use: automatic decoding of encoded character strings:

**oct2unichar**(**remove\_bom**(MyEncodedCharacterSequence),

**get\_stringencoding**(MyEncodedCharacterSequence))

# C.6 Other functions

## C.6.1 The random number generator function

**rnd([in float** seed**]) return float**

The **rnd** function returns a (pseudo) random number less than 1 but greater or equal to 0. The random number generator is initialized per test component and for the control part by means of an optional seed value (a numerical float value). If no new seed is provided, the last generated number will be used as seed for the next random number. Without a previous initialization a value calculated from the system time will be used as seed value when **rnd** is used the first time in a test component or the control part.

Each time the **rnd** function is initialized with the same seed value, it shall repeat the same sequence of random numbers.

NOTE: For the purpose of keeping parallel testing deterministic, each test component, as well as the control part has its own random seed. This allows for better reproduciblity of test executions. Thus, the rnd function will always use the seed of the component or control part which calls it.

To produce a random integers in a given range, the following formula can be used:

**float2in**t(**int2floa**t(*upperbound* - *lowerbound* +1)\***rnd**()) + *lowerbound*

// Here, *upperbound* and *lowerbound* denote highest and lowest number in range.

In addition to the general error causes in clause 16.1.2, error causes are:

* seed is **infinity**, **-infinity** or **not\_a\_number**.

## C.6.2 The testcasename function

**testcasename**() **return charstring**

The **testcasename** function shall return the unqualified name of the actually executing test case.

EXAMPLE 1:

**module** MyTCModule {

:

**testcase** MyTestCase1 () **runs** **on** MTC **system** TSI

{

**var** **charstring** v\_TCname := **testcasename** ();

// will return the charstring "MyTestCase1"

:

}

:

**testcase** MyTestCase2 () runs on MTC system TSI

{

:

}

:

}

**module** MyTSModule {

:

**function** MyStartAPTC() **runs** **on** PTC {

**var** **charstring** v\_TCname := **testcasename** ();

// will return charstring "MyTestCase1", if the function is  
 // called by a test component during the execution of MyTestCase1

// will return charstring "MyTestCase2", if the function is  
 // called by a test component when MyTestCase2 is being executed

}

:

}

When the function **testcasename** is called if the control part is being executed but no testcase, it shall return the empty string.

EXAMPLE 2:

**module** MyModule {

:

**control**

{

**var** **charstring** v\_TCname := **testcasename** () // will return charstring ""

:

}

:

}

The general error causes in clause 16.1.2 apply.

## C.6.3 The hostId function

**hostid**(**in charstring** idkind := "Ipv4orIPv6") **return charstring**

The **hostid** function shall return the host id of the test component or module control executing the **hostid** function in form of a character string. The **in** parameter idkind allows to specify the expected id format to be returned.

Predefined idkind values are:

* "Ipv4orIPv6": The contents of the returned character string is an Ipv4 address. If no Ipv4 address, but an Ipv6 address is available, a character string representation of the Ipv6 address is returned.
* "Ipv4": The contents of the returned character string shall be an Ipv4 address.
* "Ipv6": The contents of the returned characterstring shall be an Ipv6 address.

The **hostid** function shall return the empty string, if it cannot retrieve any host id or a host id of a kind different from the kind defined by the actual idkind parameter.

The general error causes in clause 16.1.2 apply.

EXAMPLE:

// assume

**testcase** MyTestCase () **runs** **on** MTC **system** TSI

{

:

**var** **charstring** v\_MyHostId := **hostid** ("Ipv4");

:

}

// assume further the following statement in module control

**execute**(MyTestCase(), -, "127.0.0.1"**)**;

// In this setting, v\_MyHostId will have the value "127.0.0.1" after the execution of oolea

Annex D (normative):  
Preprocessing macros

This annex defines a set of preprocessing macros. A preprocessing macro is a macro that is replaced by a preprocessor or a compiler with a **charstring** or **integer** value respectively before compilation. Preprocessing macros shall not be replaced inside literal **charstring** values and templates and not in TTCN-3 comments. In the TTCN-3 code, it can be used like a **charstring** or an **integer** value respectively.

# D.1 Preprocessing macro \_\_MODULE\_\_

The **\_\_MODULE\_\_** preprocessing macro denotes the module name in which the macro is used. A preproceessor or compiler shall replace all occurrences of **\_\_MODULE\_\_** with the actual module name in form of a **charstring** value.

# D.2 Preprocessing macro \_\_FILE\_\_

The **\_\_FILE\_\_** preprocessing macro denotes the canonical (absolute) file name, i.e. the full path and the basic file name, in which the macro is used. A preproceessor or compiler shall replace all occurrences of **\_\_FILE\_\_** with the actual canonical (absolute) file name in form of a **charstring** value.

NOTE: The format of the canonical file name depends on the operating system and is not specified by the present document.

EXAMPLE:

**const** **charstring** MyConst:= **\_\_FILE\_\_**;

//MyConst is for example "/home/myhome/MyTest.ttcn"

# D.3 Preprocessing macro \_\_BFILE\_\_

The **\_\_BFILE\_\_** preprocessing macro denotes the basic (relative) file name, i.e. without path, in which the macro is used. A preproceessor or compiler shall replace all occurrences of **\_\_BFILE\_\_** with the actual basic (relative) file name in form of a **charstring** value.

NOTE: The format of the basic file name depends on the operating system and is not specified by the present document.

EXAMPLE:

**const** **charstring** MyConst:= **\_\_BFILE\_\_**;

// MyConst is for example "MyTest.ttcn"

# D.4 Preprocessing macro \_\_LINE\_\_

The **\_\_LINE\_\_** preprocessing macro denotes the line number of the file in which the macro is used. A preproceessor or compiler shall replace each occurrence of **\_\_LINE\_\_** with the actual line number in form of an **integer** value.

A file starts with line number **1**. Each newline shall increase the line number by **1** (see clause A.1.5.1). Also newlines of commented lines shall increase the line number by **1**.

# D.5 Preprocessing macro \_\_SCOPE\_\_

The **\_\_SCOPE\_\_** preprocessing macro denotes the unqualified name of the lowest named basic scope unit in which the macro is used. According to clause 5.2, basic scope units of TTCN-3 are module definitions part, module control part, component types, functions, altsteps, test cases, statement blocks, templates and user defined named types. Statement blocks have no name and therefore, a **\_\_SCOPE\_\_** preprocessing macro used in a statement block refers to the next higher named basic scope unit.

A preprocessor or compiler shall replace all occurrences of **\_\_SCOPE\_\_** with a **charstring** value which includes:

1. the module name, if the lowest named scope unit is the module definitions part;
2. "**control**", if the lowest named scope unit is the module control part;
3. a component type name, if the lowest named scope unit is a component type definition;
4. a test case name, if the lowest named scope unit is a test case definition;
5. an altstep name, if the lowest named scope is an altstep definition;
6. a function name, if the lowest named scope is a function definition;
7. a template name, if the lowest named scope is a template definition (local or global); or
8. the type name, if the lowest named scope is a user defined named type definition.

NOTE: The **\_\_SCOPE\_\_** preprocessing macro cannot be used to retrieve the names of other kinds of definitions, like for example names of groups of definitions or names of global constants.

EXAMPLE 1: Using \_\_SCOPE\_\_ in constant and template definitions

**module** MyModule

{

**const** **charstring** MyConst := \_\_SCOPE\_\_; // MyConst contains "MyModule"

**template** **charstring** MyTemplate := \_\_SCOPE\_\_; // MyTemplate contains "MyTemplate"

**type** **record** MyRecord1

{

**charstring** field11,

**charstring** field12

}

**template** MyRecord1 MyTemplate1 (charstring p := \_\_SCOPE\_\_) :=

{

field11 := p,

field12 := \_\_SCOPE\_\_ // field12 contains "MyTemplate1"

}

**function** MyFunction() {

**var** **template** MyRecord1 v\_Myvar1 := MyTemplate1;

// field11 of MyTemplate1 will contain the default value of parameter p,

// i.e. "MyTemplate1"

};

}

EXAMPLE 2: Using \_\_SCOPE\_\_ in a structured type scope

**type** **record** MyRecord2 {

**charstring** field21,

**charstring** field22 ("a", "b", \_\_SCOPE\_\_)

// list constrained field: a legal values are "a", "b" or "MyRecord2"

}

**template** MyRecord2 MyTemplate2 := {

field21 := "a",

field22 := "MyRecord2" // a valid specific value matching

}

**template** MyRecord2 MyTemplate3 := {

field21 := "a",

field22 := \_\_SCOPE\_\_

// Causes an error as \_\_SCOPE\_\_ is replaced with "MyTemplate3",

// which is violating the list constraint of field22

}

EXAMPLE 3: Using \_\_SCOPE\_\_ in an embedded structured type scope

**type** **record** MyRecord3 {

**charstring** field31,

**record** {

**charstring** field321 ("a", "b", \_\_SCOPE\_\_)

// list constrained field: a legal value shall be "a", "b" or "MyRecord3"

} field32

}

**template** MyRecord3 MyTemplate4 :=

{

field31 := "a",

field32 :=

{

field321 := "MyRecord3" // a valid specific value matching

}

}

**template** MyRecord3 MyTemplate5 :=

{

field31 := "a",

field32 :=

{

field321 := \_\_SCOPE\_\_

// Causes and error as \_\_SCOPE\_\_ is replaced with "MyTemplate5",

// which is violating the list constraint of field321

}

}

Annex E (informative):  
Library of Useful Types

# E.1 Limitations

Names of types added to this library are to be unique within the whole language and within the library (i.e. are not to be one of the names defined in annex C). Names defined in this library are not to be used by TTCN‑3 users as identifiers of other definitions than given in this annex.

NOTE: Therefore type definitions given in this annex may be repeated in TTCN‑3 modules but no type distinct from the one specified in this annex can be defined with one of the identifiers used in this annex.

# E.2 Useful TTCN‑3 types

## E.2.1 Useful simple basic types

### E.2.1.0 Signed and unsigned single byte integers

These types support integer values of the range from -128 to 127 for the signed and from 0 to 255 for the unsigned type. The value notation for these types is the same as the value notation for the integer type. Values of these types are to be encoded and decoded as they were represented on a single byte within the system independently from the actual representation form used.

NOTE: Encoding of values of these types may be the same or may differ from each other and from the encoding of the integer type (the root type of these useful types) depending on the actual encoding rules used. Details of encoding rules are out of the scope of the present document.

Type definitions for these types are:

**type integer** byte (-128 .. 127) **with** { **variant** "8 bit" };

**type integer** unsignedbyte (0 .. 255) **with** { **variant** "unsigned 8 bit" };

### E.2.1.1 Signed and unsigned short integers

These types support integer values of the range from -32 768 to 32 767 for the signed and from 0 to 65 535 for the unsigned type. The value notation for these types is the same as the value notation for the integer type. Values of these types are to be encoded and decoded as they were represented on two bytes within the system independently from the actual representation form used.

NOTE: Encoding of values of these types may be the same or may differ from each other and from the encoding of the integer type (the root type of these useful types) depending on the actual encoding rules used. Details of encoding rules are out of the scope of the present document.

Type definitions for these types are:

**type integer** short (-32768 .. 32767) **with** { **variant** "16 bit" };

**type integer** unsignedshort (0 .. 65535) **with** { **variant** "unsigned 16 bit" };

### E.2.1.2 Signed and unsigned long integers

These types support integer values of the range from -2 147 483 648 to 2 147 483 647 for the signed and from 0 to 4 294 967 295 for the unsigned type. The value notation for these types is the same as the value notation for the integer type. Values of these types are to be encoded and decoded as they were represented on four bytes within the system independently from the actual representation form used.

NOTE: Encoding of values of these types may be the same or may differ from each other and from the encoding of the integer type (the root type of these useful types) depending on the actual encoding rules used. Details of encoding rules are out of the scope of the present document.

Type definitions for these types are:

**type integer** long (-2147483648 .. 2147483647)  
 **with** { **variant** "32 bit" };

**type integer** unsignedlong (0 .. 4294967295)  
 **with** { **variant** "unsigned 32 bit" };

### E.2.1.3 Signed and unsigned longlong integers

These types support integer values of the range from -9 223 372 036 854 775 808 to 9 223 372 036 854 775 807 for the signed and from 0 to 18 446 744 073 709 551 615 for the unsigned type. The value notation for these types is the same as the value notation for the integer type. Values of these types are to be encoded and decoded as they were represented on eight bytes within the system independently from the actual representation form used.

NOTE: Encoding of values of these types may be the same or may differ from each other and from the encoding of the integer type (the root type of these useful types) depending on the actual encoding rules used. Details of encoding rules are out of the scope of the present document.

Type definitions for these types are:

**type integer** longlong (-9223372036854775808 .. 9223372036854775807)  
 **with** { **variant** "64 bit" };

**type integer** unsignedlonglong (0 .. 18446744073709551615)  
 **with** { **variant** "unsigned 64 bit" };

### E.2.1.4 IEEE 754 floats

These types support the ANSI/IEEE 754 [6] for binary floating-point arithmetic. The type IEEE 754 [6] float supports floating-point numbers with base 10, exponent of size 8, mantissa of size 23 and a sign bit. The type IEEE 754 [6] double supports floating-point numbers with base 10, exponent of size 11, mantissa of size 52 and a sign bit. The type IEEE 754 [6] extfloat supports floating-point numbers with base 10, minimal exponent of size 11, minimal mantissa of size 32 and a sign bit. The type IEEE 754 [6] extdouble supports floating-point numbers with base 10, minimal exponent of size 15, minimal mantissa of size 64 and a sign bit.

Values of these types are to be encoded and decoded according to the IEEE 754 [6] definitions. The value notation for these types is the same as the value notation for the float type (base 10).

NOTE: Precise encoding of values of this type depends on the actual encoding rules used. Details of encoding rules are out of the scope of the present document.

Type definitions for these types are:

**type** **float** IEEE754float **with** { **variant** "IEEE754 float" };

**type** **float** IEEE754double **with** { **variant** "IEEE754 double" };

**type** **float** IEEE754extfloat **with** { **variant** "IEEE754 extended float" };

**type** **float** IEEE754extdouble **with** { **variant** "IEEE754 extended double" };

## E.2.2 Useful character string types

### E.2.2.0 UTF-8 character string "utf8string"

This type supports the whole character set of the TTCN‑3 type **universal charstring** (see paragraph d) of clause 6.1.1). Its distinguished values are zero, one, or more characters from this set. Values of this type are entirely (e.g. each character of the value individually) to be encoded and decoded according to the UCS Transformation Format 8 (UTF-8) as defined in annex R of ISO/IEC 10646 [2]. The value notation for this type is the same as the value notation for the **universal charstring** type.

The type definition for this type is:

**type** **universal** **charstring** utf8string **with** { **variant** "UTF-8" };

### E.2.2.1 BMP character string "bmpstring"

This type supports the Basic Multilingual Plane (BMP) character set of ISO/IEC 10646 [2]. The BMP represents all characters of plane 00 of group 00 of the Universal Multiple-octet coded Character Set. Its distinguished values are zero, one, or more characters from the BMP. Values of this type are entirely (e.g. each character of the value individually) to be encoded and decoded according to the UTF-16 coded representation form (see clause 9.2 of ISO/IEC 10646 [2]). The value notation for this type is the same as the value notation for the **universal charstring** type.

NOTE: The type "bmpstring" supports a subset of the TTCN‑3 type **universal charstring.**

The type definition for this type is:

**type** **universal charstring** **bmpstring** ( char ( 0,0,0,0 ) .. char ( 0,0,255,255) )

**with** { **variant** "UTF-16" };

### E.2.2.2 UTF-16 character string "utf16string"

This type supports all characters of planes 00 to 16 of group 00 of the Universal Multiple-octet coded Character Set (see ISO/IEC 10646 [2]). Its distinguished values are zero, one, or more characters from this set. Values of this type are entirely (e.g. each character of the value individually) to be encoded and decoded according to the UCS Transformation Format 16 (UTF-16) as defined in annex Q of ISO/IEC 10646 [2]. The value notation for this type is the same as the value notation for the **universal charstring** type.

NOTE: The type "utf16string" supports a subset of the TTCN‑3 type **universal charstring.**

The type definition for this type is:

**type** **universal charstring** **utf16string** ( char ( 0,0,0,0 ) .. char ( 0,16,255,255) )  
 **with** { **variant** "UTF-16" };

### E.2.2.3 ISO/IEC 10646 character string "iso8859string"

This type supports all characters in all alphabets defined in the multiparty standard ISO/IEC 10646 [2]. Its distinguished values are zero, one, or more characters from the ISO/IEC 10646 [2] character set. Values of this type are entirely (e.g. each character of the value individually) to be encoded and decoded according to the coded representation as specified in ISO/IEC 10646 [2] (an 8-bit coding). The value notation for this type is the same as the value notation for the **universal charstring** type.

NOTE 1: The type "iso8859string" supports a subset of the TTCN‑3 type **universal charstring.**

NOTE 2: In each ISO/IEC 10646 [2] alphabet the lower part of the character set table (positions 02/00 to 07/14) is compatible with the Recommendation ITU‑T T.50 [4] character set. Hence all extra language specific characters are defined for the upper part of the character table only (positions 10/00 to 15/15).

The type definition for this type is:

**type** **universal charstring** **iso8859string** ( char ( 0,0,0,0 ) .. char ( 0,0,0,255) )  
 **with** { **variant** "8 bit" };

### E.2.2.4 Status values for TTCN-3 objects

Type and constants defined in this clause support the secure usage of the checkstate port operation defined in clause 22.5.5.

The type definition for this type is:

**type** **charstring** objState ("Started", "Halted", "Stopped", "Connected", "Mapped", "Linked");

Useful constant definitions for working with object states are:

**const** objState STARTED := "Started";

**const** objState HALTED := "Halted";

**const** objState STOPPED := "Stopped";

**const** objState CONNECTED := "Connected";

**const** objState MAPPED := "Mapped";

**const** objState LINKED := "Linked";

### E.2.2.5 Template kinds of TTCN-3 objects

Type and constants defined in this clause support the secure usage of the predefined istemplatekind function, described in clause C.3.5.

The type definition for this type is:

**type** **charstring** TemplateKind ("value", "list", "complement", "AnyValue", "?", "AnyValueOrNone", "\*", "range", "subset", "superset", "omit", "@encoded", "AnyElement", "AnyElementsOrNone", "permutation", "length", "ifpresent", "pattern");

Useful constant definitions for working with template kinds are:

**const** TemplateKind VALUE := "value";

**const** TemplateKind LIST := "list";

**const** TemplateKind COMPLEMENT := "complement";

**const** TemplateKind ANY\_VALUE := "AnyValue";

**const** TemplateKind ANY\_VALUE\_OR\_NONE := "AnyValueOrNone";

**const** TemplateKind RANGE := "range";

**const** TemplateKind SUBSET := "subset";

**const** TemplateKind SUPERSET := "superset";

**const** TemplateKind OMIT := "omit";

**const** TemplateKind ENCODED := "@encoded";

**const** TemplateKind ANY\_ELEMENT := "AnyElement";

**const** TemplateKind ANY\_ELEMENTS\_OR\_NONE := "AnyElementsOrNone";

**const** TemplateKind PERMUTATION := "permutation";

**const** TemplateKind LENGTH := "length";

**const** TemplateKind IFPRESENT := "ifpresent";

**const** TemplateKind PATTERN := "pattern";

## E.2.3 Useful structured types

### E.2.3.0 Fixed-point decimal literal

This type supports the use of fixed-point decimal literal as defined in the IDL Syntax and Semantics version 2.6 [i.10]. It is specified by an integer part, a decimal point and a fraction part. The integer and fraction parts both consist of a sequence of decimal (base 10) digits. The number of digits is stored in "digits" and the size of the fraction part is given in "scale". The digits itself are stored in "value\_". Value notation for this type is the same as the value notation for the record type. Values of this type are to be encoded and decoded as IDL fixed point decimal values.

NOTE: Precise encoding of values of this type depends on the actual encoding rules used. Details of encoding rules are out of the scope of the present document.

The type definition for this type is:

**type record** **IDLfixed** {  
 **unsignedshort** digits,  
 **short** scale,  
 **charstring** value\_  
 }  
 **with** { **variant** "IDL:fixed FORMAL/01-12-01 v.2.6" };

## E.2.4 Useful atomic string types

### E.2.4.1 Single Recommendation ITU‑T T.50 character type

A type whose distinguished values are single characters of the version of Recommendation ITU‑T T.50 [4] complying to the International Reference Version (IRV) as specified in clause 8.2 of Recommendation ITU‑T T.50 [4] (see also note 1 to clause 6.1.1).

The type definition for this type is:

**type** **charstring** char646 **length (1)**;

NOTE: The special string "8 bit" defined in clause 27.5 may be used with this type to specify a given encoding for its values. Also, other properties of the base type can be changed by using attribute mechanisms.

### E.2.4.2 Single universal character type

A type whose distinguished values are single characters from ISO/IEC 10646 [2].

The type definition for this type is:

**type universal** **charstring** uchar **length (1)**;

NOTE: Special strings defined in clause 27.5 except "8 bit" may be used with this type to specify a given encoding for its values. Also, other properties of the base type can be changed by using attribute mechanisms.

### E.2.4.3 Single bit type

A type whose distinguished values are single binary digits.

The type definition for this type is:

**type bitstring** bit **length** (1);

### E.2.4.4 Single hex type

A type whose distinguished values are single hexadecimal digits.

The type definition for this type is:

**type hexstring** hex **length** (1);

### E.2.4.5 Single octet type

A type whose distinguished values are pairs of hexadecimal digits.

The type definition for this type is:

**type octetstring** octet **length** (1);

Annex F (informative):  
Operations on TTCN‑3 active objects

This annex describes in a short form the semantics of operations on active objects in TTCN‑3 being test components, timers and ports. This dynamic behaviour is written in the form of state machines with:

* the states being named and identified as nodes;
* the initial state being identified by an incoming arrow;
* transitions between states connecting two states (not necessarily different states) and identified as arrows;
* transitions being marked with the enabling condition for that transition (i.e. operation or statement calls) and the resulting condition (for example a test case error), both are separated by '/':
* operation and statement calls are the TTCN‑3 operations and statements applicable to the object (written in bold);
* error as a resulting condition means testcase error (written in bold);
* null as a resulting condition means that except of a possible state change no other results apply (written in bold);
* match/no match refers to the matching result of a transition (written in bold);
* concrete values are boolean or float results (written in bold italics);
* all other resulting conditions are textually described (written in standard font);
* notes are used to explain further details of the state machine.

For further details, please refer to the operational semantics of TTCN‑3 [1]. In case of any contradiction between this annex and the operational semantics of TTCN‑3 [1] the latter takes precedence.

# F.1 Test components

## F.1.1 Test component references

Variables of test component types, the **self** and **mtc** operations are used to reference test components. The **start**, **stop**, **done** and **running** operations are not directly applied on test components but on component references. The test system has to decide if the operation requested should affect the component object itself or other action is appropriate (e.g. an error occurs when the reference of a stopped PTC is used in a component start operation). The **create** operation used to create PTCs returns a unique reference to the created PTC, which is typically bound to a variable of component type. The behaviour related to variables of component type themselves is shown in figure F.1.



NOTE: Whenever a test component enters its error state, the error verdict is assigned to its local verdict, the test case terminates and the overall test case result will be error.

Figure F.1: Handling of test component references

## F.1.2 Dynamic behaviour of PTCs

PTCs can be of non-alive type or alive-type. Non-alive type PTCs can be in Inactive, Running and Killed states. Their dynamic behaviour is shown in figure F.2.



NOTE 1: (a) Stop can be either a stop, self.stop or a stop from another test component.  
(b) Kill can be either a kill, self.kill, a kill from another test component or a kill from the test system  
 (in error cases).

NOTE 2: (a) Stop can be from another test component only.   
(b) Kill can be from another test component or from the test system (in error cases) only.

NOTE 3: Whenever a test component enters its error state, the error verdict is assigned to its local verdict,  
the test case terminates and the overall test case result will be error.

Figure F.2: Dynamic behaviour of non-alive type PTCs

Alive-type PTCs can be in Inactive, Running, Stopped and Killed states. Their dynamic behaviour is shown in figure F.3.



NOTE 1: (a) Stop can be either a stop, self.stop or a stop from another test component.  
(b) Kill can be either a kill, self.kill, a kill from another test component or a kill from the test system  
 (in error cases).

NOTE 2: (a) Stop can be from another test component only.  
(b) Kill can be from another test component or from the test system (in error cases) only.

NOTE 3: Whenever a test component enters its error state, the error verdict is assigned to its local verdict,  
the test case terminates and the overall test case result will be error.

Figure F.3: Dynamic behaviour of alive-type PTCs

## F.1.3 Dynamic behaviour of the MTC

The MTC can be in Running or Killed state. The dynamic behaviour of the MTC is shown in figure F.4.



NOTE 1: (a) Stop can be either a stop, self.stop, a stop from another test component.  
(b) Kill can be either a kill, self.kill, a kill from another test component or a kill from the test system  
 (in error cases).

NOTE 2: All remaining PTCs are to be killed as well and the testcase terminates.

NOTE 3: Whenever the MTC enters its error state, the error verdict is assigned to its local verdict,  
the test case terminates and the overall test case result will be error.

Figure F.4: Dynamic behaviour of the MTC

# F.2 Timers

Timers can be in Inactive, Running or Expired state. The dynamic behaviour of a timer is shown in figure F.5.



NOTE 1: For any scope unit, all timers in that scope being in Running state constitute the running-timer list.

NOTE 2: For any scope unit, all timers in that scope being in Expired state constitute the timeout-list.

NOTE 3: Whenever a timer enters its error state, the test component it belongs to enters also its error state,  
assigns a local error verdict, the test case terminates and the overall test case result will be error.

Figure F.5: Dynamic behaviour of timers

# F.3 Ports

Ports can be in Started or Stopped state. As their behaviour is rather complex, the state machine has been split into a state machine giving the dynamic behaviour of configuration operations (i.e. connect, disconnect, map and unmap), of port controlling operations (i.e. start, stop and clear) and of communication operations (i.e. send, receive, call, getcall, raise, catch, reply, getreply and check). As trigger is a shorthand for an alt together with receive it is not considered here.

## F.3.1 Configuration Operations

The port configuration operations (i.e. connect, disconnect, map and unmap) are indifferent to the state of the port. They show the behaviour shown in figure F.6.



NOTE 1: When creating a PTC the ports of that PTC are created and started; when creating the MTC the ports of the MTC and the ports of the TSI are created and started.

NOTE 2: Whenever a port enters its error state, the test component it belongs to enters also its error state, assigns a local error verdict, the test case terminates and the overall test case result will be error.

Figure F.6: Dynamic behaviour of ports: port configuration operations

The transitions do not change the main state of the port, i.e. the port remains in the Started or Stopped state.

## F.3.2 Port Controlling Operations

The results of port controlling operations are shown in figure F.7.



NOTE: When creating a PTC the ports of that PTC are created and started; when creating the MTC the ports of the MTC and the ports of the TSI are created and started.

Figure F.7: Dynamic behaviour of ports: port controlling operations

## F.3.3 Communication Operations

The results of the communication operations send, receive, call, getcall, raise, catch, reply, getreply, check are shown in figure F.8.



NOTE 1: When creating a PTC the ports of that PTC are created and started; when creating a MTC the ports of the MTC and the ports of the TSI are created and started.

NOTE 2: A unique receiver exists if there is only one link for this port or if the to address expression references a test component whose port is linked to this port (a terminated test component is not a legal receiver).

NOTE 3: Whenever a port enters its error state, the test component it belongs to enters also its error state, assigns a local error verdict, the test case terminates and the overall test case result will be error.

NOTE 4: As trigger is a shorthand for an alt together with receive it is not considered here.

Figure F.8: Dynamic behaviour of ports: communication operations

Annex G (informative):  
Deprecated language features

# G.1 Group style definition of module parameters

Previous versions of the present document (up to and including V2.2.1) required to use a group-like syntax shown in the example below to declare module parameters. The module parameter syntax has been unified with constant and variable declaration syntax in this version but group-like syntax is not fully removed to leave a time period for tool providers and users to change from the old syntax to the new one. The group-like syntax of module parameter declarations may be fully removed in a future edition of the standard.

EXAMPLE (superfluous syntax):

**module** MyModuleWithParameters

{

**modulepar** { **integer** TS\_Par0, TS\_Par1 := 0;

**boolean** TS\_Par2 := true

"};

**modulepar** { **hexstring** TS\_Par3 };

}

# G.2 Recursive import

Previous versions of the present document (up to and including V2.2.1) allowed to import named definitions implicitly, via importing other definitions of the same module using them in a **recursive** mode. This feature is deprecated and may be fully removed in a future edition of the present document.

# G.3 Using **all** in port type definitions

Previous versions of the present document (up to and including V2.2.1) allowed to use the **all** keyword in port type definitions instead of an explicit list of types and signatures allowed via the given port. This feature is deprecated and may be fully removed in a future edition of the present document.

# G.4 sizeof for length of lists

Previous versions of the present document (up to and including V3.2.2) allowed to use the built-in function **sizeof** to compute the length of **record of**, **set of**, and **array**. This has been replaced by **lengthof**. The use of **sizeof** for list like types is deprecated and is planned to be fully removed in the next published version.

# G.5 sizeoftype predefined function

The previous version of the present document (up to and including V3.3.1) defined the **sizeoftype** predefined function. This feature is deprecated in this version of the standard and may be fully removed in the next published version.

# G.6 Mixed ports

Previous versions of the present document (up to and including V3.2.2) allowed to use **mixed** ports. This feature is deprecated and may be fully removed in a future edition of the present document.

# G.7 External constants

Previous versions of the present document (up to and including V3.4.1) allowed to use **external** **const**ants. This feature is deprecated and may be fully removed in a future edition of the present document.

# G.8 Prefixing enumerated values

Previous versions of the present document (up to and including V4.2.1) did not explicitly specify how to resolve name conflicts between imported enumerated values and global names defined in the importing or in another TTCN-3 module. Some tool implementations resolved this issue by allowing prefixing enumerated values with the name of the module in which the given enumerated type is defined. Version 4.3.1 added in clause 8.2.3.1 a rule to resolve such name clashes, therefore prefixing enumerated values is deprecated.

# G.9 Record of/arrays not compatible to record; set of not compatible with set

Previous versions of the present document (up to and including V4.3.1) did define special cases when record of types and single-dimension arrays would be compatible with record types. These rules are deprecated.

# G.10 The "UCS-2" predefined variant attribute string

Previous versions of the present document (up to and including V4.6.1) declared the "UCS-2 variant attribute string to support the UCS-2 coded representation form of ISO/IEC 10646:2003 (see clause 14.1 9.2 of ISO/IEC 10646 (2003) [i.14]). The use of this string is deprecated, as it is replaced by the predefined variant attribute string "UTF-16".

Similarly, the "UCS-2" and "UCS-4" values of string\_encoding and serialization parameters, defined in earlier versions of the present document for the **oct2unichar**, **unichar2oct**, **encvalue\_unichar** and **decvalue\_unichar** predefined functions are deprecated.

# G.11 Prefixing identifiers of local definitions with module identifiers

Previous versions of the present document (up to and including V4.6.1) did not exclude the possibility to prefix identifier of definitions without global visibility (e.g. templates defined in functions or test cases) with the local module identifier. Prefixing identifiers of local definitions with module identifiers is deprecated and may be fully removed in a future edition of the present document.

Annex H (informative):  
Bibliography

* ETSI ES 201 873-1 (V1.1.2): "Methods for Testing and Specification (MTS); The Tree and Tabular Combined Notation version 3; Part 1: TTCN‑3 Core Language", 2001.
* ETSI ES 201 873-1 (V2.2.1): "Methods for Testing and Specification (MTS); The Testing and Test Control Notation version 3; Part 1: TTCN‑3 Core Language", 2003.
* ETSI ES 201 873-1 (V3.1.1): "Methods for Testing and Specification (MTS); The Testing and Test Control Notation version 3; Part 1: TTCN‑3 Core Language", 2005.
* ETSI ES 201 873-1 (V3.2.1): "Methods for Testing and Specification (MTS); The Testing and Test Control Notation version 3; Part 1: TTCN‑3 Core Language", 2007.
* ETSI ES 201 873-1 (V3.3.2): "Methods for Testing and Specification (MTS); The Testing and Test Control Notation version 3; Part 1: TTCN‑3 Core Language", 2008.
* ETSI ES 201 873-1 (V3.4.1): "Methods for Testing and Specification (MTS); The Testing and Test Control Notation version 3; Part 1: TTCN‑3 Core Language", 2008.
* ETSI ES 201 873-1 (V4.1.1): "Methods for Testing and Specification (MTS); The Testing and Test Control Notation version 3; Part 1: TTCN‑3 Core Language", 2009.
* ETSI ES 201 873-1 (V4.2.1): "Methods for Testing and Specification (MTS); The Testing and Test Control Notation version 3; Part 1: TTCN‑3 Core Language", 2010.
* ETSI ES 201 873-1 (V4.3.1): "Methods for Testing and Specification (MTS); The Testing and Test Control Notation version 3; Part 1: TTCN‑3 Core Language", 2011.
* ETSI ES 201 873-1 (V4.4.1): "Methods for Testing and Specification (MTS); The Testing and Test Control Notation version 3; Part 1: TTCN‑3 Core Language", 2012.
* ETSI ES 201 873-1 (V4.5.1): "Methods for Testing and Specification (MTS); The Testing and Test Control Notation version 3; Part 1: TTCN‑3 Core Language", 2013.
* ETSI ES 201 873-1 (V4.6.1): "Methods for Testing and Specification (MTS); The Testing and Test Control Notation version 3; Part 1: TTCN‑3 Core Language", 2014.

# History

|  |  |  |
| --- | --- | --- |
| **Document history** | | |
| V1.1.1 | March 2001 | Publication |
| V1.1.2 | June 2001 | Publication |
| V2.2.1 | February 2003 | Publication |
| V3.1.1 | June 2005 | Publication |
| V3.2.1 | February 2007 | Publication |
| V3.3.2 | April 2008 | Publication |
| V3.4.1 | September 2008 | Publication |
| V4.1.1 | June 2009 | Publication |
| V4.2.1 | July 2010 | Publication |
| V4.3.1 | June 2011 | Publication |
| V4.4.1 | April 2012 | Publication |
| V4.5.1 | April 2013 | Publication |
|  |  |  |
| V4.6.1 | June 2014 | Publication |
| V4.6.2 | July 2014 | Interim draft version for TB MTS and 3GPP use.  CRs included (8):[0006698](http://forge.etsi.org/mantis/view.php?id=6698" \o "[closed] Missing functionality to cast \"template\" to \"template (present)\"), [0006706](http://forge.etsi.org/mantis/view.php?id=6706" \o "[closed] Encoding in oct2unichar, unichar2oct, encvalue_unichar, decvalue_unichar), [0006697](http://forge.etsi.org/mantis/view.php?id=6697" \o "[closed] Missing functionality to check absence of an object), [0006699](http://forge.etsi.org/mantis/view.php?id=6699" \o "[closed] Missing/invalid expansion rules for templates with template restrictions in 15.6.2), [0006690](http://forge.etsi.org/mantis/view.php?id=6690" \o "[closed] Case insensitive pattern matching), [0006700](http://forge.etsi.org/mantis/view.php?id=6700" \o "[closed] Clarification for clause 15.6.3), [0006714](http://forge.etsi.org/mantis/view.php?id=6714" \o "[closed] Expansion of LHS in case of uninitialized constructive variables), [0006715](http://forge.etsi.org/mantis/view.php?id=6715" \o "[resolved] Referencing alternatives of union templates) |
| V4.6.3 | January 2015 | Final draft for TB approval.  CRs included (71 in addition to V4.6.2): [0006792](http://forge.etsi.org/mantis/view.php?id=6792" \o "[resolved] Add hyperlinks to predefined function clauses), [0006692](http://forge.etsi.org/mantis/view.php?id=6692" \o "[closed] More detailed restriction on parameters of modified templates), [0006694](http://forge.etsi.org/mantis/view.php?id=6694" \o "[closed] clarify that only module definitions can be prefixed by module identifier), [0006693](http://forge.etsi.org/mantis/view.php?id=6693" \o "[closed] Missing rules for omitted values in complement templates), [0006677](http://forge.etsi.org/mantis/view.php?id=6677" \o "[closed] Additional rule on name class in import), [0006691](http://forge.etsi.org/mantis/view.php?id=6691" \o "[closed] Port visibility in compile time in connection operations), [0006695](http://forge.etsi.org/mantis/view.php?id=6695" \o "[closed] restriction on arithmetic operators should be put in a restriction section or should be dropped altogether), [0006753](http://forge.etsi.org/mantis/view.php?id=6753" \o "[closed] Partially initialized values in \"any from\" calls), [0006564](http://forge.etsi.org/mantis/view.php?id=6564" \o "[closed] Concatenation example using undefined rules), [0006663](http://forge.etsi.org/mantis/view.php?id=6663" \o "[closed] regexp's behaviour if both string parameters are literals), [0006802](http://forge.etsi.org/mantis/view.php?id=6802" \o "[closed] isvalue Definition is inconsistent/confusing), [0006678](http://forge.etsi.org/mantis/view.php?id=6678" \o "[closed] Reference to omitted field in the right hand side of an assignment), [0006785](http://forge.etsi.org/mantis/view.php?id=6785" \o "[closed] Change name and add description of string_encoding parameter), [0006841](http://forge.etsi.org/mantis/view.php?id=6841" \o "[closed] Contradictory wording in all from restrictions), [0006624](http://forge.etsi.org/mantis/view.php?id=6624" \o "[closed] Allow access to random seed per component.), [0006789](http://forge.etsi.org/mantis/view.php?id=6789" \o "[closed] Allow non-ISO646 (UTF-8 compatible) characters in universal charstrings), [0006727](http://forge.etsi.org/mantis/view.php?id=6727" \o "[closed] Alternative reference of unicode characters), [0006754](http://forge.etsi.org/mantis/view.php?id=6754" \o "[closed] Predefined function to identify unicode string encoding automatically), [0006775](http://forge.etsi.org/mantis/view.php?id=6775" \o "[closed] getverdict from other component), [0006702](http://forge.etsi.org/mantis/view.php?id=6702" \o "[closed] Assignment of partially initialized values of structured types), [0006709](http://forge.etsi.org/mantis/view.php?id=6709" \o "[closed] 22.3: What should happen when addresses are used on connected  ports?), [0006679](http://forge.etsi.org/mantis/view.php?id=6679" \o "[closed] More generic restriction on import from newer TTCN-3 versions), [0006708](http://forge.etsi.org/mantis/view.php?id=6708" \o "[closed] Section 23.6: the timer queue handling for timeout checking of 'any' timer), [0006782](http://forge.etsi.org/mantis/view.php?id=6782" \o "[closed] Complement matching should be allowed for template(present)-s), [0006681](http://forge.etsi.org/mantis/view.php?id=6681" \o "[closed] Restriction on types that can be used in port type definition), [0006682](http://forge.etsi.org/mantis/view.php?id=6682" \o "[closed] Strong typing compatibility rules for connect and map), [0006716](http://forge.etsi.org/mantis/view.php?id=6716" \o "[closed] ISO/IEC 10646 version), [0006684](http://forge.etsi.org/mantis/view.php?id=6684" \o "[closed] Wrong rule for forbidden mapping), [0006718](http://forge.etsi.org/mantis/view.php?id=6718" \o "[closed] Null value in the to and from clause), [0006239](http://forge.etsi.org/mantis/view.php?id=6239" \o "[closed] Restriction on verdict operation), [0006710](http://forge.etsi.org/mantis/view.php?id=6710" \o "[closed] Activate using timers declared in control block), [0006670](http://forge.etsi.org/mantis/view.php?id=6670" \o "[closed] Restrictions on the decvalue function), [0006647](http://forge.etsi.org/mantis/view.php?id=6647" \o "[closed] Additional restrictions for component.start), [0006717](http://forge.etsi.org/mantis/view.php?id=6717" \o "[closed] Values of address type in expressions and references), [0006781](http://forge.etsi.org/mantis/view.php?id=6781" \o "[closed] Type compatibility of the from and sender clause), [0006761](http://forge.etsi.org/mantis/view.php?id=6761" \o "[closed] extended type - syntactical Structure), [0006729](http://forge.etsi.org/mantis/view.php?id=6729" \o "[closed] Rules for concatenation of charstring templates), [0006704](http://forge.etsi.org/mantis/view.php?id=6704" \o "[closed] Number of matches of subset items), [0006722](http://forge.etsi.org/mantis/view.php?id=6722" \o "[closed] Visibility is not taken into account in component compatibility), [0006756](http://forge.etsi.org/mantis/view.php?id=6756" \o "[closed] External Function constraint exceptions should be revised), [0006783](http://forge.etsi.org/mantis/view.php?id=6783" \o "[closed] Wrong syntax to save exception parameters), [0006762](http://forge.etsi.org/mantis/view.php?id=6762" \o "[closed] Array indexing breaches strong typing principle), [0006778](http://forge.etsi.org/mantis/view.php?id=6778" \o "[closed] Add language string TTCN-3:2015 for the new edition), [0006646](http://forge.etsi.org/mantis/view.php?id=6646" \o "[closed] Missing semantic rules for the index and assignment notation), [0006728](http://forge.etsi.org/mantis/view.php?id=6728" \o "[closed] Rules for direct references inside patterns), [0006731](http://forge.etsi.org/mantis/view.php?id=6731" \o "[closed] Passing parameters by reference), [0006711](http://forge.etsi.org/mantis/view.php?id=6711" \o "[closed] Section 15.9: the phrasing of restriction a) must be made more precise), [0006811](http://forge.etsi.org/mantis/view.php?id=6811" \o "[closed] Missing BNF support for lower bound exclustion in length restriction), [0006814](http://forge.etsi.org/mantis/view.php?id=6814" \o "[closed] Delete TemplateList from BNF), [0006429](http://forge.etsi.org/mantis/view.php?id=6429" \o "[closed] modifies of 'record of' fields still seems to be ambiguous), [0006736](http://forge.etsi.org/mantis/view.php?id=6736" \o "[closed] new matching mechanism for binary string types), [0006645](http://forge.etsi.org/mantis/view.php?id=6645" \o "[closed] Rules for array values), [0006855](http://forge.etsi.org/mantis/view.php?id=6855" \o "[closed] Outdated note on mixed ports), [0006755](http://forge.etsi.org/mantis/view.php?id=6755" \o "[closed] Predefined function to remove BOMs from universal charstring), [0006707](http://forge.etsi.org/mantis/view.php?id=6707" \o "[closed] Section 7.1.2: Clarification of compatible types with the List operator), [0006411](http://forge.etsi.org/mantis/view.php?id=6411" \o "[closed] Example to clarify Modified Template semantics), [0006791](http://forge.etsi.org/mantis/view.php?id=6791" \o "[closed] Presence checking functions have in parameters only), [0006790](http://forge.etsi.org/mantis/view.php?id=6790" \o "[closed] Wrong predefined function references), [0006786](http://forge.etsi.org/mantis/view.php?id=6786" \o "[closed] Add the hostid predefined function to clause 16.1.2), [0006713](http://forge.etsi.org/mantis/view.php?id=6713" \o "[closed] Remove TFT from the standard), [0006703](http://forge.etsi.org/mantis/view.php?id=6703" \o "[closed] Inconsisten assignment restriction), [0006779](http://forge.etsi.org/mantis/view.php?id=6779" \o "[closed] Correct figures 6 and 7 to show borders of test system), [0006723](http://forge.etsi.org/mantis/view.php?id=6723" \o "[closed] R of regexp shall be lowercase), [0006780](http://forge.etsi.org/mantis/view.php?id=6780" \o "[closed] Sender clause should implicitly define the content of the missing from clause), [0006784](http://forge.etsi.org/mantis/view.php?id=6784" \o "[closed] Replace \"yooleany essor\" with \"preprocessor\"), [0006705](http://forge.etsi.org/mantis/view.php?id=6705" \o "[closed] Invalid restriction on subset length), [0006724](http://forge.etsi.org/mantis/view.php?id=6724" \o "[closed] Strange name of hostId), [0006725](http://forge.etsi.org/mantis/view.php?id=6725" \o "[closed] Strange character sequence for \"preprocessor\"), [0006726](http://forge.etsi.org/mantis/view.php?id=6726" \o "[closed] yoolean should be boolean), [0006676](http://forge.etsi.org/mantis/view.php?id=6676" \o "[closed] Incorrect record definition in import example), [0006680](http://forge.etsi.org/mantis/view.php?id=6680" \o "[closed] Typo in rules on importing from fother TTCN-3 editions and non-TTCN-3 modules) |
| V4.6.4 | January 2015 | Final draft for TB approval.  Correcting version and date on title page.CRs included (2 in addition to V4.6.3): [0005976](http://forge.etsi.org/mantis/view.php?id=5976" \o "[closed] Add hyperlinks to predefined function clauses), [0006792](http://forge.etsi.org/mantis/view.php?id=6792" \o "[closed] Add hyperlinks to predefined function clauses) |