## ANNEX M (informative): Change Request form

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **CHANGE REQUEST** | | | | | | | | | | | | | | | |
|  | ETSI EN 302 637-2 | | | **Version** | 1.4.1 | **CR** | | 1 | | **rev** | | | | - |  |
|  | | | | | | | | | | | | | | | |
| **CR Title** | | Description of LanePosition in the CAM standard | | | | | | | | | | | | | |
|  | |  | | | | | | | | | | | | | |
| **Original Source** | | ITS WG1 | | | | | | | | | | | | | |
|  | |  | | | | | | | | | | | | | |
| **Work Item Ref** | | REN/ITS-0010089 | | | | | **Submission date** | | | | | 22/03/2019 | | | |
| **Approving TB** | | ITS | | | | | **Approval date** | | | | | 08/04/2019 | | | |
| **Category:** | | **F** | **Release** | | | | | | | |  | | |  | |
|  | | Use **one** of the following categories: **F** (correction) **A** (correction in an earlier release) **B** (addition of feature)  **C** (functional modification of feature) **D** (editorial modification) | | | | | | | | | | |  | | |
|  | |  | | | | | | | | | | | | | |
| **Reason for change** | | | The description of LanePosition is not in line with the description of LanePosition in CDD. The CAM standard defines counting lanes from outside to inside and the CDD defines counting from inside to outside. It is unclear which definition of LanePosition prevails. | | | | | | | | | | | | |
|  | | |  | | | | | | | | | | | | |
| **Consequence if not approved** | | | It is unclear how to interpret the information provided on the lane the vehicle is in. This could lead to wrong interpretations and wrong advice to drivers. | | | | | | | | | | | | |
|  | | |  | | | | | | | | | | | | |
| **Summary of change** | | | The CAM standard should not re-define what is already defined elsewhere. Hence delete the last part of the first sentence in B.24  The DE lanePosition of the *referencePosition* of a vehicle, ~~counted from the~~  ~~outside border of the road, in the direction of the traffic flow.~~ | | | | | | | | | | | | |
|  | | |  | | | | | | | | | | | | |
| **Clauses affected** | | | B.24 | | | | | | | | | | | | |
|  | | |  | | | | | | | | | | | | |
| **Linked Change Requests** | | | See CR on for correction of ASN.1 definition of LanePosition in the CDD. | | | | | |  | | | | | | |
|  | | |  | | | | | |  | | | | | | |
|  | | |  | | | | | | | | | | | | |
| **Other comments** | | | See same CR for the DENM standard. | | | | | | | | | | | | |
|  | | |  | | | | | | | | | | | | |

# B.24 lanePosition

|  |  |
| --- | --- |
| Description | The DE lanePosition of the *referencePosition* of a vehicle.  This DE shall be present if the data is available at the originating ITS-S (see note). |
| Data setting and presentation requirements | The DE shall be presented as specified in ETSI TS 102 894-2 [2] *LanePosition.* |
| NOTE: Additional information is needed to unambiguously identify the lane position and to allow the correlation to a map. | |