|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **CHANGE REQUEST** | | | | | | | | | | | | | | |
|  | ETSI EN 302 637-2 | | | **Version** | 1.4.1 | **CR** | | 2 | **rev** | | | | - |  |
|  | | | | | | | | | | | | | | |
| **CR Title** | | Description of closedLanes in the CAM standard (B.43) | | | | | | | | | | | | |
|  | |  | | | | | | | | | | | | |
| **Original Source** | | ITS WG1 | | | | | | | | | | | | |
|  | |  | | | | | | | | | | | | |
| **Work Item Ref** | | REN/ITS-0010089 | | | | | **Submission date** | | | | 20/11/2019 | | | |
| **Approving TB** | | TC ITS | | | | | **Approval date** | | | | 17/01/2020 | | | |
| **Category:** | | **F** | **Release** | | | | | | | 1 | | |  | |
|  | | Use **one** of the following categories: **F** (correction) **A** (correction in an earlier release) **B** (addition of feature)  **C** (functional modification of feature) **D** (editorial modification) | | | | | | | | | |  | | |
|  | |  | | | | | | | | | | | | |
| **Reason for change** | | | The description of closedLines is not in line with the description of ClosedLines (A.106 and A.23) in CDD. | | | | | | | | | | | |
|  | | |  | | | | | | | | | | | |
| **Consequence if not approved** | | | It is unclear how to interpret the information provided on the closed lanes. This could lead to wrong interpretations and wrong advice to drivers. | | | | | | | | | | | |
|  | | |  | | | | | | | | | | | |
| **Summary of change** | | | The CAM standard should not re-define what is already defined elsewhere. Hence delete the part of the B.43 as it is already defined in CDD in A.106 and A.23 | | | | | | | | | | | |
|  | | |  | | | | | | | | | | | |
| **Clauses affected** | | | B.43 | | | | | | | | | | | |
|  | | |  | | | | | | | | | | | |
| **Linked Change Requests** | | | CR 102 894-2 - #0001 Correction of ASN.1 definition for Data Element [LanePosition ]. | | | | | | | | | | | |
|  | | | CR 302 637-2 - #0001 Description of LanePosition in the CAM standard. | | | | | | | | | | | |
|  | | |  | | | | | | | | | | | |
| **Other comments** | | | See similar CR for the LanePosition DE. | | | | | | | | | | | |
|  | | |  | | | | | | | | | | | |

* **section B.43**: *delete the part of the B.43 as it is already defined in CDD in A.106 and A.23*

It provides information about the opening/closure status of the lanes ahead. ~~Lanes are counted from the outside boarder of the road. If a lane is closed to traffic, the corresponding bit shall be set to 1.~~