|  |
| --- |
| **CHANGE REQUEST** |
|  | ETSI EN 302 637-2 | **Version** | 1.4.1 | **CR** | 2 | **rev** | - |  |
|  |
| **CR Title** | Description of closedLanes in the CAM standard (B.43) |
|  |  |
| **Original Source** | ITS WG1 |
|  |  |
| **Work Item Ref** | REN/ITS-0010089 | **Submission date** | 20/11/2019 |
| **Approving TB**  | TC ITS | **Approval date** | 17/01/2020 |
| **Category:** | **F** | **Release** | 1 |  |
|  | Use **one** of the following categories:**F** (correction)**A** (correction in an earlier release)**B** (addition of feature) **C** (functional modification of feature)**D** (editorial modification) |  |
|  |  |
| **Reason for change** | The description of closedLines is not in line with the description of ClosedLines (A.106 and A.23) in CDD. |
|  |  |
| **Consequence if not approved** | It is unclear how to interpret the information provided on the closed lanes. This could lead to wrong interpretations and wrong advice to drivers. |
|  |  |
| **Summary of change** | The CAM standard should not re-define what is already defined elsewhere. Hence delete the part of the B.43 as it is already defined in CDD in A.106 and A.23 |
|  |  |
| **Clauses affected** | B.43 |
|  |  |
| **Linked Change Requests** | CR 102 894-2 - #0001 Correction of ASN.1 definition for Data Element [LanePosition ]. |
|  | CR 302 637-2 - #0001 Description of LanePosition in the CAM standard. |
|  |  |
| **Other comments** | See similar CR for the LanePosition DE. |
|  |  |

* **section B.43**: *delete the part of the B.43 as it is already defined in CDD in A.106 and A.23*

It provides information about the opening/closure status of the lanes ahead. ~~Lanes are counted from the outside boarder of the road. If a lane is closed to traffic, the corresponding bit shall be set to 1.~~