|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **CHANGE REQUEST** | | | | | | | | | | | | | | | |
|  | ETSI TS 103 097 | | | **Version** | 1.3.1 | **CR** | | *10* | | **rev** | | | | - |  |
|  | | | | | | | | | | | | | | | |
| **CR Title** | | Allow the use of pduFunctionalType | | | | | | | | | | | | | |
|  | |  | | | | | | | | | | | | | |
| **Original Source** | | ITS WG5 | | | | | | | | | | | | | |
|  | |  | | | | | | | | | | | | | |
| **Work Item Ref** | | RTS/ITS-00557 | | | | | **Submission date** | | | | | 16.06.2020 | | | |
| **Approving TB** | | ITS | | | | | **Approval date** | | | | | 01.07.2020 | | | |
| **Category:** | | **B** | **Release** | | | | | | | | 1 | | |  | |
|  | | Use **one** of the following categories: **F** (correction) **A** (correction in an earlier release) **B** (addition of feature)  **C** (functional modification of feature) **D** (editorial modification) | | | | | | | | | | |  | | |
|  | |  | | | | | | | | | | | | | |
| **Reason for change** | | | The headerInfo field pduFunctionalType could be helpful in future to allow for Secure session functionality | | | | | | | | | | | | |
|  | | |  | | | | | | | | | | | | |
| **Consequence if not approved** | | | Secure session functionality provided by IEEE 1609.2b cannot be used by applications | | | | | | | | | | | | |
|  | | |  | | | | | | | | | | | | |
| **Summary of change** | | | Leave pduFunctionalType optional (instead of Absent as in CR9) so that future profiles can make use of it. | | | | | | | | | | | | |
|  | | |  | | | | | | | | | | | | |
| **Clauses affected** | | | 5.2 | | | | | | | | | | | | |
|  | | |  | | | | | | | | | | | | |
| **Linked Change Requests** | | | CR9 | | | | | |  | | | | | | |
|  | | |  | | | | | |  | | | | | | |
|  | | |  | | | | | | | | | | | | |
| **Other comments** | | |  | | | | | | | | | | | | |
|  | | |  | | | | | | | | | | | | |

# 5.2 SignedData

***Change the bullet point of*** pduFunctionalType***:***

The component pduFunctionalType, as defined in IEEE Std 1609.2 [1], present or absent according to the specification of message profiles in clause 7.