**Channel assignment in WAV file**

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | **Channel number** | | | | | | | | | |
| **Case** | **1** | **2** | **3** | **4** | **5** | **6** | **7** | **8** | **9** | **10** |
| **Stereo** | Left | Right | n/a | n/a | n/a | n/a | n/a | n/a | n/a | n/a |
| **5.1** | Left | Right | Center | Low Frequency Effects | Left Surround | Right Surround | n/a | n/a | n/a | n/a |
| **5.1.2** | Left | Right | Center | Low Frequency Effects | Left Surround | Right Surround | Top Side Left | Top Side Right | n/a | n/a |
| **7.1** | Left | Right | Center | Low Frequency Effects | Left Surround | Right Surround | Left Surround  Direct | Right Surround  Direct | n/a | n/a |
| **7.1.2** | Left | Right | Center | Low Frequency Effects | Left Surround | Right Surround | Left Surround  Direct | Right Surround  Direct | Top Side Left | Top Side Right |

IEC 62574:2020 Audio, video and multimedia systems - General channel assignment of multichannel audio

ISO/IEC 2309103:2018 Information technology — Coding-independent code points — Part 3: Audio